# SANE: Backends (Drivers)

The following table summarizes the backends/drivers distributed with sane-backends-1.0.16, and the hardware or software they support.

This is only a summary! Please consult the manpages and the author-supplied webpages for more detailed (and usually important) information concerning each backend.

If you have new information or corrections, please file a bug report with as many details as possible. Also please tell us if your scanner isn't mentioned in this list at all.

For an explanation of the tables, see the legend.

There are tables for scanners, still cameras, video cameras, APIs, and meta backends.

## Scanners

Backends: abaton, agfafocus, apple, artec, artec_eplus48u, as6e, avision, bh, canon, canon630u, canon_pp, coolscan, coolscan2, epson, fujitsu, genesys, gt68xx, hp, hp5400, hpsj5s, ibm, leo, ma1509, matsushita, microtek, microtek2, mustek, mustek_pp, mustek_usb, nec, niash, pie, plustek, plustek_pp, ricoh, s9036, sceptre, sharp, sm3600, sm3840, SnapScan, sp15c, st400, tamarack, teco1, teco2, teco3, template, u12, umax, umax1220u, umax_pp, unsupported

### Backend: abaton (unmaintained)

Manual page: sane-abaton

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Abaton | Scan 300/GS | SCSI | complete | All known modes and functions supported
Scan 300/S | SCSI | untested | Untested, use with caution

### Backend: agfafocus (unmaintained)

Manual page: sane-agfafocus

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
AGFA | Focus GS Scanner | SCSI | untested | 6 bit gray
Focus Lineart Scanner | SCSI | untested | Lineart only? Untested.
Focus II | SCSI | untested | gray only
Focus Color | SCSI | good | 3-pass
Focus Color Plus | SCSI | good | 3-pass
Siemens | S9036 | SCSI | untested | gray only

### Backend: apple (unmaintained)

Manual page: sane-apple

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Apple | Apple Scanner | SCSI | good | 4bit, 16 shades of gray
OneScanner | SCSI | basic | 8bit, 256 shades of gray. The backend needs work especially in the quantization code but it may work.
ColorOneScanner | SCSI | minimal | truecolor (needs much work) but it scans in non color modes.

### Backend: artec (unmaintained)

Link(s): http://www4.infi.net/~cpinkham/sane/sane-artec-doc.html
Manual page: sane-artec

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Artec/Ultima | AT3 | SCSI | complete | all modes working
A6000C | SCSI | complete | all modes working
A6000C PLUS | SCSI | complete | f/w <= v1.92 basic, f/w >= v1.93 OK
AT6 | SCSI | minimal | First scan works, subsequent fail until scanner power cycle.
AT12 | SCSI | complete | all modes working
AM12S | SCSI | complete | all modes working
BlackWidow | BW4800SP | SCSI | complete | rebadged Artec AT3
Plustek | OpticPro 19200S | SCSI | complete | rebadged Artec AM12S

### Backend: artec_eplus48u (0.0.10)

Link(s): http://www.angelfire.com/linux/crapsite/
Manual page: sane-artec_eplus48u

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Artec/Ultima | E+ 48U | USB | good | CIS scanner based on the GT6816 chip. Apparently all other devices are re-badged Artec scanners.
Medion/Lifetec/Tevion/Cytron | MD9693 | USB | good |
MD9705 | USB | good |
MD4394 | USB | good | Only scanners with product id 0x4003 will work; try the gt68xx backend, if your scanner has product id 0x4002
Trust | Easy Webscan 19200 | USB | good | Different product id: 0x4006
Memorex | MEM 48U | USB | good | Different product id: 0x4005
Microstar | MR 9791 | USB | good |
UMAX | AstraSlim SE | USB | good | Different product id: 0x4009
Artec/Ultima | E+ Pro | USB | minimal | Experimental! Different product id: 0x4004. Please report your results!

### Backend: as6e (0.4.2)

Link(s): http://as6edriver.sourceforge.net/
Manual page: sane-as6e

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Artec/Ultima | AS6E | Parport | basic | Requires the program 'as6edriver' to run.

### Backend: avision (Build: 167)

Link(s): http://www.exactcode.de/oss/avision/index.html
Manual page: sane-avision

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Avision | AV100CS | SCSI | untested |
AV100IIICS | SCSI | untested |
AV100S | SCSI | untested |
AV120 | USB | basic | sheetfed scanner
AV210 | USB | basic | sheetfed scanner
AV210-2 | USB | basic | sheetfed scanner
AV220 | USB | complete | duplex! sheetfed scanner
AV220-C2 | USB | untested | duplex! sheetfed scanner
AV240SC | SCSI | untested |
AV260CS | SCSI | untested |
AV360CS | SCSI | untested |
AV363CS | SCSI | untested |
AV420CS | SCSI | untested |
AV6120 | SCSI | untested |
AV610 | USB | good |
AVA6 | USB | untested | probably a CPU-less device
DS610CU Scancopier | USB | good | 1 pass, 600 dpi, A4
AV620CS | SCSI | complete | 1 pass, 600 dpi
AV620CS Plus | SCSI | complete | 1 pass, 1200 dpi
AV630CS | SCSI | complete | 1 pass, 1200 dpi - regularly tested
AV630CSL | SCSI | untested | 1 pass, 1200 dpi
AV6240 | SCSI | complete | 1 pass, ??? dpi
AV600U | USB | good | 1 pass, 600 dpi
AV600U Plus | USB | untested | 1 pass, ??? dpi
AV660S | SCSI | untested | 1 pass, ??? dpi
AV680S | SCSI | untested | 1 pass, ??? dpi
AV690U | SCSI | untested | 1 pass, 2400 dpi
AV800S | SCSI | untested | 1 pass, ??? dpi
AV810C | SCSI | untested | 1 pass, ??? dpi
AV820 | SCSI | untested | 1 pass, ??? dpi
AV820C | SCSI | good | 1 pass, ??? dpi
AV820C Plus | SCSI | untested | 1 pass, ??? dpi
AV830C | SCSI | untested | 1 pass, ??? dpi
AV830C Plus | SCSI | untested | 1 pass, ??? dpi
AV880 | SCSI | untested | 1 pass, ??? dpi
AV880C | SCSI | untested | 1 pass, ??? dpi
AV3200C | SCSI | complete | 1 pass, ??? dpi
AV3800C | SCSI | good | 1 pass, ??? dpi
AV8000S | SCSI | complete | 1 pass, 1200 dpi, A3 - regularly tested
AV8300 | USB | complete | 1 pass, 1200 dpi, A3 - duplex!
AV8350 | USB | complete | 1 pass, 1200 dpi, A3 - duplex!
AVA3 | SCSI | basic | 1 pass, 600 dpi, A3
Hewlett-Packard | ScanJet 5300C | USB | complete | 1 pass, 2400 dpi - regularly tested - some FW revisions have x-axis image scaling problems over 1200 dpi
ScanJet 5370C | USB | basic | 1 pass, 2400 dpi - some FW revisions have x-axis image scaling problems over 1200 dpi
ScanJet 7400c | USB | good | 1 pass, 2400 dpi - dual USB/SCSI interface
ScanJet 7450c | USB | good | 1 pass, 2400 dpi - dual USB/SCSI interface - regularly tested
ScanJet 7490c | USB | good | 1 pass, 1200 dpi - dual USB/SCSI interface
ScanJet 8200 | USB | good | 1 pass, 4800 (?) dpi - USB 2.0
ScanJet 8250 | USB | good | 1 pass, 4800 (?) dpi - USB 2.0
ScanJet 8290 | USB | good | 1 pass, 4800 (?) dpi - USB 2.0 and SCSI - only SCSI tested so far
Minolta | Dimage Scan Dual I | SCSI | basic |
Dimage Scan Dual II | USB | good | 1 pass, film-scanner
Elite II | USB | untested | 1 pass, film-scanner
Dimage Scan Dual III | USB | basic | 1 pass, film-scanner
Minolta-QMS | SC-110 | USB | untested |
SC-215 | USB | good |
Mitsubishi | MCA-ADFC | SCSI | untested |
S1200C | SCSI | untested |
S600C | SCSI | untested |
SS600 | SCSI | good |
Fujitsu | ScanPartner | SCSI | untested |
ScanPartner 10 | SCSI | untested |
ScanPartner 10C | SCSI | untested |
ScanPartner 15C | SCSI | untested |
ScanPartner 300C | SCSI | untested |
ScanPartner 600C | SCSI | untested |
ScanPartner 620C | SCSI | good |
ScanPartner Jr | SCSI | untested |
ScanStation | SCSI | untested |
Kodak | i30 | SCSI | untested |
i40 | SCSI | untested |
i50 | SCSI | untested |
i60 | SCSI | untested |
i80 | SCSI | untested |
iVina | 1200U | USB | untested |
Xerox | DocuMate252 | USB | untested |
DocuMate262 | USB | untested |

### Backend: bh (1.0-4)

Link(s): http://www.martoneconsulting.com/sane-bh.html
Manual page: sane-bh
Comment: Supports Copiscan II scanners with Remote SCSI Controller (RSC) interface

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Bell and Howell | COPISCAN II 6338 | SCSI | good | Duplex Scanner with ACE - development model
COPISCAN II 2135 | SCSI | untested | Simplex Scanner
COPISCAN II 2137(A) | SCSI | good | Simplex Scanner (with ACE) - limited testing
COPISCAN II 2138A | SCSI | untested | Simplex Scanner with ACE
COPISCAN II 3238 | SCSI | untested | Simplex Scanner
COPISCAN II 3338(A) | SCSI | untested | Simplex Scanner (with ACE)

### Backend: canon (1.12)

Link(s): http://www.rzg.mpg.de/~mpd/sane/
Manual page: sane-canon

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Canon | CanoScan 300 | SCSI | good | 1 pass; flatbed scanner
CanoScan 600 | SCSI | good | 1 pass; flatbed scanner
CanoScan 620S | SCSI | good | 1 pass; flatbed scanner
CanoScan 1200S | SCSI | good | 1 pass; flatbed scanner
CanoScan 2700F | SCSI | good | 1 pass; film scanner
CanoScan 2710S | SCSI | good | 1 pass; 36bit film scanner

### Backend: canon630u (0.1)

Link(s): http://canon-fb630u.sourceforge.net/
Manual page: sane-canon630u

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Canon | CanoScan fb630u | USB | good | OK
CanoScan fb636u | USB | untested | hopefully works

### Backend: canon_pp (0.33)

Link(s): http://canon-fb330p.sourceforge.net
Manual page: sane-canon_pp

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Canon | CanoScan FB310P | Parport (ECP) | unsupported | Rebadged Avision, different command set
CanoScan FB610P | Parport (ECP) | unsupported | Rebadged Avision, different command set
CanoScan FB320P | Parport (ECP) | basic | Newly added support
CanoScan FB620P | Parport (ECP) | basic | Newly added support
CanoScan FB330P | Parport (ECP) | good |
CanoScan FB630P | Parport (ECP) | good |
CanoScan N340P | Parport (ECP) | good |
CanoScan N640P | Parport (ECP) | good |
CanoScan N640P ex | Parport (ECP) | good | Just an N640P in a different box?

### Backend: coolscan (0.4.3)

Link(s): http://andreas.rick.free.fr/sane/
Manual page: sane-coolscan

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Nikon | LS-20 | SCSI | basic | The LS-20 has been replaced by the LS-30
LS-30 | SCSI | basic | alpha: only 24/30 bit RGB + 32/40 bit RGBI
LS-2000 | SCSI | basic | alpha: only 24/36 bit + RGB 32/48 bit RGBI
LS-1000 | SCSI | basic | Doesn't support gamma correction

### Backend: coolscan2 (0.1.8)

Link(s): http://coolscan2.sourceforge.net/
Manual page: sane-coolscan2

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Nikon | LS 30 | SCSI | complete | working -- model available to developer
LS 2000 | SCSI | good |
LS 40 ED | USB | complete |
LS 4000 ED | IEEE-1394 | good | needs linux kernel 2.4.19 or later
LS 8000 ED | IEEE-1394 | good | needs linux kernel 2.4.19 or later

### Backend: epson (0.2.42)

Link(s): http://www.khk.net/sane
Manual page: sane-epson

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Epson | GT-5000 | SCSI Parport | good |
Actionscanner II | SCSI Parport | good | US version of GT-5000
GT-6000 | SCSI Parport | good |
ES-300C | SCSI Parport | good | US version of GT-6000
GT-5500 | SCSI | good |
GT-6500 | Parport | good |
ES-600C | Parport | good | US version of GT-6500
ES-1200C | Parport | good | US version of GT-9000
GT-7000 | SCSI | good |
GT-8000 | SCSI | good |
ES-8500 | SCSI | good |
Perfection 636S | SCSI | complete | US version of GT-7000
Perfection 636U | USB | complete |
Perfection 610 | USB | complete |
Perfection 640 | USB | complete |
Perfection 1200S | SCSI | complete |
Perfection 1200U | USB | complete |
Perfection 1200Photo | USB | complete | with TPU
Perfection 1240 | SCSI USB | complete |
Perfection 1640 | SCSI USB | complete |
Perfection 1650 | USB | complete |
Perfection 1660 | USB | complete |
Perfection 2400 | USB | complete |
Perfection 2450 | USB IEEE-1394 | complete |
Perfection 3200 | USB | complete | US version of the GT-9800
Perfection 4870 | USB | complete | US version of the GT-9800
Expression 636 | SCSI | complete | US version of GT-9500
Expression 800 | SCSI | complete |
Expression 1600 | SCSI USB IEEE-1394 | complete |
Expression 1680 | SCSI USB IEEE-1394 | complete |
FilmScan 200 | SCSI | unsupported | A better backend for the FilmScan 200 can be found at http://www.vjet.demon.co.uk/scanner/
CX-3200 | USB | good |
CX-3600 | USB | good |
CX-3650 | USB | good |
CX-4600 | USB | good |
CX-5200 | USB | good |
CX-5400 | USB | good |
CX-6400 | USB | good |
RX-500 | USB | good |
RX-600 | USB | good |
RX-425 | USB | good |

### Backend: fujitsu (1.12)

Manual page: sane-fujitsu

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Fujitsu | M3096G | SCSI | good |
M3091DCd | SCSI | good |
M3092DCd | SCSI | good |
M3093GXim | SCSI | good |
M3093GDim | SCSI | good |
M4097 | SCSI | good |
ScanPartner 93GX | SCSI | good |
fi-4120C | SCSI USB | basic |
fi-4220C | SCSI USB | basic |
fi-4340C | SCSI | basic | Color scans are inverted, Flatbed option is enabled
fi-4530C | SCSI USB | basic | USB untested

### Backend: genesys (1.0)

Manual page: sane-genesys
Comment: Only the USB scanners mentioned below are currently supported.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Medion/Lifetec/Tevion/Cytron | MD5345 | USB | good | Has a Primax USB ID
MD6228 | USB | good | Has a Primax USB ID. Same as MD5345
MD6471 | USB | complete | Has a Primax USB ID. Same as MD5345
Hewlett-Packard | ScanJet 2300C | USB | complete | 600x1200 dpi max

### Backend: gt68xx (1.0-71)

Link(s): http://www.meier-geinitz.de/sane/gt68xx-backend/
Manual page: sane-gt68xx
Comment: Only the USB scanners mentioned below are supported. For other Mustek BearPaws, look at the Plustek and the MA-1509 backend.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Artec/Ultima | Ultima 2000 | USB | good | Works, only product id 0x4002 is supported
Ultima 2000 e+ | USB | good | Works, only limited testing until now
Boeder | Sm@rtScan Slim Edition | USB | good | Similar to Artec Ultima 2000
Fujitsu | 1200CUS | USB | basic | Works, but is slow. Maybe a Mustek BearPaw 2400 CU clone?
Genius | Colorpage Vivid3x | USB | good |
Colorpage Vivid3 V2 | USB | good | Same as Colorpage Vivid3x
Colorpage Vivid3xe | USB | good |
Colorpage Vivid4 | USB | good | Works.
Colorpage Vivid4x | USB | good | Works.
Colorpage Vivid4xe | USB | basic | Should work but has limited testing. Please contact me if you own such a device.
Colorpage Vivid 1200 XE | USB | good |
Googlegear | 2000 | USB | good | Same as Artec Ultima 2000.
Lexmark | X70 | USB | good | Works, some resolutions fail at 16 bit
X73 | USB | good | Works, some resolutions fail at 16 bit, same as X70
Medion/Lifetec/Tevion/Cytron | MD 4394 | USB | good | Product id 0x4002. If you have 0x4003, use artec_eplus48u backend.
MD/LT 9375 | USB | untested | Untested, but is reported to have the same ids as the Artec Ultima 2000. Please test.
MD/LT 9385 | USB | good | Similar to Artec Ultima 2000
LT 9452 | USB | good | Similar to Mustek ScanExpress 1200 UB Plus
MD 9458 | USB | good | Similar to Artec Ultima 2000 (e+?)
Mustek | BearPaw 1200 CS | USB | good |
BearPaw 1200 CU | USB | good |
BearPaw 1200 CU Plus | USB | good | Product id 0x021c
BearPaw 1200 CU Plus | USB | good | Procuct id 0x021b.
BearPaw 1200 TA | USB | good | Transparency adapter supported
BearPaw 2400 CS | USB | untested | Probably works, reports are welcome
BearPaw 2400 CS Plus | USB | good | Works, problems with 12/16 bit modes?
BearPaw 2400 CU | USB | basic | Works, but is slow
BearPaw 2400 CU Plus | USB | good |
BearPaw 2400 TA | USB | good | Transparency adapter supported
BearPaw 2400 TA Plus | USB | good | Transparency adapter supported
BearPaw 2448 CS Plus | USB | basic | Same as 2448 TA Plus, but without TA.
BearPaw 2448 TA Plus | USB | basic | Transparency adapter supported. Slow. Brightness depends on resolution?
Plug-n-Scan 2400 MT | USB | good | Works but is slow in high resolutions. Same as BearPaw 2400 TA Plus.
Plug-n-Scan 2400 M | USB | good | Works but is slow in high resolutions. Same as BearPaw 2400 CS Plus.
ScanExpress 1200 UB Plus | USB | good |
ScanExpress 1248 UB | USB | complete |
ScanExpress A3 USB | USB | basic | Still some vertical stripes.
ScanExpress 2400 USB | USB | minimal | Should be detected but may need some more work in the code. Testers welcome.
ScanMagic 1200 UB Plus | USB | good | Same as ScanExpress 1200 UB Plus
Packard Bell | Diamond 1200 | USB | good | Similar to Mustek BearPaw 1200 (Plus)
Diamond 1200 Plus | USB | good | Product id 0x021c. Similar to Mustek BearPaw 1200 Plus
Diamond 1200 Plus | USB | good | Product id 0x021b. Similar to Mustek BearPaw 1200 Plus
Diamond 2450 | USB | good |
Plustek | OpticPro 1248U | USB | good |
OpticPro U16B | USB | good |
OpticPro U16B+ | USB | good |
OpticPro UT16B | USB | untested | Probably works. Transparency adapter not supported yet. Please contact me if you own such a device.
OpticSlim 1200 | USB | good |
OpticSlim 2400 | USB | good | Works up to 1200 dpi.
RevScan | 19200i | USB | good | Similar to Plustek OpticPro 1248U
Trust | Flat Scan USB 19200 | USB | good | Similar to Artec Ultima 2000
Compact Scan USB 19200 | USB | good | Works, if you have vendor id 0x055f and product id 0x0006, use the mustek_usb backend instead, similar to Mustek ScanExpress 1200 UB (Plus)
240TH Easy Webscan Gold | USB | good | Same as Mustek Bearpaw 2400 TA plus.
Visioneer | OneTouch 7300 | USB | good | Works upto 1200 dpi and 12 bits/color.

### Backend: hp (1.06)

Link(s): http://www.kirchgessner.net/
Manual page: sane-hp

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Hewlett-Packard | ScanJet Plus | Propietary | complete | Driver for HP parallel interface card required
ScanJet IIc | SCSI | complete |
ScanJet IIp | SCSI | complete |
ScanJet IIcx | SCSI | complete |
ScanJet 3c | SCSI | complete |
ScanJet 3p | SCSI | complete |
ScanJet 4c | SCSI | complete |
ScanJet 4p | SCSI | complete |
ScanJet 4100C | USB | complete |
ScanJet 5p | SCSI | complete |
ScanJet 5100C | Parport | complete | Requires ppscsi driver and epst module
ScanJet 5200C | Parport USB | complete | Parallel interface requires ppscsi driver and epst module
ScanJet 6100C | SCSI | complete |
ScanJet 6200C | SCSI USB | complete |
ScanJet 6250C | SCSI USB | complete |
ScanJet 6300C | SCSI USB | complete |
ScanJet 6350C | SCSI USB | complete |
ScanJet 6390C | SCSI USB | complete |
PhotoSmart PhotoScanner | SCSI | complete |

### Backend: hp5400 (1.0-2)

Link(s): http://sourceforge.net/projects/hp5400backend
Manual page: sane-hp5400
Comment: HP5400 and HP5470 scanners. Prototype backend available

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Hewlett-Packard | ScanJet 5400c | USB | basic |
ScanJet 5470c | USB | basic |
ScanJet 5490c | USB | basic |

### Backend: hpsj5s (0.03)

Link(s): http://hpsj5s.sourceforge.net/
Manual page: sane-hpsj5s

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Hewlett-Packard | ScanJet 5s | Parport (EPP) | minimal | Requires libieee1284 library. Only gray mode.

### Backend: ibm (1.0-4)

Link(s): http://www.meier-geinitz.de/sane/ibm-backend/
Manual page: sane-ibm
Comment: This backend has had only limited testing. It needs more work especially for the Ricoh scanners. Patches are welcome.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
IBM | 2456 | SCSI | basic | Was reported to work long time ago. Reports are welcome.
Ricoh | IS-410 | SCSI | untested | Untested, please report!
IS-420 | SCSI | basic | Works at least in flatbed mode.
IS-430 | SCSI | untested | Untested, please report!

### Backend: leo (1.0-10)

Link(s): http://www.zago.net/sane/#leo
Manual page: sane-leo

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
LEO | LEOScan S3 | SCSI | good | FCC ID LUZFS1130
Across Technologies | FS-1130 | SCSI | good | FCC ID LUZFS1130
Genius | FS-1130 Colorpage Scanner | SCSI | good |

### Backend: ma1509 (1.0-3)

Link(s): http://www.meier-geinitz.de/sane/ma1509-backend/
Manual page: sane-ma1509

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Mustek | BearPaw 1200 F | USB | good | Works upto 600 dpi. No support for TA and ADF yet.
Fujitsu | fi-4110EOX2 | USB | unsupported | Uses ma1509 chip, but very different from other scanners supported by backend

### Backend: matsushita (1.0-7)

Link(s): http://www.zago.net/sane
Manual page: sane-matsushita

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Panasonic | KV-SS25 | SCSI | complete |
KV-SS25D | SCSI | complete |
KV-SS50 | SCSI | untested |
KV-SS55 | SCSI | untested |
KV-SS50EX | SCSI | untested |
KV-SS55EX | SCSI | minimal | no color, no high resolution, no automatic cropping
KV-SS850 | SCSI | untested |
KV-SS855 | SCSI | untested |
KV-S2025C | SCSI | minimal | no color, no high resolution, no automatic cropping
KV-S2045C | SCSI | minimal | no color, no high resolution, no automatic cropping
KV-S2065L | SCSI | minimal | no color, no high resolution, no automatic cropping

### Backend: microtek (0.13.1)

Link(s): http://www.mir.com/mtek/
Manual page: sane-microtek

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Microtek | Scanmaker E6 | SCSI | good |
Scanmaker E3 | SCSI | good |
Scanmaker E2 | SCSI | good | 3-pass
Scanmaker 35t+ | SCSI | good | slide-scanner
Scanmaker 45t | SCSI | good | slide-scanner
Scanmaker 35 | SCSI | good | slide-scanner
Scanmaker III | SCSI | good |
Scanmaker IISP | SCSI | good |
Scanmaker IIHR | SCSI | good | 3-pass
Scanmaker IIG | SCSI | good | gray only
Scanmaker II | SCSI | good | 3-pass
Scanmaker 600Z(S) | SCSI | untested |
Scanmaker 600G(S) | SCSI | basic | gray only (see manpage)
Color PageWiz | SCSI (Parport) | basic | sheet-fed (preliminary, see mapage)
Agfa | Arcus II | SCSI | good | Arcus *II*, not Arcus!
StudioScan | SCSI | good |
StudioScan II | SCSI | good |
StudioScan IIsi | SCSI | good |
Studiostar | SCSI | minimal | Is detected but scans are very dark
DuoScan | SCSI | basic |
Vobis | Highscreen Realscan | SCSI | good |
Genius | Colorpage-SP2 | SCSI | good | Same as Microtek Scanmaker E3

### Backend: microtek2 (0.96)

Link(s): http://karstenfestag.gmxhome.de
Manual page: sane-microtek2

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Microtek | ScanMaker E3plus | Parport | complete |
ScanMaker E3plus | SCSI | complete |
ScanMaker X6 | SCSI | complete |
ScanMaker X6EL | SCSI | basic |
ScanMaker X6USB | USB | good |
ScanMaker V300 | SCSI | good |
ScanMaker V300 | Parport | good |
ScanMaker V310 | SCSI | basic |
ScanMaker V310 | Parport | basic |
ScanMaker V600 | SCSI | basic |
ScanMaker V600 | Parport | basic |
ScanMaker 330 | SCSI | basic |
ScanMaker 630 | SCSI | basic |
ScanMaker 636 | SCSI | complete |
ScanMaker 9600XL | SCSI | good | only flatbed mode ?
Phantom 330CX | Parport | complete |
SlimScan C3 | Parport | complete |
Phantom 636 | SCSI | complete |
Phantom 636CX | Parport | complete |
SlimScan C6 | USB | complete |
ScanMaker V6USL | SCSI | complete |
ScanMaker V6USL | USB | complete |
ScanMaker X12USL | SCSI | good | only Flatbed mode ?
Vobis | HighScan | SCSI | complete | only E3plus based models
Scanport | SQ300 | Parport? | basic |
SQ2030 | Parport | basic |
SQ4836 | SCSI | basic |
Genius | ColorPage-EP | Parport | good |

### Backend: mustek (1.0-138)

Link(s): http://www.meier-geinitz.de/sane/mustek-backend/
Manual page: sane-mustek
Comment: Most Mustek SCSI scanners are supported by this backend. For USB scanners, look at the mustek_usb backend.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Mustek | Paragon MFS-6000CX | SCSI | good | 3-pass
Paragon MFS-12000CX | SCSI | good | 3-pass
Paragon MFC-600S | SCSI | complete |
Paragon 600 II CD | SCSI | complete |
Paragon 600 II ED | Parport | untested | Completely untested. If it's the same as the 600 II EP, it may work. Please contact me if you own such a device.
Paragon 600 II EP | Parport | untested | Not tested yet but should work. Please contact me if you own such a device.
ScanMagic 600 II SP | SCSI | complete |
TwainScan II SP | SCSI | complete |
Paragon MFC-800S | SCSI | complete |
Paragon 800 II SP | SCSI | complete |
Paragon MFS-6000SP | SCSI | complete |
Paragon MFS-8000SP | SCSI | complete |
Paragon MFS-1200SP | SCSI | complete |
Paragon MFS-12000SP | SCSI | complete |
ScanExpress 6000SP | SCSI | complete |
ScanExpress 12000SP | SCSI | complete |
ScanExpress 1200 FS | SCSI | untested | One report that it crashes the computer. SCSI driver issue? Please contact me if you own such a device.
ScanExpress 12000SP Plus | SCSI | complete |
Paragon 1200 III SP | SCSI | complete |
Paragon 1200 LS | SCSI | complete |
ScanMagic 9636S | SCSI | complete |
ScanMagic 9636S Plus | SCSI | complete |
ScanExpress A3 SP | SCSI | basic | Please test!
Paragon 1200 SP Pro | SCSI | good |
Paragon 1200 A3 Pro | SCSI | complete | ADF and TA untested. Please contact me if you own such equipment.
Paragon 600 II N | Proprietary | basic | Resolutions above 300 dpi may cause trouble.
Trust | Imagery 1200 | SCSI | good | 3-pass, Mustek Paragon MFS-6000CX compatible
Imagery 1200 SP | SCSI | complete | Mustek Paragon MFS-6000SP compatible
Imagery 4800 SP | SCSI | complete | Mustek Paragon 600 II CD compatible
SCSI Connect 19200 | SCSI | complete | Mustek ScanExpress 12000SP compatible
SCSI excellence series 19200 | SCSI | complete | Mustek ScanExpress 12000SP compatible
Primax | Compact 4800 SCSI | SCSI | complete | Mustek 600 II CD compatible

### Backend: mustek_pp (13)

Link(s): http://penguin-breeder.org/sane/mustek_pp/
Manual page: sane-mustek_pp
Comment: Supports CIS and CCD type parallel port scanners from Mustek.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Mustek | ScanExpress 6000 P | Parport (EPP) | good | 300 dpi CCD scanner
ScanExpress 600 SEP | Parport (EPP) | good | 300 dpi CCD scanner
ScanMagic 4800 P | Parport (EPP) | good | 300 dpi CCD scanner
600 III EP Plus | Parport (EPP) | good | 300 dpi CCD scanner
96 CP | Parport (EPP) | good | 300x600 dpi CIS scanner
ScanExpress 600 CP | Parport (EPP) | good | 300x600 dpi CIS scanner
ScanMagic 600 CP | Parport (EPP) | good | 300x600 dpi CIS scanner
ScanExpress 1200 CP | Parport (EPP) | good | 600x1200 dpi CIS scanner
ScanExpress 1200 CP+ | Parport (EPP) | good | 600x1200 dpi CIS scanner
Medion/Lifetec/Tevion/Cytron | MD 9848 | Parport (EPP) | good | 300 dpi CCD scanner
MD/LT 935x | Parport (EPP) | good | 600x1200 dpi CIS scanner
MD/LT 985x | Parport (EPP) | good | 600x1200 dpi CIS scanner
MD/LT 9890 | Parport (EPP) | good | 600x1200 dpi CIS scanner
Targa | Funline TS12 EP | Parport (EPP) | good | 600x1200 dpi CIS scanner
Funline TS6 EP | Parport (EPP) | good | 300x600 dpi CIS scanner
Trust | Easy Connect 9600+ | Parport (EPP) | good | 300x600 dpi CIS scanner
Easy Connect 19200+ | Parport (EPP) | good | 300x600 dpi CIS scanner
Viviscan | Compact II | Parport (EPP) | good | 300 dpi CCD scanner
Cybercom | 9352 | Parport (EPP) | good | 300 dpi CCD scanner
Gallery | 4800 | Parport (EPP) | good | 300 dpi CCD scanner
Network | Easy Plus 30 Bit | Parport (EPP) | good | 300 dpi CCD scanner

### Backend: mustek_usb (1.0-18)

Link(s): http://www.meier-geinitz.de/sane/mustek_usb-backend/
Manual page: sane-mustek_usb
Comment: Only the USB scanners mentioned below are supported. For BearPaws, look at the Plustek, MA-1509, and gt68xx backends.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Mustek | ScanExpress 600 CU | USB | complete |
ScanExpress 1200 CU | USB | complete |
ScanExpress 1200 CU Plus | USB | complete |
ScanExpress 1200 UB | USB | complete | For the UB Plus, see gt68xx backend
Trust | Compact Scan USB 19200 | USB | complete | Mustek 1200 UB compatible

### Backend: nec (0.12)

Link(s): http://www5a.biglobe.ne.jp/~saetaka/
Manual page: sane-nec

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
NEC | PC-IN500/4C | SCSI | good | PC-IN500/4C was sold only in JAPAN

### Backend: niash (0.2, NEW!)

Link(s): http://sourceforge.net/projects/hp3300backend
Manual page: sane-niash

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Hewlett-Packard | ScanJet 3300c | USB | complete |
ScanJet 3400c | USB | complete | If you use Linux 2.6, version 2.6.8 or newer is necessary.
ScanJet 4300c | USB | complete | If you use Linux 2.6, version 2.6.8 or newer is necessary.
Agfa | Snapscan Touch | USB | complete |

### Backend: pie (1.0)

Link(s): http://www.munton.demon.co.uk/sane
Manual page: sane-pie

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Devcom | 9636PRO | SCSI | good |
9636S | SCSI | untested |
9630S | SCSI | untested |
PIE | ScanAce 1236S | SCSI | good |
ScanAce 1230S | SCSI | good |
ScanAce II | SCSI | untested |
ScanAce III | SCSI | good |
ScanAce Plus | SCSI | untested |
ScanAce II Plus | SCSI | untested |
ScanAce III Plus | SCSI | untested |
ScanAce V | SCSI | untested |
ScanAce ScanMedia | SCSI | untested |
ScanAce ScanMedia II | SCSI | untested |
ScanAce 630S | SCSI | untested |
ScanAce 636S | SCSI | untested |
Adlib | JetScan630 | SCSI | good |
JetScan636PRO | SCSI | untested |

### Backend: plustek (0.49)

Link(s): http://www.gjaeger.de/scanner/plustek/
Manual page: sane-plustek

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Plustek | OpticPro U12 | USB | complete | NOTE: Devices with product ID 0x0001 are not supported!
OpticPro UT12 | USB | complete | Note: Devices with product ID 0x0001 are not supported!
OpticPro UT16 | USB | complete |
OpticPro U24 | USB | complete |
OpticPro UT24 | USB | complete |
Genius | Colorpage HR6 V2 | USB | complete |
Colorpage HR7 | USB | complete |
Colorpage HR6A | USB | untested |
Colorpage HR7LE | USB | untested |
Colorpage HR6X | USB | untested |
Mustek | BearPaw 1200 | USB | complete | both product versions are supported, see backends' man-page
BearPaw 2400 | USB | complete |
Hewlett-Packard | ScanJet 2100C | USB | complete |
ScanJet 2200C | USB | complete |
Epson | Perfection 1250 | USB | complete |
Perfection 1250Photo | USB | good | TPA scans not perfect
Perfection 1260 | USB | complete |
Perfection 1260Photo | USB | good | TPA scans not perfect
Umax | UMAX 3400 | USB | complete | there are some UMAX 3400 outside the U.S. which are not supported, as they use another chipset than the LM983x
UMAX Astranet ia101 | USB | complete | seems to be a renamed UMAX 3400
UMAX 3450 | USB | complete |
UMAX 5400 | USB | complete |
Compaq | S4-100 | USB | complete | Identical to UMAX 3400
Canon | CanoScan N650U/N656U | USB | complete |
CanoScan N1220U | USB | complete |
CanoScan N670U/N676U | USB | complete |
CanoScan N1240U | USB | complete |
CanoScan LiDE20 | USB | complete |
CanoScan LiDE30 | USB | complete |
CanoScan D660U | USB | good | TPA scans not perfect

### Backend: plustek_pp (0.43)

Link(s): http://www.gjaeger.de/scanner/plustek_pp/
Manual page: sane-plustek_pp

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Plustek | OpticPro 4800P | Parport (SPP, EPP) | complete |
OpticPro 4830P | Parport (SPP, EPP) | complete |
OpticPro 600P/6000P | Parport (SPP, EPP) | complete |
OpticPro 4831P | Parport (SPP, EPP) | complete |
OpticPro 9630P | Parport (SPP, EPP) | complete |
OpticPro 9630PL | Parport (SPP, EPP) | complete | use driver-switch mov=1
OpticPro 9600P | Parport (SPP, EPP) | complete |
OpticPro 1236P | Parport (SPP, EPP) | complete | reported as OpticPro 12000P/96000P
OpticPro 12000P/96000P | Parport (SPP, EPP) | complete |
OpticPro 9636P | Parport (SPP, EPP) | complete | use driver-switch mov=4
OpticPro 9636P+/Turbo | Parport (SPP, EPP) | complete | use driver-switch mov=3
OpticPro 9636T | Parport (SPP, EPP) | complete |
OpticPro 12000T | Parport (SPP, EPP) | complete |
OpticPro AI3 | Parport (SPP, EPP) | basic | use driver-switch mov=5, poor picture quality
OpticPro P8 | Parport | untested |
OpticPro P12 | Parport (SPP, EPP) | complete |
OpticPro PT12 | Parport (SPP, EPP) | complete |
Primax | Colorado 4800 | Parport (SPP, EPP) | untested | same as OpticPro 4800P
Compact 4800 Direct | Parport (SPP, EPP) | complete | use driver-switch mov=2
Compact 4800 Direct-30 | Parport (SPP, EPP) | complete | same as OpticPro 4830P, use driver-switch mov=7
Compact 9600 Direct-30 | Parport (SPP, EPP) | complete | same as OpticPro 9630P
Genius | Colorpage Vivid III V2 | Parport (SPP, EPP) | complete | Reported as PT12
Colorpage Vivid Pro II Film | Parport (SPP, EPP) | complete | Reported as OP9636T/12000T
Colorpage HR6X EPP | Parport (SPP, EPP) | good | Negative scanning does not work correctly
Aries | Scan-It Pro 4800 | Parport (SPP, EPP) | complete | use driver-switch mov=2
BrightScan | BrighScan OpticPro | Parport (SPP, EPP) | complete | Reported as P12

### Backend: ricoh (unmaintained)

Manual page: sane-ricoh

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Ricoh | Ricoh IS50 | SCSI | basic |
Ricoh IS60 | SCSI | basic |

### Backend: s9036 (unmaintained)

Manual page: sane-s9036

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Siemens | 9036 Flatbed scanner | SCSI | basic |

### Backend: sceptre (1.0-10)

Link(s): http://www.zago.net/sane/
Manual page: sane-sceptre

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Sceptre | Vividscan S1200 | SCSI | basic |
Komodo | S1200 | SCSI | untested | rebadged Sceptre S1200

### Backend: sharp (0.32)

Link(s): http://www.satzbau-gmbh.de/staff/abel/sane-sharp.html
Manual page: sane-sharp

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Sharp | JX-610 | SCSI | good |
JX-250 | SCSI | good |
JX-320 | SCSI | good |
JX-325 | SCSI | untested |
JX-330 | SCSI | good |
JX-350 | SCSI | good |

### Backend: sm3600 (0.1)

Link(s): http://sm3600.sourceforge.net/
Manual page: sane-sm3600

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Microtek | ScanMaker 3600 | USB | basic | works
ScanMaker 3700 | USB | basic | works
ScanMaker 3750 | USB | basic | works (told)

### Backend: sm3840 (1.1, NEW!)

Link(s): http://www.ziplabel.com/sm3840/
Manual page: sane-sm3840
Comment: This reverse-engineered backend supports the USB ScanMaker 3840 model

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Microtek | ScanMaker 3840 | USB | good | 8 and 16 bit, color and grayscale
ScanMaker 4800 | USB | good | Same hardware as SM3840, different color box

### Backend: SnapScan (1.4)

Link(s): http://snapscan.sourceforge.net/
Manual page: sane-snapscan
Comment: Supported bit depths: 24 bit (color), 8 bit (gray)

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
AGFA | SnapScan | SCSI | good |
SnapScan 300 | SCSI | good |
SnapScan 310 | SCSI | good |
SnapScan 600 | SCSI | good | Optional ADF supported.
Arcus 1200 | SCSI | good | Optional transparency unit supported.
SnapScan 1236s | SCSI | good | Optional ADF and transparency unit supported.
SnapScan 1236u | USB | good | Optional ADF and transparency unit supported.
SnapScan 1212u | USB | good |
SnapScan e10 | USB | good |
SnapScan e20 | USB | good |
SnapScan e25 | USB | good |
SnapScan e26 | USB | good |
SnapScan e40 | USB | good |
SnapScan e42 | USB | good |
SnapScan e50 | USB | good | Optional tranparency unit supported
SnapScan e52 | USB | good | Optional tranparency unit supported
SnapScan e60 | USB | untested |
Benq (Acer) | 300f | SCSI | good |
310s | SCSI | good |
610s | SCSI | good |
610plus | SCSI | good |
620s | SCSI | good |
310u | USB | good |
320u | USB | good |
340u | USB | good |
620u | USB | good | Optional tranparency unit supported
640u | USB | good | Optional tranparency unit supported
640bu | USB | good |
640BT | USB | good | Optional tranparency unit supported
1240 | USB | good | Optional tranparency unit supported
3300 | USB | good |
4300 | USB | good |
5000 | USB | basic | Working up to 600 DPI
5300 | USB | basic | Problems with firmware upload reported
Guillemot / Hercules | Maxi Scan A4 Deluxe (SCSI) | SCSI | good | Rebadged SnapScan 310s.
Scan@home Touch 1248 (USB) | USB | good | Rebadged Benq 3300.
Maxi Scan A4 USB 640U | USB | good | Rebadged Benq 640U.
Maxi A4 36 bit | USB | good | Rebadged Benq 620U, needs Benq firmware file u96v???.bin
Mitsubishi | Diamondview 648UT | USB | good | Rebadged Benq 320u.
Diamondview 650U | USB | good | Rebadged Benq 4300.
Epson | Perfection 660 | USB | good |
Perfection 1270 | USB | good |
Perfection 1670 | USB | good |
Perfection 2480 | USB | good |
Perfection 2580 | USB | basic | Problems with preview scans reported, unplugging transparency unit seems to help

### Backend: sp15c (unmaintained)

Manual page: sane-sp15c

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Fujitsu | ScanPartner 15C | SCSI | good |
ScanPartner 600C | SCSI | good |

### Backend: st400 (1.6)

Link(s): http://www.informatik.uni-oldenburg.de/~ingo/sane/
Manual page: sane-st400

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Siemens | ST400 | SCSI | basic | 6 bit gray
ST800 | SCSI | basic | 6 bit gray

### Backend: tamarack (unmaintained)

Manual page: sane-tamarack

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Tamarack | Artiscan 6000C | SCSI | good | 3 pass, 300 DPI
Artiscan 8000C | SCSI | good | 3 pass, 400 DPI
Artiscan 12000C | SCSI | good | 3 pass, 600 DPI

### Backend: teco1 (1.0-10)

Link(s): http://www.zago.net/sane/#teco
Manual page: sane-teco1

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Relisys | RELI 2412 | SCSI | complete | sub model VM3530+
AVEC 2400 | SCSI | complete | sub model VM3520
RELI 4830 | SCSI | good | sub model VM4542
AVEC 2412 | SCSI | complete | sub model VM3520+
AVEC 4800 | SCSI | untested | sub model VM4530
AVEC 4816 | SCSI | untested | sub model VM4530+
RELI DS6 | SCSI | untested | sub model VM3420
RELI DS15 | SCSI | untested | sub model VM3440
RELI 2400 | SCSI | untested | sub model VM3530
RELI 4816 | SCSI | complete | sub model VM4540
RELI 9600 | SCSI | untested | sub model VM6530
RELI 9612 | SCSI | untested | sub model VM6530*
RELI 9624 | SCSI | untested | sub model VM6530+
RELI 9630 | SCSI | untested | sub model VM6540
Actown | ACT Scan I 30 | SCSI | untested | sub model VM3520A
Dextra | DF-600P | SCSI | good | sub model VM3510
DF-1200T+ | SCSI | untested | sub model VM3530+
DF-4830T | SCSI | untested | sub model VM4542
DF-9624 | SCSI | untested | sub model VM6530+

### Backend: teco2 (1.0-9)

Link(s): http://gkall.hobby.nl/teco2.html
Manual page: sane-teco2

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Relisys | AVEC Super 3 | SCSI | untested | sub model VM3575
AVEC II S3 | SCSI | good | sub model VM3564
SCORPIO Super 3 | SCSI | good | sub model VM3575
APOLLO Express 3 | SCSI | basic | sub model VM356A
APOLLO Express 6 | SCSI | good | sub model VM6565
SCORPIO Pro | SCSI | good | sub model VM6575
SCORPIO Pro-S | SCSI | untested | sub model VM6586
Primax | Jewel 4800 | SCSI | good | sub model VM356A
Profi 9600 | SCSI | basic | sub model VM6575
Profi 19200 | SCSI | good | sub model VM6586
Mustek | ScanMagic 4830S | SCSI | untested | sub model VM3575

### Backend: teco3 (1.0-1)

Link(s): http://www.zago.net/sane/#teco3
Manual page: sane-teco3

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Relisys | Infinity Scorpio | SCSI | good | sub model VM3552
Plustek | OpticPro 2400SP | SCSI | untested | sub model VM3552
PIOTECH | Splendeur 3024 | SCSI | good | sub model VM3552
Trust | Imagery 2400 SP | SCSI | good | sub model VM3552
Imagery 4800 SP+ | SCSI | good | sub model VM3552
Imagery 9600 SP | SCSI | untested | sub model VM3552

### Backend: template (0.42, NEW!)

Link(s): http://www.luser.com/temp/, http://www.luser.com/b/
Manual page: sane-template
Comment: This backend supports only the USB and SCSI models

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
TemPlate | Templ Z | SCSI | untested | With Z-Axis scrolling
Templ ZS | USB | unsupported | No support yet, but we have docs.
Templ ZQ | USB | minimal |
Templ ZY | SCSI | basic |
Templ ZZ | SCSI | good |
ArmorPlate | AmplScan II | SCSI | complete | AmplScan *II*, not AmplScan!

### Backend: u12 (0.02)

Link(s): http://www.gjaeger.de/scanner/u12/
Manual page: sane-u12

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Plustek | OpticPro U12 | USB | basic | Note: Only devices with product ID 0x0001 are supported!
OpticPro UT12 | USB | basic | Note: Only devices with product ID 0x0001 are supported!
OpticPro 1212U | USB | basic |
RevScan | RevScan Orange R48Ti | USB | basic | Rebadged Plustek OpticPro UT12
Genius | ColorPage HR6 V1 | USB | basic |
ColorPage Vivid III USB | USB | untested | Note: Device has Plustek vendor and product ID (0x07b3/0x0001)

### Backend: umax (1.0-41)

Link(s): http://www.rauch-domain.de/sane-umax/index.html
Manual page: sane-umax

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
UMAX | Vista S6 | SCSI | good | OK
Vista S6E | SCSI | good | OK
UMAX S-6E | SCSI | good | OK
UMAX S-6EG | SCSI | good | OK
Vista-S8 | SCSI | good | OK
Supervista S-12 | SCSI | good | OK
UMAX S-12 | SCSI | good | OK
UMAX S-12G | SCSI | good | OK
Astra 600S | SCSI | good | OK
Astra 610S | SCSI | good | OK
Astra 1200S | SCSI | good | OK
Astra 1220S | SCSI | good | OK
Astra 2100S | SCSI | good | OK
Astra 2200 (SU) | SCSI | good | OK
Astra 2200 (SU) | USB | good | OK, needs USB control messages
Astra 2400S | SCSI | good | OK
Astra 6400 | IEEE-1394 | unsupported | will propably work one day
Astra 6450 | IEEE-1394 | unsupported | will propably work one day
Astra MX3 | SCSI | good | OK
Astra MX3 | USB | good | OK, needs USB control messages
Mirage D-16L | SCSI | good | OK
Mirage II | SCSI | good | OK
Mirage IIse | SCSI | good | OK
PSD | SCSI | good | OK
PowerLook | SCSI | good | OK, SCSI-ID=PS-2400X
PL-II | SCSI | good | OK
PowerLook III | SCSI | good | OK
PowerLook 270 | SCSI | unsupported | incompatible
PowerLook 270plus | SCSI | unsupported | incompatible
PowerLook 1100 | IEEE-1394 | unsupported | will propably work one day
PowerLook 2000 | SCSI | good | OK
PowerLook 2100XL | SCSI | good | OK
PowerLook 3000 | SCSI | good | OK
Gemini D-16 | SCSI | good | OK
UMAX VT600 | SCSI | untested | may work, please test and give feedback
Vista-T630 | SCSI | good | OK for some firmwareversions, on others only lineart OK
UC 630 | SCSI | good | Version 2.8 OK, others only lineart OK
UG 630 | SCSI | good | OK
UG 80 | SCSI | good | OK
UC 840 | SCSI | good | Version 1.6 OK, others only lineart OK
UC 1200S | SCSI | untested | may work, please test and give feedback
UC 1200SE | SCSI | good | Version 3.0 OK, others unknown
UC 1260 | SCSI | good | Version 1.6 OK, others unknown
Linotype Hell | Jade | SCSI | good | OK, SCSI-ID=LinoHell Office
Jade | SCSI | good | OK, SCSI-ID=LinoHell JADE
Jade2 | SCSI | good | OK, SCSI-ID=LinoHell Office2
Saphir | SCSI | untested | support disabled until tested - please contact author
Saphir2 | SCSI | good | OK, SCSI-ID=LinoHell SAPHIR2
Saphir3 | SCSI | good | OK, SCSI-ID=LinoHell SAPHIR3
Saphir Ultra | SCSI | untested | support disabled until tested - please contact author
Saphir Ultra II | SCSI | good | OK, SCSI-ID=Linotype SAPHIR4
Saphir HiRes | SCSI | untested | support disabled until tested - please contact author
Opal | SCSI | untested | support disabled until tested - please contact author
Opal2 | SCSI | good | OK; SCSI-ID=LinoHell OPAL2
Opal Ultra | SCSI | untested | support disabled until tested - please contact author
Linoscan 1400 | SCSI | good | OK, SCSI-ID=HDM LS4H1S
Vobis | Highscreen Scanboostar Premium | SCSI | good | OK, SCSI-ID=LinoHell Office2
EDGE | KTX-9600US | SCSI | untested | no feedback
Epson | Perfection 600 | SCSI | good | OK, SCSI-ID=EPSON Perfection600
Escom | Image Scanner 256 | SCSI | good | OK, SCSI-ID=UMAX UG 80
Escort | Galleria 600 | SCSI | untested | untested, SCSI-ID=ESCORT Galleria 600S
Genius | ColorPage-HR5 (Pro) | SCSI | good | OK, SCSI-ID=KYE ColorPage-HR5
Nikon | AX-110 / Scantouch 110 | SCSI | untested | may work, please test and give feedback
AX-210 | SCSI | good | OK
TriGem | PowerScanII | SCSI | good | OK

### Backend: umax1220u (1.0.1)

Link(s): http://umax1220u-sane.sourceforge.net
Manual page: sane-umax1220u

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
UMAX | Astra 1220U | USB | good | OK
Astra 1600U | USB | minimal | Is reported to be the same as the 2000U. Sort of scans, but colors all messed up.
Astra 2000U | USB | minimal | Sort of scans, but colors all messed up.
Astra 2100 U | USB | minimal | Colours are distorted, there are vertical colour stripes, and the image is shadowed inches to its left.

### Backend: umax_pp (1)

Link(s): http://umax1220p.sourceforge.net/
Manual page: sane-umax_pp

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
UMAX | Astra 1220P | Parport (EPP/ECP) | good |
Astra 2000P | Parport (EPP/ECP) | good |
Astra 1600P | Parport (EPP/ECP) | good |
Astra 600P | Parport (SPP/ECP) | unsupported | untested, but should be close to 610P
Astra 610P | Parport (SPP/ECP) | good |
Hewlett-Packard | Scanjet 3200C | Parport (EPP/ECP) | good | works (relabelled 1220P and 2000P)

### Backend: unsupported (2005-07-30)

Link(s): /contrib.html
Comment: The devices mentioned here are not supported by any SANE backend. However, there may be links to information about them or stand-alone programs.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Agfa | 1212 P | Parport | unsupported | Most probably unsupported.
DuoScan f40 | USB IEEE-1394 | unsupported | Unsupported. See link for details.
DuoScan T2000XL | SCSI | unsupported | Unsupported. Same as Microtek ArtixScan 2020?
DuoScan T2500 | SCSI IEEE-1384 | unsupported | Unsupported. Same as Microtek Artixscan 2500f
Ambir | Visigo A4 | USB | unsupported | Not supported. See link for details.
Artec/Ultima | 1236 USB | USB | unsupported | Unsupported. Vendor/product 0x05d8/0x4001. See link for details.
AM12e+ | Parport | unsupported | Unsupported. Chipset unknown. Maybe similar to SCSI version or as6e?
E+ Pro | USB | unsupported | Not supported. Work is ongoing to support it by the artec_eplus48u backend. See link for details..
Ultima 2000 (0x4001) | USB | unsupported | Same name, but different ids: vendor/product 0x05d8/0x4001 is not supported. The scanner with product id 0x4002 is supported by the gt68xx backend.
Avigramm | Minidoc | USB | unsupported | Not supported. See link for details.
Avision | DS310F | Parport | unsupported | Probably not supported. Scanner/printer/copier combination.
iVina FB2400 | USB | unsupported | Not supported. No chipset information available. Same as UMAX Astra 6700.
iVina 1600 | USB | unsupported | GL646 based, to be added to genesys backend. Same as UMAX Astra 4500.
iVina FB1800 | USB | unsupported | GL646/GL660 based. Same as UMAX Astra 4700.
Benq (Acer) | 310p | Parport | unsupported | Unsupported. No details about the protocol known.
320p | Parport | unsupported | Unsupported. No details about the protocol known.
610p | Parport | unsupported | Unsupported. No details about the protocol known.
620p | Parport | unsupported | Unsupported. No details about the protocol known.
620pt | Parport | unsupported | Unsupported. No details about the protocol known.
640p | Parport | unsupported | Unsupported. Someone is working to ge this scanner supported. See link for details.
Boeder | Sm@rtScan Office | Parport USB | unsupported | Unsupported. See link for details.
Brother | MFC 4600 | Parport USB | unsupported | Unsupported. However there is a project to support this scanner/printer/fax combination. See link.
Canon | CanoScan 3000 | USB | unsupported | GL660+GL646 based.
CanoScan 3000ex | USB | unsupported | GL660+GL646 based.
CanoScan 3000F | USB | unsupported | GL660+GL646 based.
CanoScan 3200F | USB | unsupported | Probably unsupported. See link.
CanoScan 4200F | USB | unsupported | Probably unsupported. See link.
CanoScan 5000F | USB | unsupported | Unsupported. See link for details.
CanoScan 5200F | USB | unsupported | Probably unsupported. See link for details.
CanoScan 8000F | USB | unsupported | Not supported. USB Vendor/product 0x04a9/0x220f. See link for more information. With transparency adapter.
CanoScan 8400F | USB | unsupported | GL841 based, to be added to genesys backend
CanoScan 9900F | USB | unsupported | Probably unsupported, similar to 8000F. Vendor/product 0x04a9/0x2210. 3200x6400 dpi USB2. With transparency adapter.
CanoScan D646U | USB | unsupported | Probably not supported. USB Vendor/product 0x04a9/0x220b. See link for more information and test program.
CanoScan D646U ex | USB | unsupported | Probably not supported. See D646.
CanoScan D1250U2 | USB | unsupported | Not supported. However, someone started working on this scanner and some information is available (see link).
CanoScan D2400UF | USB | unsupported | Not supported. See link.
CanoScan FB620U | USB | unsupported | Probably not supported. Vendor/product 0x4a9/0x2202. Some information is available.
CanoScan FB1210U | USB | unsupported | Not supported. Vendor/product 0x4a9/0x2205. However, a stand-alone program for FreeBSD is available.
CanoScan LiDE 35 | USB | unsupported | GL841 based, to be added to genesys backend. Same as LiDE 50.
CanoScan LiDE 40 | USB | unsupported | GL841 based, to be added to genesys backend. Same as LiDE 50.
CanoScan LiDE 50 | USB | unsupported | GL841 based, to be added to genesys backend
CanoScan LiDE 80 | USB | unsupported | GL841 based, to be added to genesys backend
CanoScan LiDE 500F | USB | unsupported | GL841 based, to be added to genesys backend
DR-2080C | USB SCSI | unsupported | Probably not supported. Pass-trough (ADF) scanner.
DR-3020C | SCSI | unsupported | Not supported. High-speed pass-trough (ADF) scanner.
DR-3060 | SCSI | unsupported | Probably not supported. High-speed pass-trough (ADF) scanner.
DR-3080C | SCSI | unsupported | Probably not supported. High-speed pass-trough (ADF) color scanner.
DR-6080 | USB SCSI | unsupported | Probably not supported. High-speed pass-trough (ADF) scanner.
DR-9080C | SCSI | unsupported | Probably not supported. High-speed pass-trough (ADF) color scanner. Similar to DR-6080C, but can scan in color.
FS4000 | USB SCSI | unsupported | Not supported. USB Vendor/product 0x04a9/0x3042. See link for more details.
IS 12 | USB | unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers.
IS 22 | Parport | unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers.
IS 32 | USB | unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers.
IS 52 | ? | unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers.
PIXMA MP110 | USB | unsupported | Probably not supported. See link for details.
Chinon | DS-3000 | Parport Serial Port | unsupported | Unsupported at the moment, but a backend is in preparation. See link.
Compaq | S200 | USB | unsupported | Not supported. 2400x1200 dpi. Vendor=0x049f, Product=0x0021. One bulk-in, one bulk-out and one interrupt endpoint. Type-number: U0001-HB21, another type nr on the inside: 75100512-00
Compeye | Simplex 1236C | Parport USB | unsupported | Unsupported. See link for details.
Corex | Cardscan 500 | USB | unsupported | Probably not supported. Businesscard reader. Vendor/product: 0x08f0/0x0001.
Dell | A920 | USB | unsupported | Probably not supported. See link for details.
A960 | USB | unsupported | Probably not supported. See link for details.
922 | USB | unsupported | Probably not supported. See link for details.
1600n | USB Ethernet | unsupported | Probably not supported. See link for details.
Epson | GT-F600 | USB | unsupported | Unsupported. Doesn't speak ESC/I. Closely related to the GT-9400. It will be supported by epkowa backeend in future.
Perfection 4180 | USB | unsupported | Unsupported. Doesn't speak ESC/I. Closely related to the GT-9400. It will be supported by epkowa backeend in future.
E-Lux | j-6121 | Parport | unsupported | Probably unsupported. Sold 1998. Same as E-Lux j-6121.
Enhans | j-6121 | Parport | unsupported | Probably unsupported. Sold 1998. Same as E-Lux j-6121.
M-3630 A | Parport | unsupported | Probably unsupported.
Fujitsu | fi-4010C | USB | unsupported | Unsupported. Vendor/product: 0x04c5, 0x1029. Maybe similar to fi-4220C?
fi-4110CU | USB | unsupported | Unsupported. Vendor/product unknown. Maybe similar to fi-4220C?
Genius | ColorPage-Slim 1200 USB2 | USB | unsupported | Unsupported. See link for details.
ColorPage HR6X Slim | USB | unsupported | GL646 based, to be added to genesys backend
ColorPage HR7X | USB | unsupported | GL646 based, to be added to genesys backend
ColorPage HR8 | USB | unsupported | GL841 based, to be added to genesys backend
ColorPage-SF600 | USB | unsupported | Unsupported. See link for details.
Guillemot | SCAN@HOME 48 USB | USB | unsupported | Probably unsupported. See link for details.
Maxi Scan A4 Parallel 36 bit | Parport | unsupported | Probably unsupported. Identical to the Benq Prisa 620P.
Hercules | SCAN@HOME 48 USB | USB | unsupported | Probably unsupported. See link for details.
Hewlett-Packard | Photo Scanner 1000 | USB | unsupported | Not supported by SANE. However, it's detected as mass storage device so just mounting it is reported to work. See link for devices data.
Photosmart 1200 Photo | USB | unsupported | Probably not supported by SANE. No details known. 10x15 cm. Maybe similar to Photo Scanner 1000?
Photosmart S20 (C5101A) | USB | unsupported | Not supported yet by SANE, but a backend is under development. See link for details.
Photosmart S20xi (C7150A) | USB | unsupported | Not supported yet by SANE, but a backend is under development. See link for details.
ScanJet 2400c | USB | unsupported | GL646 based, to be added to genesys backend
HP3500C | USB | unsupported | Doesn't work yet but support by the hp_rts88x backend is planned.
HP3530C | USB | unsupported | Doesn't work yet but support by the hp_rts88x backend is planned.
HP3570C | USB | unsupported | Doesn't work yet but support by the hp_rts88x backend is planned.
ScanJet 3670c | USB | unsupported | GL646 based, to be added to genesys backend
ScanJet 3690c | USB | unsupported | Probably GL646_HP based, maybe can be added to genesys backend
ScanJet 3970c | USB | unsupported | Unsupported. See link for details.
ScanJet 4070 Photosmart | USB | unsupported | Unsupported. See link for details.
ScanJet 4500C | USB | unsupported | Maybe GL841_HP, but not confirmed, maybe can be added to genesys backend
ScanJet 4570C | USB | unsupported | Maybe GL841_HP, but not confirmed, maybe can be added to genesys backend
ScanJet 4600 | USB | unsupported | Not supported. See link for details.
ScanJet 4670 | USB | unsupported | Not supported. See link for details.
ScanJet 5500C | USB | unsupported | Maybe GL841_HP, but not confirmed, maybe can be added to genesys backend
ScanJet 5530C Photosmart | USB | unsupported | Maybe GL841_HP, but not confirmed, maybe can be added to genesys backend
ScanJet 5550C | USB | unsupported | Maybe GL841_HP, but not confirmed, maybe can be added to genesys backend
ScanJet 5590 | USB | unsupported | Not supported. See link for details.
IBM | ADF Color Scanner | Proprietary | unsupported | Unsupported. Uses proprietary ISA card. Maybe the same as the Plustek Spectra ADF?
Kodak | i30 | USB | unsupported | Probably unsupported. See link for details.
Snapshot Photo Scanner 1 | Parport | unsupported | Unsupported. FCC ID HWF96PHS
Lexmark | Photo 3150 | USB | unsupported | Unsupported. See link for details.
X74 | USB | unsupported | Unsupported. See link for details.
X75 | USB | unsupported | Unsupported. See link for details.
X75 PrinTrio | USB | unsupported | Unsupported. See link for details.
X83 | USB | unsupported | Unsupported. Vendor/product 0x043d/0x003d. GL640.
X1130 | USB | unsupported | Unsupported.
X1150 | USB | unsupported | Unsupported.
X1180 | USB | unsupported | Unsupported.
X1185 | USB | unsupported | Unsupported.
X5130 | USB | unsupported | Unsupported.
X5250 | USB | unsupported | Unsupported.
Logitech | PageScan Color | Parport | unsupported | Most probably unsupported.
PageScan USB | USB | unsupported | Probably unsupported. See link for details.
Medion/Lifetec/Tevion/Cytron | MD 6190 | USB | unsupported | Probably unsupported. There seem to exist two different scanners with that name. See link for details.
MD 40420 | USB | unsupported | Probably unsupported. See link for details.
MD 41260 | USB | unsupported | Probably unsupported. See link for details.
MD 41985 | USB | unsupported | Probably unsupported. See link for details.
MD 42666 | USB | unsupported | Probably unsupported. See link for details.
MD 90009 | USB | unsupported | Probably unsupported. See link for details.
Memorex | 6136u | USB | unsupported | Probably unsupported.
6142u | USB | unsupported | Probably unsupported. Same as Visioneer Onetouch 4400. See link for details.
MaxxScan 6122 | USB Parport | unsupported | Unsupported. See link for details.
SCF 9612P | Parport | unsupported | Probably unsupported. See link for details.
Microtek | ArtixScan 2020 | SCSI | unsupported | Unsupported. Same as Agfa DuoScan T2000XL?
Artixscan 2500f | SCSI IEEE-1384 | unsupported | Unsupported. Same as Agfa DuoScan T2500?
ArtixScan 4000tf | USB | unsupported | Unsupported. Uses ALI M5611B.
FilmScan 35 | USB | unsupported | Probably unsupported. See link for details.
ScanMaker 336 CX | SCSI | unsupported | Probably unsupported. Seems to be similar to the Microtek 330 CX and is detected by the microtek2 backend. Scanning doesn't seem to work however.
Scanmaker 1850S | SCSI | unsupported | Unsupported. See link for details.
ScanMaker 3630 | USB | unsupported | Unsupported. Doesn't seem to be compatible to 3600 series, see link.
ScanMaker 3800 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 3830 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 4700 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 4850 | USB | unsupported | Probably unsupported. See link for details.
ScanMaker 4900 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 5 | SCSI | unsupported | Probably unsupported. See link for more details.
ScanMaker 5600 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 5700 | USB | unsupported | Unsupported. Uses ALI M5615 like the ScanMaker 4700.
ScanMaker 5800 | USB | unsupported | Unsupported. See link for details.
ScanMaker 5900 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 6000 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 6100 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 6700 | USB IEEE-1394 | unsupported | Unsupported. See link.
ScanMaker 8700 | USB IEEE-1394 | unsupported | Unsupported. See link for details.
ScanMaker 9600XL | USB SCSI IEEE-1394 | unsupported | Probably unsupported.
ScanMaker 9800XL | USB SCSI IEEE-1394 | unsupported | Unsupported. See link.
ScanMaker i320 | USB | unsupported | Unsupported. See link.
ScanMaker s400 | USB | unsupported | Unsupported. See link.
ScanPort 3000 | USB | unsupported | Unsupported. Vendor/Product ids: 0x04a7/0x0224. Realtek RTS8801B?. See link for details.
Konica Minolta | Dual Scan III | USB | unsupported | Unsupported. May work with vuescan. See link for details.
Dual Scan IV | USB | unsupported | Unsupported. Works with vuescan. See link for details.
DiMAGE Scan Elite 5400 | USB IEEE-1394 | unsupported | Probably unsupported. May work with vuescan. See link for details.
DiMAGE Scan Elite 5400 2 | USB | unsupported | Probably unsupported. See link for details.
DiMAGE Scan Multi Pro | IEEE-1394 | unsupported | Probably unsupported. See link for details.
Mustek | 1200 III EP | Parport | unsupported | Probably not supported. quarlewm at jmu dot edu offers to temporarily loan such a scanner to anyone who is interested in writing a driver.
1800 A3 Pro-1 | USB | unsupported | Not supported but someone wants to start writing a backend. See link. Vendor/Product ids: 0x055f/0x0401. No information about this scanner on any Mustek website.
2400 M | USB | unsupported | Probably unsupported. No details known.
BearPaw 1248CU | USB | unsupported | Probably unsupported. No details known.
BearPaw 2400 TA Pro | USB | unsupported | Not supported. See link for some information.
BearPaw 2448 CU Pro | USB | unsupported | Not supported. See link for some information.
BearPaw 2448 TA Pro | USB | unsupported | Not supported. See link for some information.
BearPaw 4800 TA Pro | USB | unsupported | Not supported. See link for some information.
BearPaw 4800 TA Pro II | USB | unsupported | Not supported. See link for some information.
P 3600 A3 Pro | USB | unsupported | Not supported. Maybe similar to the 1800 A3 Pro-1?. See link.
Paragon 800 II EP | Parport | unsupported | Not supported. Maybe similar to 600 II EP (SCSI_over-parport)? In this case it could be supported by the mustek SCSI backend.
ScanExpress 600 USB | USB | unsupported | Unsupported. Vendor/Product 0x055f/0x873. Programming information is available.
ScanExpress 1200 USB | USB | unsupported | Unsupported. Vendor/Product 0x055f/0x0003. Programming information is available.
ScanExpress 1200 USB Plus | USB | unsupported | Unsupported. Vendor/Product 0x055f/0x0007.
ScanExpress 12000 P | Parport | unsupported | Not supported. Asic 1505/05.
ScanExpress A3 EP | Parport | unsupported | Not supported. Maybe it will be supported by the mustek_pp backend in future.
ScanExpress CardSmart | USB | unsupported | Probably unsupported. USB business card scanner. Maybe works as USB storage device?
ScanMagic 9636P | Parport | unsupported | Probably not supported. Same as Mustek 12000 P?. ASIC 1505.
NEC | Petiscan | USB | unsupported | Most probably unsupported. See link for details. Vendor ID is 0x0475 (Relisys/Teco). Not know if it is similar to other Relisys/Teco USB scanners.
Nikon | LS 50 ED | USB | unsupported | Most probably unsupported. See link for details.
Coolscan V ED | USB | unsupported | Most probably unsupported. See link for details.
Super Coolscan LS-5000 ED | USB | unsupported | Most probably unsupported. See link for details.
Olivetti | Job-Jet M400 | USB | unsupported | Probably not supported. See link for details.
Olympus | ES-10S | SCSI | unsupported | Probably not supported. See link for details.
Optrox | PhotoMaker 3 | Parport | unsupported | Probably not supported.
Panasonic | KV-SS905C | ? | unsupported | might be supported by matsushita backend.
KV-S2026C | ? | unsupported | might be supported by matsushita backend.
KV-S2046C | ? | unsupported | might be supported by matsushita backend.
KV-S2055W | ? | unsupported | might be supported by matsushita backend.
KV-S2055L | ? | unsupported | might be supported by matsushita backend.
KV-S2065W | ? | unsupported | might be supported by matsushita backend.
KV-S3065CW | ? | unsupported | might be supported by matsushita backend.
KV-S3065CL | ? | unsupported | might be supported by matsushita backend.
KV-S3085 | ? | unsupported | might be supported by matsushita backend.
KV-S3105C | ? | unsupported | might be supported by matsushita backend.
KV-S6040W | ? | unsupported | might be supported by matsushita backend.
KV-S6045W | ? | unsupported | might be supported by matsushita backend.
KV-S6050W | ? | unsupported | might be supported by matsushita backend.
KV-S6055W | ? | unsupported | might be supported by matsushita backend.
KV-S7065C | ? | unsupported | might be supported by matsushita backend.
Pentax | DSmobile USB | USB | unsupported | Probably not supported. Some information is available.
PIE | Primefilm 1800u | USB | unsupported | Not supported. Vendor/product 0x05e3/0x0120. See link for details.
Primefilm 3600PRO | USB IEEE-1394 | unsupported | Probably not supported.
Powerslide 3600 | USB IEEE-1394 | unsupported | Probably unsupported. Film scanner that can scan directly from the magazine.
Plustek | OpticBook 3600 | USB | unsupported | GL842 based (similar to GL841?), maybe ca be added to genesys backend. Bookscanner.
OpticFilm 7200 | USB | unsupported | GL841 based, to be added to genesys backend
OpticPro A3U | USB | unsupported | Uses Plustek ASIC P99002
OpticPro S6 | USB | unsupported | Uses RealTek chipset (RTL8801D)
OpticPro S12 | USB | unsupported |
OpticPro ST12 | USB | unsupported |
OpticPro ST16 | USB | unsupported | GL646 based, to be added to genesys backend
OpticPro UA18 | USB | unsupported | Probably LM983x based.
OpticPro S24 | USB | unsupported | GL646 based, to be added to genesys backend
OpticPro ST24 | USB | unsupported | GL646 based, to be added to genesys backend
OpticPro S28 | USB | unsupported | GL841 based, to be added to genesys backend
OpticPro ST28 | USB | unsupported | GL841 based, to be added to genesys backend
OpticPro ST48 | USB | unsupported | GL841 based, to be added to genesys backend
OpticPro ST64 | USB | unsupported | No further information available.
OpticSlim 2420 | USB | unsupported | GL841 based, to be added to genesys backend
OpticSlim M12 | USB | unsupported | Uses the GT6816 chipset. May be supported by the gt68xx backend in future. See link for details.
OpticWorks 2000 | Parport | unsupported | Multifunction device. No further information available.
OptiCard 600+ | USB | unsupported | Business card reader. No further information available.
Spectra ADF | Proprietary | unsupported | Unsupported. Uses proprietary ISA card that also provides power and is labelled GPS-1 PAGE-A from Taiwan. Other labels on the scanner include ADF Color Scanner and SF600AS. Maybe the same as the IBM ADF Color Scanner?
Primax | Colorado 600U | USB | unsupported | Not supported. Some information is available.
Colorado 2400U | USB | unsupported | Probably unsupported. See link for details.
Primascan Colorado 2600u | USB | unsupported | Unsupported. Same as Visioneer Onetouch 4400. See link for details.
Colorado Direct 600 | Parport | unsupported | Not supported. However, a stand-alone program is available.
Colorado Direct 9600 | Parport | unsupported | Not supported. However, a stand-alone program is available.
Colorado USB 9600 | USB | unsupported | Not supported. See link for details.
OneTouch 5300 | Parport | unsupported | Not supported.
Slim-Line 1200 | USB | unsupported | Maybe GL646.
Prolink | Winscan Pro 2448U | USB | unsupported | Not supported. Some information is available. Vendor=0x06dc product=0x0014. RealTek RTS8801.
Quato | X-Finity | SCSI | unsupported | Probably not supported. No details yet. Originally manufactured by PFU?
X-Finity Ultra | USB IEEE-1394 | unsupported | Probably not supported. No details yet.
Reflecta | DigitDia 3600 | USB IEEE-1394 | unsupported | GL841 based, to be added to genesys backend. Film scanner that can scan directly from the magazine.
iScan 1800 | USB | unsupported | Probably unsupported. See link for details.
ProScan 4000 | USB IEEE-1394 | unsupported | Probably unsupported. See link for details.
Relisys | Eclipse 1200U | USB | unsupported | Probably unsupported. See link for details.
Scorpio Ultra 3 | USB | unsupported | Probably unsupported. See link for details.
Episode | USB | unsupported | Probably unsupported. See link for details.
Sicos | DMS 2000 | proprietary | unsupported | Not supported until now. Work on a backend has started, contact the author for details (see link)
SmartScan 3600 | USB IEEE-1394 | unsupported | Probably not supported. Same as PIE Primefilm 2600 PRO.
Spot Technology | Maxiscan A4 | proprietary | unsupported | Not supported until now. Work on a backend has started, see link for more information.
ScanTak 2c | proprietary | unsupported | Not supported. Work on a backend has started, see link for more information.
ScanTak 3c | proprietary | unsupported | Not supported. Work on a backend has started, see link for more information.
Syscan | TravelScan 460/464 | USB | unsupported | Not supported. Some information is available. See link for details.
TravelScan FS-531 | USB | unsupported | Not supported. May work with the Plustek backend in future. See link for details.
TravelScan Pro | USB | unsupported | Probably not supported. Some information is available.
Tamarack | Artiscan 9600 | Parport | unsupported | Unsupported at the moment. See link for a project for that scanner taht may support it in future.
Artiscan 9600 pro 36 | Parport | unsupported | Unsupported at the moment. See link for a project for that scanner.
TCE | MK600U | USB | unsupported | Not supported. Some information is available.
S450 | Parport | unsupported | Not supported by SANE but is reported to work with pxscan (see link).
Teco | VM6509F | USB | unsupported | Probably unsupported. See link for details.
Tiny | FU661E | USB | unsupported | Unsupported. See link for details.
Trust | CombiScan 19200 | Parport USB | unsupported | Unsupported. See link for details.
SCSI Scan 19200 -Excellence Series- | SCSI | unsupported | Unsupported. See link for details.
UMAX | Astra 3000 | USB | unsupported | Probably not supported. See link for details.
Astra 3400 | USB | unsupported | Model ID 0x0050 not supported. See link for details.
Astra 3600 | USB | unsupported | Probably not supported. See link for details.
Astra 4000 | USB | unsupported | Not supported. See link for details.
Astra 4400 | USB | unsupported | Probably not supported. See link for details.
Astra 4450 | USB | unsupported | Probably not supported. See link for details.
Astra 4500 | USB | unsupported | GL646 based, to be added to genesys backend. Avision iVina FB1600 clone
Astra 4600 | USB | unsupported | Probably not supported, no details known.
Astra 4700 | USB | unsupported | GL646/GL660 based. Avision iVina FB1800 clone.
Astra 6700 | USB | unsupported | Not supported. No chipset information available. Same as Avision iVina FB2400.
AstraSlim | USB | unsupported | Probably not supported currently. See link for more details.
AstraSlim 1200 SE | USB | unsupported | Probably not supported currently. May be supported in future. See link for more details.
AstraSlim 6000 | USB | unsupported | Probably not supported currently. See link for more details.
Powerlook 180 | USB | unsupported | Probably not supported. See link for details.
Powerlook 1000 USB | USB | unsupported | Probably not supported. No further information available.
Vantas | 3000 | USB | unsupported | Not supported. See link for more details.
Visioneer | 6200 | USB | unsupported | Not supported. Is reported to use the E5 chipset. Uses a Primax ID. See link for some details. Looks similar to Primascan Colorado 2600u.
Onetouch 4400 | USB | unsupported | Not supported. E5 chipset? Vendor/product 0x0461/0x0347.See link for more details.
OneTouch 4800 USB | USB | unsupported | Unsupported. Vendor/Product ids: 0x04a7/0x0224. Seems to use Realtek RTS8801B. Same as Microtek Scanport 3000. See link for details.
OneTouch 5300 USB | USB | unsupported | Not supported. Vendor/product ids 0x04a7/0x0226. Chipset is RTS8801B(?). See link for output of /proc/bus/usb/devices.
OneTouch 5800 USB | USB | unsupported | Unsupported. 48 bit scanner, doesn't work with viceo backend. RTS8801C. Vendor/product 0x04a7/0x0226.
OneTouch 6600 | USB | unsupported | Unsupported. See link for details.
Onetouch 7100 | USB | unsupported | GL646 based, to be added to genesys backend
OneTouch 8100 | USB | unsupported | Unsupported. See link for details.
Onetouch 8700 | USB | unsupported | Not supported. See link for details.
Onetouch 8900 | USB | unsupported | Not supported. Same as 8920 but without TA?
Onetouch 8920 | USB | unsupported | Not supported. Same as 8700 and 8900 but includes a TA. Uses a Primax ID. Chipset is RTS8801C. See link for output of /proc/bus/usb/devices.
Onetouch 9000 | USB | unsupported | Not supported. See link for details.
Onetouch 9020 | USB | unsupported | Not supported. See link for details.
Onetouch Pro 8800 | USB | unsupported | Probably not supported. See link for details.
Onetouch Pro 8820 | USB | unsupported | Probably not supported. See link for details.
PaperPort 3100b | Parport | unsupported | Most probably not supported. See link for details.
PaperPort 6100 | Parport | unsupported | Most probably not supported. More details would be appreciated.
PaperPort OneTouch | Parport | unsupported | Most probably not supported. See link for details.
Primascan Colorado 2600u | USB | unsupported | Not supported. See Visioneer Onetouch 4400.
Strobe XP 100 | USB | unsupported | Not supported but may work in future. See link for details.
Xerox | 2400 Onetouch | USB | unsupported | Probably GL646_HP based, maybe can be added to genesys backend
DocuImage 620S | SCSI | unsupported | Not supported. See link for more details.
WorkCentre 470cx | Parport | unsupported | Not supported. See link for more details.
WorkCentre M15i | USB | unsupported | Not supported. See link for more details.
WorkCentre XK35c | USB Parport | unsupported | Not supported. See link for more details.
WorkCentre XK50cx | USB | unsupported | Not supported. See link for more details.
WorkCentre Pro 412 | USB Parport | unsupported | Not supported. See link for more details.
WorkCentre PE16 | USB Parport | unsupported | Not supported. See link for more details.

## Still Cameras

Backends: dc25, dc210, dc240, dmc

### Backend: dc25 (1.2)

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-dc25

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Kodak | DC25 | Serial port | complete |
DC20 | Serial port | basic | DC-20 untested by author but reported to work

### Backend: dc210 (0.0)

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-dc210

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Kodak | DC210 | Serial port | basic |

### Backend: dc240 (0.0)

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-dc240

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Kodak | DC240 | Serial port | good | Use gphoto2 backend to get USB support

### Backend: dmc (unmaintained)

Manual page: sane-dmc

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Polaroid | DMC | SCSI | good |

## Video Cameras

Backends: qcam, unsupported

### Backend: qcam (unmaintained)

Manual page: sane-qcam

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Connectix | Color QuickCam | Parport | good | Requires root privileges.
Greyscale QuickCam | Parport | minimal | Requires root privileges. Partly working.

### Backend: unsupported (2005-07-30)

Link(s): /contrib.html
Comment: The devices mentioned here are not supported by any SANE backend. However, there may be links to information about them or stand-alone programs.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Biolux | 654 (micrOcular) | USB | unsupported | Not supported yet. See link for more details.
Grandtek Scopecam | 8x30 Binocular & Digital Camera | USB | unsupported | Not Supported yet. See link for more details.

## APIs

Backends: gphoto2, pint, pnm, template, test, v4l

### Backend: gphoto2 (0.0)

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-gphoto2
Description: Multiple cameras supported by the gphoto2 libraries
Comment: The long-term plan is to support all the cameras supported by the gphoto2 libraries (currently over 140 models). However, at this stage, only a handful of cameras are definitely known to work with SANE. Other cameras will probably work if the native file format is EXIF or JPEG. Testers welcome!

### Backend: pint (unmaintained)

Manual page: sane-pint
Description: Scanners with the machine-independent PINT interface
Comment: Haven't been tested for a long time. Handle with care.

### Backend: pnm (1.0.8)

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-pnm
Description: Reads PNM files
Comment: Used for debugging frontends. Obsolete, use test backend instead.

### Backend: template (0.42, NEW!)

Link(s): http://www.luser.com/temp/, http://www.luser.com/b/
Manual page: sane-template
Comment: This backend supports only the USB and SCSI models
Description: Interface to FrObYz API
Comment: Only FrObYz version 2.0 is supported!

### Backend: test (1.0-26)

Link(s): http://www.meier-geinitz.de/sane/test-backend/
Manual page: sane-test
Description: Frontend-tester
Comment: Backend for testing frontends. Also serves as example for SANE backend options.

### Backend: v4l (1.0-3)

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-v4l
Description: Interface to Video For Linux API
Comment: Supports video cameras and other devices accessed by the v4l kernel API, e.g. bttv devices. Quite a lot of known bugs.

## Meta Backends

Backends: dll, net

### Backend: dll (1.0.11)

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-dll
Description: Dynamic loading of shared-library backends.

### Backend: net (1.0.13)

Link(s): http://www.penguin-breeder.org/?page=sane-net
Manual page: sane-net
Description: Network access to saned servers
Comment: Can be used to access any scanner supported by SANE over the net. Supports IPv4 and IPv6.

### Legend:

> Backend:
>   Name of the backend, in parentheses if available: Version of backend/driver; newer versions may be available from their home sites.
>   NEW! means brand-new to the current release of SANE.
>   UNMAINTAINED means that nobody maintains that backend. Expect no new features or newly supported devices. You are welcome to take over maintainership.
> Link(s):
>   Link(s) to more extensive and detailed information, if it exists, or the email address of the author or maintainer.
> Manual Page:
>   A link to the man-page online, if it exists.
> Comment:
>   More information about the backend or model, e.g. the level of support and possible problems.
> Manufacturer:
>   Manufacturer, vendor or brand name of the device.
> Model:
>   Name of the the device.
> Interface:
>   How the device is connected to the computer.
> Status:
>   Indicates how many of the features the device provides are supported by SANE.
>   - unsupported means the device is not supported at least by this backend. It may be supported by other backends, however.
>   - untested means the device may be supported but couldn't be tested. Be very careful and report success/failure.
>   - minimal means that the device is detected and scans at least in one mode. But the quality is bad or important features won't work.
>   - basic means it works at least in the most important modes but quality is not perfect.
>   - good means the device is usable for day-to-day work. Some rather exotic features may be missing.
>   - complete means the backends supports everything the device can do.
> Description:
>   The scope of application of the backend.

SANE homepage
This page was last updated on Mon Aug 8 08:22:53 2005