| # SANE-umax advanced options

> Index Frontend options: Standard options Advanced options Supported scanners: Power Look series Mirage series Astra series Vista series UC series others Not listed scanners UMAX scanner clones UMAX parallel port scanners Configuration Speed of UMAX scanners SANE-umax homepage SANE homepage XSane homepage | This backend dynamically enabeles the options that are supported by the scanner in dependence of the scanning-mode and other options. Here is an example of the frontend XSane:
> Advanced options | Remark
> Set exposure time | Enable selection of exposure time, if not enabled, scanner uses default values. *
> Cal. exposure time | Define exposure time for calibration. *
> Scan exposure time | Define exposure time for scan. *
> Set lamp density | Enable selection of lamp density, if not enabled, scanner automatically selects a value. *
> Cal. lamp density | Define lamp density for calibration. *
> Set scan lamp density | Enable selection of lamp density for scan, if not enabled scanner uses the value that was used for calibration. *
> Scan lamp density | Define lamp density for scan. *
> lamp on | Turn on scanner lamp. *
> lamp off | Turn off scanner lamp. *
> lamp off at exit | Turn off scanner lamp when program exits (when sane_close is called) *
* only available for some scanners This page has been changed on 5th. february 2001

> Author: Oliver Rauch