# SANE: Supported Devices

The following table summarizes the devices supported by sane-backends-1.0.16.

This is only a summary! Please consult the manpages and the author-supplied webpages for more detailed (and usually important) information concerning each backend.

If you have new information or corrections, please file a bug report with as many details as possible. Also please tell us if your scanner isn't mentioned in this list at all.

For an explanation of the tables, see the legend.

There are tables for scanners, still cameras, video cameras, APIs, and meta backends.

## Scanners

Manufacturers: Abaton, Acer Peripherals, Across Technologies, Actown, Adlib, AGFA, Ambir, Apple, Aries, ArmorPlate, Artec/Ultima, Avigramm, Avision, Bell and Howell, Benq (Acer), BlackWidow, Boeder, BrightScan, Brother, Canon, Chinon, Compaq, Compeye, Corex, Cybercom, Dell, Devcom, Dextra, E-Lux, EDGE, Enhans, Epson, Escom, Escort, Fujitsu, Gallery, Genius, Googlegear, Guillemot, Guillemot / Hercules, Hercules, Hewlett-Packard, IBM, iVina, Kodak, Komodo, Konica Minolta, LEO, Lexmark, Linotype Hell, Logitech, Medion/Lifetec/Tevion/Cytron, Memorex, Microstar, Microtek, Minolta, Minolta-QMS, Mitsubishi, Mustek, NEC, Network, Nikon, Olivetti, Olympus, Optrox, Packard Bell, Panasonic, Pentax, PIE, PIOTECH, Plustek, Primax, Prolink, Quato, Reflecta, Relisys, RevScan, Ricoh, Scanport, Sceptre, Sharp, Sicos, Siemens, Spot Technology, Syscan, Tamarack, Targa, TCE, Teco, TemPlate, Tiny, TriGem, Trust, UMAX, Vantas, Visioneer, Viviscan, Vobis, Vuego, Xerox

### Manufacturer: Abaton

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Scan 300/GS | SCSI | complete | All known modes and functions supported | abaton (unmaintained) | sane-abaton
Scan 300/S | SCSI | untested | Untested, use with caution | abaton (unmaintained) | sane-abaton

### Manufacturer: Acer Peripherals

Comment: Company was renamed to Benq.

### Manufacturer: Across Technologies

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
FS-1130 | SCSI | good | FCC ID LUZFS1130 | leo (1.0-10) | sane-leo

### Manufacturer: Actown

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
ACT Scan I 30 | SCSI | untested | sub model VM3520A | teco1 (1.0-10) | sane-teco1

### Manufacturer: Adlib

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
JetScan630 | SCSI | good |  | pie (1.0) | sane-pie
JetScan636PRO | SCSI | untested |  | pie (1.0) | sane-pie

### Manufacturer: AGFA

Link(s): http://www.agfa.com/, http://www.agfa.com

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
1212 P | Parport | unsupported | Most probably unsupported. | unsupported (2005-07-30) | ?
Arcus 1200 | SCSI | good | Optional transparency unit supported. | SnapScan (1.4) | sane-snapscan
Arcus II | SCSI | good | Arcus *II*, not Arcus! | microtek (0.13.1) | sane-microtek
DuoScan | SCSI | basic |  | microtek (0.13.1) | sane-microtek
DuoScan f40 | USB IEEE-1394 | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
DuoScan T2000XL | SCSI | unsupported | Unsupported. Same as Microtek ArtixScan 2020? | unsupported (2005-07-30) | ?
DuoScan T2500 | SCSI IEEE-1384 | unsupported | Unsupported. Same as Microtek Artixscan 2500f | unsupported (2005-07-30) | ?
Focus Color | SCSI | good | 3-pass | agfafocus (unmaintained) | sane-agfafocus
Focus Color Plus | SCSI | good | 3-pass | agfafocus (unmaintained) | sane-agfafocus
Focus GS Scanner | SCSI | untested | 6 bit gray | agfafocus (unmaintained) | sane-agfafocus
Focus II | SCSI | untested | gray only | agfafocus (unmaintained) | sane-agfafocus
Focus Lineart Scanner | SCSI | untested | Lineart only? Untested. | agfafocus (unmaintained) | sane-agfafocus
SnapScan | SCSI | good |  | SnapScan (1.4) | sane-snapscan
SnapScan 300 | SCSI | good |  | SnapScan (1.4) | sane-snapscan
SnapScan 310 | SCSI | good |  | SnapScan (1.4) | sane-snapscan
SnapScan 600 | SCSI | good | Optional ADF supported. | SnapScan (1.4) | sane-snapscan
SnapScan 1212u | USB | good |  | SnapScan (1.4) | sane-snapscan
SnapScan 1236s | SCSI | good | Optional ADF and transparency unit supported. | SnapScan (1.4) | sane-snapscan
SnapScan 1236u | USB | good | Optional ADF and transparency unit supported. | SnapScan (1.4) | sane-snapscan
SnapScan e10 | USB | good |  | SnapScan (1.4) | sane-snapscan
SnapScan e20 | USB | good |  | SnapScan (1.4) | sane-snapscan
SnapScan e25 | USB | good |  | SnapScan (1.4) | sane-snapscan
SnapScan e26 | USB | good |  | SnapScan (1.4) | sane-snapscan
SnapScan e40 | USB | good |  | SnapScan (1.4) | sane-snapscan
SnapScan e42 | USB | good |  | SnapScan (1.4) | sane-snapscan
SnapScan e50 | USB | good | Optional tranparency unit supported | SnapScan (1.4) | sane-snapscan
SnapScan e52 | USB | good | Optional tranparency unit supported | SnapScan (1.4) | sane-snapscan
SnapScan e60 | USB | untested |  | SnapScan (1.4) | sane-snapscan
Snapscan Touch | USB | complete |  | niash (0.2, NEW!) | sane-niash
StudioScan | SCSI | good |  | microtek (0.13.1) | sane-microtek
StudioScan II | SCSI | good |  | microtek (0.13.1) | sane-microtek
StudioScan IIsi | SCSI | good |  | microtek (0.13.1) | sane-microtek
Studiostar | SCSI | minimal | Is detected but scans are very dark | microtek (0.13.1) | sane-microtek

### Manufacturer: Ambir

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Visigo A4 | USB | unsupported | Not supported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Apple

Link(s): http://developer.apple.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Apple Scanner | SCSI | good | 4bit, 16 shades of gray | apple (unmaintained) | sane-apple
ColorOneScanner | SCSI | minimal | truecolor (needs much work) but it scans in non color modes. | apple (unmaintained) | sane-apple
OneScanner | SCSI | basic | 8bit, 256 shades of gray. The backend needs work especially in the quantization code but it may work. | apple (unmaintained) | sane-apple

### Manufacturer: Aries

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Scan-It Pro 4800 | Parport (SPP, EPP) | complete | use driver-switch mov=2 | plustek_pp (0.43) | sane-plustek_pp

### Manufacturer: ArmorPlate

Link(s): http://www.armorplate.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
AmplScan II | SCSI | complete | AmplScan *II*, not AmplScan! | template (0.42, NEW!) | sane-template

### Manufacturer: Artec/Ultima

Link(s): http://www.artecusa.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
1236 USB | USB | unsupported | Unsupported. Vendor/product 0x05d8/0x4001. See link for details. | unsupported (2005-07-30) | ?
A6000C | SCSI | complete | all modes working | artec (unmaintained) | sane-artec
A6000C PLUS | SCSI | complete | f/w <= v1.92 basic, f/w >= v1.93 OK | artec (unmaintained) | sane-artec
AM12e+ | Parport | unsupported | Unsupported. Chipset unknown. Maybe similar to SCSI version or as6e? | unsupported (2005-07-30) | ?
AM12S | SCSI | complete | all modes working | artec (unmaintained) | sane-artec
AS6E | Parport | basic | Requires the program 'as6edriver' to run. | as6e (0.4.2) | sane-as6e
AT3 | SCSI | complete | all modes working | artec (unmaintained) | sane-artec
AT6 | SCSI | minimal | First scan works, subsequent fail until scanner power cycle. | artec (unmaintained) | sane-artec
AT12 | SCSI | complete | all modes working | artec (unmaintained) | sane-artec
E+ 48U | USB | good | CIS scanner based on the GT6816 chip. Apparently all other devices are re-badged Artec scanners. | artec_eplus48u (0.0.10) | sane-artec_eplus48u
E+ Pro | USB | minimal | Experimental! Different product id: 0x4004. Please report your results! | artec_eplus48u (0.0.10) | sane-artec_eplus48u
Ultima 2000 | USB | good | Works, only product id 0x4002 is supported | gt68xx (1.0-71) | sane-gt68xx
Ultima 2000 (0x4001) | USB | unsupported | Same name, but different ids: vendor/product 0x05d8/0x4001 is not supported. The scanner with product id 0x4002 is supported by the gt68xx backend. | unsupported (2005-07-30) | ?
Ultima 2000 e+ | USB | good | Works, only limited testing until now | gt68xx (1.0-71) | sane-gt68xx

### Manufacturer: Avigramm

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Minidoc | USB | unsupported | Not supported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Avision

Link(s): http://www.avision.com, http://www.avision.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
AV100CS | SCSI | untested |  | avision (Build: 167) | sane-avision
AV100IIICS | SCSI | untested |  | avision (Build: 167) | sane-avision
AV100S | SCSI | untested |  | avision (Build: 167) | sane-avision
AV120 | USB | basic | sheetfed scanner | avision (Build: 167) | sane-avision
AV210 | USB | basic | sheetfed scanner | avision (Build: 167) | sane-avision
AV210-2 | USB | basic | sheetfed scanner | avision (Build: 167) | sane-avision
AV220 | USB | complete | duplex! sheetfed scanner | avision (Build: 167) | sane-avision
AV220-C2 | USB | untested | duplex! sheetfed scanner | avision (Build: 167) | sane-avision
AV240SC | SCSI | untested |  | avision (Build: 167) | sane-avision
AV260CS | SCSI | untested |  | avision (Build: 167) | sane-avision
AV360CS | SCSI | untested |  | avision (Build: 167) | sane-avision
AV363CS | SCSI | untested |  | avision (Build: 167) | sane-avision
AV420CS | SCSI | untested |  | avision (Build: 167) | sane-avision
AV600U | USB | good | 1 pass, 600 dpi | avision (Build: 167) | sane-avision
AV600U Plus | USB | untested | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV610 | USB | good |  | avision (Build: 167) | sane-avision
AV620CS | SCSI | complete | 1 pass, 600 dpi | avision (Build: 167) | sane-avision
AV620CS Plus | SCSI | complete | 1 pass, 1200 dpi | avision (Build: 167) | sane-avision
AV630CS | SCSI | complete | 1 pass, 1200 dpi - regularly tested | avision (Build: 167) | sane-avision
AV630CSL | SCSI | untested | 1 pass, 1200 dpi | avision (Build: 167) | sane-avision
AV660S | SCSI | untested | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV680S | SCSI | untested | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV690U | SCSI | untested | 1 pass, 2400 dpi | avision (Build: 167) | sane-avision
AV800S | SCSI | untested | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV810C | SCSI | untested | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV820 | SCSI | untested | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV820C | SCSI | good | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV820C Plus | SCSI | untested | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV830C | SCSI | untested | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV830C Plus | SCSI | untested | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV880 | SCSI | untested | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV880C | SCSI | untested | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV3200C | SCSI | complete | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV3800C | SCSI | good | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV6120 | SCSI | untested |  | avision (Build: 167) | sane-avision
AV6240 | SCSI | complete | 1 pass, ??? dpi | avision (Build: 167) | sane-avision
AV8000S | SCSI | complete | 1 pass, 1200 dpi, A3 - regularly tested | avision (Build: 167) | sane-avision
AV8300 | USB | complete | 1 pass, 1200 dpi, A3 - duplex! | avision (Build: 167) | sane-avision
AV8350 | USB | complete | 1 pass, 1200 dpi, A3 - duplex! | avision (Build: 167) | sane-avision
AVA3 | SCSI | basic | 1 pass, 600 dpi, A3 | avision (Build: 167) | sane-avision
AVA6 | USB | untested | probably a CPU-less device | avision (Build: 167) | sane-avision
DS310F | Parport | unsupported | Probably not supported. Scanner/printer/copier combination. | unsupported (2005-07-30) | ?
DS610CU Scancopier | USB | good | 1 pass, 600 dpi, A4 | avision (Build: 167) | sane-avision
iVina 1600 | USB | unsupported | GL646 based, to be added to genesys backend. Same as UMAX Astra 4500. | unsupported (2005-07-30) | ?
iVina FB1800 | USB | unsupported | GL646/GL660 based. Same as UMAX Astra 4700. | unsupported (2005-07-30) | ?
iVina FB2400 | USB | unsupported | Not supported. No chipset information available. Same as UMAX Astra 6700. | unsupported (2005-07-30) | ?

### Manufacturer: Bell and Howell

Link(s): http://www.bhscanners.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
COPISCAN II 2135 | SCSI | untested | Simplex Scanner | bh (1.0-4) | sane-bh
COPISCAN II 2137(A) | SCSI | good | Simplex Scanner (with ACE) - limited testing | bh (1.0-4) | sane-bh
COPISCAN II 2138A | SCSI | untested | Simplex Scanner with ACE | bh (1.0-4) | sane-bh
COPISCAN II 3238 | SCSI | untested | Simplex Scanner | bh (1.0-4) | sane-bh
COPISCAN II 3338(A) | SCSI | untested | Simplex Scanner (with ACE) | bh (1.0-4) | sane-bh
COPISCAN II 6338 | SCSI | good | Duplex Scanner with ACE - development model | bh (1.0-4) | sane-bh

### Manufacturer: Benq (Acer)

Link(s): http://www.benq.com
Comment: Formerly Acer Peripherals

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
300f | SCSI | good |  | SnapScan (1.4) | sane-snapscan
310p | Parport | unsupported | Unsupported. No details about the protocol known. | unsupported (2005-07-30) | ?
310s | SCSI | good |  | SnapScan (1.4) | sane-snapscan
310u | USB | good |  | SnapScan (1.4) | sane-snapscan
320p | Parport | unsupported | Unsupported. No details about the protocol known. | unsupported (2005-07-30) | ?
320u | USB | good |  | SnapScan (1.4) | sane-snapscan
340u | USB | good |  | SnapScan (1.4) | sane-snapscan
610p | Parport | unsupported | Unsupported. No details about the protocol known. | unsupported (2005-07-30) | ?
610plus | SCSI | good |  | SnapScan (1.4) | sane-snapscan
610s | SCSI | good |  | SnapScan (1.4) | sane-snapscan
620p | Parport | unsupported | Unsupported. No details about the protocol known. | unsupported (2005-07-30) | ?
620pt | Parport | unsupported | Unsupported. No details about the protocol known. | unsupported (2005-07-30) | ?
620s | SCSI | good |  | SnapScan (1.4) | sane-snapscan
620u | USB | good | Optional tranparency unit supported | SnapScan (1.4) | sane-snapscan
640BT | USB | good | Optional tranparency unit supported | SnapScan (1.4) | sane-snapscan
640bu | USB | good |  | SnapScan (1.4) | sane-snapscan
640p | Parport | unsupported | Unsupported. Someone is working to ge this scanner supported. See link for details. | unsupported (2005-07-30) | ?
640u | USB | good | Optional tranparency unit supported | SnapScan (1.4) | sane-snapscan
1240 | USB | good | Optional tranparency unit supported | SnapScan (1.4) | sane-snapscan
3300 | USB | good |  | SnapScan (1.4) | sane-snapscan
4300 | USB | good |  | SnapScan (1.4) | sane-snapscan
5000 | USB | basic | Working up to 600 DPI | SnapScan (1.4) | sane-snapscan
5300 | USB | basic | Problems with firmware upload reported | SnapScan (1.4) | sane-snapscan

### Manufacturer: BlackWidow

Link(s): http://www.blackwidow.co.uk/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
BW4800SP | SCSI | complete | rebadged Artec AT3 | artec (unmaintained) | sane-artec

### Manufacturer: Boeder

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Sm@rtScan Office | Parport USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
Sm@rtScan Slim Edition | USB | good | Similar to Artec Ultima 2000 | gt68xx (1.0-71) | sane-gt68xx

### Manufacturer: BrightScan

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
BrighScan OpticPro | Parport (SPP, EPP) | complete | Reported as P12 | plustek_pp (0.43) | sane-plustek_pp

### Manufacturer: Brother

Link(s): http://www.brother.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
MFC 4600 | Parport USB | unsupported | Unsupported. However there is a project to support this scanner/printer/fax combination. See link. | unsupported (2005-07-30) | ?

### Manufacturer: Canon

Link(s): http://www.canon.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
CanoScan 300 | SCSI | good | 1 pass; flatbed scanner | canon (1.12) | sane-canon
CanoScan 600 | SCSI | good | 1 pass; flatbed scanner | canon (1.12) | sane-canon
CanoScan 620S | SCSI | good | 1 pass; flatbed scanner | canon (1.12) | sane-canon
CanoScan 1200S | SCSI | good | 1 pass; flatbed scanner | canon (1.12) | sane-canon
CanoScan 2700F | SCSI | good | 1 pass; film scanner | canon (1.12) | sane-canon
CanoScan 2710S | SCSI | good | 1 pass; 36bit film scanner | canon (1.12) | sane-canon
CanoScan 3000 | USB | unsupported | GL660+GL646 based. | unsupported (2005-07-30) | ?
CanoScan 3000ex | USB | unsupported | GL660+GL646 based. | unsupported (2005-07-30) | ?
CanoScan 3000F | USB | unsupported | GL660+GL646 based. | unsupported (2005-07-30) | ?
CanoScan 3200F | USB | unsupported | Probably unsupported. See link. | unsupported (2005-07-30) | ?
CanoScan 4200F | USB | unsupported | Probably unsupported. See link. | unsupported (2005-07-30) | ?
CanoScan 5000F | USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
CanoScan 5200F | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
CanoScan 8000F | USB | unsupported | Not supported. USB Vendor/product 0x04a9/0x220f. See link for more information. With transparency adapter. | unsupported (2005-07-30) | ?
CanoScan 8400F | USB | unsupported | GL841 based, to be added to genesys backend | unsupported (2005-07-30) | ?
CanoScan 9900F | USB | unsupported | Probably unsupported, similar to 8000F. Vendor/product 0x04a9/0x2210. 3200x6400 dpi USB2. With transparency adapter. | unsupported (2005-07-30) | ?
CanoScan D646U | USB | unsupported | Probably not supported. USB Vendor/product 0x04a9/0x220b. See link for more information and test program. | unsupported (2005-07-30) | ?
CanoScan D646U ex | USB | unsupported | Probably not supported. See D646. | unsupported (2005-07-30) | ?
CanoScan D660U | USB | good | TPA scans not perfect | plustek (0.49) | sane-plustek
CanoScan D1250U2 | USB | unsupported | Not supported. However, someone started working on this scanner and some information is available (see link). | unsupported (2005-07-30) | ?
CanoScan D2400UF | USB | unsupported | Not supported. See link. | unsupported (2005-07-30) | ?
CanoScan FB310P | Parport (ECP) | unsupported | Rebadged Avision, different command set | canon_pp (0.33) | sane-canon_pp
CanoScan FB320P | Parport (ECP) | basic | Newly added support | canon_pp (0.33) | sane-canon_pp
CanoScan FB330P | Parport (ECP) | good |  | canon_pp (0.33) | sane-canon_pp
CanoScan FB610P | Parport (ECP) | unsupported | Rebadged Avision, different command set | canon_pp (0.33) | sane-canon_pp
CanoScan FB620P | Parport (ECP) | basic | Newly added support | canon_pp (0.33) | sane-canon_pp
CanoScan FB620U | USB | unsupported | Probably not supported. Vendor/product 0x4a9/0x2202. Some information is available. | unsupported (2005-07-30) | ?
CanoScan FB630P | Parport (ECP) | good |  | canon_pp (0.33) | sane-canon_pp
CanoScan fb630u | USB | good | OK | canon630u (0.1) | sane-canon630u
CanoScan fb636u | USB | untested | hopefully works | canon630u (0.1) | sane-canon630u
CanoScan FB1210U | USB | unsupported | Not supported. Vendor/product 0x4a9/0x2205. However, a stand-alone program for FreeBSD is available. | unsupported (2005-07-30) | ?
CanoScan LiDE 35 | USB | unsupported | GL841 based, to be added to genesys backend. Same as LiDE 50. | unsupported (2005-07-30) | ?
CanoScan LiDE 40 | USB | unsupported | GL841 based, to be added to genesys backend. Same as LiDE 50. | unsupported (2005-07-30) | ?
CanoScan LiDE 50 | USB | unsupported | GL841 based, to be added to genesys backend | unsupported (2005-07-30) | ?
CanoScan LiDE 80 | USB | unsupported | GL841 based, to be added to genesys backend | unsupported (2005-07-30) | ?
CanoScan LiDE 500F | USB | unsupported | GL841 based, to be added to genesys backend | unsupported (2005-07-30) | ?
CanoScan LiDE20 | USB | complete |  | plustek (0.49) | sane-plustek
CanoScan LiDE30 | USB | complete |  | plustek (0.49) | sane-plustek
CanoScan N340P | Parport (ECP) | good |  | canon_pp (0.33) | sane-canon_pp
CanoScan N640P | Parport (ECP) | good |  | canon_pp (0.33) | sane-canon_pp
CanoScan N640P ex | Parport (ECP) | good | Just an N640P in a different box? | canon_pp (0.33) | sane-canon_pp
CanoScan N650U/N656U | USB | complete |  | plustek (0.49) | sane-plustek
CanoScan N670U/N676U | USB | complete |  | plustek (0.49) | sane-plustek
CanoScan N1220U | USB | complete |  | plustek (0.49) | sane-plustek
CanoScan N1240U | USB | complete |  | plustek (0.49) | sane-plustek
DR-2080C | USB SCSI | unsupported | Probably not supported. Pass-trough (ADF) scanner. | unsupported (2005-07-30) | ?
DR-3020C | SCSI | unsupported | Not supported. High-speed pass-trough (ADF) scanner. | unsupported (2005-07-30) | ?
DR-3060 | SCSI | unsupported | Probably not supported. High-speed pass-trough (ADF) scanner. | unsupported (2005-07-30) | ?
DR-3080C | SCSI | unsupported | Probably not supported. High-speed pass-trough (ADF) color scanner. | unsupported (2005-07-30) | ?
DR-6080 | USB SCSI | unsupported | Probably not supported. High-speed pass-trough (ADF) scanner. | unsupported (2005-07-30) | ?
DR-9080C | SCSI | unsupported | Probably not supported. High-speed pass-trough (ADF) color scanner. Similar to DR-6080C, but can scan in color. | unsupported (2005-07-30) | ?
FS4000 | USB SCSI | unsupported | Not supported. USB Vendor/product 0x04a9/0x3042. See link for more details. | unsupported (2005-07-30) | ?
IS 12 | USB | unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers. | unsupported (2005-07-30) | ?
IS 22 | Parport | unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers. | unsupported (2005-07-30) | ?
IS 32 | USB | unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers. | unsupported (2005-07-30) | ?
IS 52 | ? | unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers. | unsupported (2005-07-30) | ?
PIXMA MP110 | USB | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Chinon

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
DS-3000 | Parport Serial Port | unsupported | Unsupported at the moment, but a backend is in preparation. See link. | unsupported (2005-07-30) | ?

### Manufacturer: Compaq

Link(s): http://www.compaq.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
S4-100 | USB | complete | Identical to UMAX 3400 | plustek (0.49) | sane-plustek
S200 | USB | unsupported | Not supported. 2400x1200 dpi. Vendor=0x049f, Product=0x0021. One bulk-in, one bulk-out and one interrupt endpoint. Type-number: U0001-HB21, another type nr on the inside: 75100512-00 | unsupported (2005-07-30) | ?

### Manufacturer: Compeye

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Simplex 1236C | Parport USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Corex

Link(s): http://www.cardscan.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Cardscan 500 | USB | unsupported | Probably not supported. Businesscard reader. Vendor/product: 0x08f0/0x0001. | unsupported (2005-07-30) | ?

### Manufacturer: Cybercom

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
9352 | Parport (EPP) | good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp

### Manufacturer: Dell

Link(s): http://www.dell.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
922 | USB | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?
1600n | USB Ethernet | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?
A920 | USB | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?
A960 | USB | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Devcom

Link(s): http://www.blackwidow.co.uk/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
9630S | SCSI | untested |  | pie (1.0) | sane-pie
9636PRO | SCSI | good |  | pie (1.0) | sane-pie
9636S | SCSI | untested |  | pie (1.0) | sane-pie

### Manufacturer: Dextra

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
DF-600P | SCSI | good | sub model VM3510 | teco1 (1.0-10) | sane-teco1
DF-1200T+ | SCSI | untested | sub model VM3530+ | teco1 (1.0-10) | sane-teco1
DF-4830T | SCSI | untested | sub model VM4542 | teco1 (1.0-10) | sane-teco1
DF-9624 | SCSI | untested | sub model VM6530+ | teco1 (1.0-10) | sane-teco1

### Manufacturer: E-Lux

Comment: E-Lux and Enhans seem to have been purchased by dysan, now known as MEMOREX

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
j-6121 | Parport | unsupported | Probably unsupported. Sold 1998. Same as E-Lux j-6121. | unsupported (2005-07-30) | ?

### Manufacturer: EDGE

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
KTX-9600US | SCSI | untested | no feedback | umax (1.0-41) | sane-umax

### Manufacturer: Enhans

Comment: E-Lux and Enhans seem to have been purchased by dysan, now known as MEMOREX

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
j-6121 | Parport | unsupported | Probably unsupported. Sold 1998. Same as E-Lux j-6121. | unsupported (2005-07-30) | ?
M-3630 A | Parport | unsupported | Probably unsupported. | unsupported (2005-07-30) | ?

### Manufacturer: Epson

Link(s): http://www.epson.com/, http://www.epson.com

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Actionscanner II | SCSI Parport | good | US version of GT-5000 | epson (0.2.42) | sane-epson
CX-3200 | USB | good |  | epson (0.2.42) | sane-epson
CX-3600 | USB | good |  | epson (0.2.42) | sane-epson
CX-3650 | USB | good |  | epson (0.2.42) | sane-epson
CX-4600 | USB | good |  | epson (0.2.42) | sane-epson
CX-5200 | USB | good |  | epson (0.2.42) | sane-epson
CX-5400 | USB | good |  | epson (0.2.42) | sane-epson
CX-6400 | USB | good |  | epson (0.2.42) | sane-epson
ES-300C | SCSI Parport | good | US version of GT-6000 | epson (0.2.42) | sane-epson
ES-600C | Parport | good | US version of GT-6500 | epson (0.2.42) | sane-epson
ES-1200C | Parport | good | US version of GT-9000 | epson (0.2.42) | sane-epson
ES-8500 | SCSI | good |  | epson (0.2.42) | sane-epson
Expression 636 | SCSI | complete | US version of GT-9500 | epson (0.2.42) | sane-epson
Expression 800 | SCSI | complete |  | epson (0.2.42) | sane-epson
Expression 1600 | SCSI USB IEEE-1394 | complete |  | epson (0.2.42) | sane-epson
Expression 1680 | SCSI USB IEEE-1394 | complete |  | epson (0.2.42) | sane-epson
FilmScan 200 | SCSI | unsupported | A better backend for the FilmScan 200 can be found at http://www.vjet.demon.co.uk/scanner/ | epson (0.2.42) | sane-epson
GT-5000 | SCSI Parport | good |  | epson (0.2.42) | sane-epson
GT-5500 | SCSI | good |  | epson (0.2.42) | sane-epson
GT-6000 | SCSI Parport | good |  | epson (0.2.42) | sane-epson
GT-6500 | Parport | good |  | epson (0.2.42) | sane-epson
GT-7000 | SCSI | good |  | epson (0.2.42) | sane-epson
GT-8000 | SCSI | good |  | epson (0.2.42) | sane-epson
GT-F600 | USB | unsupported | Unsupported. Doesn't speak ESC/I. Closely related to the GT-9400. It will be supported by epkowa backeend in future. | unsupported (2005-07-30) | ?
Perfection 600 | SCSI | good | OK, SCSI-ID=EPSON Perfection600 | umax (1.0-41) | sane-umax
Perfection 610 | USB | complete |  | epson (0.2.42) | sane-epson
Perfection 636S | SCSI | complete | US version of GT-7000 | epson (0.2.42) | sane-epson
Perfection 636U | USB | complete |  | epson (0.2.42) | sane-epson
Perfection 640 | USB | complete |  | epson (0.2.42) | sane-epson
Perfection 660 | USB | good |  | SnapScan (1.4) | sane-snapscan
Perfection 1200Photo | USB | complete | with TPU | epson (0.2.42) | sane-epson
Perfection 1200S | SCSI | complete |  | epson (0.2.42) | sane-epson
Perfection 1200U | USB | complete |  | epson (0.2.42) | sane-epson
Perfection 1240 | SCSI USB | complete |  | epson (0.2.42) | sane-epson
Perfection 1250 | USB | complete |  | plustek (0.49) | sane-plustek
Perfection 1250Photo | USB | good | TPA scans not perfect | plustek (0.49) | sane-plustek
Perfection 1260 | USB | complete |  | plustek (0.49) | sane-plustek
Perfection 1260Photo | USB | good | TPA scans not perfect | plustek (0.49) | sane-plustek
Perfection 1270 | USB | good |  | SnapScan (1.4) | sane-snapscan
Perfection 1640 | SCSI USB | complete |  | epson (0.2.42) | sane-epson
Perfection 1650 | USB | complete |  | epson (0.2.42) | sane-epson
Perfection 1660 | USB | complete |  | epson (0.2.42) | sane-epson
Perfection 1670 | USB | good |  | SnapScan (1.4) | sane-snapscan
Perfection 2400 | USB | complete |  | epson (0.2.42) | sane-epson
Perfection 2450 | USB IEEE-1394 | complete |  | epson (0.2.42) | sane-epson
Perfection 2480 | USB | good |  | SnapScan (1.4) | sane-snapscan
Perfection 2580 | USB | basic | Problems with preview scans reported, unplugging transparency unit seems to help | SnapScan (1.4) | sane-snapscan
Perfection 3200 | USB | complete | US version of the GT-9800 | epson (0.2.42) | sane-epson
Perfection 4180 | USB | unsupported | Unsupported. Doesn't speak ESC/I. Closely related to the GT-9400. It will be supported by epkowa backeend in future. | unsupported (2005-07-30) | ?
Perfection 4870 | USB | complete | US version of the GT-9800 | epson (0.2.42) | sane-epson
RX-425 | USB | good |  | epson (0.2.42) | sane-epson
RX-500 | USB | good |  | epson (0.2.42) | sane-epson
RX-600 | USB | good |  | epson (0.2.42) | sane-epson

### Manufacturer: Escom

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Image Scanner 256 | SCSI | good | OK, SCSI-ID=UMAX UG 80 | umax (1.0-41) | sane-umax

### Manufacturer: Escort

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Galleria 600 | SCSI | untested | untested, SCSI-ID=ESCORT Galleria 600S | umax (1.0-41) | sane-umax

### Manufacturer: Fujitsu

Link(s): http://www.fujitsu.com, http://www.fujitsu.com/services/computing/peripheral/scanners/product/, http://www.fujitsu.com/, http://www.fcpa.fujitsu.com/products/scanners/, http://www.fujitsu.ca/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
1200CUS | USB | basic | Works, but is slow. Maybe a Mustek BearPaw 2400 CU clone? | gt68xx (1.0-71) | sane-gt68xx
fi-4010C | USB | unsupported | Unsupported. Vendor/product: 0x04c5, 0x1029. Maybe similar to fi-4220C? | unsupported (2005-07-30) | ?
fi-4110CU | USB | unsupported | Unsupported. Vendor/product unknown. Maybe similar to fi-4220C? | unsupported (2005-07-30) | ?
fi-4110EOX2 | USB | unsupported | Uses ma1509 chip, but very different from other scanners supported by backend | ma1509 (1.0-3) | sane-ma1509
fi-4120C | SCSI USB | basic |  | fujitsu (1.12) | sane-fujitsu
fi-4220C | SCSI USB | basic |  | fujitsu (1.12) | sane-fujitsu
fi-4340C | SCSI | basic | Color scans are inverted, Flatbed option is enabled | fujitsu (1.12) | sane-fujitsu
fi-4530C | SCSI USB | basic | USB untested | fujitsu (1.12) | sane-fujitsu
M3091DCd | SCSI | good |  | fujitsu (1.12) | sane-fujitsu
M3092DCd | SCSI | good |  | fujitsu (1.12) | sane-fujitsu
M3093GDim | SCSI | good |  | fujitsu (1.12) | sane-fujitsu
M3093GXim | SCSI | good |  | fujitsu (1.12) | sane-fujitsu
M3096G | SCSI | good |  | fujitsu (1.12) | sane-fujitsu
M4097 | SCSI | good |  | fujitsu (1.12) | sane-fujitsu
ScanPartner | SCSI | untested |  | avision (Build: 167) | sane-avision
ScanPartner 10 | SCSI | untested |  | avision (Build: 167) | sane-avision
ScanPartner 10C | SCSI | untested |  | avision (Build: 167) | sane-avision
ScanPartner 15C | SCSI | good |  | sp15c (unmaintained) | sane-sp15c
ScanPartner 93GX | SCSI | good |  | fujitsu (1.12) | sane-fujitsu
ScanPartner 300C | SCSI | untested |  | avision (Build: 167) | sane-avision
ScanPartner 600C | SCSI | good |  | sp15c (unmaintained) | sane-sp15c
ScanPartner 620C | SCSI | good |  | avision (Build: 167) | sane-avision
ScanPartner Jr | SCSI | untested |  | avision (Build: 167) | sane-avision
ScanStation | SCSI | untested |  | avision (Build: 167) | sane-avision

### Manufacturer: Gallery

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
4800 | Parport (EPP) | good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp

### Manufacturer: Genius

Link(s): http://www.genius-kye.com/, http://www.geniusmouse.co.uk/, http://www.geniusnet.com.tw/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
ColorPage HR6 V1 | USB | basic |  | u12 (0.02) | sane-u12
Colorpage HR6 V2 | USB | complete |  | plustek (0.49) | sane-plustek
Colorpage HR6A | USB | untested |  | plustek (0.49) | sane-plustek
Colorpage HR6X | USB | untested |  | plustek (0.49) | sane-plustek
Colorpage HR6X EPP | Parport (SPP, EPP) | good | Negative scanning does not work correctly | plustek_pp (0.43) | sane-plustek_pp
ColorPage HR6X Slim | USB | unsupported | GL646 based, to be added to genesys backend | unsupported (2005-07-30) | ?
Colorpage HR7 | USB | complete |  | plustek (0.49) | sane-plustek
Colorpage HR7LE | USB | untested |  | plustek (0.49) | sane-plustek
ColorPage HR7X | USB | unsupported | GL646 based, to be added to genesys backend | unsupported (2005-07-30) | ?
ColorPage HR8 | USB | unsupported | GL841 based, to be added to genesys backend | unsupported (2005-07-30) | ?
Colorpage Vivid 1200 XE | USB | good |  | gt68xx (1.0-71) | sane-gt68xx
ColorPage Vivid III USB | USB | untested | Note: Device has Plustek vendor and product ID (0x07b3/0x0001) | u12 (0.02) | sane-u12
Colorpage Vivid III V2 | Parport (SPP, EPP) | complete | Reported as PT12 | plustek_pp (0.43) | sane-plustek_pp
Colorpage Vivid Pro II Film | Parport (SPP, EPP) | complete | Reported as OP9636T/12000T | plustek_pp (0.43) | sane-plustek_pp
Colorpage Vivid3 V2 | USB | good | Same as Colorpage Vivid3x | gt68xx (1.0-71) | sane-gt68xx
Colorpage Vivid3x | USB | good |  | gt68xx (1.0-71) | sane-gt68xx
Colorpage Vivid3xe | USB | good |  | gt68xx (1.0-71) | sane-gt68xx
Colorpage Vivid4 | USB | good | Works. | gt68xx (1.0-71) | sane-gt68xx
Colorpage Vivid4x | USB | good | Works. | gt68xx (1.0-71) | sane-gt68xx
Colorpage Vivid4xe | USB | basic | Should work but has limited testing. Please contact me if you own such a device. | gt68xx (1.0-71) | sane-gt68xx
ColorPage-EP | Parport | good |  | microtek2 (0.96) | sane-microtek2
ColorPage-HR5 (Pro) | SCSI | good | OK, SCSI-ID=KYE ColorPage-HR5 | umax (1.0-41) | sane-umax
ColorPage-SF600 | USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
ColorPage-Slim 1200 USB2 | USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
Colorpage-SP2 | SCSI | good | Same as Microtek Scanmaker E3 | microtek (0.13.1) | sane-microtek
FS-1130 Colorpage Scanner | SCSI | good |  | leo (1.0-10) | sane-leo

### Manufacturer: Googlegear

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
2000 | USB | good | Same as Artec Ultima 2000. | gt68xx (1.0-71) | sane-gt68xx

### Manufacturer: Guillemot

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Maxi Scan A4 Parallel 36 bit | Parport | unsupported | Probably unsupported. Identical to the Benq Prisa 620P. | unsupported (2005-07-30) | ?
SCAN@HOME 48 USB | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Guillemot / Hercules

Link(s): http://www.guillemot.com

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Maxi A4 36 bit | USB | good | Rebadged Benq 620U, needs Benq firmware file u96v???.bin | SnapScan (1.4) | sane-snapscan
Maxi Scan A4 Deluxe (SCSI) | SCSI | good | Rebadged SnapScan 310s. | SnapScan (1.4) | sane-snapscan
Maxi Scan A4 USB 640U | USB | good | Rebadged Benq 640U. | SnapScan (1.4) | sane-snapscan
Scan@home Touch 1248 (USB) | USB | good | Rebadged Benq 3300. | SnapScan (1.4) | sane-snapscan

### Manufacturer: Hercules

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
SCAN@HOME 48 USB | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Hewlett-Packard

Link(s): http://www.hp.com, http://www.hp.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
HP3500C | USB | unsupported | Doesn't work yet but support by the hp_rts88x backend is planned. | unsupported (2005-07-30) | ?
HP3530C | USB | unsupported | Doesn't work yet but support by the hp_rts88x backend is planned. | unsupported (2005-07-30) | ?
HP3570C | USB | unsupported | Doesn't work yet but support by the hp_rts88x backend is planned. | unsupported (2005-07-30) | ?
Photo Scanner 1000 | USB | unsupported | Not supported by SANE. However, it's detected as mass storage device so just mounting it is reported to work. See link for devices data. | unsupported (2005-07-30) | ?
Photosmart 1200 Photo | USB | unsupported | Probably not supported by SANE. No details known. 10x15 cm. Maybe similar to Photo Scanner 1000? | unsupported (2005-07-30) | ?
PhotoSmart PhotoScanner | SCSI | complete |  | hp (1.06) | sane-hp
Photosmart S20 (C5101A) | USB | unsupported | Not supported yet by SANE, but a backend is under development. See link for details. | unsupported (2005-07-30) | ?
Photosmart S20xi (C7150A) | USB | unsupported | Not supported yet by SANE, but a backend is under development. See link for details. | unsupported (2005-07-30) | ?
ScanJet 3c | SCSI | complete |  | hp (1.06) | sane-hp
ScanJet 3p | SCSI | complete |  | hp (1.06) | sane-hp
ScanJet 4c | SCSI | complete |  | hp (1.06) | sane-hp
ScanJet 4p | SCSI | complete |  | hp (1.06) | sane-hp
ScanJet 5p | SCSI | complete |  | hp (1.06) | sane-hp
ScanJet 5s | Parport (EPP) | minimal | Requires libieee1284 library. Only gray mode. | hpsj5s (0.03) | sane-hpsj5s
ScanJet 2100C | USB | complete |  | plustek (0.49) | sane-plustek
ScanJet 2200C | USB | complete |  | plustek (0.49) | sane-plustek
ScanJet 2300C | USB | complete | 600x1200 dpi max | genesys (1.0) | sane-genesys
ScanJet 2400c | USB | unsupported | GL646 based, to be added to genesys backend | unsupported (2005-07-30) | ?
Scanjet 3200C | Parport (EPP/ECP) | good | works (relabelled 1220P and 2000P) | umax_pp (1) | sane-umax_pp
ScanJet 3300c | USB | complete |  | niash (0.2, NEW!) | sane-niash
ScanJet 3400c | USB | complete | If you use Linux 2.6, version 2.6.8 or newer is necessary. | niash (0.2, NEW!) | sane-niash
ScanJet 3670c | USB | unsupported | GL646 based, to be added to genesys backend | unsupported (2005-07-30) | ?
ScanJet 3690c | USB | unsupported | Probably GL646_HP based, maybe can be added to genesys backend | unsupported (2005-07-30) | ?
ScanJet 3970c | USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
ScanJet 4070 Photosmart | USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
ScanJet 4100C | USB | complete |  | hp (1.06) | sane-hp
ScanJet 4300c | USB | complete | If you use Linux 2.6, version 2.6.8 or newer is necessary. | niash (0.2, NEW!) | sane-niash
ScanJet 4500C | USB | unsupported | Maybe GL841_HP, but not confirmed, maybe can be added to genesys backend | unsupported (2005-07-30) | ?
ScanJet 4570C | USB | unsupported | Maybe GL841_HP, but not confirmed, maybe can be added to genesys backend | unsupported (2005-07-30) | ?
ScanJet 4600 | USB | unsupported | Not supported. See link for details. | unsupported (2005-07-30) | ?
ScanJet 4670 | USB | unsupported | Not supported. See link for details. | unsupported (2005-07-30) | ?
ScanJet 5100C | Parport | complete | Requires ppscsi driver and epst module | hp (1.06) | sane-hp
ScanJet 5200C | Parport USB | complete | Parallel interface requires ppscsi driver and epst module | hp (1.06) | sane-hp
ScanJet 5300C | USB | complete | 1 pass, 2400 dpi - regularly tested - some FW revisions have x-axis image scaling problems over 1200 dpi | avision (Build: 167) | sane-avision
ScanJet 5370C | USB | basic | 1 pass, 2400 dpi - some FW revisions have x-axis image scaling problems over 1200 dpi | avision (Build: 167) | sane-avision
ScanJet 5400c | USB | basic |  | hp5400 (1.0-2) | sane-hp5400
ScanJet 5470c | USB | basic |  | hp5400 (1.0-2) | sane-hp5400
ScanJet 5490c | USB | basic |  | hp5400 (1.0-2) | sane-hp5400
ScanJet 5500C | USB | unsupported | Maybe GL841_HP, but not confirmed, maybe can be added to genesys backend | unsupported (2005-07-30) | ?
ScanJet 5530C Photosmart | USB | unsupported | Maybe GL841_HP, but not confirmed, maybe can be added to genesys backend | unsupported (2005-07-30) | ?
ScanJet 5550C | USB | unsupported | Maybe GL841_HP, but not confirmed, maybe can be added to genesys backend | unsupported (2005-07-30) | ?
ScanJet 5590 | USB | unsupported | Not supported. See link for details. | unsupported (2005-07-30) | ?
ScanJet 6100C | SCSI | complete |  | hp (1.06) | sane-hp
ScanJet 6200C | SCSI USB | complete |  | hp (1.06) | sane-hp
ScanJet 6250C | SCSI USB | complete |  | hp (1.06) | sane-hp
ScanJet 6300C | SCSI USB | complete |  | hp (1.06) | sane-hp
ScanJet 6350C | SCSI USB | complete |  | hp (1.06) | sane-hp
ScanJet 6390C | SCSI USB | complete |  | hp (1.06) | sane-hp
ScanJet 7400c | USB | good | 1 pass, 2400 dpi - dual USB/SCSI interface | avision (Build: 167) | sane-avision
ScanJet 7450c | USB | good | 1 pass, 2400 dpi - dual USB/SCSI interface - regularly tested | avision (Build: 167) | sane-avision
ScanJet 7490c | USB | good | 1 pass, 1200 dpi - dual USB/SCSI interface | avision (Build: 167) | sane-avision
ScanJet 8200 | USB | good | 1 pass, 4800 (?) dpi - USB 2.0 | avision (Build: 167) | sane-avision
ScanJet 8250 | USB | good | 1 pass, 4800 (?) dpi - USB 2.0 | avision (Build: 167) | sane-avision
ScanJet 8290 | USB | good | 1 pass, 4800 (?) dpi - USB 2.0 and SCSI - only SCSI tested so far | avision (Build: 167) | sane-avision
ScanJet IIc | SCSI | complete |  | hp (1.06) | sane-hp
ScanJet IIcx | SCSI | complete |  | hp (1.06) | sane-hp
ScanJet IIp | SCSI | complete |  | hp (1.06) | sane-hp
ScanJet Plus | Propietary | complete | Driver for HP parallel interface card required | hp (1.06) | sane-hp

### Manufacturer: IBM

Link(s): http://www.ibm.com/, http://www.ibm.com

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
2456 | SCSI | basic | Was reported to work long time ago. Reports are welcome. | ibm (1.0-4) | sane-ibm
ADF Color Scanner | Proprietary | unsupported | Unsupported. Uses proprietary ISA card. Maybe the same as the Plustek Spectra ADF? | unsupported (2005-07-30) | ?

### Manufacturer: iVina

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
1200U | USB | untested |  | avision (Build: 167) | sane-avision

### Manufacturer: Kodak

Link(s): http://www.kodak.com

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
i30 | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
i30 | SCSI | untested |  | avision (Build: 167) | sane-avision
i40 | SCSI | untested |  | avision (Build: 167) | sane-avision
i50 | SCSI | untested |  | avision (Build: 167) | sane-avision
i60 | SCSI | untested |  | avision (Build: 167) | sane-avision
i80 | SCSI | untested |  | avision (Build: 167) | sane-avision
Snapshot Photo Scanner 1 | Parport | unsupported | Unsupported. FCC ID HWF96PHS | unsupported (2005-07-30) | ?

### Manufacturer: Komodo

Link(s): http://www.komodo.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
S1200 | SCSI | untested | rebadged Sceptre S1200 | sceptre (1.0-10) | sane-sceptre

### Manufacturer: Konica Minolta

Link(s): http://www.konicaminolta.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
DiMAGE Scan Elite 5400 | USB IEEE-1394 | unsupported | Probably unsupported. May work with vuescan. See link for details. | unsupported (2005-07-30) | ?
DiMAGE Scan Elite 5400 2 | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
DiMAGE Scan Multi Pro | IEEE-1394 | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
Dual Scan III | USB | unsupported | Unsupported. May work with vuescan. See link for details. | unsupported (2005-07-30) | ?
Dual Scan IV | USB | unsupported | Unsupported. Works with vuescan. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: LEO

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
LEOScan S3 | SCSI | good | FCC ID LUZFS1130 | leo (1.0-10) | sane-leo

### Manufacturer: Lexmark

Link(s): http://www.lexmark.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Photo 3150 | USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
X70 | USB | good | Works, some resolutions fail at 16 bit | gt68xx (1.0-71) | sane-gt68xx
X73 | USB | good | Works, some resolutions fail at 16 bit, same as X70 | gt68xx (1.0-71) | sane-gt68xx
X74 | USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
X75 | USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
X75 PrinTrio | USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
X83 | USB | unsupported | Unsupported. Vendor/product 0x043d/0x003d. GL640. | unsupported (2005-07-30) | ?
X1130 | USB | unsupported | Unsupported. | unsupported (2005-07-30) | ?
X1150 | USB | unsupported | Unsupported. | unsupported (2005-07-30) | ?
X1180 | USB | unsupported | Unsupported. | unsupported (2005-07-30) | ?
X1185 | USB | unsupported | Unsupported. | unsupported (2005-07-30) | ?
X5130 | USB | unsupported | Unsupported. | unsupported (2005-07-30) | ?
X5250 | USB | unsupported | Unsupported. | unsupported (2005-07-30) | ?

### Manufacturer: Linotype Hell

Link(s): http://www.heidelberg.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Jade | SCSI | good | OK, SCSI-ID=LinoHell JADE | umax (1.0-41) | sane-umax
Jade | SCSI | good | OK, SCSI-ID=LinoHell Office | umax (1.0-41) | sane-umax
Jade2 | SCSI | good | OK, SCSI-ID=LinoHell Office2 | umax (1.0-41) | sane-umax
Linoscan 1400 | SCSI | good | OK, SCSI-ID=HDM LS4H1S | umax (1.0-41) | sane-umax
Opal | SCSI | untested | support disabled until tested - please contact author | umax (1.0-41) | sane-umax
Opal Ultra | SCSI | untested | support disabled until tested - please contact author | umax (1.0-41) | sane-umax
Opal2 | SCSI | good | OK; SCSI-ID=LinoHell OPAL2 | umax (1.0-41) | sane-umax
Saphir | SCSI | untested | support disabled until tested - please contact author | umax (1.0-41) | sane-umax
Saphir HiRes | SCSI | untested | support disabled until tested - please contact author | umax (1.0-41) | sane-umax
Saphir Ultra | SCSI | untested | support disabled until tested - please contact author | umax (1.0-41) | sane-umax
Saphir Ultra II | SCSI | good | OK, SCSI-ID=Linotype SAPHIR4 | umax (1.0-41) | sane-umax
Saphir2 | SCSI | good | OK, SCSI-ID=LinoHell SAPHIR2 | umax (1.0-41) | sane-umax
Saphir3 | SCSI | good | OK, SCSI-ID=LinoHell SAPHIR3 | umax (1.0-41) | sane-umax

### Manufacturer: Logitech

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
PageScan Color | Parport | unsupported | Most probably unsupported. | unsupported (2005-07-30) | ?
PageScan USB | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Medion/Lifetec/Tevion/Cytron

Link(s): http://www.medion.com, http://www.medion.com/, http://www.medion.de/
Comment: Sold by Aldi and Tchibo.

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
LT 9452 | USB | good | Similar to Mustek ScanExpress 1200 UB Plus | gt68xx (1.0-71) | sane-gt68xx
MD 4394 | USB | good | Product id 0x4002. If you have 0x4003, use artec_eplus48u backend. | gt68xx (1.0-71) | sane-gt68xx
MD 6190 | USB | unsupported | Probably unsupported. There seem to exist two different scanners with that name. See link for details. | unsupported (2005-07-30) | ?
MD 9458 | USB | good | Similar to Artec Ultima 2000 (e+?) | gt68xx (1.0-71) | sane-gt68xx
MD 9848 | Parport (EPP) | good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp
MD 40420 | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
MD 41260 | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
MD 41985 | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
MD 42666 | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
MD 90009 | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
MD/LT 935x | Parport (EPP) | good | 600x1200 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
MD/LT 985x | Parport (EPP) | good | 600x1200 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
MD/LT 9375 | USB | untested | Untested, but is reported to have the same ids as the Artec Ultima 2000. Please test. | gt68xx (1.0-71) | sane-gt68xx
MD/LT 9385 | USB | good | Similar to Artec Ultima 2000 | gt68xx (1.0-71) | sane-gt68xx
MD/LT 9890 | Parport (EPP) | good | 600x1200 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
MD4394 | USB | good | Only scanners with product id 0x4003 will work; try the gt68xx backend, if your scanner has product id 0x4002 | artec_eplus48u (0.0.10) | sane-artec_eplus48u
MD5345 | USB | good | Has a Primax USB ID | genesys (1.0) | sane-genesys
MD6228 | USB | good | Has a Primax USB ID. Same as MD5345 | genesys (1.0) | sane-genesys
MD6471 | USB | complete | Has a Primax USB ID. Same as MD5345 | genesys (1.0) | sane-genesys
MD9693 | USB | good |  | artec_eplus48u (0.0.10) | sane-artec_eplus48u
MD9705 | USB | good |  | artec_eplus48u (0.0.10) | sane-artec_eplus48u

### Manufacturer: Memorex

Link(s): http://www.artecusa.com/, http://www.memorex.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
6136u | USB | unsupported | Probably unsupported. | unsupported (2005-07-30) | ?
6142u | USB | unsupported | Probably unsupported. Same as Visioneer Onetouch 4400. See link for details. | unsupported (2005-07-30) | ?
MaxxScan 6122 | USB Parport | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
MEM 48U | USB | good | Different product id: 0x4005 | artec_eplus48u (0.0.10) | sane-artec_eplus48u
SCF 9612P | Parport | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Microstar

Link(s): http://www.microstar.de/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
MR 9791 | USB | good |  | artec_eplus48u (0.0.10) | sane-artec_eplus48u

### Manufacturer: Microtek

Link(s): http://www.microtek.com/
Comment: Microtek makes a wide variety of devices.

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
ArtixScan 2020 | SCSI | unsupported | Unsupported. Same as Agfa DuoScan T2000XL? | unsupported (2005-07-30) | ?
Artixscan 2500f | SCSI IEEE-1384 | unsupported | Unsupported. Same as Agfa DuoScan T2500? | unsupported (2005-07-30) | ?
ArtixScan 4000tf | USB | unsupported | Unsupported. Uses ALI M5611B. | unsupported (2005-07-30) | ?
Color PageWiz | SCSI (Parport) | basic | sheet-fed (preliminary, see mapage) | microtek (0.13.1) | sane-microtek
FilmScan 35 | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
Phantom 330CX | Parport | complete |  | microtek2 (0.96) | sane-microtek2
Phantom 636 | SCSI | complete |  | microtek2 (0.96) | sane-microtek2
Phantom 636CX | Parport | complete |  | microtek2 (0.96) | sane-microtek2
ScanMaker 5 | SCSI | unsupported | Probably unsupported. See link for more details. | unsupported (2005-07-30) | ?
Scanmaker 35 | SCSI | good | slide-scanner | microtek (0.13.1) | sane-microtek
Scanmaker 35t+ | SCSI | good | slide-scanner | microtek (0.13.1) | sane-microtek
Scanmaker 45t | SCSI | good | slide-scanner | microtek (0.13.1) | sane-microtek
ScanMaker 330 | SCSI | basic |  | microtek2 (0.96) | sane-microtek2
ScanMaker 336 CX | SCSI | unsupported | Probably unsupported. Seems to be similar to the Microtek 330 CX and is detected by the microtek2 backend. Scanning doesn't seem to work however. | unsupported (2005-07-30) | ?
Scanmaker 600G(S) | SCSI | basic | gray only (see manpage) | microtek (0.13.1) | sane-microtek
Scanmaker 600Z(S) | SCSI | untested |  | microtek (0.13.1) | sane-microtek
ScanMaker 630 | SCSI | basic |  | microtek2 (0.96) | sane-microtek2
ScanMaker 636 | SCSI | complete |  | microtek2 (0.96) | sane-microtek2
Scanmaker 1850S | SCSI | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
ScanMaker 3600 | USB | basic | works | sm3600 (0.1) | sane-sm3600
ScanMaker 3630 | USB | unsupported | Unsupported. Doesn't seem to be compatible to 3600 series, see link. | unsupported (2005-07-30) | ?
ScanMaker 3700 | USB | basic | works | sm3600 (0.1) | sane-sm3600
ScanMaker 3750 | USB | basic | works (told) | sm3600 (0.1) | sane-sm3600
ScanMaker 3800 | USB | unsupported | Unsupported. See link for more details. | unsupported (2005-07-30) | ?
ScanMaker 3830 | USB | unsupported | Unsupported. See link for more details. | unsupported (2005-07-30) | ?
ScanMaker 3840 | USB | good | 8 and 16 bit, color and grayscale | sm3840 (1.1, NEW!) | sane-sm3840
ScanMaker 4700 | USB | unsupported | Unsupported. See link for more details. | unsupported (2005-07-30) | ?
ScanMaker 4800 | USB | good | Same hardware as SM3840, different color box | sm3840 (1.1, NEW!) | sane-sm3840
ScanMaker 4850 | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
ScanMaker 4900 | USB | unsupported | Unsupported. See link for more details. | unsupported (2005-07-30) | ?
ScanMaker 5600 | USB | unsupported | Unsupported. See link for more details. | unsupported (2005-07-30) | ?
ScanMaker 5700 | USB | unsupported | Unsupported. Uses ALI M5615 like the ScanMaker 4700. | unsupported (2005-07-30) | ?
ScanMaker 5800 | USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
ScanMaker 5900 | USB | unsupported | Unsupported. See link for more details. | unsupported (2005-07-30) | ?
ScanMaker 6000 | USB | unsupported | Unsupported. See link for more details. | unsupported (2005-07-30) | ?
ScanMaker 6100 | USB | unsupported | Unsupported. See link for more details. | unsupported (2005-07-30) | ?
ScanMaker 6700 | USB IEEE-1394 | unsupported | Unsupported. See link. | unsupported (2005-07-30) | ?
ScanMaker 8700 | USB IEEE-1394 | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
ScanMaker 9600XL | USB SCSI IEEE-1394 | unsupported | Probably unsupported. | unsupported (2005-07-30) | ?
ScanMaker 9600XL | SCSI | good | only flatbed mode ? | microtek2 (0.96) | sane-microtek2
ScanMaker 9800XL | USB SCSI IEEE-1394 | unsupported | Unsupported. See link. | unsupported (2005-07-30) | ?
Scanmaker E2 | SCSI | good | 3-pass | microtek (0.13.1) | sane-microtek
Scanmaker E3 | SCSI | good |  | microtek (0.13.1) | sane-microtek
ScanMaker E3plus | SCSI | complete |  | microtek2 (0.96) | sane-microtek2
ScanMaker E3plus | Parport | complete |  | microtek2 (0.96) | sane-microtek2
Scanmaker E6 | SCSI | good |  | microtek (0.13.1) | sane-microtek
ScanMaker i320 | USB | unsupported | Unsupported. See link. | unsupported (2005-07-30) | ?
Scanmaker II | SCSI | good | 3-pass | microtek (0.13.1) | sane-microtek
Scanmaker IIG | SCSI | good | gray only | microtek (0.13.1) | sane-microtek
Scanmaker IIHR | SCSI | good | 3-pass | microtek (0.13.1) | sane-microtek
Scanmaker III | SCSI | good |  | microtek (0.13.1) | sane-microtek
Scanmaker IISP | SCSI | good |  | microtek (0.13.1) | sane-microtek
ScanMaker s400 | USB | unsupported | Unsupported. See link. | unsupported (2005-07-30) | ?
ScanMaker V6USL | USB | complete |  | microtek2 (0.96) | sane-microtek2
ScanMaker V6USL | SCSI | complete |  | microtek2 (0.96) | sane-microtek2
ScanMaker V300 | Parport | good |  | microtek2 (0.96) | sane-microtek2
ScanMaker V300 | SCSI | good |  | microtek2 (0.96) | sane-microtek2
ScanMaker V310 | Parport | basic |  | microtek2 (0.96) | sane-microtek2
ScanMaker V310 | SCSI | basic |  | microtek2 (0.96) | sane-microtek2
ScanMaker V600 | Parport | basic |  | microtek2 (0.96) | sane-microtek2
ScanMaker V600 | SCSI | basic |  | microtek2 (0.96) | sane-microtek2
ScanMaker X6 | SCSI | complete |  | microtek2 (0.96) | sane-microtek2
ScanMaker X6EL | SCSI | basic |  | microtek2 (0.96) | sane-microtek2
ScanMaker X6USB | USB | good |  | microtek2 (0.96) | sane-microtek2
ScanMaker X12USL | SCSI | good | only Flatbed mode ? | microtek2 (0.96) | sane-microtek2
ScanPort 3000 | USB | unsupported | Unsupported. Vendor/Product ids: 0x04a7/0x0224. Realtek RTS8801B?. See link for details. | unsupported (2005-07-30) | ?
SlimScan C3 | Parport | complete |  | microtek2 (0.96) | sane-microtek2
SlimScan C6 | USB | complete |  | microtek2 (0.96) | sane-microtek2

### Manufacturer: Minolta

Link(s): http://www.minolta.com

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Dimage Scan Dual I | SCSI | basic |  | avision (Build: 167) | sane-avision
Dimage Scan Dual II | USB | good | 1 pass, film-scanner | avision (Build: 167) | sane-avision
Dimage Scan Dual III | USB | basic | 1 pass, film-scanner | avision (Build: 167) | sane-avision
Elite II | USB | untested | 1 pass, film-scanner | avision (Build: 167) | sane-avision

### Manufacturer: Minolta-QMS

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
SC-110 | USB | untested |  | avision (Build: 167) | sane-avision
SC-215 | USB | good |  | avision (Build: 167) | sane-avision

### Manufacturer: Mitsubishi

Link(s): http://www.mitsubishi.com

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Diamondview 648UT | USB | good | Rebadged Benq 320u. | SnapScan (1.4) | sane-snapscan
Diamondview 650U | USB | good | Rebadged Benq 4300. | SnapScan (1.4) | sane-snapscan
MCA-ADFC | SCSI | untested |  | avision (Build: 167) | sane-avision
S600C | SCSI | untested |  | avision (Build: 167) | sane-avision
S1200C | SCSI | untested |  | avision (Build: 167) | sane-avision
SS600 | SCSI | good |  | avision (Build: 167) | sane-avision

### Manufacturer: Mustek

Link(s): http://www.mustek.com/, http://www.mustek.com.tw/, http://www.mustek.de/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
96 CP | Parport (EPP) | good | 300x600 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
600 III EP Plus | Parport (EPP) | good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp
1200 III EP | Parport | unsupported | Probably not supported. quarlewm at jmu dot edu offers to temporarily loan such a scanner to anyone who is interested in writing a driver. | unsupported (2005-07-30) | ?
1800 A3 Pro-1 | USB | unsupported | Not supported but someone wants to start writing a backend. See link. Vendor/Product ids: 0x055f/0x0401. No information about this scanner on any Mustek website. | unsupported (2005-07-30) | ?
2400 M | USB | unsupported | Probably unsupported. No details known. | unsupported (2005-07-30) | ?
BearPaw 1200 | USB | complete | both product versions are supported, see backends' man-page | plustek (0.49) | sane-plustek
BearPaw 1200 CS | USB | good |  | gt68xx (1.0-71) | sane-gt68xx
BearPaw 1200 CU | USB | good |  | gt68xx (1.0-71) | sane-gt68xx
BearPaw 1200 CU Plus | USB | good | Procuct id 0x021b. | gt68xx (1.0-71) | sane-gt68xx
BearPaw 1200 CU Plus | USB | good | Product id 0x021c | gt68xx (1.0-71) | sane-gt68xx
BearPaw 1200 F | USB | good | Works upto 600 dpi. No support for TA and ADF yet. | ma1509 (1.0-3) | sane-ma1509
BearPaw 1200 TA | USB | good | Transparency adapter supported | gt68xx (1.0-71) | sane-gt68xx
BearPaw 1248CU | USB | unsupported | Probably unsupported. No details known. | unsupported (2005-07-30) | ?
BearPaw 2400 | USB | complete |  | plustek (0.49) | sane-plustek
BearPaw 2400 CS | USB | untested | Probably works, reports are welcome | gt68xx (1.0-71) | sane-gt68xx
BearPaw 2400 CS Plus | USB | good | Works, problems with 12/16 bit modes? | gt68xx (1.0-71) | sane-gt68xx
BearPaw 2400 CU | USB | basic | Works, but is slow | gt68xx (1.0-71) | sane-gt68xx
BearPaw 2400 CU Plus | USB | good |  | gt68xx (1.0-71) | sane-gt68xx
BearPaw 2400 TA | USB | good | Transparency adapter supported | gt68xx (1.0-71) | sane-gt68xx
BearPaw 2400 TA Plus | USB | good | Transparency adapter supported | gt68xx (1.0-71) | sane-gt68xx
BearPaw 2400 TA Pro | USB | unsupported | Not supported. See link for some information. | unsupported (2005-07-30) | ?
BearPaw 2448 CS Plus | USB | basic | Same as 2448 TA Plus, but without TA. | gt68xx (1.0-71) | sane-gt68xx
BearPaw 2448 CU Pro | USB | unsupported | Not supported. See link for some information. | unsupported (2005-07-30) | ?
BearPaw 2448 TA Plus | USB | basic | Transparency adapter supported. Slow. Brightness depends on resolution? | gt68xx (1.0-71) | sane-gt68xx
BearPaw 2448 TA Pro | USB | unsupported | Not supported. See link for some information. | unsupported (2005-07-30) | ?
BearPaw 4800 TA Pro | USB | unsupported | Not supported. See link for some information. | unsupported (2005-07-30) | ?
BearPaw 4800 TA Pro II | USB | unsupported | Not supported. See link for some information. | unsupported (2005-07-30) | ?
P 3600 A3 Pro | USB | unsupported | Not supported. Maybe similar to the 1800 A3 Pro-1?. See link. | unsupported (2005-07-30) | ?
Paragon 600 II CD | SCSI | complete |  | mustek (1.0-138) | sane-mustek
Paragon 600 II ED | Parport | untested | Completely untested. If it's the same as the 600 II EP, it may work. Please contact me if you own such a device. | mustek (1.0-138) | sane-mustek
Paragon 600 II EP | Parport | untested | Not tested yet but should work. Please contact me if you own such a device. | mustek (1.0-138) | sane-mustek
Paragon 600 II N | Proprietary | basic | Resolutions above 300 dpi may cause trouble. | mustek (1.0-138) | sane-mustek
Paragon 800 II EP | Parport | unsupported | Not supported. Maybe similar to 600 II EP (SCSI_over-parport)? In this case it could be supported by the mustek SCSI backend. | unsupported (2005-07-30) | ?
Paragon 800 II SP | SCSI | complete |  | mustek (1.0-138) | sane-mustek
Paragon 1200 A3 Pro | SCSI | complete | ADF and TA untested. Please contact me if you own such equipment. | mustek (1.0-138) | sane-mustek
Paragon 1200 III SP | SCSI | complete |  | mustek (1.0-138) | sane-mustek
Paragon 1200 LS | SCSI | complete |  | mustek (1.0-138) | sane-mustek
Paragon 1200 SP Pro | SCSI | good |  | mustek (1.0-138) | sane-mustek
Paragon MFC-600S | SCSI | complete |  | mustek (1.0-138) | sane-mustek
Paragon MFC-800S | SCSI | complete |  | mustek (1.0-138) | sane-mustek
Paragon MFS-1200SP | SCSI | complete |  | mustek (1.0-138) | sane-mustek
Paragon MFS-6000CX | SCSI | good | 3-pass | mustek (1.0-138) | sane-mustek
Paragon MFS-6000SP | SCSI | complete |  | mustek (1.0-138) | sane-mustek
Paragon MFS-8000SP | SCSI | complete |  | mustek (1.0-138) | sane-mustek
Paragon MFS-12000CX | SCSI | good | 3-pass | mustek (1.0-138) | sane-mustek
Paragon MFS-12000SP | SCSI | complete |  | mustek (1.0-138) | sane-mustek
Plug-n-Scan 2400 M | USB | good | Works but is slow in high resolutions. Same as BearPaw 2400 CS Plus. | gt68xx (1.0-71) | sane-gt68xx
Plug-n-Scan 2400 MT | USB | good | Works but is slow in high resolutions. Same as BearPaw 2400 TA Plus. | gt68xx (1.0-71) | sane-gt68xx
ScanExpress 600 CP | Parport (EPP) | good | 300x600 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
ScanExpress 600 CU | USB | complete |  | mustek_usb (1.0-18) | sane-mustek_usb
ScanExpress 600 SEP | Parport (EPP) | good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp
ScanExpress 600 USB | USB | unsupported | Unsupported. Vendor/Product 0x055f/0x873. Programming information is available. | unsupported (2005-07-30) | ?
ScanExpress 1200 CP | Parport (EPP) | good | 600x1200 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
ScanExpress 1200 CP+ | Parport (EPP) | good | 600x1200 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
ScanExpress 1200 CU | USB | complete |  | mustek_usb (1.0-18) | sane-mustek_usb
ScanExpress 1200 CU Plus | USB | complete |  | mustek_usb (1.0-18) | sane-mustek_usb
ScanExpress 1200 FS | SCSI | untested | One report that it crashes the computer. SCSI driver issue? Please contact me if you own such a device. | mustek (1.0-138) | sane-mustek
ScanExpress 1200 UB | USB | complete | For the UB Plus, see gt68xx backend | mustek_usb (1.0-18) | sane-mustek_usb
ScanExpress 1200 UB Plus | USB | good |  | gt68xx (1.0-71) | sane-gt68xx
ScanExpress 1200 USB | USB | unsupported | Unsupported. Vendor/Product 0x055f/0x0003. Programming information is available. | unsupported (2005-07-30) | ?
ScanExpress 1200 USB Plus | USB | unsupported | Unsupported. Vendor/Product 0x055f/0x0007. | unsupported (2005-07-30) | ?
ScanExpress 1248 UB | USB | complete |  | gt68xx (1.0-71) | sane-gt68xx
ScanExpress 2400 USB | USB | minimal | Should be detected but may need some more work in the code. Testers welcome. | gt68xx (1.0-71) | sane-gt68xx
ScanExpress 6000 P | Parport (EPP) | good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp
ScanExpress 6000SP | SCSI | complete |  | mustek (1.0-138) | sane-mustek
ScanExpress 12000 P | Parport | unsupported | Not supported. Asic 1505/05. | unsupported (2005-07-30) | ?
ScanExpress 12000SP | SCSI | complete |  | mustek (1.0-138) | sane-mustek
ScanExpress 12000SP Plus | SCSI | complete |  | mustek (1.0-138) | sane-mustek
ScanExpress A3 EP | Parport | unsupported | Not supported. Maybe it will be supported by the mustek_pp backend in future. | unsupported (2005-07-30) | ?
ScanExpress A3 SP | SCSI | basic | Please test! | mustek (1.0-138) | sane-mustek
ScanExpress A3 USB | USB | basic | Still some vertical stripes. | gt68xx (1.0-71) | sane-gt68xx
ScanExpress CardSmart | USB | unsupported | Probably unsupported. USB business card scanner. Maybe works as USB storage device? | unsupported (2005-07-30) | ?
ScanMagic 600 CP | Parport (EPP) | good | 300x600 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
ScanMagic 600 II SP | SCSI | complete |  | mustek (1.0-138) | sane-mustek
ScanMagic 1200 UB Plus | USB | good | Same as ScanExpress 1200 UB Plus | gt68xx (1.0-71) | sane-gt68xx
ScanMagic 4800 P | Parport (EPP) | good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp
ScanMagic 4830S | SCSI | untested | sub model VM3575 | teco2 (1.0-9) | sane-teco2
ScanMagic 9636P | Parport | unsupported | Probably not supported. Same as Mustek 12000 P?. ASIC 1505. | unsupported (2005-07-30) | ?
ScanMagic 9636S | SCSI | complete |  | mustek (1.0-138) | sane-mustek
ScanMagic 9636S Plus | SCSI | complete |  | mustek (1.0-138) | sane-mustek
TwainScan II SP | SCSI | complete |  | mustek (1.0-138) | sane-mustek

### Manufacturer: NEC

Link(s): http://www.nevt.co.jp/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
PC-IN500/4C | SCSI | good | PC-IN500/4C was sold only in JAPAN | nec (0.12) | sane-nec
Petiscan | USB | unsupported | Most probably unsupported. See link for details. Vendor ID is 0x0475 (Relisys/Teco). Not know if it is similar to other Relisys/Teco USB scanners. | unsupported (2005-07-30) | ?

### Manufacturer: Network

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Easy Plus 30 Bit | Parport (EPP) | good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp

### Manufacturer: Nikon

Link(s): http://www.nikon.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
AX-110 / Scantouch 110 | SCSI | untested | may work, please test and give feedback | umax (1.0-41) | sane-umax
AX-210 | SCSI | good | OK | umax (1.0-41) | sane-umax
Coolscan V ED | USB | unsupported | Most probably unsupported. See link for details. | unsupported (2005-07-30) | ?
LS 30 | SCSI | complete | working -- model available to developer | coolscan2 (0.1.8) | sane-coolscan2
LS 40 ED | USB | complete |  | coolscan2 (0.1.8) | sane-coolscan2
LS 50 ED | USB | unsupported | Most probably unsupported. See link for details. | unsupported (2005-07-30) | ?
LS 2000 | SCSI | good |  | coolscan2 (0.1.8) | sane-coolscan2
LS 4000 ED | IEEE-1394 | good | needs linux kernel 2.4.19 or later | coolscan2 (0.1.8) | sane-coolscan2
LS 8000 ED | IEEE-1394 | good | needs linux kernel 2.4.19 or later | coolscan2 (0.1.8) | sane-coolscan2
LS-20 | SCSI | basic | The LS-20 has been replaced by the LS-30 | coolscan (0.4.3) | sane-coolscan
LS-30 | SCSI | basic | alpha: only 24/30 bit RGB + 32/40 bit RGBI | coolscan (0.4.3) | sane-coolscan
LS-1000 | SCSI | basic | Doesn't support gamma correction | coolscan (0.4.3) | sane-coolscan
LS-2000 | SCSI | basic | alpha: only 24/36 bit + RGB 32/48 bit RGBI | coolscan (0.4.3) | sane-coolscan
Super Coolscan LS-5000 ED | USB | unsupported | Most probably unsupported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Olivetti

Link(s): http://www.olivetti.com

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Job-Jet M400 | USB | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Olympus

Link(s): http://www.olympus.com

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
ES-10S | SCSI | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Optrox

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
PhotoMaker 3 | Parport | unsupported | Probably not supported. | unsupported (2005-07-30) | ?

### Manufacturer: Packard Bell

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Diamond 1200 | USB | good | Similar to Mustek BearPaw 1200 (Plus) | gt68xx (1.0-71) | sane-gt68xx
Diamond 1200 Plus | USB | good | Product id 0x021b. Similar to Mustek BearPaw 1200 Plus | gt68xx (1.0-71) | sane-gt68xx
Diamond 1200 Plus | USB | good | Product id 0x021c. Similar to Mustek BearPaw 1200 Plus | gt68xx (1.0-71) | sane-gt68xx
Diamond 2450 | USB | good |  | gt68xx (1.0-71) | sane-gt68xx

### Manufacturer: Panasonic

Link(s): http://www.panasonic.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
KV-S2025C | SCSI | minimal | no color, no high resolution, no automatic cropping | matsushita (1.0-7) | sane-matsushita
KV-S2026C | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-S2045C | SCSI | minimal | no color, no high resolution, no automatic cropping | matsushita (1.0-7) | sane-matsushita
KV-S2046C | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-S2055L | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-S2055W | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-S2065L | SCSI | minimal | no color, no high resolution, no automatic cropping | matsushita (1.0-7) | sane-matsushita
KV-S2065W | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-S3065CL | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-S3065CW | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-S3085 | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-S3105C | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-S6040W | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-S6045W | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-S6050W | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-S6055W | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-S7065C | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?
KV-SS25 | SCSI | complete |  | matsushita (1.0-7) | sane-matsushita
KV-SS25D | SCSI | complete |  | matsushita (1.0-7) | sane-matsushita
KV-SS50 | SCSI | untested |  | matsushita (1.0-7) | sane-matsushita
KV-SS50EX | SCSI | untested |  | matsushita (1.0-7) | sane-matsushita
KV-SS55 | SCSI | untested |  | matsushita (1.0-7) | sane-matsushita
KV-SS55EX | SCSI | minimal | no color, no high resolution, no automatic cropping | matsushita (1.0-7) | sane-matsushita
KV-SS850 | SCSI | untested |  | matsushita (1.0-7) | sane-matsushita
KV-SS855 | SCSI | untested |  | matsushita (1.0-7) | sane-matsushita
KV-SS905C | ? | unsupported | might be supported by matsushita backend. | unsupported (2005-07-30) | ?

### Manufacturer: Pentax

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
DSmobile USB | USB | unsupported | Probably not supported. Some information is available. | unsupported (2005-07-30) | ?

### Manufacturer: PIE

Link(s): http://www.scanace.com/
Comment: Pacific Image Electronics

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Powerslide 3600 | USB IEEE-1394 | unsupported | Probably unsupported. Film scanner that can scan directly from the magazine. | unsupported (2005-07-30) | ?
Primefilm 1800u | USB | unsupported | Not supported. Vendor/product 0x05e3/0x0120. See link for details. | unsupported (2005-07-30) | ?
Primefilm 3600PRO | USB IEEE-1394 | unsupported | Probably not supported. | unsupported (2005-07-30) | ?
ScanAce 630S | SCSI | untested |  | pie (1.0) | sane-pie
ScanAce 636S | SCSI | untested |  | pie (1.0) | sane-pie
ScanAce 1230S | SCSI | good |  | pie (1.0) | sane-pie
ScanAce 1236S | SCSI | good |  | pie (1.0) | sane-pie
ScanAce II | SCSI | untested |  | pie (1.0) | sane-pie
ScanAce II Plus | SCSI | untested |  | pie (1.0) | sane-pie
ScanAce III | SCSI | good |  | pie (1.0) | sane-pie
ScanAce III Plus | SCSI | untested |  | pie (1.0) | sane-pie
ScanAce Plus | SCSI | untested |  | pie (1.0) | sane-pie
ScanAce ScanMedia | SCSI | untested |  | pie (1.0) | sane-pie
ScanAce ScanMedia II | SCSI | untested |  | pie (1.0) | sane-pie
ScanAce V | SCSI | untested |  | pie (1.0) | sane-pie

### Manufacturer: PIOTECH

Link(s): http://www.image-land.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Splendeur 3024 | SCSI | good | sub model VM3552 | teco3 (1.0-1) | sane-teco3

### Manufacturer: Plustek

Link(s): http://www.plustek.com/, http://www.plustek.de/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
OptiCard 600+ | USB | unsupported | Business card reader. No further information available. | unsupported (2005-07-30) | ?
OpticBook 3600 | USB | unsupported | GL842 based (similar to GL841?), maybe ca be added to genesys backend. Bookscanner. | unsupported (2005-07-30) | ?
OpticFilm 7200 | USB | unsupported | GL841 based, to be added to genesys backend | unsupported (2005-07-30) | ?
OpticPro 600P/6000P | Parport (SPP, EPP) | complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 1212U | USB | basic |  | u12 (0.02) | sane-u12
OpticPro 1236P | Parport (SPP, EPP) | complete | reported as OpticPro 12000P/96000P | plustek_pp (0.43) | sane-plustek_pp
OpticPro 1248U | USB | good |  | gt68xx (1.0-71) | sane-gt68xx
OpticPro 2400SP | SCSI | untested | sub model VM3552 | teco3 (1.0-1) | sane-teco3
OpticPro 4800P | Parport (SPP, EPP) | complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 4830P | Parport (SPP, EPP) | complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 4831P | Parport (SPP, EPP) | complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 9600P | Parport (SPP, EPP) | complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 9630P | Parport (SPP, EPP) | complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 9630PL | Parport (SPP, EPP) | complete | use driver-switch mov=1 | plustek_pp (0.43) | sane-plustek_pp
OpticPro 9636P | Parport (SPP, EPP) | complete | use driver-switch mov=4 | plustek_pp (0.43) | sane-plustek_pp
OpticPro 9636P+/Turbo | Parport (SPP, EPP) | complete | use driver-switch mov=3 | plustek_pp (0.43) | sane-plustek_pp
OpticPro 9636T | Parport (SPP, EPP) | complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 12000P/96000P | Parport (SPP, EPP) | complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 12000T | Parport (SPP, EPP) | complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro 19200S | SCSI | complete | rebadged Artec AM12S | artec (unmaintained) | sane-artec
OpticPro A3U | USB | unsupported | Uses Plustek ASIC P99002 | unsupported (2005-07-30) | ?
OpticPro AI3 | Parport (SPP, EPP) | basic | use driver-switch mov=5, poor picture quality | plustek_pp (0.43) | sane-plustek_pp
OpticPro P8 | Parport | untested |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro P12 | Parport (SPP, EPP) | complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro PT12 | Parport (SPP, EPP) | complete |  | plustek_pp (0.43) | sane-plustek_pp
OpticPro S6 | USB | unsupported | Uses RealTek chipset (RTL8801D) | unsupported (2005-07-30) | ?
OpticPro S12 | USB | unsupported |  | unsupported (2005-07-30) | ?
OpticPro S24 | USB | unsupported | GL646 based, to be added to genesys backend | unsupported (2005-07-30) | ?
OpticPro S28 | USB | unsupported | GL841 based, to be added to genesys backend | unsupported (2005-07-30) | ?
OpticPro ST12 | USB | unsupported |  | unsupported (2005-07-30) | ?
OpticPro ST16 | USB | unsupported | GL646 based, to be added to genesys backend | unsupported (2005-07-30) | ?
OpticPro ST24 | USB | unsupported | GL646 based, to be added to genesys backend | unsupported (2005-07-30) | ?
OpticPro ST28 | USB | unsupported | GL841 based, to be added to genesys backend | unsupported (2005-07-30) | ?
OpticPro ST48 | USB | unsupported | GL841 based, to be added to genesys backend | unsupported (2005-07-30) | ?
OpticPro ST64 | USB | unsupported | No further information available. | unsupported (2005-07-30) | ?
OpticPro U12 | USB | basic | Note: Only devices with product ID 0x0001 are supported! | u12 (0.02) | sane-u12
OpticPro U12 | USB | complete | NOTE: Devices with product ID 0x0001 are not supported! | plustek (0.49) | sane-plustek
OpticPro U16B | USB | good |  | gt68xx (1.0-71) | sane-gt68xx
OpticPro U16B+ | USB | good |  | gt68xx (1.0-71) | sane-gt68xx
OpticPro U24 | USB | complete |  | plustek (0.49) | sane-plustek
OpticPro UA18 | USB | unsupported | Probably LM983x based. | unsupported (2005-07-30) | ?
OpticPro UT12 | USB | basic | Note: Only devices with product ID 0x0001 are supported! | u12 (0.02) | sane-u12
OpticPro UT12 | USB | complete | Note: Devices with product ID 0x0001 are not supported! | plustek (0.49) | sane-plustek
OpticPro UT16 | USB | complete |  | plustek (0.49) | sane-plustek
OpticPro UT16B | USB | untested | Probably works. Transparency adapter not supported yet. Please contact me if you own such a device. | gt68xx (1.0-71) | sane-gt68xx
OpticPro UT24 | USB | complete |  | plustek (0.49) | sane-plustek
OpticSlim 1200 | USB | good |  | gt68xx (1.0-71) | sane-gt68xx
OpticSlim 2400 | USB | good | Works up to 1200 dpi. | gt68xx (1.0-71) | sane-gt68xx
OpticSlim 2420 | USB | unsupported | GL841 based, to be added to genesys backend | unsupported (2005-07-30) | ?
OpticSlim M12 | USB | unsupported | Uses the GT6816 chipset. May be supported by the gt68xx backend in future. See link for details. | unsupported (2005-07-30) | ?
OpticWorks 2000 | Parport | unsupported | Multifunction device. No further information available. | unsupported (2005-07-30) | ?
Spectra ADF | Proprietary | unsupported | Unsupported. Uses proprietary ISA card that also provides power and is labelled GPS-1 PAGE-A from Taiwan. Other labels on the scanner include ADF Color Scanner and SF600AS. Maybe the same as the IBM ADF Color Scanner? | unsupported (2005-07-30) | ?

### Manufacturer: Primax

Link(s): http://www.primax.nl/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Colorado 600U | USB | unsupported | Not supported. Some information is available. | unsupported (2005-07-30) | ?
Colorado 2400U | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
Colorado 4800 | Parport (SPP, EPP) | untested | same as OpticPro 4800P | plustek_pp (0.43) | sane-plustek_pp
Colorado Direct 600 | Parport | unsupported | Not supported. However, a stand-alone program is available. | unsupported (2005-07-30) | ?
Colorado Direct 9600 | Parport | unsupported | Not supported. However, a stand-alone program is available. | unsupported (2005-07-30) | ?
Colorado USB 9600 | USB | unsupported | Not supported. See link for details. | unsupported (2005-07-30) | ?
Compact 4800 Direct | Parport (SPP, EPP) | complete | use driver-switch mov=2 | plustek_pp (0.43) | sane-plustek_pp
Compact 4800 Direct-30 | Parport (SPP, EPP) | complete | same as OpticPro 4830P, use driver-switch mov=7 | plustek_pp (0.43) | sane-plustek_pp
Compact 4800 SCSI | SCSI | complete | Mustek 600 II CD compatible | mustek (1.0-138) | sane-mustek
Compact 9600 Direct-30 | Parport (SPP, EPP) | complete | same as OpticPro 9630P | plustek_pp (0.43) | sane-plustek_pp
Jewel 4800 | SCSI | good | sub model VM356A | teco2 (1.0-9) | sane-teco2
OneTouch 5300 | Parport | unsupported | Not supported. | unsupported (2005-07-30) | ?
Primascan Colorado 2600u | USB | unsupported | Unsupported. Same as Visioneer Onetouch 4400. See link for details. | unsupported (2005-07-30) | ?
Profi 9600 | SCSI | basic | sub model VM6575 | teco2 (1.0-9) | sane-teco2
Profi 19200 | SCSI | good | sub model VM6586 | teco2 (1.0-9) | sane-teco2
Slim-Line 1200 | USB | unsupported | Maybe GL646. | unsupported (2005-07-30) | ?

### Manufacturer: Prolink

Link(s): http://www.fida.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Winscan Pro 2448U | USB | unsupported | Not supported. Some information is available. Vendor=0x06dc product=0x0014. RealTek RTS8801. | unsupported (2005-07-30) | ?

### Manufacturer: Quato

Link(s): http://www.quato.de/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
X-Finity | SCSI | unsupported | Probably not supported. No details yet. Originally manufactured by PFU? | unsupported (2005-07-30) | ?
X-Finity Ultra | USB IEEE-1394 | unsupported | Probably not supported. No details yet. | unsupported (2005-07-30) | ?

### Manufacturer: Reflecta

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
DigitDia 3600 | USB IEEE-1394 | unsupported | GL841 based, to be added to genesys backend. Film scanner that can scan directly from the magazine. | unsupported (2005-07-30) | ?
iScan 1800 | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
ProScan 4000 | USB IEEE-1394 | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Relisys

Link(s): http://www.relisys.com/, http://www.tecoimage.com.tw/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
APOLLO Express 3 | SCSI | basic | sub model VM356A | teco2 (1.0-9) | sane-teco2
APOLLO Express 6 | SCSI | good | sub model VM6565 | teco2 (1.0-9) | sane-teco2
AVEC 2400 | SCSI | complete | sub model VM3520 | teco1 (1.0-10) | sane-teco1
AVEC 2412 | SCSI | complete | sub model VM3520+ | teco1 (1.0-10) | sane-teco1
AVEC 4800 | SCSI | untested | sub model VM4530 | teco1 (1.0-10) | sane-teco1
AVEC 4816 | SCSI | untested | sub model VM4530+ | teco1 (1.0-10) | sane-teco1
AVEC II S3 | SCSI | good | sub model VM3564 | teco2 (1.0-9) | sane-teco2
AVEC Super 3 | SCSI | untested | sub model VM3575 | teco2 (1.0-9) | sane-teco2
Eclipse 1200U | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
Episode | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?
Infinity Scorpio | SCSI | good | sub model VM3552 | teco3 (1.0-1) | sane-teco3
RELI 2400 | SCSI | untested | sub model VM3530 | teco1 (1.0-10) | sane-teco1
RELI 2412 | SCSI | complete | sub model VM3530+ | teco1 (1.0-10) | sane-teco1
RELI 4816 | SCSI | complete | sub model VM4540 | teco1 (1.0-10) | sane-teco1
RELI 4830 | SCSI | good | sub model VM4542 | teco1 (1.0-10) | sane-teco1
RELI 9600 | SCSI | untested | sub model VM6530 | teco1 (1.0-10) | sane-teco1
RELI 9612 | SCSI | untested | sub model VM6530* | teco1 (1.0-10) | sane-teco1
RELI 9624 | SCSI | untested | sub model VM6530+ | teco1 (1.0-10) | sane-teco1
RELI 9630 | SCSI | untested | sub model VM6540 | teco1 (1.0-10) | sane-teco1
RELI DS6 | SCSI | untested | sub model VM3420 | teco1 (1.0-10) | sane-teco1
RELI DS15 | SCSI | untested | sub model VM3440 | teco1 (1.0-10) | sane-teco1
SCORPIO Pro | SCSI | good | sub model VM6575 | teco2 (1.0-9) | sane-teco2
SCORPIO Pro-S | SCSI | untested | sub model VM6586 | teco2 (1.0-9) | sane-teco2
SCORPIO Super 3 | SCSI | good | sub model VM3575 | teco2 (1.0-9) | sane-teco2
Scorpio Ultra 3 | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: RevScan

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
19200i | USB | good | Similar to Plustek OpticPro 1248U | gt68xx (1.0-71) | sane-gt68xx
RevScan Orange R48Ti | USB | basic | Rebadged Plustek OpticPro UT12 | u12 (0.02) | sane-u12

### Manufacturer: Ricoh

Link(s): http://www.ricoh.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
IS-410 | SCSI | untested | Untested, please report! | ibm (1.0-4) | sane-ibm
IS-420 | SCSI | basic | Works at least in flatbed mode. | ibm (1.0-4) | sane-ibm
IS-430 | SCSI | untested | Untested, please report! | ibm (1.0-4) | sane-ibm
Ricoh IS50 | SCSI | basic |  | ricoh (unmaintained) | sane-ricoh
Ricoh IS60 | SCSI | basic |  | ricoh (unmaintained) | sane-ricoh

### Manufacturer: Scanport

Link(s): http://www.scanport.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
SQ300 | Parport? | basic |  | microtek2 (0.96) | sane-microtek2
SQ2030 | Parport | basic |  | microtek2 (0.96) | sane-microtek2
SQ4836 | SCSI | basic |  | microtek2 (0.96) | sane-microtek2

### Manufacturer: Sceptre

Link(s): http://www.sceptre.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Vividscan S1200 | SCSI | basic |  | sceptre (1.0-10) | sane-sceptre

### Manufacturer: Sharp

Link(s): http://sharp-world.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
JX-250 | SCSI | good |  | sharp (0.32) | sane-sharp
JX-320 | SCSI | good |  | sharp (0.32) | sane-sharp
JX-325 | SCSI | untested |  | sharp (0.32) | sane-sharp
JX-330 | SCSI | good |  | sharp (0.32) | sane-sharp
JX-350 | SCSI | good |  | sharp (0.32) | sane-sharp
JX-610 | SCSI | good |  | sharp (0.32) | sane-sharp

### Manufacturer: Sicos

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
DMS 2000 | proprietary | unsupported | Not supported until now. Work on a backend has started, contact the author for details (see link) | unsupported (2005-07-30) | ?
SmartScan 3600 | USB IEEE-1394 | unsupported | Probably not supported. Same as PIE Primefilm 2600 PRO. | unsupported (2005-07-30) | ?

### Manufacturer: Siemens

Link(s): http://www.siemens.com/, http://www.siemens.de/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
9036 Flatbed scanner | SCSI | basic |  | s9036 (unmaintained) | sane-s9036
S9036 | SCSI | untested | gray only | agfafocus (unmaintained) | sane-agfafocus
ST400 | SCSI | basic | 6 bit gray | st400 (1.6) | sane-st400
ST800 | SCSI | basic | 6 bit gray | st400 (1.6) | sane-st400

### Manufacturer: Spot Technology

Comment: Spot seems have gone out of business.

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Maxiscan A4 | proprietary | unsupported | Not supported until now. Work on a backend has started, see link for more information. | unsupported (2005-07-30) | ?
ScanTak 2c | proprietary | unsupported | Not supported. Work on a backend has started, see link for more information. | unsupported (2005-07-30) | ?
ScanTak 3c | proprietary | unsupported | Not supported. Work on a backend has started, see link for more information. | unsupported (2005-07-30) | ?

### Manufacturer: Syscan

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
TravelScan 460/464 | USB | unsupported | Not supported. Some information is available. See link for details. | unsupported (2005-07-30) | ?
TravelScan FS-531 | USB | unsupported | Not supported. May work with the Plustek backend in future. See link for details. | unsupported (2005-07-30) | ?
TravelScan Pro | USB | unsupported | Probably not supported. Some information is available. | unsupported (2005-07-30) | ?

### Manufacturer: Tamarack

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Artiscan 6000C | SCSI | good | 3 pass, 300 DPI | tamarack (unmaintained) | sane-tamarack
Artiscan 8000C | SCSI | good | 3 pass, 400 DPI | tamarack (unmaintained) | sane-tamarack
Artiscan 9600 | Parport | unsupported | Unsupported at the moment. See link for a project for that scanner taht may support it in future. | unsupported (2005-07-30) | ?
Artiscan 9600 pro 36 | Parport | unsupported | Unsupported at the moment. See link for a project for that scanner. | unsupported (2005-07-30) | ?
Artiscan 12000C | SCSI | good | 3 pass, 600 DPI | tamarack (unmaintained) | sane-tamarack

### Manufacturer: Targa

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Funline TS6 EP | Parport (EPP) | good | 300x600 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
Funline TS12 EP | Parport (EPP) | good | 600x1200 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp

### Manufacturer: TCE

Link(s): http://www.tce.com.br/
Comment: Brasilian vendor.

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
MK600U | USB | unsupported | Not supported. Some information is available. | unsupported (2005-07-30) | ?
S450 | Parport | unsupported | Not supported by SANE but is reported to work with pxscan (see link). | unsupported (2005-07-30) | ?

### Manufacturer: Teco

Link(s): http://www.tecoimage.com.tw/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
VM6509F | USB | unsupported | Probably unsupported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: TemPlate

Link(s): http://www.template.com/, http://www.template.de/
Comment: TemPlate scanners are sometimes labeled "TMP "

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Templ Z | SCSI | untested | With Z-Axis scrolling | template (0.42, NEW!) | sane-template
Templ ZQ | USB | minimal |  | template (0.42, NEW!) | sane-template
Templ ZS | USB | unsupported | No support yet, but we have docs. | template (0.42, NEW!) | sane-template
Templ ZY | SCSI | basic |  | template (0.42, NEW!) | sane-template
Templ ZZ | SCSI | good |  | template (0.42, NEW!) | sane-template

### Manufacturer: Tiny

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
FU661E | USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: TriGem

Link(s): http://www.nikon.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
PowerScanII | SCSI | good | OK | umax (1.0-41) | sane-umax

### Manufacturer: Trust

Link(s): http://www.trust-site.com, http://www.trust-site.com/home/
Comment: Carefully check the model names. Trust uses similar names for completely different hardware.

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
240TH Easy Webscan Gold | USB | good | Same as Mustek Bearpaw 2400 TA plus. | gt68xx (1.0-71) | sane-gt68xx
CombiScan 19200 | Parport USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
Compact Scan USB 19200 | USB | complete | Mustek 1200 UB compatible | mustek_usb (1.0-18) | sane-mustek_usb
Compact Scan USB 19200 | USB | good | Works, if you have vendor id 0x055f and product id 0x0006, use the mustek_usb backend instead, similar to Mustek ScanExpress 1200 UB (Plus) | gt68xx (1.0-71) | sane-gt68xx
Easy Connect 9600+ | Parport (EPP) | good | 300x600 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
Easy Connect 19200+ | Parport (EPP) | good | 300x600 dpi CIS scanner | mustek_pp (13) | sane-mustek_pp
Easy Webscan 19200 | USB | good | Different product id: 0x4006 | artec_eplus48u (0.0.10) | sane-artec_eplus48u
Flat Scan USB 19200 | USB | good | Similar to Artec Ultima 2000 | gt68xx (1.0-71) | sane-gt68xx
Imagery 1200 | SCSI | good | 3-pass, Mustek Paragon MFS-6000CX compatible | mustek (1.0-138) | sane-mustek
Imagery 1200 SP | SCSI | complete | Mustek Paragon MFS-6000SP compatible | mustek (1.0-138) | sane-mustek
Imagery 2400 SP | SCSI | good | sub model VM3552 | teco3 (1.0-1) | sane-teco3
Imagery 4800 SP | SCSI | complete | Mustek Paragon 600 II CD compatible | mustek (1.0-138) | sane-mustek
Imagery 4800 SP+ | SCSI | good | sub model VM3552 | teco3 (1.0-1) | sane-teco3
Imagery 9600 SP | SCSI | untested | sub model VM3552 | teco3 (1.0-1) | sane-teco3
SCSI Connect 19200 | SCSI | complete | Mustek ScanExpress 12000SP compatible | mustek (1.0-138) | sane-mustek
SCSI excellence series 19200 | SCSI | complete | Mustek ScanExpress 12000SP compatible | mustek (1.0-138) | sane-mustek
SCSI Scan 19200 -Excellence Series- | SCSI | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: UMAX

Link(s): http://www.umax.com/, http://www.umax.com.tw/, http://www.umax.de/en, http://www.umax-europe.com, http://www.umaxjapan.co.jp, http://www.umax.com.cn

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Astra 600P | Parport (SPP/ECP) | unsupported | untested, but should be close to 610P | umax_pp (1) | sane-umax_pp
Astra 600S | SCSI | good | OK | umax (1.0-41) | sane-umax
Astra 610P | Parport (SPP/ECP) | good |  | umax_pp (1) | sane-umax_pp
Astra 610S | SCSI | good | OK | umax (1.0-41) | sane-umax
Astra 1200S | SCSI | good | OK | umax (1.0-41) | sane-umax
Astra 1220P | Parport (EPP/ECP) | good |  | umax_pp (1) | sane-umax_pp
Astra 1220S | SCSI | good | OK | umax (1.0-41) | sane-umax
Astra 1220U | USB | good | OK | umax1220u (1.0.1) | sane-umax1220u
Astra 1600P | Parport (EPP/ECP) | good |  | umax_pp (1) | sane-umax_pp
Astra 1600U | USB | minimal | Is reported to be the same as the 2000U. Sort of scans, but colors all messed up. | umax1220u (1.0.1) | sane-umax1220u
Astra 2000P | Parport (EPP/ECP) | good |  | umax_pp (1) | sane-umax_pp
Astra 2000U | USB | minimal | Sort of scans, but colors all messed up. | umax1220u (1.0.1) | sane-umax1220u
Astra 2100 U | USB | minimal | Colours are distorted, there are vertical colour stripes, and the image is shadowed inches to its left. | umax1220u (1.0.1) | sane-umax1220u
Astra 2100S | SCSI | good | OK | umax (1.0-41) | sane-umax
Astra 2200 (SU) | USB | good | OK, needs USB control messages | umax (1.0-41) | sane-umax
Astra 2200 (SU) | SCSI | good | OK | umax (1.0-41) | sane-umax
Astra 2400S | SCSI | good | OK | umax (1.0-41) | sane-umax
Astra 3000 | USB | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?
Astra 3400 | USB | unsupported | Model ID 0x0050 not supported. See link for details. | unsupported (2005-07-30) | ?
Astra 3600 | USB | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?
Astra 4000 | USB | unsupported | Not supported. See link for details. | unsupported (2005-07-30) | ?
Astra 4400 | USB | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?
Astra 4450 | USB | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?
Astra 4500 | USB | unsupported | GL646 based, to be added to genesys backend. Avision iVina FB1600 clone | unsupported (2005-07-30) | ?
Astra 4600 | USB | unsupported | Probably not supported, no details known. | unsupported (2005-07-30) | ?
Astra 4700 | USB | unsupported | GL646/GL660 based. Avision iVina FB1800 clone. | unsupported (2005-07-30) | ?
Astra 6400 | IEEE-1394 | unsupported | will propably work one day | umax (1.0-41) | sane-umax
Astra 6450 | IEEE-1394 | unsupported | will propably work one day | umax (1.0-41) | sane-umax
Astra 6700 | USB | unsupported | Not supported. No chipset information available. Same as Avision iVina FB2400. | unsupported (2005-07-30) | ?
Astra MX3 | USB | good | OK, needs USB control messages | umax (1.0-41) | sane-umax
Astra MX3 | SCSI | good | OK | umax (1.0-41) | sane-umax
AstraSlim | USB | unsupported | Probably not supported currently. See link for more details. | unsupported (2005-07-30) | ?
AstraSlim 1200 SE | USB | unsupported | Probably not supported currently. May be supported in future. See link for more details. | unsupported (2005-07-30) | ?
AstraSlim 6000 | USB | unsupported | Probably not supported currently. See link for more details. | unsupported (2005-07-30) | ?
AstraSlim SE | USB | good | Different product id: 0x4009 | artec_eplus48u (0.0.10) | sane-artec_eplus48u
Gemini D-16 | SCSI | good | OK | umax (1.0-41) | sane-umax
Mirage D-16L | SCSI | good | OK | umax (1.0-41) | sane-umax
Mirage II | SCSI | good | OK | umax (1.0-41) | sane-umax
Mirage IIse | SCSI | good | OK | umax (1.0-41) | sane-umax
PL-II | SCSI | good | OK | umax (1.0-41) | sane-umax
PowerLook | SCSI | good | OK, SCSI-ID=PS-2400X | umax (1.0-41) | sane-umax
Powerlook 180 | USB | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?
PowerLook 270 | SCSI | unsupported | incompatible | umax (1.0-41) | sane-umax
PowerLook 270plus | SCSI | unsupported | incompatible | umax (1.0-41) | sane-umax
Powerlook 1000 USB | USB | unsupported | Probably not supported. No further information available. | unsupported (2005-07-30) | ?
PowerLook 1100 | IEEE-1394 | unsupported | will propably work one day | umax (1.0-41) | sane-umax
PowerLook 2000 | SCSI | good | OK | umax (1.0-41) | sane-umax
PowerLook 2100XL | SCSI | good | OK | umax (1.0-41) | sane-umax
PowerLook 3000 | SCSI | good | OK | umax (1.0-41) | sane-umax
PowerLook III | SCSI | good | OK | umax (1.0-41) | sane-umax
PSD | SCSI | good | OK | umax (1.0-41) | sane-umax
Supervista S-12 | SCSI | good | OK | umax (1.0-41) | sane-umax
UC 630 | SCSI | good | Version 2.8 OK, others only lineart OK | umax (1.0-41) | sane-umax
UC 840 | SCSI | good | Version 1.6 OK, others only lineart OK | umax (1.0-41) | sane-umax
UC 1200S | SCSI | untested | may work, please test and give feedback | umax (1.0-41) | sane-umax
UC 1200SE | SCSI | good | Version 3.0 OK, others unknown | umax (1.0-41) | sane-umax
UC 1260 | SCSI | good | Version 1.6 OK, others unknown | umax (1.0-41) | sane-umax
UG 80 | SCSI | good | OK | umax (1.0-41) | sane-umax
UG 630 | SCSI | good | OK | umax (1.0-41) | sane-umax
UMAX 3400 | USB | complete | there are some UMAX 3400 outside the U.S. which are not supported, as they use another chipset than the LM983x | plustek (0.49) | sane-plustek
UMAX 3450 | USB | complete |  | plustek (0.49) | sane-plustek
UMAX 5400 | USB | complete |  | plustek (0.49) | sane-plustek
UMAX Astranet ia101 | USB | complete | seems to be a renamed UMAX 3400 | plustek (0.49) | sane-plustek
UMAX S-6E | SCSI | good | OK | umax (1.0-41) | sane-umax
UMAX S-6EG | SCSI | good | OK | umax (1.0-41) | sane-umax
UMAX S-12 | SCSI | good | OK | umax (1.0-41) | sane-umax
UMAX S-12G | SCSI | good | OK | umax (1.0-41) | sane-umax
UMAX VT600 | SCSI | untested | may work, please test and give feedback | umax (1.0-41) | sane-umax
Vista S6 | SCSI | good | OK | umax (1.0-41) | sane-umax
Vista S6E | SCSI | good | OK | umax (1.0-41) | sane-umax
Vista-S8 | SCSI | good | OK | umax (1.0-41) | sane-umax
Vista-T630 | SCSI | good | OK for some firmwareversions, on others only lineart OK | umax (1.0-41) | sane-umax

### Manufacturer: Vantas

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
3000 | USB | unsupported | Not supported. See link for more details. | unsupported (2005-07-30) | ?

### Manufacturer: Visioneer

Link(s): http://www.visioneer.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
6200 | USB | unsupported | Not supported. Is reported to use the E5 chipset. Uses a Primax ID. See link for some details. Looks similar to Primascan Colorado 2600u. | unsupported (2005-07-30) | ?
Onetouch 4400 | USB | unsupported | Not supported. E5 chipset? Vendor/product 0x0461/0x0347.See link for more details. | unsupported (2005-07-30) | ?
OneTouch 4800 USB | USB | unsupported | Unsupported. Vendor/Product ids: 0x04a7/0x0224. Seems to use Realtek RTS8801B. Same as Microtek Scanport 3000. See link for details. | unsupported (2005-07-30) | ?
OneTouch 5300 USB | USB | unsupported | Not supported. Vendor/product ids 0x04a7/0x0226. Chipset is RTS8801B(?). See link for output of /proc/bus/usb/devices. | unsupported (2005-07-30) | ?
OneTouch 5800 USB | USB | unsupported | Unsupported. 48 bit scanner, doesn't work with viceo backend. RTS8801C. Vendor/product 0x04a7/0x0226. | unsupported (2005-07-30) | ?
OneTouch 6600 | USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
Onetouch 7100 | USB | unsupported | GL646 based, to be added to genesys backend | unsupported (2005-07-30) | ?
OneTouch 7300 | USB | good | Works upto 1200 dpi and 12 bits/color. | gt68xx (1.0-71) | sane-gt68xx
OneTouch 8100 | USB | unsupported | Unsupported. See link for details. | unsupported (2005-07-30) | ?
Onetouch 8700 | USB | unsupported | Not supported. See link for details. | unsupported (2005-07-30) | ?
Onetouch 8900 | USB | unsupported | Not supported. Same as 8920 but without TA? | unsupported (2005-07-30) | ?
Onetouch 8920 | USB | unsupported | Not supported. Same as 8700 and 8900 but includes a TA. Uses a Primax ID. Chipset is RTS8801C. See link for output of /proc/bus/usb/devices. | unsupported (2005-07-30) | ?
Onetouch 9000 | USB | unsupported | Not supported. See link for details. | unsupported (2005-07-30) | ?
Onetouch 9020 | USB | unsupported | Not supported. See link for details. | unsupported (2005-07-30) | ?
Onetouch Pro 8800 | USB | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?
Onetouch Pro 8820 | USB | unsupported | Probably not supported. See link for details. | unsupported (2005-07-30) | ?
PaperPort 3100b | Parport | unsupported | Most probably not supported. See link for details. | unsupported (2005-07-30) | ?
PaperPort 6100 | Parport | unsupported | Most probably not supported. More details would be appreciated. | unsupported (2005-07-30) | ?
PaperPort OneTouch | Parport | unsupported | Most probably not supported. See link for details. | unsupported (2005-07-30) | ?
Primascan Colorado 2600u | USB | unsupported | Not supported. See Visioneer Onetouch 4400. | unsupported (2005-07-30) | ?
Strobe XP 100 | USB | unsupported | Not supported but may work in future. See link for details. | unsupported (2005-07-30) | ?

### Manufacturer: Viviscan

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Compact II | Parport (EPP) | good | 300 dpi CCD scanner | mustek_pp (13) | sane-mustek_pp

### Manufacturer: Vobis

Link(s): http://www.vobis.de/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
HighScan | SCSI | complete | only E3plus based models | microtek2 (0.96) | sane-microtek2
Highscreen Realscan | SCSI | good |  | microtek (0.13.1) | sane-microtek
Highscreen Scanboostar Premium | SCSI | good | OK, SCSI-ID=LinoHell Office2 | umax (1.0-41) | sane-umax

### Manufacturer: Vuego

Comment: Company was renamed to Benq.

### Manufacturer: Xerox

Link(s): http://www.xerox.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
2400 Onetouch | USB | unsupported | Probably GL646_HP based, maybe can be added to genesys backend | unsupported (2005-07-30) | ?
DocuImage 620S | SCSI | unsupported | Not supported. See link for more details. | unsupported (2005-07-30) | ?
DocuMate252 | USB | untested |  | avision (Build: 167) | sane-avision
DocuMate262 | USB | untested |  | avision (Build: 167) | sane-avision
WorkCentre 470cx | Parport | unsupported | Not supported. See link for more details. | unsupported (2005-07-30) | ?
WorkCentre M15i | USB | unsupported | Not supported. See link for more details. | unsupported (2005-07-30) | ?
WorkCentre PE16 | USB Parport | unsupported | Not supported. See link for more details. | unsupported (2005-07-30) | ?
WorkCentre Pro 412 | USB Parport | unsupported | Not supported. See link for more details. | unsupported (2005-07-30) | ?
WorkCentre XK35c | USB Parport | unsupported | Not supported. See link for more details. | unsupported (2005-07-30) | ?
WorkCentre XK50cx | USB | unsupported | Not supported. See link for more details. | unsupported (2005-07-30) | ?

## Still Cameras

Manufacturers: Kodak, Polaroid

### Manufacturer: Kodak

Link(s): http://www.kodak.com/global/en/service/digCam/dc25/dc25.shtml, http://www.kodak.com/global/en/service/digCam/dc210/dc210.shtml, http://www.kodak.com/global/en/service/products/ekn006568.jhtml

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
DC20 | Serial port | basic | DC-20 untested by author but reported to work | dc25 (1.2) | sane-dc25
DC25 | Serial port | complete |  | dc25 (1.2) | sane-dc25
DC210 | Serial port | basic |  | dc210 (0.0) | sane-dc210
DC240 | Serial port | good | Use gphoto2 backend to get USB support | dc240 (0.0) | sane-dc240

### Manufacturer: Polaroid

Link(s): http://www.polaroid.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
DMC | SCSI | good |  | dmc (unmaintained) | sane-dmc

## Video Cameras

Manufacturers: Biolux, Connectix, Grandtek Scopecam

### Manufacturer: Biolux

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
654 (micrOcular) | USB | unsupported | Not supported yet. See link for more details. | unsupported (2005-07-30) | ?

### Manufacturer: Connectix

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Color QuickCam | Parport | good | Requires root privileges. | qcam (unmaintained) | sane-qcam
Greyscale QuickCam | Parport | minimal | Requires root privileges. Partly working. | qcam (unmaintained) | sane-qcam

### Manufacturer: Grandtek Scopecam

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
8x30 Binocular & Digital Camera | USB | unsupported | Not Supported yet. See link for more details. | unsupported (2005-07-30) | ?

## APIs

Backends: gphoto2, pint, pnm, template, test, v4l

### Backend: gphoto2 (0.0)

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-gphoto2
Description: Multiple cameras supported by the gphoto2 libraries
Comment: The long-term plan is to support all the cameras supported by the gphoto2 libraries (currently over 140 models). However, at this stage, only a handful of cameras are definitely known to work with SANE. Other cameras will probably work if the native file format is EXIF or JPEG. Testers welcome!

### Backend: pint (unmaintained)

Manual page: sane-pint
Description: Scanners with the machine-independent PINT interface
Comment: Haven't been tested for a long time. Handle with care.

### Backend: pnm (1.0.8)

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-pnm
Description: Reads PNM files
Comment: Used for debugging frontends. Obsolete, use test backend instead.

### Backend: template (0.42, NEW!)

Link(s): http://www.luser.com/temp/, http://www.luser.com/b/
Manual page: sane-template
Comment: This backend supports only the USB and SCSI models
Description: Interface to FrObYz API
Comment: Only FrObYz version 2.0 is supported!

### Backend: test (1.0-26)

Link(s): http://www.meier-geinitz.de/sane/test-backend/
Manual page: sane-test
Description: Frontend-tester
Comment: Backend for testing frontends. Also serves as example for SANE backend options.

### Backend: v4l (1.0-3)

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-v4l
Description: Interface to Video For Linux API
Comment: Supports video cameras and other devices accessed by the v4l kernel API, e.g. bttv devices. Quite a lot of known bugs.

## Meta Backends

Backends: dll, net

### Backend: dll (1.0.11)

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-dll
Description: Dynamic loading of shared-library backends.

### Backend: net (1.0.13)

Link(s): http://www.penguin-breeder.org/?page=sane-net
Manual page: sane-net
Description: Network access to saned servers
Comment: Can be used to access any scanner supported by SANE over the net. Supports IPv4 and IPv6.

### Legend:

> Model:
>   Name of the the device.
> Interface:
>   How the device is connected to the computer.
> Status:
>   Indicates how many of the features the device provides are supported by SANE.
>   - unsupported means the device is not supported at least by this backend. It may be supported by other backends, however.
>   - untested means the device may be supported but couldn't be tested. Be very careful and report success/failure.
>   - minimal means that the device is detected and scans at least in one mode. But the quality is bad or important features won't work.
>   - basic means it works at least in the most important modes but quality is not perfect.
>   - good means the device is usable for day-to-day work. Some rather exotic features may be missing.
>   - complete means the backends supports everything the device can do.
> Comment:
>   More information about the backend or model, e.g. the level of support and possible problems.
> Backend:
>   Name of the backend, in parentheses if available: Version of backend/driver; newer versions may be available from their home sites.
>   NEW! means brand-new to the current release of SANE.
>   UNMAINTAINED means that nobody maintains that backend. Expect no new features or newly supported devices. You are welcome to take over maintainership.
> Manual Page:
>   A link to the man-page online, if it exists.
> Manufacturer:
>   Manufacturer, vendor or brand name of the device.
> Description:
>   The scope of application of the backend.

SANE homepage
This page was last updated on Mon Aug 8 08:22:53 2005