# SANE: Devices Supported by External Backends

The following table summarizes the devices that are supported by external backends.

This is only a summary! Please consult the manpages and the author-supplied webpages for more detailed (and usually important) information concerning each backend.

If you have new information or corrections, please file a bug report with as many details as possible. Also please tell us if your scanner isn't mentioned in this list at all.

For an explanation of the tables, see the legend.

There are tables for scanners, still cameras, video cameras, APIs, and meta backends.

## Scanners

Manufacturers: ArmorPlate, Benq, Brother, EPSON, Genius, Hewlett Packard, Hewlett-Packard, IBM, LG Electronics, Mustek, Network, Primax, Samsung, Storm, TemPlate, Visioneer

### Manufacturer: ArmorPlate

Link(s): http://www.armorplate.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
AmplScan II | SCSI | complete | AmplScan *II*, not AmplScan! | template (0.42, NEW!) | sane-template

### Manufacturer: Benq

Link(s): http://www.benq.com
Comment: Formerly Acer Peripherals

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
ScanWit 2720S | SCSI | basic | Usable, but not complete | scanwit | ?

### Manufacturer: Brother

Link(s): http://www.brother.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
DCP-110C | USB | untested | No report yet. | brother2 | ?
DCP-310CN | USB | untested | No report yet. | brother2 | ?
DCP-1000 | USB | untested | No report yet. | brother | ?
DCP-1400 | USB | untested | No report yet. | brother | ?
DCP-4020C | USB | untested | No report yet. | brother | ?
DCP-7010 | USB | untested | No report yet. | brother2 | ?
DCP-7020 | USB | untested | No report yet. | brother2 | ?
DCP-7025 | USB | good |  | brother2 | ?
DCP-8020 | USB | untested | No report yet. | brother | ?
DCP-8025D | USB | good |  | brother | ?
DCP-8040 | USB | untested | No report yet. | brother | ?
DCP-8045D | USB | good |  | brother | ?
FAX-2850 | USB | untested | No report yet. | brother | ?
FAX-2900 | USB | untested | No report yet. | brother | ?
FAX-3800 | USB | untested | No report yet. | brother | ?
FAX-4100 | USB | untested | No report yet. | brother | ?
FAX-4750e | USB | untested | No report yet. | brother | ?
FAX-5750e | USB | untested | No report yet. | brother | ?
FAX1800C | USB | untested | No report yet. | brother | ?
FAX1815C | USB | untested | No report yet. | brother | ?
FAX1820C | USB | untested | No report yet. | brother | ?
FAX1920CN | USB | untested | No report yet. | brother | ?
MFC-210C | USB | untested | No report yet. | brother2 | ?
MFC-410CN | USB | untested | No report yet. | brother2 | ?
MFC-420CN | USB | untested | No report yet. | brother2 | ?
MFC-580 | USB | good |  | brother | ?
MFC-590 | USB | good |  | brother | ?
MFC-620CN | USB | untested | No report yet. | brother2 | ?
MFC-890 | USB | good |  | brother | ?
MFC-3100C | USB | untested | No report yet. | brother | ?
MFC-3200C | USB | untested | No report yet. | brother | ?
MFC-3220C | USB | untested | No report yet. | brother | ?
MFC-3240C | USB | untested | No report yet. | brother2 | ?
MFC-3320CN | USB | untested | No report yet. | brother | ?
MFC-3340CN | USB | untested | No report yet. | brother2 | ?
MFC-3420C | USB | good |  | brother | ?
MFC-3820CN | USB | untested | No report yet. | brother | ?
MFC-4420C | USB | untested | No report yet. | brother | ?
MFC-4800 | USB | good |  | brother | ?
MFC-4820C | USB | good |  | brother | ?
MFC-5100C | USB | good |  | brother | ?
MFC-5200C | USB | good |  | brother | ?
MFC-5440CN | USB | untested | No report yet. | brother2 | ?
MFC-5840CN | USB | untested | No report yet. | brother2 | ?
MFC-6800 | USB | untested | No report yet. | brother | ?
MFC-7220 | USB | untested | No report yet. | brother2 | ?
MFC-7225N | USB | untested | No report yet. | brother2 | ?
MFC-7420 | USB | untested | No report yet. | brother2 | ?
MFC-7820N | USB | untested | No report yet. | brother2 | ?
MFC-8220 | USB | untested | No report yet. | brother | ?
MFC-8420 | USB | good |  | brother | ?
MFC-8440 | USB | good |  | brother | ?
MFC-8500 | USB | untested | No report yet. | brother | ?
MFC-8820D | USB | good | Is reported to work well with backend version 0.0.12. | brother | ?
MFC-8840D | USB | untested | No report yet. | brother | ?
MFC-9030 | USB | untested | No report yet. | brother | ?
MFC-9070 | USB | untested | No report yet. | brother | ?
MFC-9160 | USB | good | Is reported to work well with backend version 0.0.12. | brother | ?
MFC-9180 | USB | untested | No report yet. | brother | ?
MFC-9660 | USB | untested | No report yet. | brother | ?
MFC-9700 | USB | untested | No report yet. | brother | ?
MFC-9760 | USB | untested | No report yet. | brother | ?
MFC-9800 | USB | untested | No report yet. | brother | ?
MFC-9860 | USB | untested | No report yet. | brother | ?
MFC-9880 | USB | untested | No report yet. | brother | ?

### Manufacturer: EPSON

Link(s): http://www.epson.com/
Comment:

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Actionscanner II | parallel | untested | overseas version of the GT-5000 | epkowa (1.15.0) | sane-epkowa
AcuLaser CX11 | USB | complete | overseas version of the LP-A500 | epkowa (1.15.0) | sane-epkowa
CC-500L | USB | unsupported | all-in-one | epkowa (1.15.0) | sane-epkowa
CC-550L | USB | unsupported | all-in-one | epkowa (1.15.0) | sane-epkowa
CC-570L | USB | untested | all-in-one | epkowa (1.15.0) | sane-epkowa
CC-600PX | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
CC-700 | USB | unsupported | all-in-one | epkowa (1.15.0) | sane-epkowa
ES-300C | SCSI parallel | untested | overseas version of the GT-6000 | epkowa (1.15.0) | sane-epkowa
ES-600C | parallel | untested | overseas version of the GT-5400 | epkowa (1.15.0) | sane-epkowa
ES-800C | SCSI | untested | overseas version of the GT-8000 | epkowa (1.15.0) | sane-epkowa
ES-1000C | ? | unsupported | overseas version of the GT-8500 | epkowa (1.15.0) | sane-epkowa
ES-1200C | parallel | untested | overseas version of the GT-9000 | epkowa (1.15.0) | sane-epkowa
ES-2000 | SCSI USB | complete | IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
ES-2200 | SCSI USB | complete | IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
ES-6000 | SCSI | complete |  | epkowa (1.15.0) | sane-epkowa
ES-6000H | SCSI | complete | IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
ES-6000HS | SCSI | complete | IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
ES-7000H | SCSI USB | complete | IEEE1394 untested; 100Base-TX/10Base-T unsupported | epkowa (1.15.0) | sane-epkowa
ES-8000 | SCSI | untested |  | epkowa (1.15.0) | sane-epkowa
ES-8500 | SCSI USB | complete | IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
ES-9000H | SCSI | complete | IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
ES-10000G | USB | complete | IEEE1394 untested 100Base-TX/10Base-T unsupported | epkowa (1.15.0) | sane-epkowa
Expression 636 | SCSI | untested | overseas version of the GT-9500 | epkowa (1.15.0) | sane-epkowa
Expression 800 | SCSI | untested | overseas version of the GT-9600 | epkowa (1.15.0) | sane-epkowa
Expression 836XL | SCSI | untested | overseas version of the ES-8000 | epkowa (1.15.0) | sane-epkowa
Expression 1600 | SCSI USB | complete | overseas version of the ES-2000 IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
Expression 1640XL | SCSI USB | complete | overseas version of the ES-8500 IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
Expression 1680 | SCSI USB | complete | overseas version of the ES-2200 IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
Expression 10000XL | USB | complete | overseas version of the ES-10000G IEEE1394 untested; 100Base-TX/10Base-T unsupported | epkowa (1.15.0) | sane-epkowa
F-3200 | USB IEEE1394 | unsupported | Film scanner | epkowa (1.15.0) | sane-epkowa
FilmScan 200 | SCSI | unsupported | A better backend for the FilmScan 200 can be found at http://www.vjet.demon.co.uk/scanner/. | epkowa (1.15.0) | sane-epkowa
GT-4000 | ? | untested |  | epkowa (1.15.0) | sane-epkowa
GT-5000 | parallel | untested |  | epkowa (1.15.0) | sane-epkowa
GT-5400 | parallel | untested |  | epkowa (1.15.0) | sane-epkowa
GT-5500 | SCSI | untested |  | epkowa (1.15.0) | sane-epkowa
GT-6000 | SCSI Parport | untested |  | epkowa (1.15.0) | sane-epkowa
GT-6500 | parallel | untested | overseas version of the GT-5400 | epkowa (1.15.0) | sane-epkowa
GT-6600U | USB | complete |  | epkowa (1.15.0) | sane-epkowa
GT-6700U | USB | complete |  | epkowa (1.15.0) | sane-epkowa
GT-7000S | SCSI | untested |  | epkowa (1.15.0) | sane-epkowa
GT-7000U | USB | untested |  | epkowa (1.15.0) | sane-epkowa
GT-7200U | USB | complete | requires a DFSG non-free module also supported by the plustek backend | epkowa (1.15.0) | sane-epkowa
GT-7300U | USB | complete | requires a DFSG non-free module also supported by the plustek backend | epkowa (1.15.0) | sane-epkowa
GT-7400U | USB | unsupported | may be supported by the snapscan backend | epkowa (1.15.0) | sane-epkowa
GT-7600S | SCSI | complete | SCSI version of the GT-7600U | epkowa (1.15.0) | sane-epkowa
GT-7600U | USB | complete | USB version of the GT-7600S | epkowa (1.15.0) | sane-epkowa
GT-7600UF | USB | complete | GT-7600U with TPU option bundled | epkowa (1.15.0) | sane-epkowa
GT-7700U | USB | complete |  | epkowa (1.15.0) | sane-epkowa
GT-8000 | SCSI | untested |  | epkowa (1.15.0) | sane-epkowa
GT-8200U | USB | complete |  | epkowa (1.15.0) | sane-epkowa
GT-8200UF | USB | complete |  | epkowa (1.15.0) | sane-epkowa
GT-8300UF | USB | complete |  | epkowa (1.15.0) | sane-epkowa
GT-8400UF | USB | unsupported |  | epkowa (1.15.0) | sane-epkowa
GT-8500 | ? | untested |  | epkowa (1.15.0) | sane-epkowa
GT-8700 | SCSI USB | complete |  | epkowa (1.15.0) | sane-epkowa
GT-8700F | SCSI USB | complete | GT-8700U with TPU option bundled | epkowa (1.15.0) | sane-epkowa
GT-9000 | parallel | untested |  | epkowa (1.15.0) | sane-epkowa
GT-9300UF | USB | complete |  | epkowa (1.15.0) | sane-epkowa
GT-9400UF | USB | complete | requires a DFSG non-free module | epkowa (1.15.0) | sane-epkowa
GT-9500 | SCSI | untested |  | epkowa (1.15.0) | sane-epkowa
GT-9600 | SCSI | untested |  | epkowa (1.15.0) | sane-epkowa
GT-9700F | USB | complete | IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
GT-9800F | USB | complete | IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
GT-10000 | SCSI | complete | overseas version of the ES-6000 | epkowa (1.15.0) | sane-epkowa
GT-10000+ | SCSI | complete | overseas version of the ES-6000H IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
GT-12000 | SCSI | untested | overseas version of the ES-8000 | epkowa (1.15.0) | sane-epkowa
GT-15000 | SCSI USB | complete | overseas version of the ES-7000H IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
GT-30000 | SCSI | complete | overseas version of the ES-9000H IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
GT-F500 | USB | complete |  | epkowa (1.15.0) | sane-epkowa
GT-F550 | USB | good |  | epkowa (1.15.0) | sane-epkowa
GT-F600 | USB | good | only scans up to 2400dpi requires a DFSG non-free module | epkowa (1.15.0) | sane-epkowa
GT-X700 | USB | complete | IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
GT-X800 | USB IEEE1394 | complete |  | epkowa (1.15.0) | sane-epkowa
LP-7900CS | ? | untested | business all-in-one; scanner is a ES-7000H | epkowa (1.15.0) | sane-epkowa
LP-9000CCH | ? | untested | business all-in-one; scanner is a ES-9000H | epkowa (1.15.0) | sane-epkowa
LP-9000CCS | ? | untested | business all-in-one; scanner is a ES-7000H | epkowa (1.15.0) | sane-epkowa
LP-9000CFH | ? | untested | business all-in-one; scanner is a ES-9000H | epkowa (1.15.0) | sane-epkowa
LP-9500CCS | ? | untested | business all-in-one; scanner is a ES-7000H | epkowa (1.15.0) | sane-epkowa
LP-9500CFH | ? | untested | business all-in-one; scanner is a ES-9000H | epkowa (1.15.0) | sane-epkowa
LP-9500CH2 | ? | untested | business all-in-one; scanner is a ES-9000H | epkowa (1.15.0) | sane-epkowa
LP-9800CCH | ? | untested | business all-in-one; scanner is a ES-9000H | epkowa (1.15.0) | sane-epkowa
LP-9800CCS | ? | untested | business all-in-one; scanner is a ES-7000H | epkowa (1.15.0) | sane-epkowa
LP-9800CFH | ? | untested | business all-in-one; scanner is a ES-9000H | epkowa (1.15.0) | sane-epkowa
LP-A500 | USB | complete | business all-in-one | epkowa (1.15.0) | sane-epkowa
Perfection 600 | SCSI | unsupported | rebadged UMAX Astra 1200S supported by the umax backend | epkowa (1.15.0) | sane-epkowa
Perfection 610 | USB | complete | overseas version of the GT-6600U | epkowa (1.15.0) | sane-epkowa
Perfection 636S | SCSI | untested | overseas version of the GT-7000S | epkowa (1.15.0) | sane-epkowa
Perfection 636U | USB | untested | overseas version of the GT-7000U | epkowa (1.15.0) | sane-epkowa
Perfection 640U | USB | complete | overseas version of the GT-6700U | epkowa (1.15.0) | sane-epkowa
Perfection 660 | USB | unsupported | supported by the snapscan backend | epkowa (1.15.0) | sane-epkowa
Perfection 1200S | SCSI | complete | overseas version of the GT-7600S | epkowa (1.15.0) | sane-epkowa
Perfection 1200U | USB | complete | overseas version of the GT-7600U | epkowa (1.15.0) | sane-epkowa
Perfection 1200U PHOTO | USB | complete | overseas version of the GT-7600UF | epkowa (1.15.0) | sane-epkowa
Perfection 1240U | USB | complete | overseas version of the GT-7700U | epkowa (1.15.0) | sane-epkowa
Perfection 1250 | USB | complete | overseas version of the GT-7200U requires a DFSG non-free module also supported by the plustek backend | epkowa (1.15.0) | sane-epkowa
Perfection 1250 PHOTO | USB | complete | Perfection 1250 with TPU option bundled requires a DFSG non-free module also supported by the plustek backend | epkowa (1.15.0) | sane-epkowa
Perfection 1260 | USB | complete | overseas version of the GT-7300U requires a DFSG non-free module also supported by the plustek backend | epkowa (1.15.0) | sane-epkowa
Perfection 1260 PHOTO | USB | complete | Perfection 1260 with TPU option bundled requires a DFSG non-free module also supported by the plustek backend | epkowa (1.15.0) | sane-epkowa
Perfection 1270 | USB | unsupported | may be supported by the snapscan backend | epkowa (1.15.0) | sane-epkowa
Perfection 1640SU | SCSI USB | complete | overseas version of the GT-8700 | epkowa (1.15.0) | sane-epkowa
Perfection 1640SU PHOTO | SCSI USB | complete | overseas version of the GT-8700F | epkowa (1.15.0) | sane-epkowa
Perfection 1650 | USB | complete | overseas version of the GT-8200U | epkowa (1.15.0) | sane-epkowa
Perfection 1650 PHOTO | USB | complete | overseas version of the GT-8200UF | epkowa (1.15.0) | sane-epkowa
Perfection 1660 PHOTO | USB | complete | overseas version of the GT-8300UF | epkowa (1.15.0) | sane-epkowa
Perfection 1670 | USB | unsupported | supported by the snapscan backend | epkowa (1.15.0) | sane-epkowa
Perfection 2400 PHOTO | USB | complete | overseas version of the GT-9300UF | epkowa (1.15.0) | sane-epkowa
Perfection 2450 PHOTO | USB | complete | overseas version of the GT-9700F IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
Perfection 2480 PHOTO | USB | complete | overseas version of the GT-F500 requires a DFSG non-free module also supported by the snapscan backend | epkowa (1.15.0) | sane-epkowa
Perfection 2580 PHOTO | USB | complete | overseas version of the GT-F550 requires a DFSG non-free module also supported by the snapscan backend | epkowa (1.15.0) | sane-epkowa
Perfection 3170 PHOTO | USB | complete | overseas version of the GT-9400UF requires a DFSG non-free module | epkowa (1.15.0) | sane-epkowa
Perfection 3200 PHOTO | USB | complete | overseas version of the GT-9800F IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
Perfection 4180 PHOTO | USB | good | overseas version of the GT-F600 only scans up to 2400dpi requires a DFSG non-free module | epkowa (1.15.0) | sane-epkowa
Perfection 4870 PHOTO | USB | complete | overseas version of the GT-X700 IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
Perfection 4990 PHOTO | USB | complete | overseas version of the GT-X800 IEEE1394 untested | epkowa (1.15.0) | sane-epkowa
PM-A700 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
PM-A850 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
PM-A870 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
PM-A900 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
PX-A550 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX1500 | USB | unsupported | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX3100 | USB | untested | overseas version of the CC-570 all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX3200 | USB | untested | overseas version of the CC-570 all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX3500 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX3600 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX3650 | USB | unsupported | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX4500 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX4600 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX5100 | USB | complete | overseas version of the CC-600PX all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX5200 | USB | complete | overseas version of the CC-600PX all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX5300 | USB | complete | overseas version of the CC-600PX all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX5400 | USB | complete | overseas version of the CC-600PX all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX6300 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX6400 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX6500 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus CX6600 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus Photo RX420 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus Photo RX425 | USB | unsupported | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus Photo RX430 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus Photo RX500 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus Photo RX510 | USB | complete | all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus Photo RX600 | USB | complete | overseas version of the PM-A850 all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus Photo RX610 | USB | complete | overseas version of the PM-A850 all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus Photo RX620 | USB | complete | overseas version of the PM-A870 all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus Photo RX630 | USB | complete | overseas version of the PM-A870 all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus Photo RX700 | USB | complete | overseas version of the PM-A900 all-in-one | epkowa (1.15.0) | sane-epkowa
Stylus Scan 2000 | ? | unsupported |  | epkowa (1.15.0) | sane-epkowa
Stylus Scan 2500 | USB | untested |  | epkowa (1.15.0) | sane-epkowa

### Manufacturer: Genius

Link(s): http://www.genius-kye.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
ColorPage-Vivid Pro II | Parport (EPP) | basic | Similar to Primax Colorado Direct 9600, but with EICI 091000 ASIC | geniusvp2 | ?
Colorpage-Vivid+ | Parport | untested |  | primax | ?
Vivid Pro USB | USB | basic | Linux 2.4 only, needs a kernel patch. | viceo (0.6) | ?

### Manufacturer: Hewlett Packard

Link(s): http://www.hp.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
ScanJet 3770 | USB | good |  | hp3770 | ?
ScanJet 8200 | USB | good |  | hp8200 | ?

### Manufacturer: Hewlett-Packard

Link(s): http://www.hp.com/, http://www.hp.com/go/all-in-one

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
HP4400C | USB | basic | grayscale 300DPI only | hp_rts88xx | ?
HP4470C | USB | basic | grayscale 300DPI only, XPA/bed mode | hp_rts88xx | ?
Most HP OfficeJet, LaserJet, and PSC (Printer/Scanner/Copier) multi-function peripherals | Parport(ECP) USB JetDirect | good | Distributed with the HP OfficeJet Linux driver (hpoj) | hpoj | ?
Most HP OfficeJet, LaserJet, and PSC (Printer/Scanner/Copier) multi-function peripherals | Parport(ECP) USB JetDirect | good | Distributed with the HP Linux Imaging and Printing Project (hplip), see table on website for product support status | hpaio | ?
ScanJet 4200c | USB | minimal | 8bpp, 150/300/600 dpi only, and scanned image needs postprocessing | hp4200 | ?

### Manufacturer: IBM

Link(s): http://www.ibm.com/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
IdeaScan 2000 USB | USB | basic | Linux 2.4 only, needs a kernel patch. | viceo (0.6) | ?

### Manufacturer: LG Electronics

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Scanworks 600U | USB | basic | Linux 2.4 only, needs a kernel patch. | viceo (0.6) | ?

### Manufacturer: Mustek

Comment: Other models may also be supported.

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
CG-6000 | Proprietary | untested | Old handscanner. Hasn't been tested for a long time but once worked. See link for the linux kernel driver that's necessary to run the scanner. | lhii | ?

### Manufacturer: Network

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Scanny MM100 | Parport | good |  | primax | ?

### Manufacturer: Primax

Link(s): http://www.primax.nl/

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Colorado 2200 USB | USB | untested | Untested. See link for details. Linux 2.4 only, needs a kernel patch. | viceo (0.6) | ?
Colorado Direct 300 | Parport | good |  | primax | ?
Colorado Direct 600/30bit | Parport | untested |  | primax | ?
Colorado USB 19200 | USB | basic | Linux 2.4 only, needs a kernel patch. | viceo (0.6) | ?

### Manufacturer: Samsung

Link(s): http://www.samsung.com/
Comment: Multi Function Peripheral. External backend made by Samsung.

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
For models not mentioned, check their website | USB | untested | No information received about supported status | samsung | ?
SCX-4016 | Parport USB | untested | No information received about supported status | samsung | ?
SCX-4100 | Parport USB | good | Is reported to work. | samsung | ?
SCX-4216F | Parport USB | untested | No information received about supported status | samsung | ?
SCX-4720F | Parport USB | untested | No information received about supported status | samsung | ?
SCX-6220 | Parport USB | untested | No information received about supported status | samsung | ?
SCX-6320F | Parport USB | untested | No information received about supported status | samsung | ?
SF-565P | Parport USB | untested | No information received about supported status | samsung | ?
SF-755P | Parport USB | untested | No information received about supported status | samsung | ?

### Manufacturer: Storm

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
ImageWave | Parport | untested |  | primax | ?
Totalscan | Parport | untested |  | primax | ?

### Manufacturer: TemPlate

Link(s): http://www.template.com/, http://www.template.de/
Comment: TemPlate scanners are sometimes labeled "TMP "

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Templ Z | SCSI | untested | With Z-Axis scrolling | template (0.42, NEW!) | sane-template
Templ ZQ | USB | minimal |  | template (0.42, NEW!) | sane-template
Templ ZS | USB | unsupported | No support yet, but we have docs. | template (0.42, NEW!) | sane-template
Templ ZY | SCSI | basic |  | template (0.42, NEW!) | sane-template
Templ ZZ | SCSI | good |  | template (0.42, NEW!) | sane-template

### Manufacturer: Visioneer

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
OneTouch 6100 | USB | basic | Linux 2.4 only, needs a kernel patch. | viceo (0.6) | ?
OneTouch 7600 | USB | basic | Linux 2.4 only, needs a kernel patch. | viceo (0.6) | ?
OneTouch 8600 | USB | basic | Linux 2.4 only, needs a kernel patch. | viceo (0.6) | ?

## Still Cameras

Manufacturers: (none)

## Video Cameras

Manufacturers: Aiptek, Digital Dream, Konica

### Manufacturer: Aiptek

Link(s): http://www.aiptek.com.tw

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
Aiptek Pencam | USB | minimal | usb vid 0c0553 pid 0x0202, image is OK for CIF and QCIF, VGA and QVGA untested, streaming video is a problem | stv680 | ?

### Manufacturer: Digital Dream

Link(s): http://www.digitaldreamco.com/en/index.shtml

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
l' espion XS | USB | untested | usb vid 0x1183 pid 0x0001 | stv680 | ?

### Manufacturer: Konica

Link(s): http://www.konicaminolta.com

Model | Interface | Status | Comment | Backend | Manpage
--- | --- | --- | --- | --- | ---
e-mini | USB | untested | usb vid 0x04c8 pid 0x0722 | stv680 | ?

## APIs

Backends: template, v4l2

### Backend: template (0.42, NEW!)

Link(s): http://www.luser.com/temp/, http://www.luser.com/b/
Manual page: sane-template
Comment: This backend supports only the USB and SCSI models
Description: Interface to FrObYz API
Comment: Only FrObYz version 2.0 is supported!

### Backend: v4l2

Link(s): http://video.inodes.org/sane-v4l2/
Comment: The status of this backend is unknown. It hasn't been updated for years. The v4l2 API is now in Linux 2.5 but it's not clear if the v4l2 backend is compatible to that API.
Description: Interface to Video For Linux 2 API

## Meta Backends

Backends: (none)

### Legend:

> Model:
>   Name of the the device.
> Interface:
>   How the device is connected to the computer.
> Status:
>   Indicates how many of the features the device provides are supported by SANE.
>   - unsupported means the device is not supported at least by this backend. It may be supported by other backends, however.
>   - untested means the device may be supported but couldn't be tested. Be very careful and report success/failure.
>   - minimal means that the device is detected and scans at least in one mode. But the quality is bad or important features won't work.
>   - basic means it works at least in the most important modes but quality is not perfect.
>   - good means the device is usable for day-to-day work. Some rather exotic features may be missing.
>   - complete means the backends supports everything the device can do.
> Comment:
>   More information about the backend or model, e.g. the level of support and possible problems.
> Backend:
>   Name of the backend, in parentheses if available: Version of backend/driver; newer versions may be available from their home sites.
>   NEW! means brand-new to the current release of SANE.
>   UNMAINTAINED means that nobody maintains that backend. Expect no new features or newly supported devices. You are welcome to take over maintainership.
> Manual Page:
>   A link to the man-page online, if it exists.
> Manufacturer:
>   Manufacturer, vendor or brand name of the device.
> Description:
>   The scope of application of the backend.

SANE homepage
This page was last updated on Mon Aug 8 08:22:53 2005