           install-memo  -  Installs  a  new Memo Pad entry onto your
           Palm handheld.

## SECTION

           pilot-link: Userland Conduits

## SYNOPSIS

           install-memo [-p|--port <port>]  [--version]  [-q|--quiet]
           [-?|--help]  [--usage] [-c|--category name] [-r|--replace]
           [-t|--title] [-f|--file STRING]

## DESCRIPTION

           install-memo allows the user to write one or more files as
           a new memo or memos, respectively, onto the Palm handheld.

## OPTIONS

       INSTALL-MEMO OPTIONS
           -c, --category category
                  Install memo(s) to category defined by category  by
                  default.  Normally  install-memo  uses  the Unfiled
                  category as the default category if no category  is
                  chosen.

           -f, --file STRING
                  File containing the target memo entry

           -r, --replace
                  Replace  all memos in the category specified by the
                  -c category option.

           -t --title
                  Use the filename as the title for the  memo.  (Nor-
                  mally,  the  first  line  of  a memo is used as the
                  title if one is not supplied with the -t option).

       CONDUIT OPTIONS
           -p, --portport
                  Use device file <port> to communicate with the Palm
                  handheld.  If  this  is not specified, install-memo
                  will look for the $PILOTPORT environment  variable.
                  If neither are found or supplied, install-memo will
                  print the usage information.

           -v, --version
                  Display version of install-memo  and  exit  without
                  connecting.

       HELP OPTIONS
           -h, --help
                  Display the help synopsis for install-memo and exit
                  without connecting.

                  necting.

## USAGE

           The  program will connect to the Palm handheld, and create
           memo entries for each file(s)  given  on  the  commandline
           into the Memo Pad application on the Palm.

## AUTHOR

           install-memo  was  originally  written  by  Damien P. Neil
           neild@rpi.edu.

           This manual page was written by Neil Williams  linux@code-
           help.co.uk

## BUGS

       KNOWN BUGS
           The  Palm  Device has a maximum length of 4,096 bytes (4k)
           on memopad entries, if you wish to retain the  ability  to
           edit  the Memo (add/remove/change data within the memo) on
           the Palm itself. You can create a  memo  entry  of  65,490
           bytes in size (the absolute maximum) if you do not need to
           edit the memo entry any further on the Palm device itself.
           Any  memo  larger  than  4,096  bytes and less than 65,490
           bytes will not be editable on the  Palm  itself.  Consider
           these memo entries "read-only".

           This  is not specifically a "bug", but a limitation in the
           PalmOS design itself.

       REPORTING BUGS
           Report bugs at http://bugs.pilot-link.org/

## COPYRIGHT

           This program is free software;  you  can  redistribute  it
           and/or modify it under the terms of the GNU General Public
           License as published  by  the  Free  Software  Foundation;
           either  version  2 of the License, or (at your option) any
           later version.

           This program is distributed in the hope that  it  will  be
           useful, but WITHOUT ANY WARRANTY; without even the implied
           warranty of MERCHANTABILITY or FITNESS  FOR  A  PARTICULAR
           PURPOSE.  See  the  GNU  General  Public  License for more
           details.

           You should have received a copy of the GNU General  Public
           License along with this program; if not, write to the Free
           Software Foundation, Inc., 59  Temple  Place,  Suite  330,
           Boston, MA 02111-1307 USA

## SEE ALSO

           memos(1), pilot-link(7).