Next: 13. Telescope and CCD Up: Fitsblink 2.1 user manual Previous: 11. Blinking
Subsections

- 12.1 Detection of stars
  - 12.1.1 Parameters
  - 12.1.2 Star list format
  - 12.1.3 Loading a star list
  - 12.1.4 Right mouse button
  - 12.1.5 Non-interactive mode
- 12.2 Star matching
  - 12.2.1 You need some catalog
  - 12.2.2 How it works
  - 12.2.3 What if matching fails?
  - 12.2.4 Non-interactive mode
- 12.3 Astrometry
- 12.4 Sending a report
- 12.5 Settings

# 12. Astrometry

With `fitsblink` it is possible to measure star positions. To do this, it is first necessary to detect stars on the image, then to find a match between the detected stars and stars from a catalog, and to make a transformation between the two sets of stars.

## 12.1 Detection of stars

You start star detection of the currently displayed image by choosing the Detect stars item in the Astrometry menu. Detection of stars has two steps: in the first step sky background levels are determined as a function of position inside the image, and in the second step stars are actually counted and their positions and intensities are determined. A list of these quantities, along with a star ID number, is stored in a memory. It is possible to store the results of star detection into a file by choosing the Save star list item. Format of the output file is fairly simple: input file name followed by a list of stars. For each star, there is a star ID, an x coordinate, a y coordinate and star intensity. If star matching is performed (see subsection 12.2) successfully Save star list also outputs celestial star coordinates expressed in decimal degrees.

Note that the stars which touch the edge of image are not reported.

### 12.1.1 Parameters

There are only five parameters concerning star detection that can be changed. You can find them in the Astrometry Options window. You can set Sigma above background value, which is a sensitivity threshold expressed in units of standard deviation of the image background level. Typically you will use values between 3.0 and 5.0. The Minimal accepted intensity is a threshold value expressed in pixel intensity units. A star is not detected if its total intensity is less than the minimal accepted intensity. This parameter is less important (and a bit redundant) and you can keep it close to zero. The Minimal star size in pixels is mostly used to prevent detection of hot pixels as stars. Normally you will keep this value equal 2.

In certain applications it may be desired that the stars lying close to the image edge are not detected. This can be handled by the Insensitive edge parameter. It defines the number of pixels from each of the image edges where the stars are not reported. Finally, the Background grid size determines the size of grid elements inside which background values are determined. This value should not be too big, otherwise gradients in background level may not be detected. Also, it should not be too small or background will be affected by bright stars and other objects more than you want. Values between 30 and 50 should be fine for most cases.

### 12.1.2 Star list format

Here are first few lines from the `98kd3r5.dat` file.

    Input file name: 98kd3r5.fts.gz
        0  203.41  425.36    33961.00 222.426891  0.361738 g 03261330   0.10  11.76
        1  340.29  487.03    21952.00 222.393445  0.289046 g 03261311   0.10  12.39
        2  211.92  187.61     5991.00 222.553634  0.356243 g 03270218   0.35  13.91
        3  198.20  369.38     4987.00 222.456765  0.364289 g 03260027   0.08  14.42
        4   62.06   97.30     4557.00 222.602409  0.435737 g 03270409   0.07  14.39
        5  219.05  256.28     4551.00 222.516988  0.352721 g 03270212   0.21  14.54
        6  339.95  424.35     4321.00 222.426869  0.288976
        7  251.13  269.00     3627.00 222.510071  0.335679 g 03270167   0.12  14.88
        8  332.75   64.77     2982.00 222.618637  0.291364 g 03270098   0.11  15.07
        9  254.19  111.81     1924.00 222.593878  0.333415
       10  150.39  232.54     1657.00 222.529929  0.389214 g 03270315   0.41  15.38
       11  172.09  507.79     1654.00 222.383064  0.378755

In the first line there is the name of the image that was used to produce the star list. Columns for the following rows have the following meanings:

1.
  Star ID for this image;
2.
  Star x coordinate;
3.
  Star y coordinate;
4.
  Star intensity (sum of pixels belonging to a star minus the local background)
5.
  Right ascension in decimal degrees.
6.
  Declination in decimal degrees
7.
  If match with a catalog star is found, a single letter tells catalog which was used. For now `g` stands for the GSC and `u` stands for the USNO SA.
8.
  If the catalog is GSC, here is a star ID for this catalog.
9.
  Residual expressed in arc seconds.
10.
  Star magnitude from the catalog.

Only first four columns are always present, columns from 5 on appear only if the coordinate transformation between image and catalog coordinates was successfully made and a matching catalog star was found.

### 12.1.3 Loading a star list

Star list can be also imported. Choose Load star list item and select the wanted file name. Please note that the first line in the input file is ignored. `Fitsblink` reads star lists it has produced, but it should be an easy exercise to convert any star list to the desired format: you need a star id in the first column, x and y coordinates in the second and third column and star intensity (not magnitude) in the fourth column.

### 12.1.4 Right mouse button

After succesfully detecting stars or importing of a star list you can display star coordinates by pointing a cursor to it and pressing the right mouse button.

###
12.1.5 Non-interactive mode

Extraction of star lists is often desired in a noninteractive mode. It is possible to use `fitsblink` in such a mode. You need a soft link named `starcount` (do `ln -s fitsblink starcount`), which points to the `fitsblink` program. If you run `fitsblink` using the name `starcount`, it will perform star counting on the input image. Command line parameters are:

- `-l logname` name of the log file;
- `-m gridsize` size of the grid element for background determination;
- `-s threshold` intensity threshold expressed in units of background variation;
- `-i intensity` absolute intensity threshold;
- `-c starsize` minimum star linear size (in pixels).

##
12.2 Star matching

After the star detection, it is possible to match the detected stars with stars from a star catalog. This is an operation which can easily fail if you do something wrong. You should practice on one of the test images distributed together with the `fitsblink` program. Parameters needed for star matching (WCS values) can be either read from the FITS file header or input manually by choosing the Edit parameters item from the Astrometry menu. The pixel size values should be correct within few percent. Also, center coordinates should not be off by more than half of field. The rotation angle does not need to be changed because `fitsblink` finds (or does not find) a match regardless of image orientation.

Figure 2: Edit parameters window.

### 12.2.1 You need some catalog

To do star matching, you need at least one of the supported star catalogs. Currently `fitsblink` reads GSC 1.1 and USNO SA 1.0 catalogs. Both are distributed on CD-ROM and must be purchased separately. You need to mount the CD-ROM somewhere in the directory structure of your computer and make sure that you are allowed to read it. You choose the catalogs and set their paths in a window which appears after you choose the Catalogs item from the Astrometry menu (fig. 3).

Figure 3: Catalogs window.

### 12.2.2 How it works

Matching subroutine uses constellations of stars from star lists extracted from both the CCD image and the catalog. In the initial phase, it only uses a subset of bright stars from both images. For each star in this subset it forms a constellation using the nearest stars from the subset. Then it tries to find a constellation of stars from the catalog which completely or partly matches the reference constellation. Each attempt of matching is given a value which indicates a level of similarity between the reference constellation and the constellation under investigation. The maximum value that can be achieved is n(n+1)/2, where n is the number you type in Number of stars in constellation field of the Astrometry options form. This number is never actually reached because stars from the CCD image never exactly match stars from the catalogue.

If the match is successful, a bilinear transformation between the coordinate system is calculated and results of matching are presented in a window. It is possible to write the newly calculated WCS values directly into the FITS header (see also non-interactive mode). This is only possible for the noncompressed images, because the cfitsio library does not write the compressed images yet.

Figure 4: Display of input and calculated WCS coordinates.

### 12.2.3 What if matching fails?

There may be many reasons why matching between star lists extracted from a CCD image and a catalog fails. They are the following:

- Wrong image coordinates. Although `fitsblink` is tolerant to small discrepancies of image center coordinates, it can not search a very wide field around the assumed center coordinates. Catalog image is extended 30 % in each of four directions, so it covers 2.56 times the area that CCD image has. Anything outside this can not be matched.

- Wrong pixel angular sizes. The algorithm for star detection is not scale insensitive, as is, for example, `match` written by Michael Richmond. So, you need to know actual pixel dimensions rather accurately, to some 1 %. If you poorly know pixel dimensions, you should recall Astrometry options input form and enlarge Maximal positional error in pixels value to 20 or 40 pixels. You will get some warnings, but you can ignore them. If you do this, star matching routine will be more tolerant. If matching succeeds, you will get the calculated pixel sizes and you should use these values in the future. However, if you don't know angular pixel size with better then 10 % accuracy, you really should rethink your intention to do astrometry.

- Bad choice of star catalog. If angular dimensions of your CCD image are very small (15' or less), it may happen that you will not have enough comparison stars from the catalog. It is better to use USNO SA catalog for small fields. On the other side, in large fields there will be a lot of bright stars which are typically absent from the USNO SA catalog, so the program will not find comparison stars in the catalog. So, for large fields, it is better to use GSC catalog.

If you are reasonably sure about the correctness of the star field coordinates as well as the pixel size(s) and you still can not get a match, try the following in Astrometry options form:

1.
  Decrease Minimal value to accept constellation. This helps if you don't have enough stars either on the CCD image or in the catalog. If you decrease this value too much, you will get a lot of false matches and the coordinate transformation you will get will be wrong.
2.
  Increase Number of bright stars in initial matching. This may help if the CCD field and the catalog field only partially overlap or if you get a lot of spurious objects near some bright star or star cluster. Increasing this number too much may increase processing time dramatically.
3.
  Increase Number of stars in constellation. Bigger constellations are more likely to have some stars in common. Increases processing time. Do not use more than 20 stars.
4.
  Increasing Maximal positional error in pixels will treat incorrect pixel sizes but also increase matching time and possibly cause false matches.

Do the above parameter adjustment in the order as described here. As your despair increases, start to combine changes of different parameters until you finally get a match.

###
12.2.4 Non-interactive mode

Star matching with a catalog can be done also in a command line mode. By making a link `catalog` which points to `fitsblink` it is possible to run `fitsblink` with a command `catalog`. Output file name will be made automatically by stripping off whatever follows the last ``.'' and replacing it by an extension `dat`. Some attention is required here because there are chances that the output `.dat` file gets the same name as the input `.dat` file. This may not be desired in some cases. A possible solution for this is to rename the input `.dat` file.

- `-l` log file name
- `-b` number of bright stars
- `-a` right ascension of the center pixel (in decimal degrees)
- `-d` declination (in decimal degrees)
- `-w` width of a pixel (in arc seconds)
- `-h` height of a pixel (in arc seconds)
- `-x` number of pixels in x direction
- `-y` number of pixels in y direction
- `-f` name of the input star list
- `-n` number of stars in constellation
- `-m` minimal constellation value
- `-e` allowed arror in pixels
- `-i` allowed intensity error (factor)
- `-r` residual in arc-seconds
- `-c` catalog name and path (eg. `usno:/cdrom`, can be also `gscn:` for GSC North or `gscs:` for GSC South)
- `-W` write newly calculated WCS values into the FITS file header

Here is a command line useful for the example image `98kd3r5.fts.gz`:

    catalog -f 98kd3r5.dat -a 222.5 -d 0.366 -w 1.92 -h 1.92 \
    	-c gscn:/cdrom -x 356 -y 541

The backslash above means continuation of the command line. Please note again that the center coordinates are specified in DECIMAL degrees. Default values for catalog matching are the same as in the interactive mode. As in the interactive mode, it is not possible to write the WCS values into the header (the -W option) if the image file is compressed.

##
12.3 Astrometry

Finally! You successfully made all of the previous steps and you want to do astrometry of the asteroid you just imaged. Go to the Astrometry menu and choose the Do astrometry item. When inside the image, cursor shape will change from a box to a cross. Now point to some of the objects (red circles) and click left button on it. You will be asked for the object designation. When you enter it and click on the OK button, a window with the report suitable for sending to MPC (Minor Planet Center) will appear. At this point you can either send the report immediatelly or proceed with further astrometry. Coordinates are for the equinox J2000.

##
12.4 Sending a report

The report window is used for editing and sending astrometry positions to the MPC. It is shown in fig. 5

Figure 5: Astrometry report window.

Sending astrometry reports to MPC requires certain format. `Fitsblink` writes information about the measurement in this format. Additionally, you have to give some basic information about you and about the measurement. If this information is present in the header of the image file or in the `.fitsblinkrc` file, it will be inserted in the message if you press the Insert header button. Otherwise you will have to type this information by yourself. You can use the Send astrometry report form as a primitive line editor and add additional information to the file which will be sent. When you press the Send button and comfirm your decision, the message is sent to whatever addresses you wrote into To: and CC: fields. So, be careful with this.

## 12.5 Settings

The following default settings can be written into file `$HOME/.fitsblinkrc` by `fitsblink` and then read at the start-up time.

Figure 6: Catalog paths: these are the places where the supported catalogs can be found.

Figure 7: Observatory settings: Observatory code, observer name(s), telescope name and size and instrument type.

Figure 8: Display settings: color or grey level and delay between blinking images.

Figure 9: Mail defaults.

Figure 10: Telescope control commands.

Figure 11: Camera control commands.

Figure 12: Help system.

Next: 13. Telescope and CCD Up: Fitsblink 2.1 user manual Previous: 11. Blinking