- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16CE625
| Bank 0 |  | Bank 1 |
INDF | 0x000
TMR0 | 0x001
PCL | 0x002
STATUS | 0x003
FSR | 0x004
PORTA | 0x005
PORTB | 0x006
PCLATH | 0x00A
INTCON | 0x00B
PIR1 | 0x00C
CMCON | 0x01F
OPTION_REG | 0x081
TRISA | 0x085
TRISB | 0x086
PIE1 | 0x08C
PCON | 0x08E
EEINTF | 0x090
VRCON | 0x09F
The mirror of [PCL, STATUS, ...] are not shown.

SFR

SFR with alias name.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.