- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC10F222
CONFIG (address:0x0FFF, mask:0xFFFF)
IOSCFS -- Internal Oscillator Frequency Select bit
| IOSCFS = 4MHZ | 0x0FFE | 4 MHz. |
| IOSCFS = 8MHZ | 0x0FFF | 8 MHz. |
IOFSCS -- Internal Oscillator Frequency Select bit
| IOFSCS = 4MHZ | 0x0FFE | 4 MHz. |
| IOFSCS = 8MHZ | 0x0FFF | 8 MHz. |
MCPU -- Master Clear Pull-up Enable bit
| MCPU = ON | 0x0FFD | Pull-up enabled. |
| MCPU = OFF | 0x0FFF | Pull-up disabled. |
WDTE -- Watchdog Timer Enable bit
| WDTE = OFF | 0x0FFB | WDT disabled. |
| WDTE = ON | 0x0FFF | WDT enabled. |
CP -- Code protection bit
| CP = ON | 0x0FF7 | Code protection on. |
| CP = OFF | 0x0FFF | Code protection off. |
MCLRE -- GP3/MCLR Pin Function Select bit
| MCLRE = OFF | 0x0FEF | GP3/MCLR pin function is digital I/O, MCLR internally tied to VDD. |
| MCLRE = ON | 0x0FFF | GP3/MCLR pin function is MCLR. |

This page generated automatically by the device-help.pl program (2012-12-22 23:50:57 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.