- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16C505
| Coff ID of device | 0x2505 |
| Number of ROM/FLASH pages | 2 (512 words/pages)
| Last address of ROM/FLASH | 0x03FF (1024 words)
| Address space of User ID | 0x0400 - 0x0403 (4 bytes)
| Address of Configuration Word | 0x0FFF (1 word)
| Number of RAM Banks | 4 (32 bytes/banks)
| Number of SFRs | 8
| Size of GPRs | 120 bytes
| Joint size of SFRs + GPRs | 128 bytes

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.