- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16CR83
| Bank 0 |  | Bank 1 |
| SFR 0x000 - 0x006 7 bytes Unimplemented 0x007 SFR 0x008 - 0x00B 4 bytes GPR 0x00C - 0x02F 36 bytes Unimplemented 0x030 - 0x07F 80 bytes |  | SFR 0x080 - 0x086 7 bytes Unimplemented 0x087 SFR 0x088 - 0x08B 4 bytes Unimplemented 0x08C - 0x0FF 116 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

| SFR 11 bytes GPR 36 bytes Shared 0 bytes Unimplemented 81 bytes |  | SFR 11 bytes GPR 0 bytes Shared 0 bytes Unimplemented 117 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

Special Function Register.

General-purpose RAM.

Shared RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.