- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F527
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |
| SFR 0x000 - 0x00B 12 bytes Shared 0x00C - 0x00F 4 bytes GPR 0x010 - 0x01F 16 bytes |  | SFR 0x020 - 0x02A 11 bytes GPR 0x02B Shared 0x02C - 0x02F 4 bytes GPR 0x030 - 0x03F 16 bytes |  | SFR 0x040 Unimplemented 0x041 SFR 0x042 - 0x044 3 bytes GPR 0x045 - 0x04B 7 bytes Shared 0x04C - 0x04F 4 bytes GPR 0x050 - 0x05F 16 bytes |  | SFR 0x060 - 0x069 10 bytes GPR 0x06A - 0x06B 2 bytes Shared 0x06C - 0x06F 4 bytes GPR 0x070 - 0x07F 16 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

| SFR 12 bytes GPR 16 bytes Shared 4 bytes Unimplemented 0 bytes |  | SFR 11 bytes GPR 17 bytes Shared 4 bytes Unimplemented 0 bytes |  | SFR 4 bytes GPR 23 bytes Shared 4 bytes Unimplemented 1 bytes |  | SFR 10 bytes GPR 18 bytes Shared 4 bytes Unimplemented 0 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

Special Function Register.

General-purpose RAM.

Shared RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.