- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F687
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |
INDF | 0x000
TMR0 | 0x001
PCL | 0x002
STATUS | 0x003
FSR | 0x004
PORTA | 0x005
PORTB | 0x006
PORTC | 0x007
PCLATH | 0x00A
INTCON | 0x00B
PIR1 | 0x00C
PIR2 | 0x00D
TMR1TMR1L | 0x00E
TMR1H | 0x00F
T1CON | 0x010
SSPBUF | 0x013
SSPCON | 0x014
RCSTA | 0x018
TXREG | 0x019
RCREG | 0x01A
ADRESH | 0x01E
ADCON0 | 0x01F
OPTION_REG | 0x081
TRISA | 0x085
TRISB | 0x086
TRISC | 0x087
PIE1 | 0x08C
PIE2 | 0x08D
PCON | 0x08E
OSCCON | 0x08F
OSCTUNE | 0x090
MSKSSPADD SSPMSK | 0x093
SSPSTAT | 0x094
WPUWPUA | 0x095
IOCIOCA | 0x096
WDTCON | 0x097
TXSTA | 0x098
SPBRG | 0x099
SPBRGH | 0x09A
BAUDCTL | 0x09B
ADRESL | 0x09E
ADCON1 | 0x09F
EEDATEEDATA | 0x10C
EEADR | 0x10D
WPUB | 0x115
IOCB | 0x116
VRCON | 0x118
CM1CON0 | 0x119
CM2CON0 | 0x11A
CM2CON1 | 0x11B
ANSEL | 0x11E
ANSELH | 0x11F
EECON1 | 0x18C
EECON2 | 0x18D
SRCON | 0x19E
The mirror of [PCL, STATUS, ...] are not shown.

SFR

SFR with alias name.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.