- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC10F206
| Bank 0 |
| SFR 0x000 - 0x007 8 bytes GPR 0x008 - 0x01F 24 bytes |

| SFR 8 bytes GPR 24 bytes Unimplemented 0 bytes |

Special Function Register.

General-purpose RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:57 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.