- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC18F46J53
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |  | Bank 4 |  | Bank 5 |  | Bank 6 |  | Bank 7 |  | Bank 8 |  | Bank 9 |  | Bank 10 |  | Bank 11 |  | Bank 12 |  | Bank 13 |  | Bank 14 |  | Bank 15 |
| GPR 0x000 - 0x0FF 256 bytes |  | GPR 0x100 - 0x1FF 256 bytes |  | GPR 0x200 - 0x2FF 256 bytes |  | GPR 0x300 - 0x3FF 256 bytes |  | GPR 0x400 - 0x4FF 256 bytes |  | GPR 0x500 - 0x5FF 256 bytes |  | GPR 0x600 - 0x6FF 256 bytes |  | GPR 0x700 - 0x7FF 256 bytes |  | GPR 0x800 - 0x8FF 256 bytes |  | GPR 0x900 - 0x9FF 256 bytes |  | GPR 0xA00 - 0xAFF 256 bytes |  | GPR 0xB00 - 0xBFF 256 bytes |  | GPR 0xC00 - 0xCFF 256 bytes |  | GPR 0xD00 - 0xDFF 256 bytes |  | GPR 0xE00 - 0xEAF 176 bytes Unimplemented 0xEB0 - 0xEB7 8 bytes SFR 0xEB8 - 0xEBC 5 bytes Unimplemented 0xEBD - 0xEBE 2 bytes SFR 0xEBF - 0xECD 15 bytes Unimplemented 0xECE - 0xED0 3 bytes SFR 0xED1 - 0xED8 8 bytes Unimplemented 0xED9 - 0xEE0 8 bytes SFR 0xEE1 - 0xEE4 4 bytes Unimplemented 0xEE5 SFR 0xEE6 - 0xEEA 5 bytes Unimplemented 0xEEB - 0xEF1 7 bytes SFR 0xEF2 - 0xEF4 3 bytes Unimplemented 0xEF5 - 0xEF6 2 bytes SFR 0xEF7 - 0xEF8 2 bytes Unimplemented 0xEF9 - 0xEFB 3 bytes SFR 0xEFC - 0xEFF 4 bytes |  | SFR 0xF00 - 0xF42 67 bytes Unimplemented 0xF43 SFR 0xF44 - 0xFD3 144 bytes Unimplemented 0xFD4 SFR 0xFD5 - 0xFFF 43 bytes |

| SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 46 bytes GPR 176 bytes Unimplemented 34 bytes |  | SFR 254 bytes GPR 0 bytes Unimplemented 2 bytes |

Special Function Register.

General-purpose RAM.

In this place no RAM.

Special Function Register on Access Area.

General-purpose RAM on Access Area.

In this place no RAM on Access Area.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:59 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.