- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F723A
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |
| SFR 0x000 - 0x007 8 bytes Unimplemented 0x008 SFR 0x009 - 0x01F 23 bytes GPR 0x020 - 0x06F 80 bytes Shared 0x070 - 0x07F 16 bytes |  | SFR 0x080 - 0x087 8 bytes Unimplemented 0x088 SFR 0x089 - 0x096 14 bytes Unimplemented 0x097 SFR 0x098 - 0x099 2 bytes Unimplemented 0x09A - 0x09B 2 bytes SFR 0x09C - 0x09D 2 bytes Unimplemented 0x09E SFR 0x09F GPR 0x0A0 - 0x0EF 80 bytes Shared 0x0F0 - 0x0FF 16 bytes |  | SFR 0x100 Unimplemented 0x101 SFR 0x102 - 0x104 3 bytes Unimplemented 0x105 - 0x107 3 bytes SFR 0x108 - 0x10F 8 bytes Unimplemented 0x110 - 0x11F 16 bytes GPR 0x120 - 0x12F 16 bytes Unimplemented 0x130 - 0x16F 64 bytes Shared 0x170 - 0x17F 16 bytes |  | SFR 0x180 Unimplemented 0x181 SFR 0x182 - 0x186 5 bytes Unimplemented 0x187 - 0x189 3 bytes SFR 0x18A - 0x18C 3 bytes Unimplemented 0x18D - 0x1EF 99 bytes Shared 0x1F0 - 0x1FF 16 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

| SFR 31 bytes GPR 80 bytes Shared 16 bytes Unimplemented 1 bytes |  | SFR 27 bytes GPR 80 bytes Shared 16 bytes Unimplemented 5 bytes |  | SFR 12 bytes GPR 16 bytes Shared 16 bytes Unimplemented 84 bytes |  | SFR 9 bytes GPR 0 bytes Shared 16 bytes Unimplemented 103 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

Special Function Register.

General-purpose RAM.

Shared RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.