- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F707
CONFIG1 (address:0x2007, mask:0xFFFF)
FOSC -- Oscillator Selection bits
| FOSC = LP_OSC | 0x3FF8 | LP oscillator: Low-power crystal on RA6/OSC2/CLKOUT and RA7/OSC1/CLKIN. |
| FOSC = XT_OSC | 0x3FF9 | XT oscillator: Crystal/resonator on RA6/OSC2/CLKIN and RA7/OSC1/CLKIN. |
| FOSC = HS_OSC | 0x3FFA | HS oscillator: High Speed crystal/resonator on RA6/OSC2/CLKOUT and RA7/OSC1/CLKIN. |
| FOSC = EC_OSC | 0x3FFB | EC oscillator: I/O function on RA6/OSC2/CLKOUT pin, CLKIN on RA7/OSC1/CLKIN. |
| FOSC = INTOSCIO | 0x3FFC | INTOSCIO oscillator: I/O function on RA6/OSC2/CLKOUT and RA7/OSC1/CLKIN pins. |
| FOSC = INTOSC | 0x3FFD | INTOSC oscillator: CLKOUT function on RA6/OSC2/CLKOUT pin, I/O function on RA7/OSC1/CLKIN. |
| FOSC = EXTRCIO | 0x3FFE | RCIO oscillator: I/O function on RA6/OSC2/CLKOUT pin, RC on RA7/OSC1/CLKIN. |
| FOSC = EXTRC | 0x3FFF | RC oscillator: CLKOUT function on RA6/OSC2/CLKOUT pin, RC on RA7/OSC1/CLKIN. |
WDTE -- Watchdog Timer Enable bit
| WDTE = OFF | 0x3FF7 | WDT disabled and can be enabled by SWDTEN bit of the WDTCON register. |
| WDTE = ON | 0x3FFF | WDT enabled. |
PWRTE -- Power-up Timer Enable bit
| PWRTE = ON | 0x3FEF | PWRT enabled. |
| PWRTE = OFF | 0x3FFF | PWRT disabled. |
MCLRE -- RE3/MCLR Pin Function Select bit
| MCLRE = OFF | 0x3FDF | RE3/MCLR pin function is digital input, MCLR internally tied to VDD. |
| MCLRE = ON | 0x3FFF | RE3/MCLR pin function is MCLR. |
CP -- Code Protection bit
| CP = ON | 0x3FBF | Program memory code protection is enabled. |
| CP = OFF | 0x3FFF | Program memory code protection is disabled. |
BOREN -- Brown-out Reset Selection bits
| BOREN = OFF | 0x3CFF | BOR disabled (Preconditioned State). |
| BOREN = NSLEEP | 0x3EFF | BOR enabled during operation and disabled in Sleep. |
| BOREN = ON | 0x3FFF | BOR enabled. |
BORV -- Brown-out Reset Voltage Selection bit
| BORV = 25 | 0x3BFF | Brown-out Reset Voltage (VBOR) set to 2.5 V nominal. |
| BORV = 19 | 0x3FFF | Brown-out Reset Voltage (VBOR) set to 1.9 V nominal. |
PLLEN -- INTOSC PLLEN Enable Bit
| PLLEN = OFF | 0x2FFF | INTOSC Frequency is 500 kHz. |
| PLLEN = ON | 0x3FFF | INTOSC Frequency is 16 MHz (32x). |
CONFIG2 (address:0x2008, mask:0xFFFF)
VCAPEN -- Voltage Regulator Capacitor Enable bits
| VCAPEN = RA0 | 0x3FCF | VCAP functionality is enabled on RA0. |
| VCAPEN = RA5 | 0x3FDF | VCAP functionality is enabled on RA5. |
| VCAPEN = RA6 | 0x3FEF | VCAP functionality is enabled on RA6. |
| VCAPEN = OFF | 0x3FFF | All VCAP pin functions are disabled. |

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.