- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16C74B
| Bank 0 |  | Bank 1 |
| SFR 0x000 - 0x01F 32 bytes GPR 0x020 - 0x07F 96 bytes |  | SFR 0x080 - 0x08E 15 bytes Unimplemented 0x08F - 0x091 3 bytes SFR 0x092 - 0x094 3 bytes Unimplemented 0x095 - 0x097 3 bytes SFR 0x098 - 0x099 2 bytes Unimplemented 0x09A - 0x09E 5 bytes SFR 0x09F GPR 0x0A0 - 0x0FF 96 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

| SFR 32 bytes GPR 96 bytes Shared 0 bytes Unimplemented 0 bytes |  | SFR 21 bytes GPR 96 bytes Shared 0 bytes Unimplemented 11 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

Special Function Register.

General-purpose RAM.

Shared RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.