- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F1938
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |  | Bank 4 |  | Bank 5 |  | Bank 6 |  | Bank 7 |  | Bank 8 |  | Bank 15 |  | Bank 31 |
INDF0 | 0x000
INDF1 | 0x001
PCL | 0x002
STATUS | 0x003
FSR0FSR0L | 0x004
FSR0H | 0x005
FSR1FSR1L | 0x006
FSR1H | 0x007
BSR | 0x008
WREG | 0x009
PCLATH | 0x00A
INTCON | 0x00B
PORTA | 0x00C
PORTB | 0x00D
PORTC | 0x00E
PORTE | 0x010
PIR1 | 0x011
PIR2 | 0x012
PIR3 | 0x013
TMR0 | 0x015
TMR1TMR1L | 0x016
TMR1H | 0x017
T1CON | 0x018
T1GCON | 0x019
TMR2 | 0x01A
PR2 | 0x01B
T2CON | 0x01C
CPSCON0 | 0x01E
CPSCON1 | 0x01F
TRISA | 0x08C
TRISB | 0x08D
TRISC | 0x08E
TRISE | 0x090
PIE1 | 0x091
PIE2 | 0x092
PIE3 | 0x093
OPTION_REG | 0x095
PCON | 0x096
WDTCON | 0x097
OSCTUNE | 0x098
OSCCON | 0x099
OSCSTAT | 0x09A
ADRESADRESL | 0x09B
ADRESH | 0x09C
ADCON0 | 0x09D
ADCON1 | 0x09E
LATA | 0x10C
LATB | 0x10D
LATC | 0x10E
LATE | 0x110
CM1CON0 | 0x111
CM1CON1 | 0x112
CM2CON0 | 0x113
CM2CON1 | 0x114
CMOUT | 0x115
BORCON | 0x116
FVRCON | 0x117
DACCON0 | 0x118
DACCON1 | 0x119
SRCON0 | 0x11A
SRCON1 | 0x11B
APFCON | 0x11D
ANSELA | 0x18C
ANSELB | 0x18D
EEADREEADRL | 0x191
EEADRH | 0x192
EEDATEEDATL | 0x193
EEDATH | 0x194
EECON1 | 0x195
EECON2 | 0x196
RCREG | 0x199
TXREG | 0x19A
SPBRGSPBRGL | 0x19B
SPBRGH | 0x19C
RCSTA | 0x19D
TXSTA | 0x19E
BAUDCON | 0x19F
WPUB | 0x20D
WPUE | 0x210
SSPBUF | 0x211
SSPADD | 0x212
SSPMSK | 0x213
SSPSTAT | 0x214
SSPCONSSPCON1 | 0x215
SSPCON2 | 0x216
SSPCON3 | 0x217
CCPR1L | 0x291
CCPR1H | 0x292
CCP1CON | 0x293
PWM1CON | 0x294
CCP1ASECCP1AS | 0x295
PSTR1CON | 0x296
CCPR2L | 0x298
CCPR2H | 0x299
CCP2CON | 0x29A
PWM2CON | 0x29B
CCP2ASECCP2AS | 0x29C
PSTR2CON | 0x29D
CCPTMRS0 | 0x29E
CCPTMRS1 | 0x29F
CCPR3L | 0x311
CCPR3H | 0x312
CCP3CON | 0x313
PWM3CON | 0x314
CCP3ASECCP3AS | 0x315
PSTR3CON | 0x316
CCPR4L | 0x318
CCPR4H | 0x319
CCP4CON | 0x31A
CCPR5L | 0x31C
CCPR5H | 0x31D
CCP5CON | 0x31E
IOCBP | 0x394
IOCBN | 0x395
IOCBF | 0x396
TMR4 | 0x415
PR4 | 0x416
T4CON | 0x417
TMR6 | 0x41C
PR6 | 0x41D
T6CON | 0x41E
LCDCON | 0x791
LCDPS | 0x792
LCDREF | 0x793
LCDCST | 0x794
LCDRL | 0x795
LCDSE0 | 0x798
LCDSE1 | 0x799
LCDDATA0 | 0x7A0
LCDDATA1 | 0x7A1
LCDDATA3 | 0x7A3
LCDDATA4 | 0x7A4
LCDDATA6 | 0x7A6
LCDDATA7 | 0x7A7
LCDDATA9 | 0x7A9
LCDDATA10 | 0x7AA
STATUS_SHAD | 0xFE4
WREG_SHAD | 0xFE5
BSR_SHAD | 0xFE6
PCLATH_SHAD | 0xFE7
FSR0L_SHAD | 0xFE8
FSR0H_SHAD | 0xFE9
FSR1L_SHAD | 0xFEA
FSR1H_SHAD | 0xFEB
STKPTR | 0xFED
TOSL | 0xFEE
TOSH | 0xFEF
The mirror of [PCL, STATUS, ...] are not shown.

SFR

SFR with alias name.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.