- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16LF1459
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |  | Bank 4 |  | Bank 7 |  | Bank 12 |  | Bank 13 |  | Bank 29 |  | Bank 31 |
INDF0 | 0x000
INDF1 | 0x001
PCL | 0x002
STATUS | 0x003
FSR0FSR0L | 0x004
FSR0H | 0x005
FSR1FSR1L | 0x006
FSR1H | 0x007
BSR | 0x008
WREG | 0x009
PCLATH | 0x00A
INTCON | 0x00B
PORTA | 0x00C
PORTB | 0x00D
PORTC | 0x00E
PIR1 | 0x011
PIR2 | 0x012
TMR0 | 0x015
TMR1TMR1L | 0x016
TMR1H | 0x017
T1CON | 0x018
T1GCON | 0x019
TMR2 | 0x01A
PR2 | 0x01B
T2CON | 0x01C
TRISA | 0x08C
TRISB | 0x08D
TRISC | 0x08E
PIE1 | 0x091
PIE2 | 0x092
OPTION_REG | 0x095
PCON | 0x096
WDTCON | 0x097
OSCTUNE | 0x098
OSCCON | 0x099
OSCSTAT | 0x09A
ADRESADRESL | 0x09B
ADRESH | 0x09C
ADCON0 | 0x09D
ADCON1 | 0x09E
ADCON2 | 0x09F
LATA | 0x10C
LATB | 0x10D
LATC | 0x10E
CM1CON0 | 0x111
CM1CON1 | 0x112
CM2CON0 | 0x113
CM2CON1 | 0x114
CMOUT | 0x115
BORCON | 0x116
FVRCON | 0x117
DACCON0 | 0x118
DACCON1 | 0x119
APFCON | 0x11D
ANSELA | 0x18C
ANSELB | 0x18D
ANSELC | 0x18E
PMADRPMADRL | 0x191
PMADRH | 0x192
PMDATPMDATL | 0x193
PMDATH | 0x194
PMCON1 | 0x195
PMCON2 | 0x196
RCREG | 0x199
TXREG | 0x19A
SPBRGL | 0x19B
SPBRGH | 0x19C
RCSTA | 0x19D
TXSTA | 0x19E
BAUDCON | 0x19F
WPUA | 0x20C
WPUB | 0x20D
SSP1BUFSSPBUF | 0x211
SSP1ADDSSPADD | 0x212
SSP1MSKSSPMSK | 0x213
SSP1STATSSPSTAT | 0x214
SSP1CON1SSPCON SSPCON1 | 0x215
SSP1CON2SSPCON2 | 0x216
SSP1CON3SSPCON3 | 0x217
IOCAP | 0x391
IOCAN | 0x392
IOCAF | 0x393
IOCBP | 0x394
IOCBN | 0x395
IOCBF | 0x396
CLKRCON | 0x39A
ACTCON | 0x39B
PWM1DCL | 0x611
PWM1DCH | 0x612
PWM1CONPWM1CON0 | 0x613
PWM2DCL | 0x614
PWM2DCH | 0x615
PWM2CONPWM2CON0 | 0x616
CWG1DBR | 0x691
CWG1DBF | 0x692
CWG1CON0 | 0x693
CWG1CON1 | 0x694
CWG1CON2 | 0x695
UCON | 0xE8E
USTAT | 0xE8F
UIR | 0xE90
UCFG | 0xE91
UIE | 0xE92
UEIR | 0xE93
UFRMUFRMH | 0xE94
UFRML | 0xE95
UADDR | 0xE96
UEIE | 0xE97
UEP0 | 0xE98
UEP1 | 0xE99
UEP2 | 0xE9A
UEP3 | 0xE9B
UEP4 | 0xE9C
UEP5 | 0xE9D
UEP6 | 0xE9E
UEP7 | 0xE9F
STATUS_SHAD | 0xFE4
WREG_SHAD | 0xFE5
BSR_SHAD | 0xFE6
PCLATH_SHAD | 0xFE7
FSR0L_SHAD | 0xFE8
FSR0H_SHAD | 0xFE9
FSR1L_SHAD | 0xFEA
FSR1H_SHAD | 0xFEB
STKPTR | 0xFED
TOSL | 0xFEE
TOSH | 0xFEF
The mirror of [PCL, STATUS, ...] are not shown.

SFR

SFR with alias name.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.