- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC18F26J50
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |  | Bank 4 |  | Bank 5 |  | Bank 6 |  | Bank 7 |  | Bank 8 |  | Bank 9 |  | Bank 10 |  | Bank 11 |  | Bank 12 |  | Bank 13 |  | Bank 14 |  | Bank 15 |
| GPR 0x000 - 0x0FF 256 bytes |  | GPR 0x100 - 0x1FF 256 bytes |  | GPR 0x200 - 0x2FF 256 bytes |  | GPR 0x300 - 0x3FF 256 bytes |  | GPR 0x400 - 0x4FF 256 bytes |  | GPR 0x500 - 0x5FF 256 bytes |  | GPR 0x600 - 0x6FF 256 bytes |  | GPR 0x700 - 0x7FF 256 bytes |  | GPR 0x800 - 0x8FF 256 bytes |  | GPR 0x900 - 0x9FF 256 bytes |  | GPR 0xA00 - 0xAFF 256 bytes |  | GPR 0xB00 - 0xBFF 256 bytes |  | GPR 0xC00 - 0xCFF 256 bytes |  | GPR 0xD00 - 0xDFF 256 bytes |  | GPR 0xE00 - 0xEBF 192 bytes Unimplemented 0xEC0 - 0xEC5 6 bytes SFR 0xEC6 - 0xED3 14 bytes Unimplemented 0xED4 - 0xED6 3 bytes SFR 0xED7 - 0xED8 2 bytes Unimplemented 0xED9 - 0xEE6 14 bytes SFR 0xEE7 - 0xEEA 4 bytes Unimplemented 0xEEB SFR 0xEEC - 0xEEE 3 bytes Unimplemented 0xEEF - 0xEF1 3 bytes SFR 0xEF2 - 0xEF3 2 bytes Unimplemented 0xEF4 - 0xEF5 2 bytes SFR 0xEF6 - 0xEF7 2 bytes Unimplemented 0xEF8 - 0xEFA 3 bytes SFR 0xEFB - 0xEFF 5 bytes |  | Unimplemented 0xF00 - 0xF25 38 bytes SFR 0xF26 - 0xF39 20 bytes Unimplemented 0xF3A - 0xF3B 2 bytes SFR 0xF3C - 0xF42 7 bytes Unimplemented 0xF43 - 0xF47 5 bytes SFR 0xF48 - 0xF4F 8 bytes Unimplemented 0xF50 - 0xF51 2 bytes SFR 0xF52 - 0xF53 2 bytes Unimplemented 0xF54 - 0xF5F 12 bytes SFR 0xF60 - 0xF6B 12 bytes Unimplemented 0xF6C - 0xF6F 4 bytes SFR 0xF70 - 0xF82 19 bytes Unimplemented 0xF83 - 0xF84 2 bytes SFR 0xF85 - 0xF86 2 bytes Unimplemented 0xF87 SFR 0xF88 - 0xF8B 4 bytes Unimplemented 0xF8C - 0xF8D 2 bytes SFR 0xF8E - 0xF94 7 bytes Unimplemented 0xF95 - 0xF96 2 bytes SFR 0xF97 - 0xFD3 61 bytes Unimplemented 0xFD4 SFR 0xFD5 - 0xFFF 43 bytes |

| SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 32 bytes GPR 192 bytes Unimplemented 32 bytes |  | SFR 185 bytes GPR 0 bytes Unimplemented 71 bytes |

Special Function Register.

General-purpose RAM.

In this place no RAM.

Special Function Register on Access Area.

General-purpose RAM on Access Area.

In this place no RAM on Access Area.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:59 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.