- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC18F86J10
| Coff ID of device | 0xC610 |
| Last address of ROM/FLASH | 0x00FFF7 (65528 bytes)
| Address space of Configuration Bytes | 0x00FFF8 - 0x00FFFD (6 bytes)
| Address space of Device ID | 0x3FFFFE - 0x3FFFFF (2 bytes)
| Number of RAM Banks | 16 (256 bytes/banks)
| Number of SFRs | 151
| Size of GPRs | 2048 bytes
| Joint size of SFRs + GPRs | 2199 bytes
| Last address of lower Access RAM | 0x5F

This page generated automatically by the device-help.pl program (2012-12-22 23:51:00 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.