- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16LF1902
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |  | Bank 4 |  | Bank 5 |  | Bank 6 |  | Bank 7 |  | Bank 8 |  | Bank 9 |  | Bank 10 |  | Bank 11 |  | Bank 12 |  | Bank 13 |  | Bank 14 |  | Bank 15 |  | Bank 16 |  | Bank 17 |  | Bank 18 |  | Bank 19 |  | Bank 20 |  | Bank 21 |  | Bank 22 |  | Bank 23 |  | Bank 24 |  | Bank 25 |  | Bank 26 |  | Bank 27 |  | Bank 28 |  | Bank 29 |  | Bank 30 |  | Bank 31 |
| SFR 0x000 - 0x00E 15 bytes Unimplemented 0x00F SFR 0x010 - 0x012 3 bytes Unimplemented 0x013 - 0x014 2 bytes SFR 0x015 - 0x019 5 bytes Unimplemented 0x01A - 0x01F 6 bytes GPR 0x020 - 0x06F 80 bytes linear0: 0x2000 80 bytes Shared 0x070 - 0x07F 16 bytes |  | SFR 0x080 - 0x08E 15 bytes Unimplemented 0x08F SFR 0x090 - 0x092 3 bytes Unimplemented 0x093 - 0x094 2 bytes SFR 0x095 - 0x097 3 bytes Unimplemented 0x098 SFR 0x099 - 0x09E 6 bytes Unimplemented 0x09F GPR 0x0A0 - 0x0BF 32 bytes linear0: 0x2050 32 bytes Unimplemented 0x0C0 - 0x0EF 48 bytes Shared 0x0F0 - 0x0FF 16 bytes |  | SFR 0x100 - 0x10E 15 bytes Unimplemented 0x10F - 0x115 7 bytes SFR 0x116 - 0x117 2 bytes Unimplemented 0x118 - 0x16F 88 bytes Shared 0x170 - 0x17F 16 bytes |  | SFR 0x180 - 0x18D 14 bytes Unimplemented 0x18E - 0x190 3 bytes SFR 0x191 - 0x196 6 bytes Unimplemented 0x197 - 0x1EF 89 bytes Shared 0x1F0 - 0x1FF 16 bytes |  | SFR 0x200 - 0x20B 12 bytes Unimplemented 0x20C SFR 0x20D Unimplemented 0x20E - 0x20F 2 bytes SFR 0x210 Unimplemented 0x211 - 0x26F 95 bytes Shared 0x270 - 0x27F 16 bytes |  | SFR 0x280 - 0x28B 12 bytes Unimplemented 0x28C - 0x2EF 100 bytes Shared 0x2F0 - 0x2FF 16 bytes |  | SFR 0x300 - 0x30B 12 bytes Unimplemented 0x30C - 0x36F 100 bytes Shared 0x370 - 0x37F 16 bytes |  | SFR 0x380 - 0x38B 12 bytes Unimplemented 0x38C - 0x393 8 bytes SFR 0x394 - 0x396 3 bytes Unimplemented 0x397 - 0x3EF 89 bytes Shared 0x3F0 - 0x3FF 16 bytes |  | SFR 0x400 - 0x40B 12 bytes Unimplemented 0x40C - 0x46F 100 bytes Shared 0x470 - 0x47F 16 bytes |  | SFR 0x480 - 0x48B 12 bytes Unimplemented 0x48C - 0x4EF 100 bytes Shared 0x4F0 - 0x4FF 16 bytes |  | SFR 0x500 - 0x50B 12 bytes Unimplemented 0x50C - 0x56F 100 bytes Shared 0x570 - 0x57F 16 bytes |  | SFR 0x580 - 0x58B 12 bytes Unimplemented 0x58C - 0x5EF 100 bytes Shared 0x5F0 - 0x5FF 16 bytes |  | SFR 0x600 - 0x60B 12 bytes Unimplemented 0x60C - 0x66F 100 bytes Shared 0x670 - 0x67F 16 bytes |  | SFR 0x680 - 0x68B 12 bytes Unimplemented 0x68C - 0x6EF 100 bytes Shared 0x6F0 - 0x6FF 16 bytes |  | SFR 0x700 - 0x70B 12 bytes Unimplemented 0x70C - 0x76F 100 bytes Shared 0x770 - 0x77F 16 bytes |  | SFR 0x780 - 0x78B 12 bytes Unimplemented 0x78C - 0x790 5 bytes SFR 0x791 - 0x795 5 bytes Unimplemented 0x796 - 0x797 2 bytes SFR 0x798 - 0x799 2 bytes Unimplemented 0x79A - 0x79F 6 bytes SFR 0x7A0 - 0x7A1 2 bytes Unimplemented 0x7A2 SFR 0x7A3 - 0x7A4 2 bytes Unimplemented 0x7A5 SFR 0x7A6 - 0x7A7 2 bytes Unimplemented 0x7A8 SFR 0x7A9 - 0x7AA 2 bytes Unimplemented 0x7AB SFR 0x7AC Unimplemented 0x7AD - 0x7AE 2 bytes SFR 0x7AF Unimplemented 0x7B0 - 0x7B1 2 bytes SFR 0x7B2 Unimplemented 0x7B3 - 0x7B4 2 bytes SFR 0x7B5 Unimplemented 0x7B6 - 0x7EF 58 bytes Shared 0x7F0 - 0x7FF 16 bytes |  | SFR 0x800 - 0x80B 12 bytes Unimplemented 0x80C - 0x86F 100 bytes Shared 0x870 - 0x87F 16 bytes |  | SFR 0x880 - 0x88B 12 bytes Unimplemented 0x88C - 0x8EF 100 bytes Shared 0x8F0 - 0x8FF 16 bytes |  | SFR 0x900 - 0x90B 12 bytes Unimplemented 0x90C - 0x96F 100 bytes Shared 0x970 - 0x97F 16 bytes |  | SFR 0x980 - 0x98B 12 bytes Unimplemented 0x98C - 0x9EF 100 bytes Shared 0x9F0 - 0x9FF 16 bytes |  | SFR 0xA00 - 0xA0B 12 bytes Unimplemented 0xA0C - 0xA6F 100 bytes Shared 0xA70 - 0xA7F 16 bytes |  | SFR 0xA80 - 0xA8B 12 bytes Unimplemented 0xA8C - 0xAEF 100 bytes Shared 0xAF0 - 0xAFF 16 bytes |  | SFR 0xB00 - 0xB0B 12 bytes Unimplemented 0xB0C - 0xB6F 100 bytes Shared 0xB70 - 0xB7F 16 bytes |  | SFR 0xB80 - 0xB8B 12 bytes Unimplemented 0xB8C - 0xBEF 100 bytes Shared 0xBF0 - 0xBFF 16 bytes |  | SFR 0xC00 - 0xC0B 12 bytes Unimplemented 0xC0C - 0xC6F 100 bytes Shared 0xC70 - 0xC7F 16 bytes |  | SFR 0xC80 - 0xC8B 12 bytes Unimplemented 0xC8C - 0xCEF 100 bytes Shared 0xCF0 - 0xCFF 16 bytes |  | SFR 0xD00 - 0xD0B 12 bytes Unimplemented 0xD0C - 0xD6F 100 bytes Shared 0xD70 - 0xD7F 16 bytes |  | SFR 0xD80 - 0xD8B 12 bytes Unimplemented 0xD8C - 0xDEF 100 bytes Shared 0xDF0 - 0xDFF 16 bytes |  | SFR 0xE00 - 0xE0B 12 bytes Unimplemented 0xE0C - 0xE6F 100 bytes Shared 0xE70 - 0xE7F 16 bytes |  | SFR 0xE80 - 0xE8B 12 bytes Unimplemented 0xE8C - 0xEEF 100 bytes Shared 0xEF0 - 0xEFF 16 bytes |  | SFR 0xF00 - 0xF0B 12 bytes Unimplemented 0xF0C - 0xF6F 100 bytes Shared 0xF70 - 0xF7F 16 bytes |  | SFR 0xF80 - 0xF8B 12 bytes Unimplemented 0xF8C - 0xFE3 88 bytes SFR 0xFE4 - 0xFEB 8 bytes Unimplemented 0xFEC SFR 0xFED - 0xFEF 3 bytes Shared 0xFF0 - 0xFFF 16 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

| SFR 23 bytes GPR 80 bytes Shared 16 bytes Unimplemented 9 bytes |  | SFR 27 bytes GPR 32 bytes Shared 16 bytes Unimplemented 53 bytes |  | SFR 17 bytes GPR 0 bytes Shared 16 bytes Unimplemented 95 bytes |  | SFR 20 bytes GPR 0 bytes Shared 16 bytes Unimplemented 92 bytes |  | SFR 14 bytes GPR 0 bytes Shared 16 bytes Unimplemented 98 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 15 bytes GPR 0 bytes Shared 16 bytes Unimplemented 97 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 31 bytes GPR 0 bytes Shared 16 bytes Unimplemented 81 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 12 bytes GPR 0 bytes Shared 16 bytes Unimplemented 100 bytes |  | SFR 23 bytes GPR 0 bytes Shared 16 bytes Unimplemented 89 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

Special Function Register.

General-purpose RAM.

Shared RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:59 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.