- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16LF1526
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |  | Bank 4 |  | Bank 5 |  | Bank 6 |  | Bank 7 |  | Bank 8 |  | Bank 9 |  | Bank 11 |  | Bank 12 |  | Bank 31 |
INDF0 | 0x000
INDF1 | 0x001
PCL | 0x002
STATUS | 0x003
FSR0FSR0L | 0x004
FSR0H | 0x005
FSR1FSR1L | 0x006
FSR1H | 0x007
BSR | 0x008
WREG | 0x009
PCLATH | 0x00A
INTCON | 0x00B
PORTA | 0x00C
PORTB | 0x00D
PORTC | 0x00E
PORTD | 0x00F
PORTE | 0x010
PIR1 | 0x011
PIR2 | 0x012
PIR3 | 0x013
PIR4 | 0x014
TMR0 | 0x015
TMR1TMR1L | 0x016
TMR1H | 0x017
T1CON | 0x018
T1GCON | 0x019
TMR2 | 0x01A
PR2 | 0x01B
T2CON | 0x01C
TRISA | 0x08C
TRISB | 0x08D
TRISC | 0x08E
TRISD | 0x08F
TRISE | 0x090
PIE1 | 0x091
PIE2 | 0x092
PIE3 | 0x093
PIE4 | 0x094
OPTION_REG | 0x095
PCON | 0x096
WDTCON | 0x097
OSCCON | 0x099
OSCSTAT | 0x09A
ADRESADRESL | 0x09B
ADRESH | 0x09C
ADCON0 | 0x09D
ADCON1 | 0x09E
LATA | 0x10C
LATB | 0x10D
LATC | 0x10E
LATD | 0x10F
LATE | 0x110
BORCON | 0x116
FVRCON | 0x117
APFCON | 0x11D
ANSELA | 0x18C
ANSELB | 0x18D
ANSELD | 0x18F
ANSELE | 0x190
PMADRPMADRL | 0x191
PMADRH | 0x192
PMDATPMDATL | 0x193
PMDATH | 0x194
PMCON1 | 0x195
PMCON2 | 0x196
RC1REGRCREG RCREG1 | 0x199
TX1REGTXREG TXREG1 | 0x19A
SP1BRGLSPBRG SPBRGL SPBRGL1 | 0x19B
SP1BRGHSPBRGH SPBRGH1 | 0x19C
RC1STARCSTA RCSTA1 | 0x19D
TX1STATXSTA TXSTA1 | 0x19E
BAUD1CONBAUDCON BAUDCON1 | 0x19F
WPUB | 0x20D
WPUD | 0x20F
WPUE | 0x210
SSP1BUFSSPBUF | 0x211
SSP1ADDSSPADD | 0x212
SSP1MSKSSPMSK | 0x213
SSP1STATSSPSTAT | 0x214
SSP1CON1SSPCON SSPCON1 | 0x215
SSP1CON2SSPCON2 | 0x216
SSP1CON3SSPCON3 | 0x217
SSP2BUF | 0x219
SSP2ADD | 0x21A
SSP2MSK | 0x21B
SSP2STAT | 0x21C
SSP2CON1 | 0x21D
SSP2CON2 | 0x21E
SSP2CON3 | 0x21F
PORTF | 0x28C
PORTG | 0x28D
CCPR1CCPR1L | 0x291
CCPR1H | 0x292
CCP1CON | 0x293
CCPR2CCPR2L | 0x298
CCPR2H | 0x299
CCP2CON | 0x29A
CCPTMRS0 | 0x29D
CCPTMRS1 | 0x29E
CCPTMRS2 | 0x29F
TRISF | 0x30C
TRISG | 0x30D
CCPR3CCPR3L | 0x311
CCPR3H | 0x312
CCP3CON | 0x313
CCPR4CCPR4L | 0x318
CCPR4H | 0x319
CCP4CON | 0x31A
CCPR5CCPR5L | 0x31C
CCPR5H | 0x31D
CCP5CON | 0x31E
LATF | 0x38C
LATG | 0x38D
IOCBP | 0x394
IOCBN | 0x395
IOCBF | 0x396
ANSELF | 0x40C
ANSELG | 0x40D
TMR3TMR3L | 0x411
TMR3H | 0x412
T3CON | 0x413
T3GCON | 0x414
TMR4 | 0x415
PR4 | 0x416
T4CON | 0x417
TMR5TMR5L | 0x418
TMR5H | 0x419
T5CON | 0x41A
T5GCON | 0x41B
TMR6 | 0x41C
PR6 | 0x41D
T6CON | 0x41E
WPUG | 0x48D
RC2REGRCREG2 | 0x491
TX2REGTXREG2 | 0x492
SP2BRGSP2BRGL SPBRGL2 | 0x493
SP2BRGHSPBRGH2 | 0x494
RC2STARCSTA2 | 0x495
TX2STATXSTA2 | 0x496
BAUD2CONBAUDCON2 | 0x497
TMR8 | 0x595
PR8 | 0x596
T8CON | 0x597
TMR10 | 0x59C
PR10 | 0x59D
T10CON | 0x59E
CCPR6CCPR6L | 0x611
CCPR6H | 0x612
CCP6CON | 0x613
CCPR7CCPR7L | 0x614
CCPR7H | 0x615
CCP7CON | 0x616
CCPR8CCPR8L | 0x617
CCPR8H | 0x618
CCP8CON | 0x619
CCPR9CCPR9L | 0x61A
CCPR9H | 0x61B
CCP9CON | 0x61C
CCPR10CCPR10L | 0x61D
CCPR10H | 0x61E
CCP10CON | 0x61F
STATUS_SHAD | 0xFE4
WREG_SHAD | 0xFE5
BSR_SHAD | 0xFE6
PCLATH_SHAD | 0xFE7
FSR0L_SHAD | 0xFE8
FSR0H_SHAD | 0xFE9
FSR1L_SHAD | 0xFEA
FSR1H_SHAD | 0xFEB
STKPTR | 0xFED
TOSL | 0xFEE
TOSH | 0xFEF
The mirror of [PCL, STATUS, ...] are not shown.

SFR

SFR with alias name.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.