- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F648A
CONFIG (address:0x2007, mask:0xFFFF)
FOSC -- Oscillator Selection bits
| FOSC = LP | 0x3FEC | LP oscillator: Low-power crystal on RA6/OSC2/CLKOUT and RA7/OSC1/CLKIN. |
| FOSC = XT | 0x3FED | XT oscillator: Crystal/resonator on RA6/OSC2/CLKOUT and RA7/OSC1/CLKIN. |
| FOSC = HS | 0x3FEE | HS oscillator: High-speed crystal/resonator on RA6/OSC2/CLKOUT and RA7/OSC1/CLKIN. |
| FOSC = ECIO | 0x3FEF | EC: I/O function on RA6/OSC2/CLKOUT pin, CLKIN on RA7/OSC1/CLKIN. |
| FOSC = INTOSCIO | 0x3FFC | INTOSC oscillator: I/O function on RA6/OSC2/CLKOUT pin, I/O function on RA7/OSC1/CLKIN. |
| FOSC = INTOSCCLK | 0x3FFD | INTOSC oscillator: CLKOUT function on RA6/OSC2/CLKOUT pin, I/O function on RA7/OSC1/CLKIN. |
| FOSC = EXTRCIO | 0x3FFE | RC oscillator: I/O function on RA6/OSC2/CLKOUT pin, Resistor and Capacitor on RA7/OSC1/CLKIN. |
| FOSC = EXTRCCLK | 0x3FFF | RC oscillator: CLKOUT function on RA6/OSC2/CLKOUT pin, Resistor and Capacitor on RA7/OSC1/CLKIN. |
WDTE -- Watchdog Timer Enable bit
| WDTE = OFF | 0x3FFB | WDT disabled. |
| WDTE = ON | 0x3FFF | WDT enabled. |
PWRTE -- Power-up Timer Enable bit
| PWRTE = ON | 0x3FF7 | PWRT enabled. |
| PWRTE = OFF | 0x3FFF | PWRT disabled. |
MCLRE -- RA5/MCLR/VPP Pin Function Select bit
| MCLRE = OFF | 0x3FDF | RA5/MCLR/VPP pin function is digital input, MCLR internally tied to VDD. |
| MCLRE = ON | 0x3FFF | RA5/MCLR/VPP pin function is MCLR. |
BOREN -- Brown-out Detect Enable bit
| BOREN = OFF | 0x3FBF | BOD disabled. |
| BOREN = ON | 0x3FFF | BOD enabled. |
LVP -- Low-Voltage Programming Enable bit
| LVP = OFF | 0x3F7F | RB4/PGM pin has digital I/O function, HV on MCLR must be used for programming. |
| LVP = ON | 0x3FFF | RB4/PGM pin has PGM function, low-voltage programming enabled. |
CPD -- Data EE Memory Code Protection bit
| CPD = ON | 0x3EFF | Data memory code-protected. |
| CPD = OFF | 0x3FFF | Data memory code protection off. |
CP -- Flash Program Memory Code Protection bit
| CP = ON | 0x1FFF | 0000h to 0FFFh code-protected. |
| CP = OFF | 0x3FFF | Code protection off. |

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.