Informations about the PIC microcontrollers

- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

| name | config word size (bit) | class |
| PIC10F320 | 14 | regular |
| PIC10F322 | 14 | regular |
| PIC10LF320 | 14 | regular |
| PIC10LF322 | 14 | regular |
| PIC12C671 | 14 | regular |
| PIC12C672 | 14 | regular |
| PIC12CE673 | 14 | regular |
| PIC12CE674 | 14 | regular |
| PIC12F609 | 14 | regular |
| PIC12F615 | 14 | regular |
| PIC12F617 | 14 | regular |
| PIC12F629 | 14 | regular |
| PIC12F635 | 14 | regular |
| PIC12F675 | 14 | regular |
| PIC12F683 | 14 | regular |
| PIC12F752 | 14 | regular |
| PIC12F1501 | 16 | enhanced |
| PIC12F1822 | 16 | enhanced |
| PIC12F1840 | 16 | enhanced |
| PIC12HV609 | 14 | regular |
| PIC12HV615 | 14 | regular |
| PIC12HV752 | 14 | regular |
| PIC12LF1501 | 16 | enhanced |
| PIC12LF1552 | 16 | enhanced |
| PIC12LF1822 | 16 | enhanced |
| PIC12LF1840 | 16 | enhanced |
| PIC12LF1840T39A | 16 | enhanced |
| PIC12LF1840T48A | 16 | enhanced |
| PIC16C62A | 14 | regular |
| PIC16C62B | 14 | regular |
| PIC16C63 | 14 | regular |
| PIC16C63A | 14 | regular |
| PIC16C64A | 14 | regular |
| PIC16C65A | 14 | regular |
| PIC16C65B | 14 | regular |
| PIC16C66 | 14 | regular |
| PIC16C67 | 14 | regular |
| PIC16C71 | 14 | regular |
| PIC16C72 | 14 | regular |
| PIC16C72A | 14 | regular |
| PIC16C73A | 14 | regular |
| PIC16C73B | 14 | regular |
| PIC16C74A | 14 | regular |
| PIC16C74B | 14 | regular |
| PIC16C76 | 14 | regular |
| PIC16C77 | 14 | regular |
| PIC16C432 | 14 | regular |
| PIC16C433 | 14 | regular |
| PIC16C554 | 14 | regular |
| PIC16C557 | 14 | regular |
| PIC16C558 | 14 | regular |
| PIC16C620 | 14 | regular |
| PIC16C620A | 14 | regular |
| PIC16C621 | 14 | regular |
| PIC16C621A | 14 | regular |
| PIC16C622 | 14 | regular |
| PIC16C622A | 14 | regular |
| PIC16C642 | 14 | regular |
| PIC16C662 | 14 | regular |
| PIC16C710 | 14 | regular |
| PIC16C711 | 14 | regular |
| PIC16C712 | 14 | regular |
| PIC16C715 | 14 | regular |
| PIC16C716 | 14 | regular |
| PIC16C717 | 14 | regular |
| PIC16C745 | 14 | regular |
| PIC16C765 | 14 | regular |
| PIC16C770 | 14 | regular |
| PIC16C771 | 14 | regular |
| PIC16C773 | 14 | regular |
| PIC16C774 | 14 | regular |
| PIC16C781 | 14 | regular |
| PIC16C782 | 14 | regular |
| PIC16C923 | 14 | regular |
| PIC16C924 | 14 | regular |
| PIC16C925 | 14 | regular |
| PIC16C926 | 14 | regular |
| PIC16CE623 | 14 | regular |
| PIC16CE624 | 14 | regular |
| PIC16CE625 | 14 | regular |
| PIC16CR62 | 14 | regular |
| PIC16CR63 | 14 | regular |
| PIC16CR64 | 14 | regular |
| PIC16CR65 | 14 | regular |
| PIC16CR72 | 14 | regular |
| PIC16CR83 | 14 | regular |
| PIC16CR84 | 14 | regular |
| PIC16F72 | 14 | regular |
| PIC16F73 | 14 | regular |
| PIC16F74 | 14 | regular |
| PIC16F76 | 14 | regular |
| PIC16F77 | 14 | regular |
| PIC16F83 | 14 | regular |
| PIC16F84 | 14 | regular |
| PIC16F84A | 14 | regular |
| PIC16F87 | 14 | regular |
| PIC16F88 | 14 | regular |
| PIC16F610 | 14 | regular |
| PIC16F616 | 14 | regular |
| PIC16F627 | 14 | regular |
| PIC16F627A | 14 | regular |
| PIC16F628 | 14 | regular |
| PIC16F628A | 14 | regular |
| PIC16F630 | 14 | regular |
| PIC16F631 | 14 | regular |
| PIC16F636 | 14 | regular |
| PIC16F639 | 14 | regular |
| PIC16F648A | 14 | regular |
| PIC16F676 | 14 | regular |
| PIC16F677 | 14 | regular |
| PIC16F684 | 14 | regular |
| PIC16F685 | 14 | regular |
| PIC16F687 | 14 | regular |
| PIC16F688 | 14 | regular |
| PIC16F689 | 14 | regular |
| PIC16F690 | 14 | regular |
| PIC16F707 | 14 | regular |
| PIC16F716 | 14 | regular |
| PIC16F720 | 14 | regular |
| PIC16F721 | 14 | regular |
| PIC16F722 | 14 | regular |
| PIC16F722A | 14 | regular |
| PIC16F723 | 14 | regular |
| PIC16F723A | 14 | regular |
| PIC16F724 | 14 | regular |
| PIC16F726 | 14 | regular |
| PIC16F727 | 14 | regular |
| PIC16F737 | 14 | regular |
| PIC16F747 | 14 | regular |
| PIC16F767 | 14 | regular |
| PIC16F777 | 14 | regular |
| PIC16F785 | 14 | regular |
| PIC16F818 | 14 | regular |
| PIC16F819 | 14 | regular |
| PIC16F870 | 14 | regular |
| PIC16F871 | 14 | regular |
| PIC16F872 | 14 | regular |
| PIC16F873 | 14 | regular |
| PIC16F873A | 14 | regular |
| PIC16F874 | 14 | regular |
| PIC16F874A | 14 | regular |
| PIC16F876 | 14 | regular |
| PIC16F876A | 14 | regular |
| PIC16F877 | 14 | regular |
| PIC16F877A | 14 | regular |
| PIC16F882 | 14 | regular |
| PIC16F883 | 14 | regular |
| PIC16F884 | 14 | regular |
| PIC16F886 | 14 | regular |
| PIC16F887 | 14 | regular |
| PIC16F913 | 14 | regular |
| PIC16F914 | 14 | regular |
| PIC16F916 | 14 | regular |
| PIC16F917 | 14 | regular |
| PIC16F946 | 14 | regular |
| PIC16F1454 | 16 | enhanced |
| PIC16F1455 | 16 | enhanced |
| PIC16F1459 | 16 | enhanced |
| PIC16F1503 | 16 | enhanced |
| PIC16F1507 | 16 | enhanced |
| PIC16F1508 | 16 | enhanced |
| PIC16F1509 | 16 | enhanced |
| PIC16F1512 | 16 | enhanced |
| PIC16F1513 | 16 | enhanced |
| PIC16F1516 | 16 | enhanced |
| PIC16F1517 | 16 | enhanced |
| PIC16F1518 | 16 | enhanced |
| PIC16F1519 | 16 | enhanced |
| PIC16F1526 | 16 | enhanced |
| PIC16F1527 | 16 | enhanced |
| PIC16F1782 | 16 | enhanced |
| PIC16F1783 | 16 | enhanced |
| PIC16F1784 | 16 | enhanced |
| PIC16F1786 | 16 | enhanced |
| PIC16F1787 | 16 | enhanced |
| PIC16F1788 | 16 | enhanced |
| PIC16F1789 | 16 | enhanced |
| PIC16F1823 | 16 | enhanced |
| PIC16F1824 | 16 | enhanced |
| PIC16F1825 | 16 | enhanced |
| PIC16F1826 | 16 | enhanced |
| PIC16F1827 | 16 | enhanced |
| PIC16F1828 | 16 | enhanced |
| PIC16F1829 | 16 | enhanced |
| PIC16F1847 | 16 | enhanced |
| PIC16F1933 | 16 | enhanced |
| PIC16F1934 | 16 | enhanced |
| PIC16F1936 | 16 | enhanced |
| PIC16F1937 | 16 | enhanced |
| PIC16F1938 | 16 | enhanced |
| PIC16F1939 | 16 | enhanced |
| PIC16F1946 | 16 | enhanced |
| PIC16F1947 | 16 | enhanced |
| PIC16HV610 | 14 | regular |
| PIC16HV616 | 14 | regular |
| PIC16HV785 | 14 | regular |
| PIC16LF720 | 14 | regular |
| PIC16LF721 | 14 | regular |
| PIC16LF1454 | 16 | enhanced |
| PIC16LF1455 | 16 | enhanced |
| PIC16LF1459 | 16 | enhanced |
| PIC16LF1503 | 16 | enhanced |
| PIC16LF1507 | 16 | enhanced |
| PIC16LF1508 | 16 | enhanced |
| PIC16LF1509 | 16 | enhanced |
| PIC16LF1512 | 16 | enhanced |
| PIC16LF1513 | 16 | enhanced |
| PIC16LF1516 | 16 | enhanced |
| PIC16LF1517 | 16 | enhanced |
| PIC16LF1518 | 16 | enhanced |
| PIC16LF1519 | 16 | enhanced |
| PIC16LF1526 | 16 | enhanced |
| PIC16LF1527 | 16 | enhanced |
| PIC16LF1782 | 16 | enhanced |
| PIC16LF1783 | 16 | enhanced |
| PIC16LF1784 | 16 | enhanced |
| PIC16LF1786 | 16 | enhanced |
| PIC16LF1787 | 16 | enhanced |
| PIC16LF1788 | 16 | enhanced |
| PIC16LF1789 | 16 | enhanced |
| PIC16LF1823 | 16 | enhanced |
| PIC16LF1824 | 16 | enhanced |
| PIC16LF1825 | 16 | enhanced |
| PIC16LF1826 | 16 | enhanced |
| PIC16LF1827 | 16 | enhanced |
| PIC16LF1828 | 16 | enhanced |
| PIC16LF1829 | 16 | enhanced |
| PIC16LF1847 | 16 | enhanced |
| PIC16LF1902 | 16 | enhanced |
| PIC16LF1903 | 16 | enhanced |
| PIC16LF1904 | 16 | enhanced |
| PIC16LF1906 | 16 | enhanced |
| PIC16LF1907 | 16 | enhanced |
| PIC16LF1933 | 16 | enhanced |
| PIC16LF1934 | 16 | enhanced |
| PIC16LF1936 | 16 | enhanced |
| PIC16LF1937 | 16 | enhanced |
| PIC16LF1938 | 16 | enhanced |
| PIC16LF1939 | 16 | enhanced |
| PIC16LF1946 | 16 | enhanced |
| PIC16LF1947 | 16 | enhanced |
| PICRF675F | 14 | regular |
| PICRF675H | 14 | regular |
| PICRF675K | 14 | regular |

12 bit MCU

14 bit MCU

16 bit MCU

12 bit enhanced MCU

14 bit enhanced MCU

16 bit extended MCU

This page generated automatically by the device-help.pl program (2012-12-22 23:50:57 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.