- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC10LF320
CONFIG (address:0x2007, mask:0x3FFF)
FOSC -- Oscillator Selection bits
| FOSC = INTOSC | 0x3FFE | INTOSC oscillator: CLKIN function disabled. |
| FOSC = EC | 0x3FFF | EC: CLKIN function enabled. |
BOREN -- Brown-out Reset Enable
| BOREN = OFF | 0x3FF9 | Brown-out Reset disabled. |
| BOREN = SBODEN | 0x3FFB | Brown-out Reset controlled by the SBOREN bit in the BORCON register. |
| BOREN = NSLEEP | 0x3FFD | Brown-out Reset enabled while running and disabled in Sleep. |
| BOREN = ON | 0x3FFF | Brown-out Reset enabled. |
WDTE -- Watchdog Timer Enable
| WDTE = OFF | 0x3FE7 | WDT disabled. |
| WDTE = SWDTEN | 0x3FEF | WDT controlled by the SWDTEN bit in the WDTCON register. |
| WDTE = NSLEEP | 0x3FF7 | WDT enabled while running and disabled in Sleep. |
| WDTE = ON | 0x3FFF | WDT enabled. |
PWRTE -- Power-up Timer Enable bit
| PWRTE = ON | 0x3FDF | PWRT enabled. |
| PWRTE = OFF | 0x3FFF | PWRT disabled. |
MCLRE -- MCLR Pin Function Select bit
| MCLRE = OFF | 0x3FBF | MCLR pin function is digital input, MCLR internally tied to VDD. |
| MCLRE = ON | 0x3FFF | MCLR pin function is MCLR. |
CP -- Code Protection bit
| CP = ON | 0x3F7F | Program memory code protection is enabled. |
| CP = OFF | 0x3FFF | Program memory code protection is disabled. |
LVP -- Low-Voltage Programming Enable
| LVP = OFF | 0x3EFF | High-voltage on MCLR/VPP must be used for programming. |
| LVP = ON | 0x3FFF | Low-voltage programming enabled. |
LPBOR -- Brown-out Reset Selection bits
| LPBOR = OFF | 0x3DFF | BOR disabled. |
| LPBOR = ON | 0x3FFF | BOR enabled. |
BORV -- Brown-out Reset Voltage Selection
| BORV = HI | 0x3BFF | Brown-out Reset Voltage (Vbor), high trip point selected. |
| BORV = LO | 0x3FFF | Brown-out Reset Voltage (Vbor), low trip point selected. |
WRT -- Flash Memory Self-Write Protection
| WRT = ALL | 0x27FF | 000h to 0FFh write protected, no addresses may be modified by PMCON control. |
| WRT = HALF | 0x2FFF | 000h to 07Fh write protected, 080h to 0FFh may be modified by PMCON control. |
| WRT = BOOT | 0x37FF | 000h to 03Fh write protected, 040h to 0FFh may be modified by PMCON control. |
| WRT = OFF | 0x3FFF | Write protection off. |

This page generated automatically by the device-help.pl program (2012-12-22 23:50:57 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.