- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F913
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |
| SFR 0x000 - 0x007 8 bytes Unimplemented 0x008 SFR 0x009 - 0x01A 18 bytes Unimplemented 0x01B - 0x01D 3 bytes SFR 0x01E - 0x01F 2 bytes GPR 0x020 - 0x06F 80 bytes Shared 0x070 - 0x07F 16 bytes |  | SFR 0x080 - 0x087 8 bytes Unimplemented 0x088 SFR 0x089 - 0x099 17 bytes Unimplemented 0x09A - 0x09B 2 bytes SFR 0x09C - 0x09F 4 bytes GPR 0x0A0 - 0x0EF 80 bytes Shared 0x0F0 - 0x0FF 16 bytes |  | SFR 0x100 Unimplemented 0x101 SFR 0x102 - 0x105 4 bytes Unimplemented 0x106 SFR 0x107 - 0x111 11 bytes Unimplemented 0x112 SFR 0x113 - 0x114 2 bytes Unimplemented 0x115 SFR 0x116 - 0x117 2 bytes Unimplemented 0x118 SFR 0x119 - 0x11A 2 bytes Unimplemented 0x11B SFR 0x11C - 0x11D 2 bytes Unimplemented 0x11E - 0x11F 2 bytes GPR 0x120 - 0x16F 80 bytes Shared 0x170 - 0x17F 16 bytes |  | SFR 0x180 Unimplemented 0x181 SFR 0x182 - 0x184 3 bytes Unimplemented 0x185 - 0x189 5 bytes SFR 0x18A - 0x18D 4 bytes Unimplemented 0x18E - 0x1EF 98 bytes Shared 0x1F0 - 0x1FF 16 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

| SFR 28 bytes GPR 80 bytes Shared 16 bytes Unimplemented 4 bytes |  | SFR 29 bytes GPR 80 bytes Shared 16 bytes Unimplemented 3 bytes |  | SFR 24 bytes GPR 80 bytes Shared 16 bytes Unimplemented 8 bytes |  | SFR 8 bytes GPR 0 bytes Shared 16 bytes Unimplemented 104 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

Special Function Register.

General-purpose RAM.

Shared RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.