- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16LF1828
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |  | Bank 4 |  | Bank 5 |  | Bank 6 |  | Bank 7 |  | Bank 8 |  | Bank 31 |
INDF0 | 0x000
INDF1 | 0x001
PCL | 0x002
STATUS | 0x003
FSR0FSR0L | 0x004
FSR0H | 0x005
FSR1FSR1L | 0x006
FSR1H | 0x007
BSR | 0x008
WREG | 0x009
PCLATH | 0x00A
INTCON | 0x00B
PORTA | 0x00C
PORTB | 0x00D
PORTC | 0x00E
PIR1 | 0x011
PIR2 | 0x012
PIR3 | 0x013
TMR0 | 0x015
TMR1TMR1L | 0x016
TMR1H | 0x017
T1CON | 0x018
T1GCON | 0x019
TMR2 | 0x01A
PR2 | 0x01B
T2CON | 0x01C
CPSCON0 | 0x01E
CPSCON1 | 0x01F
TRISA | 0x08C
TRISB | 0x08D
TRISC | 0x08E
PIE1 | 0x091
PIE2 | 0x092
PIE3 | 0x093
OPTION_REG | 0x095
PCON | 0x096
WDTCON | 0x097
OSCTUNE | 0x098
OSCCON | 0x099
OSCSTAT | 0x09A
ADRESADRESL | 0x09B
ADRESH | 0x09C
ADCON0 | 0x09D
ADCON1 | 0x09E
LATA | 0x10C
LATB | 0x10D
LATC | 0x10E
CM1CON0 | 0x111
CM1CON1 | 0x112
CM2CON0 | 0x113
CM2CON1 | 0x114
CMOUT | 0x115
BORCON | 0x116
FVRCON | 0x117
DACCON0 | 0x118
DACCON1 | 0x119
SRCON0 | 0x11A
SRCON1 | 0x11B
APFCON0 | 0x11D
APFCON1 | 0x11E
ANSELA | 0x18C
ANSELB | 0x18D
ANSELC | 0x18E
EEADREEADRL | 0x191
EEADRH | 0x192
EEDATEEDATL | 0x193
EEDATH | 0x194
EECON1 | 0x195
EECON2 | 0x196
RCREG | 0x199
TXREG | 0x19A
SPBRGSPBRGL | 0x19B
SPBRGH | 0x19C
RCSTA | 0x19D
TXSTA | 0x19E
BAUDCON | 0x19F
WPUA | 0x20C
WPUB | 0x20D
WPUC | 0x20E
SSP1BUFSSPBUF | 0x211
SSP1ADDSSPADD | 0x212
SSP1MSKSSPMSK | 0x213
SSP1STATSSPSTAT | 0x214
SSP1CONSSP1CON1 SSPCON SSPCON1 | 0x215
SSP1CON2SSPCON2 | 0x216
SSP1CON3SSPCON3 | 0x217
CCPR1L | 0x291
CCPR1H | 0x292
CCP1CON | 0x293
PWM1CON | 0x294
CCP1ASECCP1AS | 0x295
PSTR1CON | 0x296
CCPR2L | 0x298
CCPR2H | 0x299
CCP2CON | 0x29A
PWM2CON | 0x29B
CCP2AS | 0x29C
PSTR2CON | 0x29D
CCPTMRSCCPTMRS0 | 0x29E
CCPR3L | 0x311
CCPR3H | 0x312
CCP3CON | 0x313
CCPR4L | 0x318
CCPR4H | 0x319
CCP4CON | 0x31A
INLVLA | 0x38C
INLVLB | 0x38D
INLVLC | 0x38E
IOCAP | 0x391
IOCAN | 0x392
IOCAF | 0x393
IOCBP | 0x394
IOCBN | 0x395
IOCBF | 0x396
CLKRCON | 0x39A
MDCON | 0x39C
MDSRC | 0x39D
MDCARL | 0x39E
MDCARH | 0x39F
TMR4 | 0x415
PR4 | 0x416
T4CON | 0x417
TMR6 | 0x41C
PR6 | 0x41D
T6CON | 0x41E
STATUS_SHAD | 0xFE4
WREG_SHAD | 0xFE5
BSR_SHAD | 0xFE6
PCLATH_SHAD | 0xFE7
FSR0L_SHAD | 0xFE8
FSR0H_SHAD | 0xFE9
FSR1L_SHAD | 0xFEA
FSR1H_SHAD | 0xFEB
STKPTR | 0xFED
TOSL | 0xFEE
TOSH | 0xFEF
The mirror of [PCL, STATUS, ...] are not shown.

SFR

SFR with alias name.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:59 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.