- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC18F6680
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |  | Bank 4 |  | Bank 5 |  | Bank 6 |  | Bank 7 |  | Bank 8 |  | Bank 9 |  | Bank 10 |  | Bank 11 |  | Bank 12 |  | Bank 13 |  | Bank 14 |  | Bank 15 |
| GPR 0x000 - 0x0FF 256 bytes |  | GPR 0x100 - 0x1FF 256 bytes |  | GPR 0x200 - 0x2FF 256 bytes |  | GPR 0x300 - 0x3FF 256 bytes |  | GPR 0x400 - 0x4FF 256 bytes |  | GPR 0x500 - 0x5FF 256 bytes |  | GPR 0x600 - 0x6FF 256 bytes |  | GPR 0x700 - 0x7FF 256 bytes |  | GPR 0x800 - 0x8FF 256 bytes |  | GPR 0x900 - 0x9FF 256 bytes |  | GPR 0xA00 - 0xAFF 256 bytes |  | GPR 0xB00 - 0xBFF 256 bytes |  | GPR 0xC00 - 0xCFF 256 bytes |  | Unimplemented 0xD00 - 0xD5F 96 bytes SFR 0xD60 - 0xD6B 12 bytes Unimplemented 0xD6C - 0xD6F 4 bytes SFR 0xD70 - 0xD7B 12 bytes Unimplemented 0xD7C - 0xD7F 4 bytes SFR 0xD80 - 0xD8B 12 bytes Unimplemented 0xD8C - 0xD8F 4 bytes SFR 0xD90 - 0xD93 4 bytes Unimplemented 0xD94 - 0xDD3 64 bytes SFR 0xDD4 - 0xDD5 2 bytes Unimplemented 0xDD6 - 0xDD7 2 bytes SFR 0xDD8 Unimplemented 0xDD9 - 0xDDF 7 bytes SFR 0xDE0 - 0xDE7 8 bytes Unimplemented 0xDE8 - 0xDEF 8 bytes SFR 0xDF0 - 0xDF3 4 bytes Unimplemented 0xDF4 - 0xDF7 4 bytes SFR 0xDF8 Unimplemented 0xDF9 SFR 0xDFA Unimplemented 0xDFB SFR 0xDFC Unimplemented 0xDFD - 0xDFF 3 bytes |  | Unimplemented 0xE00 - 0xE1F 32 bytes SFR 0xE20 - 0xE7F 96 bytes Unimplemented 0xE80 - 0xEFF 128 bytes |  | SFR 0xF00 - 0xF77 120 bytes Unimplemented 0xF78 SFR 0xF79 Unimplemented 0xF7A - 0xF7D 4 bytes SFR 0xF7E - 0xF86 9 bytes Unimplemented 0xF87 - 0xF88 2 bytes SFR 0xF89 - 0xF8F 7 bytes Unimplemented 0xF90 - 0xF91 2 bytes SFR 0xF92 - 0xF98 7 bytes Unimplemented 0xF99 - 0xF9C 4 bytes SFR 0xF9D - 0xFB6 26 bytes Unimplemented 0xFB7 - 0xFB9 3 bytes SFR 0xFBA - 0xFD3 26 bytes Unimplemented 0xFD4 SFR 0xFD5 - 0xFFF 43 bytes |

| SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 58 bytes GPR 0 bytes Unimplemented 198 bytes |  | SFR 96 bytes GPR 0 bytes Unimplemented 160 bytes |  | SFR 239 bytes GPR 0 bytes Unimplemented 17 bytes |

Special Function Register.

General-purpose RAM.

In this place no RAM.

Special Function Register on Access Area.

General-purpose RAM on Access Area.

In this place no RAM on Access Area.

This page generated automatically by the device-help.pl program (2012-12-22 23:51:01 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.