- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F77
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |
INDF | 0x000
TMR0 | 0x001
PCL | 0x002
STATUS | 0x003
FSR | 0x004
PORTA | 0x005
PORTB | 0x006
PORTC | 0x007
PORTD | 0x008
PORTE | 0x009
PCLATH | 0x00A
INTCON | 0x00B
PIR1 | 0x00C
PIR2 | 0x00D
TMR1TMR1L | 0x00E
TMR1H | 0x00F
T1CON | 0x010
TMR2 | 0x011
T2CON | 0x012
SSPBUF | 0x013
SSPCON | 0x014
CCPR1CCPR1L | 0x015
CCPR1H | 0x016
CCP1CON | 0x017
RCSTA | 0x018
TXREG | 0x019
RCREG | 0x01A
CCPR2CCPR2L | 0x01B
CCPR2H | 0x01C
CCP2CON | 0x01D
ADRES | 0x01E
ADCON0 | 0x01F
OPTION_REG | 0x081
TRISA | 0x085
TRISB | 0x086
TRISC | 0x087
TRISD | 0x088
TRISE | 0x089
PIE1 | 0x08C
PIE2 | 0x08D
PCON | 0x08E
PR2 | 0x092
SSPADD | 0x093
SSPSTAT | 0x094
TXSTA | 0x098
SPBRG | 0x099
ADCON1 | 0x09F
PMDATA | 0x10C
PMADR | 0x10D
PMDATH | 0x10E
PMADRH | 0x10F
PMCON1 | 0x18C
The mirror of [PCL, STATUS, ...] are not shown.

SFR

SFR with alias name.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.