- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC12F635
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |
| SFR 0x000 - 0x005 6 bytes Unimplemented 0x006 - 0x009 4 bytes SFR 0x00A - 0x00C 3 bytes Unimplemented 0x00D SFR 0x00E - 0x010 3 bytes Unimplemented 0x011 - 0x017 7 bytes SFR 0x018 - 0x01A 3 bytes Unimplemented 0x01B - 0x03F 37 bytes GPR 0x040 - 0x06F 48 bytes Shared 0x070 - 0x07F 16 bytes |  | SFR 0x080 - 0x085 6 bytes Unimplemented 0x086 - 0x089 4 bytes SFR 0x08A - 0x08C 3 bytes Unimplemented 0x08D SFR 0x08E - 0x090 3 bytes Unimplemented 0x091 - 0x093 3 bytes SFR 0x094 - 0x097 4 bytes Unimplemented 0x098 SFR 0x099 - 0x09D 5 bytes Unimplemented 0x09E - 0x0EF 82 bytes Shared 0x0F0 - 0x0FF 16 bytes |  | SFR 0x100 Unimplemented 0x101 SFR 0x102 - 0x104 3 bytes Unimplemented 0x105 - 0x109 5 bytes SFR 0x10A - 0x10B 2 bytes Unimplemented 0x10C - 0x10F 4 bytes SFR 0x110 - 0x114 5 bytes Unimplemented 0x115 - 0x16F 91 bytes Shared 0x170 - 0x17F 16 bytes |  | SFR 0x180 Unimplemented 0x181 SFR 0x182 - 0x184 3 bytes Unimplemented 0x185 - 0x189 5 bytes SFR 0x18A - 0x18B 2 bytes Unimplemented 0x18C - 0x1EF 100 bytes Shared 0x1F0 - 0x1FF 16 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

| SFR 15 bytes GPR 48 bytes Shared 16 bytes Unimplemented 49 bytes |  | SFR 21 bytes GPR 0 bytes Shared 16 bytes Unimplemented 91 bytes |  | SFR 11 bytes GPR 0 bytes Shared 16 bytes Unimplemented 101 bytes |  | SFR 6 bytes GPR 0 bytes Shared 16 bytes Unimplemented 106 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

Special Function Register.

General-purpose RAM.

Shared RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:57 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.