- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F74
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |
| SFR 0x000 - 0x01F 32 bytes GPR 0x020 - 0x06F 80 bytes Shared 0x070 - 0x07F 16 bytes |  | SFR 0x080 - 0x08E 15 bytes Unimplemented 0x08F - 0x091 3 bytes SFR 0x092 - 0x094 3 bytes Unimplemented 0x095 - 0x097 3 bytes SFR 0x098 - 0x099 2 bytes Unimplemented 0x09A - 0x09E 5 bytes SFR 0x09F GPR 0x0A0 - 0x0EF 80 bytes Shared 0x0F0 - 0x0FF 16 bytes |  | SFR 0x100 Unimplemented 0x101 SFR 0x102 - 0x104 3 bytes Unimplemented 0x105 - 0x109 5 bytes SFR 0x10A - 0x10F 6 bytes Unimplemented 0x110 - 0x11F 16 bytes GPR 0x120 - 0x16F 80 bytes Shared 0x170 - 0x17F 16 bytes |  | SFR 0x180 Unimplemented 0x181 SFR 0x182 - 0x184 3 bytes Unimplemented 0x185 - 0x189 5 bytes SFR 0x18A - 0x18C 3 bytes Unimplemented 0x18D - 0x19F 19 bytes GPR 0x1A0 - 0x1EF 80 bytes Shared 0x1F0 - 0x1FF 16 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

| SFR 32 bytes GPR 80 bytes Shared 16 bytes Unimplemented 0 bytes |  | SFR 21 bytes GPR 80 bytes Shared 16 bytes Unimplemented 11 bytes |  | SFR 10 bytes GPR 80 bytes Shared 16 bytes Unimplemented 22 bytes |  | SFR 7 bytes GPR 80 bytes Shared 16 bytes Unimplemented 25 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

Special Function Register.

General-purpose RAM.

Shared RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:58 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.