- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC12F529T39A
CONFIG (address:0x0FFF, mask:0x0DFF)
OSC -- Oscillator
| OSC = LP | 0x0FFC | LP Osc With 18 ms DRT. |
| OSC = XT | 0x0FFD | XT Osc With 18 ms DRT. |
| OSC = INTRC | 0x0FFE | INTRC With 1 ms DRT. |
| OSC = EXTRC | 0x0FFF | EXTRC With 1 ms DRT. |
WDT -- Watchdog Timer Enable
| WDT = OFF | 0x0FFB | Disabled. |
| WDT = ON | 0x0FFF | Enabled. |
PARITY -- Configuration Word Parity
| PARITY = CLEAR | 0x0FF7 | Parity bit clear. |
| PARITY = SET | 0x0FFF | Parity bit set. |
MCLRE -- Master Clear Enable
| MCLRE = OFF | 0x0FEF | RB3/MCLR Functions as RB3. |
| MCLRE = ON | 0x0FFF | RB3/MCLR Functions as MCLR. |
IOSCFS -- Internal Oscillator Frequency Select
| IOSCFS = 4MHz | 0x0FDF | 4 MHz INTOSC Speed. |
| IOSCFS = 8MHz | 0x0FFF | 8 MHz INTOSC Speed. |
CPDF -- Code Protection bit - Flash Data Memory
| CPDF = ON | 0x0FBF | Code protection on. |
| CPDF = OFF | 0x0FFF | Code protection off. |
CP -- Code Protect State
| CP = ENABLE | 0x097F | Enabled. |
| CP = DISABLE | 0x0EFF | Disabled. |

This page generated automatically by the device-help.pl program (2012-12-22 23:50:57 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.