- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC18F14K22
CONFIG1H (address:0x300001, mask:0x27)
FOSC -- Oscillator Selection bits
| FOSC = LP | 0xF0 | LP oscillator. |
| FOSC = XT | 0xF1 | XT oscillator. |
| FOSC = HS | 0xF2 | HS oscillator. |
| FOSC = ERCCLKOUT | 0xF3 | External RC oscillator, CLKOUT function on OSC2. |
| FOSC = ECCLKOUTH | 0xF4 | EC, CLKOUT function on OSC2 (high). |
| FOSC = ECH | 0xF5 | EC (high). |
| FOSC = ERC | 0xF7 | External RC oscillator. |
| FOSC = IRC | 0xF8 | Internal RC oscillator. |
| FOSC = IRCCLKOUT | 0xF9 | Internal RC oscillator, CLKOUT function on OSC2. |
| FOSC = ECCLKOUTM | 0xFA | EC, CLKOUT function on OSC2 (medium). |
| FOSC = ECM | 0xFB | EC (medium). |
| FOSC = ECCLKOUTL | 0xFC | EC, CLKOUT function on OSC2 (low). |
| FOSC = ECL | 0xFD | EC (low). |
PLLEN -- 4 X PLL Enable bit
| PLLEN = OFF | 0xEF | PLL is under software control. |
| PLLEN = ON | 0xFF | Oscillator multiplied by 4. |
PCLKEN -- Primary Clock Enable bit
| PCLKEN = OFF | 0xDF | Primary clock is under software control. |
| PCLKEN = ON | 0xFF | Primary clock enabled. |
FCMEN -- Fail-Safe Clock Monitor Enable
| FCMEN = OFF | 0xBF | Fail-Safe Clock Monitor disabled. |
| FCMEN = ON | 0xFF | Fail-Safe Clock Monitor enabled. |
IESO -- Internal/External Oscillator Switchover bit
| IESO = OFF | 0x7F | Oscillator Switchover mode disabled. |
| IESO = ON | 0xFF | Oscillator Switchover mode enabled. |
CONFIG2L (address:0x300002, mask:0x1F)
PWRTEN -- Power-up Timer Enable bit
| PWRTEN = ON | 0xFE | PWRT enabled. |
| PWRTEN = OFF | 0xFF | PWRT disabled. |
BOREN -- Brown-out Reset Enable bits
| BOREN = OFF | 0xF9 | Brown-out Reset disabled in hardware and software. |
| BOREN = ON | 0xFB | Brown-out Reset enabled and controlled by software (SBOREN is enabled). |
| BOREN = NOSLP | 0xFD | Brown-out Reset enabled in hardware only and disabled in Sleep mode (SBOREN is disabled). |
| BOREN = SBORDIS | 0xFF | Brown-out Reset enabled in hardware only (SBOREN is disabled). |
BORV -- Brown Out Reset Voltage bits
| BORV = 30 | 0xE7 | VBOR set to 3.0 V nominal. |
| BORV = 27 | 0xEF | VBOR set to 2.7 V nominal. |
| BORV = 22 | 0xF7 | VBOR set to 2.2 V nominal. |
| BORV = 19 | 0xFF | VBOR set to 1.9 V nominal. |
CONFIG2H (address:0x300003, mask:0x1F)
WDTEN -- Watchdog Timer Enable bit
| WDTEN = OFF | 0xFE | WDT is controlled by SWDTEN bit of the WDTCON register. |
| WDTEN = ON | 0xFF | WDT is always enabled. SWDTEN bit has no effect. |
WDTPS -- Watchdog Timer Postscale Select bits
| WDTPS = 1 | 0xE1 | 1:1. |
| WDTPS = 2 | 0xE3 | 1:2. |
| WDTPS = 4 | 0xE5 | 1:4. |
| WDTPS = 8 | 0xE7 | 1:8. |
| WDTPS = 16 | 0xE9 | 1:16. |
| WDTPS = 32 | 0xEB | 1:32. |
| WDTPS = 64 | 0xED | 1:64. |
| WDTPS = 128 | 0xEF | 1:128. |
| WDTPS = 256 | 0xF1 | 1:256. |
| WDTPS = 512 | 0xF3 | 1:512. |
| WDTPS = 1024 | 0xF5 | 1:1024. |
| WDTPS = 2048 | 0xF7 | 1:2048. |
| WDTPS = 4096 | 0xF9 | 1:4096. |
| WDTPS = 8192 | 0xFB | 1:8192. |
| WDTPS = 16384 | 0xFD | 1:16384. |
| WDTPS = 32768 | 0xFF | 1:32768. |
CONFIG3H (address:0x300005, mask:0x88)
HFOFST -- HFINTOSC Fast Start-up bit
| HFOFST = OFF | 0xF7 | The system clock is held off until the HFINTOSC is stable. |
| HFOFST = ON | 0xFF | HFINTOSC starts clocking the CPU without waiting for the oscillator to stablize. |
MCLRE -- MCLR Pin Enable bit
| MCLRE = OFF | 0x7F | RA3 input pin enabled; MCLR disabled. |
| MCLRE = ON | 0xFF | MCLR pin enabled, RA3 input pin disabled. |
CONFIG4L (address:0x300006, mask:0x85)
STVREN -- Stack Full/Underflow Reset Enable bit
| STVREN = OFF | 0xFE | Stack full/underflow will not cause Reset. |
| STVREN = ON | 0xFF | Stack full/underflow will cause Reset. |
LVP -- Single-Supply ICSP Enable bit
| LVP = OFF | 0xFB | Single-Supply ICSP disabled. |
| LVP = ON | 0xFF | Single-Supply ICSP enabled. |
BBSIZ -- Boot Block Size Select bit
| BBSIZ = OFF | 0xF7 | 1kW boot block size. |
| BBSIZ = ON | 0xFF | 2kW boot block size. |
XINST -- Extended Instruction Set Enable bit
| XINST = OFF | 0xBF | Instruction set extension and Indexed Addressing mode disabled (Legacy mode). |
| XINST = ON | 0xFF | Instruction set extension and Indexed Addressing mode enabled. |
DEBUG -- Background Debugger Enable bit
| DEBUG = ON | 0x7F | Background debugger enabled, RA0 and RA1 are dedicated to In-Circuit Debug. |
| DEBUG = OFF | 0xFF | Background debugger disabled, RA0 and RA1 configured as general purpose I/O pins. |
CONFIG5L (address:0x300008, mask:0x03)
CP0 -- Code Protection bit
| CP0 = ON | 0xFE | Block 0 code-protected. |
| CP0 = OFF | 0xFF | Block 0 not code-protected. |
CP1 -- Code Protection bit
| CP1 = ON | 0xFD | Block 1 code-protected. |
| CP1 = OFF | 0xFF | Block 1 not code-protected. |
CONFIG5H (address:0x300009, mask:0xC0)
CPB -- Boot Block Code Protection bit
| CPB = ON | 0xBF | Boot block code-protected. |
| CPB = OFF | 0xFF | Boot block not code-protected. |
CPD -- Data EEPROM Code Protection bit
| CPD = ON | 0x7F | Data EEPROM code-protected. |
| CPD = OFF | 0xFF | Data EEPROM not code-protected. |
CONFIG6L (address:0x30000A, mask:0x03)
WRT0 -- Write Protection bit
| WRT0 = ON | 0xFE | Block 0 write-protected. |
| WRT0 = OFF | 0xFF | Block 0 not write-protected. |
WRT1 -- Write Protection bit
| WRT1 = ON | 0xFD | Block 1 write-protected. |
| WRT1 = OFF | 0xFF | Block 1 not write-protected. |
CONFIG6H (address:0x30000B, mask:0xE0)
WRTC -- Configuration Register Write Protection bit
| WRTC = ON | 0xDF | Configuration registers write-protected. |
| WRTC = OFF | 0xFF | Configuration registers not write-protected. |
WRTB -- Boot Block Write Protection bit
| WRTB = ON | 0xBF | Boot block write-protected. |
| WRTB = OFF | 0xFF | Boot block not write-protected. |
WRTD -- Data EEPROM Write Protection bit
| WRTD = ON | 0x7F | Data EEPROM write-protected. |
| WRTD = OFF | 0xFF | Data EEPROM not write-protected. |
CONFIG7L (address:0x30000C, mask:0x03)
EBTR0 -- Table Read Protection bit
| EBTR0 = ON | 0xFE | Block 0 protected from table reads executed in other blocks. |
| EBTR0 = OFF | 0xFF | Block 0 not protected from table reads executed in other blocks. |
EBTR1 -- Table Read Protection bit
| EBTR1 = ON | 0xFD | Block 1 protected from table reads executed in other blocks. |
| EBTR1 = OFF | 0xFF | Block 1 not protected from table reads executed in other blocks. |
CONFIG7H (address:0x30000D, mask:0x40)
EBTRB -- Boot Block Table Read Protection bit
| EBTRB = ON | 0xBF | Boot block protected from table reads executed in other blocks. |
| EBTRB = OFF | 0xFF | Boot block not protected from table reads executed in other blocks. |

This page generated automatically by the device-help.pl program (2012-12-22 23:50:59 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.