- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC12C509
| Bank 0 |  | Bank 1 |
| Shared 0x000 - 0x00F 16 bytes GPR 0x010 - 0x01F 16 bytes |  | Shared 0x020 - 0x02F 16 bytes GPR 0x030 - 0x03F 16 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

| SFR 0 bytes GPR 16 bytes Shared 16 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 16 bytes Shared 16 bytes Unimplemented 0 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

Special Function Register.

General-purpose RAM.

Shared RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:57 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.