## Detailed command line switches

### Options ordered by feature

Setting | Brief description
--- | ---
Input options
By default, LAME accepts a PCM audio sample inside a .WAV container as the input file, in 8, 16, 24 and 32 bits integer and in IEEE FLOAT. If it is compiled with libsndfile, then it also supports the extra formats that the library supports. There is also support for RAW PCM data and and piped input
- | For piped/streamed Input, use "-" as the input and/or output file name.
--out-dir path | If no explicit output file is specified, a file will be written at given path. Ignored when using piped/streamed input
--mp1input 1 | Input file is an MPEG layer I file. Implicit if extension is .mp1
--mp2input 1 | Input file is an MPEG layer II file. Implicit if extension is .mp2
--mp3input 1 | Input file is an MPEG layer III file. Implicit if extension is .mp3
--scale number | Scale input (multiply PCM data) by number.
--scale-l number | Scale channel 0 (left) input (multiply PCM data ) by number
--scale-r number | Scale channel 1 (right) input (multiply PCM data) by number
--swap-channel | Swap input channels
--nogap file1 file2 ... | Gapless encoding for a set of contiguous files
--nogapout dir | Output dir for gapless encoding (must precede --nogap)
--nogaptags | Allow the use of VBR tags in gapless encoding
Input options for RAW PCM
-r | Assume input file is raw PCM.
-s number | Input sampling frequency in kHz
-x | Force byte-swapping of input
--bitwidth w | Input bit width is w (default 16)
--signed / --unsigned | Input is signed (default) or unsigned
--little-endian / --big-endian | Input is little-endian (default) or big-endian
-a | Downmix from stereo to mono file for mono encoding
Constant Bit Rate (CBR)
-b number | Set the bitrate in kbps, default 128 kbps
--cbr | Enforce use of constant bitrate
--comp ratio | Choose bitrate to obtain the specified compression ratio
--freeformat | Produce a free format bitstream instead of the standard one. Supported bitrates between 8 and 640 kbps. Scarce support by decoders.
Variable Bit Rate (ABR)
--abr number | Specify average bitrate desired (instead of quality)
Variable Bit Rate (VBR)
-V number | Quality setting for VBR. default number=4. Decimal values can be specified, like: 4.51 0=highest quality, bigger files. 9.999=lowest quality, smaller files
--vbr-old | Use old variable bitrate (VBR) routine
-b number | Specify a minimum allowed bitrate. default 32 kbps (See -F setting below)
-B number | Specify a maximum allowed bitrate. default 320 kbps
-F | Enforce -b option for digital silence frames too, rather than encoding them at 8 or 32 kbps.
-t | Disable VBR informational tag
-T | Enable and force writing LAME Tag
-Y | Allows -V2, -V1 and -V0 to not to encode the highest frequencies accurately, if doing so causes disproportional increases in bitrate. This is the same that CBR and ABR modes do.
Operational options
--preset type | Enables some preconfigured settings. Check below for each of the valid values
--resample sfreq | Sampling frequency of output file(kHz)- default=automatic
--priority number | Sets the process priority: 0,1 = Low priority 2 = normal priority (default) 3,4 = High priority
--flush | Flush output stream as soon as possible
--decode | Input=mp3 file, output=wav
--decode-mp3delay samples | Set the encoder delay to use to decode the input .mp3 file
-t | Disable writing wav header when using --decode
--noasm type | Disable assembly optimizations for mmx/3dnow/sse
Noise shaping & psycho acoustic algorithms
-q number | number = 0...9. Default -q 3 -q 0: Highest quality, very slow -q 9: Poor quality, but fast Please, see notes in the detailed description
-m mode | joint, simple, force, dual-mono, mono, left, right. default is j. joint = joins the best possible of MS and LR stereo simple = force LR stereo on all frames force = force MS stereo on all frames.
Filter options:
--lowpass number | Frequency(kHz), lowpass filter cutoff above freq. Range [0.001..50]kHz or [50..50000]Hz
--lowpass-width number | Frequency(kHz), lowpass window width. Range [0.001..16]kHz or [16..50000]Hz - (See further restriction in the detailed explanation)
--highpass number | Frequency(kHz), highpass filter cutoff below freq. Range [0.001..16]kHz or [16..50000]Hz (See further restriction in the detailed explanation)
--highpass-width number | Frequency(kHz), highpass window width - (See further restriction in the detailed explanation)
ID3 tag Information
--tt title | Audio/song title (max 30 chars for version 1 tag)
--ta artist | Audio/song artist (max 30 chars for version 1 tag)
--tl album | Audio/song album (max 30 chars for version 1 tag)
--ty year | Audio/song year of issue (1 to 9999)
--tc comment | User-defined text (max 30 chars for v1 tag, 28 for v1.1)
--tn track[/total] | Audio/song track number and (optionally) the total number of tracks on the original recording. (track and total each 1 to 255. just the track number creates v1.1 tag, providing a total forces v2.0).
--tg genre | Audio/song genre (name or number in list)
--ti file | Audio/song albumArt (jpeg/png/gif file, 128KB max, v2.3)
--tv id=value | Text or URL frame specified by id and value (v2.3 tag), user defined text frame syntax: --tv "TXXX=description=content"
--add-id3v2 | Force addition of version 2 tag
--id3v1-only | Add only a version 1 tag
--id3v2-only | Add only a version 2 tag
--id3v2-latin1 | Add following options in ISO-8859-1 text encoding
--id3v2-utf16 | Add following options in unicode text encoding
--space-id3v1 | Pad version 1 tag with spaces instead of nulls
--pad-id3v2-size n | Adds ID3v2 tag with n padding bytes
--genre-list | Print alphabetically sorted ID3 genre list and exit
--ignore-tag-errors | Ignore errors in values passed for tags
Note: A version 2 tag will NOT be added unless one of the input fields won't fit in a version 1 tag (e.g. the title string is longer than 30 characters), or the '--add-id3v2' or '--id3v2-only' options are used, or output is redirected to stdout.
MP3 header/stream options:
-e mode | De-emphasis n/5/c (obsolete)
-c | Mark as copyright
-o | Mark as non-original
-p | Error detection. adds 16 bit checksum to every frame (the checksum is computed correctly)
--strictly-enforce-ISO | Comply as much as possible to ISO MPEG spec
--replaygain-fast | Compute RG fast but slightly inaccurately (default)
--replaygain-accurate 1 | Compute RG more accurately and find the peak sample
--noreplaygain | Disable ReplayGain analysis
--clipdetect 1 | Enable --replaygain-accurate and print a message whether clipping occurs and how far the waveform is from full scale
Verbosity:
--disptime secs | Print progress report every secs seconds
--nohist | Disable VBR histogram display
--silent / --quiet | Don't print anything on screen
--verbose | Print a lot of useful information
--version / --license | Print License information
--help / --usage | Shows the common list of switches. Add id3 or dev to get help for a specified topic
--longhelp | Shows the complete list of switches
Experimental switches for developers. Only enabled in alpha/debug versions:
--nores | Each frame will then become independent from previous ones, but the quality will be lower.
--noshort | Disable use of short blocks
--short | Allow the use of short blocs (default)
--allshort | Use only short blocks
--shortthreshold x[,y] |
--temporal-masking x | x=0 disables, x=1 enables temporal masking effect
--notemp | Alias of --temporal-masking 0
--nssafejoint | M/S switching criterion
--nsmsfix x | M/S switching tuning [effective 0-3.5]
--interch x | Adjust inter-channel masking ratio (default 0.0). Range [0.0..1.0]
--ns-bass x | Adjust masking for sfbs 0 - 6 (long) 0 - 5 (short)
--ns-alto x | Adjust masking for sfbs 7 - 13 (long) 6 - 10 (short)
--ns-treble x | Adjust masking for sfbs 14 - 21 (long) 11 - 12 (short)
--ns-sfb21 x | Change ns-treble by x dB for sfb21
--substep |
--noath | Disable the use of ATH
--athonly | Use only ATH
--athshort | ATH only for short blocks
--athlower x | Lower the ATH by x.x dB's
--athtype x | Select ATH type curve
--vbr-new | In LAME 3.98, the new VBR was made default, and this switch is now used for experimental tweaks
--buffer-constraint x | available values for x: default, strict, maximum
Aliases and removed settings
-f | Alias of -q 7.
-h | Alias of -q 2.
-v | Alias of -V 4
-S | Alias of --silent
--alt-preset | Alias of --preset
--r3mix | Alias of -V 3
--vbr-mtrh | Alias of LAME 3.98 default vbr mode
--pad-id3v2 | Alias of --pad-id3v2-size 128
-d | No longer supported
-k | No longer supported
--cwlimit | No longer supported
--ogginput | No longer supported. Compile with libsndfile instead
-Z | Currently unused
--brief | Currently unused
--nspsytune | Currently unused

### Detailed description in alphabetical order

-a Downmix

mix the stereo input file to mono and encode as mono.

This option is only needed in the case of raw PCM stereo input (because LAME cannot determine the number of channels in the input file). To encode a stereo PCM input file as mono, use "lame -m s -a"

For WAV and AIFF input files, using "-m m" will always produce a mono .mp3 file from both mono and stereo input.

--abr n Average bitrate encoding (aka Safe VBR)

turns on encoding with a targeted average bitrate of n kbps, allowing to use frames of different sizes. The allowed range of n is 8...320 kbps, you can use any integer value within that range.

--add-id3v2 Force addition of version 2 tag

Tells LAME to add the tag information as id3v2. This implies adding both, a version 1 and a version 2 tag, if the values fit on a version 1 tag. See --id3v1-only and --id3v2-only if you want a more fine-grained control.

-b n Bitrate

Codec | sample frequencies (kHz) | bitrates (kbps)
--- | --- | ---
MPEG-1 layer III | 32, 48, 44.1 | 32 40 48 56 64 80 96 112 128 160 192 224 256 320
MPEG-2 layer III | 16, 24, 22.05 | 8 16 24 32 40 48 56 64 80 96 112 128 144 160
MPEG-2.5 layer III | 8, 12, 11.025 | 8 16 24 32 40 48 56 64

The bitrate to be used. Default for CBR is 128 kbps MPEG1, 80 kbps MPEG2.

When used with variable bitrate encodings (VBR), -b specifies the minimum bitrate to use. This is useful only if you need to circumvent a buggy hardware device with strange bitrate constrains. (You will need the -F setting too for digital silence).
Default for ABR/VBR is the minimum allowed bitrate for the MPEG version. (i.e. no limit)

-B n Max bitrate

see also option "-b" for allowed bitrates.

Maximum allowed bitrate when using VBR/ABR.

Using -B is NOT RECOMMENDED. A 128 kbps CBR bitstream, because of the bit reservoir, can actually have frames which use as many bits as a 320 kbps frame. ABR/VBR modes minimize the use of the bit reservoir, and thus need to allow 320 kbps frames to get the same flexibility as CBR streams. This is useful only if you need to circumvent a buggy hardware device with strange bitrate constrains.
Default value is the maximum allowed bitrate for the MPEG versio (i.e. no limit)

--big-endian Set the byte order to big-endian.

This switch tells LAME that the RAW pcm input is encoded in big-endian instead of little-endian.

--bitwidth Sets the bitwidth value

With RAW pcm input, this switch lets specify the bitwidth of the same (8 bits, 16 bits...)

-c copyright flag

mark the encoded file as copyrighted

--cbr Enforce constant bitrate encoding

This switch disables the VBR encoding. Examples:

    lame -V 0 --cbr input.wav

Will encode at -b 128 (ignore completely -V and encode at default bitrate)

    lame --preset 160 --cbr

Will encode at -b 160 (ignore ABR and use the specified bitrate)

    lame --abr 200 --cbr

Will encode at -b 192 (ignore ABR and use the nearest bitrate to the one specified)

--clipdetect Clipping detection

Enable --replaygain-accurate and print a message whether clipping occurs and how far in dB the waveform is from full scale.

This option is not usable if the MP3 decoder was explicitly disabled in the build of LAME.

See also: --replaygain-accurate

--comp x Indicate a compression ratio instead of a bitrate

Use this in place of the -b setting if you prefer to indicate a compression ratio (integer value). The ratio is the value of original-filesize/desired-filesize

--decode MP3 decode capability

This uses LAME's HIP2 decoder to decode an MP3 (layers 1, 2 and 3) file to a wav file.

If -t is used (disable wav header), LAME will output raw pcm in native endian format (use -x to swap bytes).

This option is not usable if the MP3 decoder was explicitly disabled in the build of LAME.

--decode-mp3delay x Indicate a different encoder delay for decoding

When decoding an mp3 file, LAME automatically corrects for the start delay that the encoder had to put into it.
This setting lets you specify a different delay than LAME's own one, so that it is possible to compensate for the delay of mp3's generated with other encoders.

--disptime secs Update the display each secs

Use this setting to change the frequency that LAME updates the display when encoding a file. Allows decimal values (like 0.5)

-e n/5/c Write the de-emphasis flag

n = (none, default)
5 = 50/15 microseconds
c = ccitt j.17

All this does is set a flag in the bitstream. If you have a PCM input file where one of the above types of (obsolete) emphasis has been applied, you can set this flag in LAME. Then the mp3 decoder should de-emphasize the output during playback, although most decoders ignore this flag.

A better solution would be to apply the de-emphasis with a standalone utility before encoding, and then encode without -e.

-F Enforce the minimum bitrate

Enforces the minimum bitrate. Without this option, passages of analog silence will be encoded at the minimum bitrate possible (32 or 8, depending on MPEG version).

--flush Flush the output stream as soon as possible

This setting forces a flush of the data written as soon as the operation has finished. This is mostly useful in case of streams. With files, it may degrade performance, since the OS has to write to disk in smaller chunks.

--freeformat Encode to freeformat stream

LAME will produce a fixed bitrate, free format bitstream. User must specify the desired bitrate in kbps, which can be any integer between 8 and 640.

Not supported by most decoders. Compliant decoders (of which there are few) are only required to support up to 320 kbps.

Decoders which can handle free format:

| Supports up to
--- | ---
MAD | 640 kbps
"lame --decode" | 640 kbps
l3dec | 310 kbps

--genre-list Print alphabetical ordered list of known genres

Tell LAME to print the list of genres with their index to be used with the --tg setting.

123 Acappella 34 Acid 74 Acid Jazz 73 Acid Punk 99 Acoustic 20 Alternative 40 Alternative Rock 26 Ambient 145 Anime 90 Avantgarde 116 Ballad 41 Bass 135 Beat 85 Bebob 96 Big Band 138 Black Metal 89 Bluegrass 0 Blues 107 Booty Bass 132 BritPop 65 Cabaret 88 Celtic 104 Chamber Music 102 Chanson 97 Chorus 136 Christian Gangsta 61 Christian Rap 141 Christian Rock 32 Classical 1 Classic Rock 112 Club 128 Club-House 57 Comedy 140 Contemporary Christian 2 Country 139 Crossover 58 Cult | 3 Dance 125 Dance Hall 50 Darkwave 22 Death Metal 4 Disco 55 Dream 127 Drum & Bass 122 Drum Solo 120 Duet 98 Easy Listening 52 Electronic 48 Ethnic 54 Eurodance 124 Euro-House 25 Euro-Techno 84 Fast Fusion 80 Folk 115 Folklore 81 Folk-Rock 119 Freestyle 5 Funk 30 Fusion 36 Game 59 Gangsta 126 Goa 38 Gospel 49 Gothic 91 Gothic Rock 6 Grunge 129 Hardcore 79 Hard Rock 137 Heavy Metal 7 Hip-Hop 35 House 100 Humour 131 Indie | 19 Industrial 33 Instrumental 46 Instrumental Pop 47 Instrumental Rock 8 Jazz 29 Jazz+Funk 146 JPop 63 Jungle 86 Latin 71 Lo-Fi 45 Meditative 142 Merengue 9 Metal 77 Musical 82 National Folk 64 Native US 133 Negerpunk 10 New Age 66 New Wave 39 Noise 11 Oldies 103 Opera 12 Other 75 Polka 134 Polsk Punk 13 Pop 53 Pop-Folk 62 Pop/Funk 109 Porn Groove 117 Power Ballad 23 Pranks 108 Primus 92 Progressive Rock 67 Psychedelic 93 Psychedelic Rock 43 Punk 121 Punk Rock | 15 Rap 68 Rave 14 R&B 16 Reggae 76 Retro 87 Revival 118 Rhythmic Soul 17 Rock 78 Rock & Roll 143 Salsa 114 Samba 110 Satire 69 Showtunes 21 Ska 111 Slow Jam 95 Slow Rock 105 Sonata 42 Soul 37 Sound Clip 24 Soundtrack 56 Southern Rock 44 Space 101 Speech 83 Swing 94 Symphonic Rock 106 Symphony 147 SynthPop 113 Tango 18 Techno 51 Techno-Industrial 130 Terror 144 Thrash Metal 60 Top 40 70 Trailer 31 Trance 72 Tribal 27 Trip-Hop 28 Vocal

--help Print the command line help.

Print the short command line help and exit.

--highpass number Use a highpass filter when encoding

Enables a highpass filter of the specified frequency when encoding the source. Range [0.001..50]kHz or [50..50000]Hz.
This is usually not required, and the gains are usually minimal. May be useful to remove an interference signal on 50Hz or 60Hz, or a DC offset. (default: disabled)
Note: The current implementation has a minimum highpass frequency of (67.5/62)% of the sample rate (I.e. 481Hz at 44Khz).

--highpass-width width Set the width of the decaying curve.

Specify the width in Hz of the decaying curve of the highpass. Range [16..50000]Hz
The minimum (and default) width is 75% of a band's width (which is 1/64th of the sample rate).
Note: See the remark in the --highpass command above.

--id3v1-only Disable the use of id3v2.

Put it before any tag setting.
This setting tells LAME to use ID3 v1 tag only, and not create an ID3v2 even if it thinks it should.

--id3v2-only Disable the user ov id3v1.

Put it before any tag setting.
This setting tells LAME to use ID3 v2 tag only. An ID3 v1 tag would not be written.

--ignore-tag-errors Ignore tag information errors

Put it before any tag setting.
This tells lame to ignore the tag information that sees as erroneous and continue encoding without those. Without this setting, errors are reported and encoding does not start.

--license Print the license page

Prints version and license information about LAME encoder.

--little-endian Set the byte order to little-endian.

This switch tells LAME that the RAW pcm input is encoded in little-endian. It is the default setting.

--longhelp Shows the detailed help

Prints a help page with all of the command-line switches and a brief explanation of them.

--lowpass number Use a lowpass filter when encoding

Enables a lowpass filter of the specified frequency when encoding the source. Range [0.001..50]kHz or [50..50000]Hz

Using a lowpass filter helps reducing the amount of data to encode. This is important in MP3 due to a limitation in very high frequencies (>16Khz). The default value depends on the target bitrate/quality. It is not recommended to change it as a general basis.

--lowpass-width width Set the width of the decaying curve.

Specify the width in Hz of the decaying curve of the lowpass. Range [0.001..16]kHz or [16..50000]Hz
The lowpass is in the center of this curve. The minimum (and default) width is 75% of a band's width (which is 1/64th of the sample rate).

-m x Channel modes

-m m | mono
-m s | forced L/R stereo
-m j | automatic switch between L/R and M/S stereo
-m f | forced mid/side stereo
-m d | dual (independent) channels

MONO is the default mode for mono input files. If "-m m" is specified for a stereo input file, the two channels will be averaged into a mono signal.

FORCED L/R STEREO encodes the left and the right signals independently, and gives more or less bits to each, depending on the currently available.

JOINT STEREO is the default mode of encoding. jstereo means the encoder can use (on a frame by frame basis) either L/R stereo or mid/side stereo. In mid/side stereo, the mid (L+R) and side (L-R) channels are encoded, and more bits are allocated to the mid channel than the side channel. When there isn't too much stereo separation, this effectively increases the bandwidth, so having higher quality with the same amount of bits.
Using mid/side stereo inappropriately can result in audible compression artifacts. Too much switching between mid/side and regular stereo can also sound bad. To determine when to switch to mid/side stereo, LAME uses a much more sophisticated algorithm than the one described in the ISO documentation.

FORCED MID/SIDE STEREO forces all frames to be encoded with mid/side stereo. It should only be used if you are sure every frame of the input file has very little stereo seperation.

DUAL CHANNEL mode is similar to encode the left and right as two mono signals. The main use of Dual channel is to encode content in two languages.

--mp1input --mp2input --mp3input MPEG layer I, II or III input file

Assume the input file is an MP1/2/3 file. LAME will decode the input file before re-encoding it. Since MP3 is a lossy format, this is not recommended in general. But it is useful for creating low bitrate mp3s from high bitrate mp3s. If the filename ends in ".mp3" LAME will assume it is an MP3. For stdin or MP3 files which don't end in .mp3 you need to use this switch.

--noasm value Disables the specified assembler instructions

When the encoder is compiled with assembler optimizations, this setting allows to disable them at runtime (They are only enabled if the CPU supports them). The purpose of this setting is to detect problems in those optimizations, and/or check the speed difference.

--nogap file1 file2 [...] Encodes multiple continuous files.

Encodes multiple files (ordered by position) which are meant to be played gaplessly.

By default, LAME will encode the files with accurate length, but the first and last frame may contain a few erroneous samples for signals that don't fade-in/out (as is the case of continuous playback).

This setting solves that by using the samples from the next/previous file to compute the encoding.

--nogapout dir Specify a directory for the output of the files encoded with --nogap

This setting should precede --nogap, and is used to specify the alternate directory where to store the encoded files. The default one is the input file directory.

--nogaptags Enables the use of VBR tags with files encoded with --nogap

Tells LAME to put VBR tags to encoded files if they are encoded in VBR or ABR modes. Else, using the --nogap option doesn't generate it.

--nohist Disable bitrate Histogram

By default, LAME will display a bitrate histogram while producing VBR mp3 files. This will disable that feature.

--noreplaygain Disable ReplayGain analysis

By default ReplayGain analysis is enabled. This switch disables it.

See also: --replaygain-accurate, --replaygain-fast

-o non-original

Mark the encoded file as a copy

-p CRC error detection

Turn on CRC error protection. It will add a cyclic redundancy check (CRC) code in each frame, allowing to detect transmission errors that could occur on the MP3 stream. However, it takes 16 bits per frame that would otherwise be used for encoding, and then will slightly reduce the sound quality.

--pad-id3v2 Pad ID3v2 tag.

Pads the ID3v2 tag with extra 128bytes to allow it to expand.

--preset x Enable one of the presets

Setting | Meaning
--- | ---
--preset medium | -V 5 --vbr-old
--preset standard | -V 2 --vbr-old
--preset extreme | -V 0 --vbr-old
--preset insane | -b 320 --vbr-old
--preset fast xxx | Adding the "fast" keyword before the mentioned presets enables the LAME 3.98 default vbr routine.
--preset number | --abr number
--preset cbr number | -b number
Old compatibility settings. Meaningless
--preset phone | -b 16 -m m
--preset phon+ / lw / mw-eu | -b 24 -m m
--preset mw-us | -b 40 -m m
--preset voice | -b 56 -m m
--preset fm / radio | -b 112
--preset hifi | -b 160
--preset cd | -b 192
--preset studio | -b 256

--priority value Set process priority

(Windows and OS/2 only)

Sets the process priority for LAME while running under Windows and/or IBM OS/2. This can be very useful to avoid the system becoming slow and/or unresponsive. By setting LAME to run in a lower priority, you leave more time for the system to update basic processing (drawing windows, polling keyboard/mouse, etc). The impact in LAME's performance is minimal if you use priority 0 to 2.

The valid parameters are:

| Priority | Windows | OS/2
--- | --- | --- | ---
0 | Low priority | IDLE_PRIORITY_CLASS | IDLE, delta = 0
1 | Medium priority | IDLE_PRIORITY_CLASS | IDLE, delta = +31
2 | Regular priority | NORMAL_PRIORITY_CLASS | REGULAR, delta = -31
3 | High priority | HIGH_PRIORITY_CLASS | REGULAR, delta = 0
4 | Maximum priority | HIGH_PRIORITY_CLASS | REGULAR, delta = +31

Note that if you call '--priority' without a parameter, then priority 0 will be assumed.

-q n Algorithm quality selection

Bitrate is of course the main influence on quality. The higher the bitrate, the higher the quality. But for a given bitrate, we have a choice of algorithms to determine the best scalefactors and Huffman coding (noise shaping).

For CBR, ABR and --vbr-old modes, the following table applies

-q 0 | Use slowest & best possible version of all algorithms.
-q 3 | Default value. Good speed, good quality
-q 7 | Very fast, ok quality. (psycho acoustics are used for pre-echo & M/S, but no noise shaping is done.
-q 9 | Disables almost all algorithms including psy-model. Poor quality.

For the default VBR mode since LAME 3.98, the following table applies

-q 0 to -q 4 | Use the best algorithm.
-q 5 to -q 9 | Use the not so good algorithm

--quiet Don't print any output in the screen

Disables the screen output. Useful for job processing or other times where screen output is undesirable.

-r Input file is raw pcm

Assume the input file is raw pcm. Sampling rate and mono/stereo must be specified on the command line. Without -r, LAME will perform several fseek()'s on the input file looking for WAV and AIFF headers.

Not supported if LAME is compiled to use LIBSNDFILE.

--replaygain-accurate Slightly more accurate ReplayGain analysis and finding the peak sample

Enable decoding on the fly. Compute "Radio" ReplayGain on the decoded data stream. Find the peak sample of the decoded data stream and store it in the file.

ReplayGain analysis does _not_ affect the content of a compressed data stream itself, it is a value stored in the header of a sound file. Information on the purpose of ReplayGain and the algorithms used is available from http://www.replaygain.org/

By default, LAME performs ReplayGain analysis on the input data (after the user-specified volume scaling). This behaviour might give slightly inaccurate results because the data on the output of a lossy compression/decompression sequence differs from the initial input data. When --replaygain-accurate is specified the mp3 stream gets decoded on the fly and the analysis is performed on the decoded data stream. Although theoretically this method gives more accurate results, it has several disadvantages:

- tests have shown that the difference between the ReplayGain values computed on the input data and decoded data is usually no greater than 0.5dB, although the minimum volume difference the human ear can perceive is about 1.0dB
- decoding on the fly significantly slows down the encoding process

The apparent advantage is that:

- with --replaygain-accurate the peak sample is determined and stored in the file. The knowledge of the peak sample can be useful to decoders (players) to prevent a negative effect called 'clipping' that introduces distortion into sound.

Only the "Radio" ReplayGain value is computed. It is stored in the LAME tag. The analysis is performed with the reference volume equal to 89dB. Note: the reference volume has been changed from 83dB on transition from version 3.95 to 3.95.1.

This option is not usable if the MP3 decoder was _explicitly_ disabled in the build of LAME. (Note: if LAME is compiled without the MP3 decoder, ReplayGain analysis is performed on the input data after user-specified volume scaling).

See also: --replaygain-fast, --noreplaygain, --clipdetect

--replaygain-fast Fast ReplayGain analysis

Compute "Radio" ReplayGain of the input data stream after user-specified volume scaling and/or resampling.

ReplayGain analysis does _not_ affect the content of a compressed data stream itself, it is a value stored in the header of a sound file. Information on the purpose of ReplayGain and the algorithms used is available from http://www.replaygain.org/

Only the "Radio" ReplayGain value is computed. It is stored in the LAME tag. The analysis is performed with the reference volume equal to 89dB. Note: the reference volume has been changed from 83dB on transition from version 3.95 to 3.95.1.

This switch is enabled by default.

See also: --replaygain-accurate, --noreplaygain

--resample n Output sampling frequency in kHz

where n = 8, 11.025, 12, 16, 22.05, 24, 32, 44.1, 48

Output sampling frequency. Resample the input if necessary.

If not specified, LAME may sometimes resample automatically when faced with extreme compression conditions (like encoding a 44.1 kHz input file at 32 kbps). To disable this automatic resampling, you have to use --resample to set the output sample rate equal to the input sample rate. In that case, LAME will not perform any extra computations.

-s n Sampling frequency in kHz

where n = sampling rate in kHz.

Required for raw PCM input files. Otherwise it will be determined from the header information in the input file.

LAME will automatically resample the input file to one of the supported MP3 sample rates if necessary.

--scale arg --scale-l arg --scale-r arg Scale the amplitude of the input file

Scales input by arg. This just multiplies the PCM data (after it has been converted to floating point) by arg.

arg > 1: increase volume
arg = 1: no effect
arg < 1: reduce volume

Use with care, since most MP3 decoders will truncate data which decodes to values greater than 32768.

The l and r variants apply the scaling only to left (channel 0) or right (channel 1) respectively.

--signed Input RAW uses signed values

Use with RAW pcm to indicate if the data is signed (values centered at zero) or unsigned (all positive values). This is the default value.

--silent Don't print any output in the screen

Disables the screen output. Useful for job processing or other times where screen output is undesirable.

--space-id3v1 Use spaces for padding.

Use spaces instead of null values for padding data in an ID3v1 tag.

--strictly-enforce-ISO Strict ISO compliance

With this option, LAME will enforce the 7680 bit limitation on total frame size. This results in many wasted bits for high bitrate encodings. Some decoders need it.

-t Disable VBR tag or disable WAV header

This setting has two different uses:

When encoding to VBR, this setting disables writing the VBR Tag (also known as XING tag). This tag is embedded by default in the frame 0 of the MP3 file. It lets VBR aware players to correctly seek and compute playing times in such files.

When decoding MP3 to WAV using --decode, this flag will disable writing the WAV header. The output will be raw pcm, native endian format. Use -x to swap bytes.

-T Force the usage of the LAME tag

By default, LAME already adds a LAME tag when encoding. This setting overrides the -t setting, and implies --nogaptags.

--unsigned Input RAW uses unsigned values

Use with RAW pcm to indicate if the data is signed (values centered at zero) or unsigned (all positive values).

--usage Print the command line help.

Print the short command line help and exit.

-V n Enable VBR encoding

Encodes using the VBR algorithm, at the indicated quality.
Decimal values can be specified, like: 4.51
0=highest quality, bigger files. 9.999=lowest quality, smaller files

Using -V 7 or higher (lower quality) is not recommended. ABR usually produces better results.

--vbr-old Uses the old VBR method of encoding

Tells LAME to encode to VBR using the old (slower) method of encoding.

--verboseProgram verbosity

Print a lot of information on screen.

--version Prints the license page

Prints version and license information about LAME encoder.

-x Swap input bytes

swap bytes in the input file (and output file when using --decode). For sorting out little endian/big endian type problems. If your encodings sound like static, try this first.

-Y Ignore noise in sbf21, like CBR mode does

Allows -V2, -V1 and -V0 to not to encode the highest frequencies accurately, if doing so causes disproportional increases in bitrate. This is the same that CBR and ABR modes do.
Due to the design of the MP3 format, to keep precision in the last scalefactor band, an encoder needs to increase the precision in all the bands (not only in this one).
The consequence is an increase of bitrate (+60kbps in some cases) compared to not keeping that precision. Generally, this band should allow for distortions, so using it shouldn't cause harm.

1. If compiled with decoding capabilities
2. HIP stands for Hip Isn't a Player and is based off of Michael Hipp's mpglib 0.2a