  
  Logitech MouseWare README File
  (c) Copyright 1995-1998 Logitech, Inc. All Rights Reserved.
  
  
  README TABLE OF CONTENTS
  
  1. Installation
   1.1  Standard Installation
   1.2  DOS Installation
   1.3  Drivers Only Installation
   1.4  Work Around Installation for Windows 9x
   1.5  Work Around Installation for Windows 3.1
   1.6  Manually Decompressing Files
  2. Uninstall Program
  3. Features
   3.1  Cloaking Feature for DOS and Windows 3.1
   3.2  Zooming in Windows 9x and NT 4.0
  4. Troubleshooting
   4.1  Detection Problems with PS/2 Pointing Devices
   4.2  Serial Port Detection Problems with Serial Pointing
   Devices under DOS and Windows 3.1
   4.3  Conflicts with other Serial Devices
   4.4  Power Management Problems
   4.5  Logitech Enhanced Mouse Control Panel is not Updated
   4.6  Scrolling/wheel related issues
   4.7  Cordless Desktop
  5. For more information
  
  ________________________________________

1.   Installation
  
  Before installing any software under Windows NT 4.0, we
  strongly recommend you create an Emergency Repair Disk using
  the Repair Disk utility provided by the system (RDISK.EXE).
  
  Please note that USB mice are only supported under Windows 98.
  
1.1  Standard Installation
  
  Windows 3.1, Windows 95 (OSR2), Windows 98 (both of them
  together from now on referred to as Windows 9x when applicable)
  and Windows NT 4.0.
  Run Setup.exe from the floppy diskette to install the MouseWare
  software.
  
1.2  DOS Installation
  
  The MouseWare installation program will only run if Windows is
  installed on your machine. If your computer runs DOS only,
  follow the instructions below:
  
  1) Insert the MouseWare diskette into the floppy drive.
  2) Change your DOS prompt to match the floppy drive being used.
  3) At the A: prompt type:
     T A: C:\Mouse [Enter]
     Or at the B: prompt type:
     T B: C:\Mouse [Enter]
  4) Pressing any key will start the copy process.
  5) When the manual install is complete, you will need to edit
     the AUTOEXEC.BAT. Please add the following lines:
     SET LMOUSE=C:\MOUSE
     C:\MOUSE\MOUSE.EXE
  6) Reboot the computer to make these changes take effect.
  
  
1.3  Drivers Only Installation
  
  Windows 9x and Windows NT 4.0 have the ability to load device
  drivers without running the Setup program. Loading the devices
  drivers this way, however, does not install the user interface
  programs such as the Logitech Enhanced Mouse Control Center.
  Using the "Have Disk" function will install only the Logitech
  mouse drivers.
  
  Please execute the following steps to perform a driver-only
  installation for Windows 95 or Windows NT 4.0:
  
  1)   Click on the "Start" button on the Windows Desktop.
  2)   Select "Settings", then "Control Panel".
  3)   From the Control Panel, double click on the Mouse Icon.
  4)   Select the "General" tab.
  5)   From the "General" tab, click on "Change".
  6)   Insert the MouseWare Disk 1 into the disk drive.
  7)   Click the "Have Disk" button.
  8)   When prompted, click the Browse button.
  9)   Double click the "drivers" folder.
  10)  Depending on the operating system, double click on the
       following folder:
    a)   Win95, for Windows 95 (OSR2)
    b)   WinNT, for Windows NT 4.0
  11)  Click the "Open" or "OK" button.
  12)  Click on the "OK" button.
  13)  Select, "Show all Devices".
  14)  Under "Manufacturers", Select "Logitech".
  15)  Under "Models", select the correct model that matches the
       pointing device type and click on the "OK" button.
  16)  If the "Confirm Device Install" box appears, click on the
       "Yes" button.
  17)  Windows should now copy the updated mouse drivers to the
       system.
  18)  Click on "Close".
  19)  Windows may request that you restart the system for the
       changes to take effect, click on "YES" to restart the
       system.
  
  Please execute the following steps to perform a driver-only
  installation for Windows 98:
  
  1)   Click on the "Start" button on the Windows 98 Desktop.
  2)   Select "Settings", then "Control Panel".
  3)   From the Control Panel, double click on the System icon.
  4)   Select the Device Manager tab.
  5)   Double click on the Mouse icon.
  6)   Double click on the Mouse Type icon.
  7)   Click on the Driver Tab.
  8)   Click on the "Update Driver" button.
  9)   From the "Update Device Driver Wizard" box click the
       "Next" button.
  10)  When asked "What do you want Windows to do?" click on
       the radio button next to:  "Display a list of all the
       drivers in a specific location, so you can select the
       driver you want."
  11)  Click on the "Next" button.
  12)  Insert the MouseWare Disk 1 into the disk drive.
  13)  Click on the "Have Disk" button.
  14)  When prompted, click the Browse button.
  15)  Double Click on the "drivers" folder.
  16)  Double Click on the "Win98" folder.
  17)  Click the "OK" button.
  18)  Click the "OK" button again.
  19)  Under "Models", select the correct model that matches
       the pointing device type and click on the "Next" button.
  
       Note: If the "Update Driver Warning" appears, click on
       the "Yes" button.
  
  20)  Click the "Next" button to copy files.
  21)  Click on the "Finish" button.
  22)  Windows 98 may request that you restart your system.
       Click on the "Yes" button to restart.

      
1.4  Work Around Installation for Windows 9x
  
  If you experience difficulty running the installation program,
  under Windows 9x, try launching the installer while running
  Windows 9x in Safe Mode.
  
  To install MouseWare manually under Windows 95, restart your
  computer and press the F8 key when "Starting Windows95"
  appears. To install MouseWare manually under Windows 98,
  restart your computer and hold down the Control Key until you
  see the Microsoft Startup Menu. Now select Safe Mode and rerun
  the MouseWare Setup program.
  
  If the Safe Mode installation fails, install MouseWare from the
  command line. Restart your system as described above and select
  "Command Prompt only" from the Microsoft Startup Menu. Insert
  the MouseWare diskette #1 into either the A: or B: drive. At
  the MS-DOS prompt type "A:" or "B:" depending on the drive you
  are using. Then type "T95 A:" or "T95 B:". This will expand all
  the compressed files. After running this you will need to load
  the drivers. See section 1.3 for a description on how to do
  this.
  
  
1.5  Work Around Installation for Windows 3.1
   
  If you experience difficulty running the installation program,
  you may want to do a manual installation. Refer to section 1.2
  and proceed with the installation for DOS.
  
  Before rebooting you need to edit the SYSTEM.INI file located
  in the WINDOWS directory. Please change the following lines to
  read as follows:
   
      [boot]
      mouse.drv=C:\MOUSE\LMOUSE.DRV
   
      [386Enh]
      mouse=C:\MOUSE\LVMD.386

  
1.6  Manually Decompressing Files
  
  Several files on the installation disk have been compressed.
  These files must be decompressed before you can use them. The
  SETUP program automatically decompresses these files during
  installation. However, should the need arise, we have provided
  a method for you to manually decompress these files. Compressed
  files have file names that end with a tilde sign (~). To
  decompress a file manually, use the LGEXPAND.EXE utility
  provided on the installation disk.
  
  For example, to decompress the file "WMOUSECC.EXE" to your hard
  disk, type:
  
  A:\lgexpand A:\WMOUSECC.EX~ C:\MOUSE\WMOUSECC.EXE
  
  Please make sure that the destination directory (C:\MOUSE in
  this example) exists before you issue this command.
  
  
2.   Uninstall Program
  
  MouseWare can be removed from Windows 9x and NT 4.0 by clicking
  the Add/Remove Programs icon in the Windows 9x or NT 4.0
  Control Panel. Select Logitech MouseWare and press the Remove
  button.
  
  Windows 9x
  Logitech MouseWare drivers will be removed from the system if
  setup finds alternate compatible drivers for a device in
  MSMOUSE.INF. Should this not be the case you can manually
  change the driver to another one as described in section 1.3.
  
  
3.   Features
  
3.1  Cloaking Feature for DOS and Windows 3.1
  
  The MouseWare DOS mouse driver works in conjunction with a
  special interface program called "Cloaking". The CLOAKING.EXE
  interface program allows the DOS mouse driver, MOUSE.EXE, to be
  loaded in extended memory, freeing valuable conventional and
  upper memory for DOS applications. CLOAKING.EXE is
  automatically installed during the standard MouseWare
  installation for Windows 3.1.
  
  Cloaking works in conjunction with a supported memory manager
  to enable the mouse driver to load in extended memory, using a
  mere 1k of conventional or upper memory.
  
  CLOAKING.EXE will work with any of the following extended
  memory managers:
  
   EMM386.EXE               Microsoft
   HIMEM.SYS                Microsoft
   RM386.EXE 3.03 or later  Helix
   QEMM386.SYS 7.1          Quarterdeck
   386MAX.SYS 5.0           Qualitas
  
  You will need to be running one of these programs in order to
  use CLOAKING.EXE. The EMM386.EXE and HIMEM.SYS programs are
  included with DOS versions 5.0 and above, and with Windows.
  
  Installing Cloaking:
  
  Under Windows 3.1, the installation program copies CLOAKING.EXE
  in the mouse directory and loads CLOAKING.EXE in your
  AUTOEXEC.BAT file. This will occur if your DOS version is 6.0
  or greater, you are running EMM386.EXE, and you are not already
  loading a version of CLOAKING.EXE.
  
  If you are running DOS only, you will need to do the changes
  manually. If you wish to install CLOAKING.EXE in the CONFIG.SYS
  file, add the line: "DEVICE=C:\MOUSE\CLOAKING.EXE" after the
  supported memory manager is loaded. If you wish to install
  cloaking in the AUTOEXEC.BAT file, add the line:
  "C:\MOUSE\CLOAKING.EXE" before the mouse driver is loaded.
  
  
3.2  Zooming in Windows 9x and NT 4.0
  
  In Windows 9x and Windows NT 4.0, some applications, as
  Office97, support the zooming. To zoom in such applications,
  just press the [Ctrl] key and roll your mouse's wheel (if any)
  or use the Universal Scroll button assignment. Be sure your
  application is Office 97 compliant and supports the zoom
  function.
  
  
4.   Troubleshooting
  
4.1  Detection Problems with PS/2 Pointing Devices
  
  If your mouse is connected to the mouse port and is not
  detected by the system, attempt the following step(s):
    
  1) Your mouse port might need to be enabled through the SETUP
     menu of your computer. Please check your computer
     documentation regarding the SETUP menu.
  
  2) If you have a mouse with both serial and mouse port
     adapters, connect the mouse to the computer through the
     serial port. Reboot and check if the mouse is detected
     properly.
  
  3) If adapter(s) were not included in your package, your mouse
     was designed to work on only one type of port (Serial OR
     PS/2). Refer to your package for the type of port your mouse
     supports.
  
  If the problem persists, please check for a possible computer
  BIOS ROM upgrade from your computer manufacturer.
  
  Some notebook systems, such as IBM ThinkPad, have both an
  external Mouse Port and an integrated Pointing Stick, which is
  connected to the Mouse Port. If your mouse is having difficulty
  running on the Mouse Port of this type of system, try using the
  serial port instead.
  
  The 500/700 series of IBM Thinkpad require you to disable the
  internal pointer stick or you may not get wheel/roller
  function.
  
4.2  Serial Port Detection Problems with Serial Pointing Devices
     under DOS and Windows 3.1
  
  If your mouse is connected to the serial port and is not
  detected by the system, add the following modification to the
  MOUSEDRV.INI file and reboot:
  
  [Technical]
  Timing=Hardware
  
  or load the DOS driver with the following parameter
  MOUSE.EXE NOINI
  
  
4.3  Conflicts with other Serial Devices
  
  1) Windows 9x
     If you have problems operating other serial devices together
     with MouseWare, in Windows 95 run Regedit.exe, edit the key:
     HKEY_LOCAL_MACHINE\SOFTWARE\Logitech\MouseWare\CurrentVersio
     n\Global\PortSearchOrder and remove the unused COM ports.
  
  2) Windows NT 4.0
     If you have problems operating other serial devices together
     with MouseWare, in Windows NT 4.0 run Regedit.exe, edit the
     key:
     HKEY_LOCAL_MACHINE\System\CurrentControlSet\Services\lsermou
     s\Parameters\Global\PortSearchOrder and remove the unused
     COM ports.
  
  3) Windows 3.1x and DOS
     In Windows 3.1 edit the parameter "PortSearchOrder" in the
     [Global] section of the file MOUSEDRV.INI located in the
     C:\MOUSE directory and remove the unused COM port.
  
  
4.4  Power Management Problems
  
  If your mouse freezes when waking your PC up from suspend, in
  Windows 9x run Regedit.exe and edit the key:
  HKEY_LOCAL_MACHINE\SOFTWARE\Logitech\MouseWare\CurrentVersion\T
  echnical\APMMode="Off"
  
  In Windows 3.1 edit the parameter "APMMode" in the [Technical]
  section of the file MOUSEDRV.INI
  
  
4.5  Logitech Enhanced Mouse Control Panel is not Updated
  
  Under Windows 9x if the Mouse properties has not been updated
  to Logitech Enhanced Mouse Control Center, verify you have
  installed MouseWare. If this does not resolve this issue, it
  may be necessary to do a registry clean-up. Remove the
  following folders in the Windows 9x Registry.
  
  Select the Start button, then Run, in the Open Line type
  
  C:\WINDOWS\REGEDIT.EXE and click on the OK button.
  
  Open the following Registry folders:
  
  HKEY_LOCAL_MACHINE\System\CurrentControlSet\Services\Class\Mous
  e\xxxx
  
  Remove all of the 0000, 0001, 0002, etc. under the Mouse folder
  until there are no folders remaining under the Mouse folder.
  Now shutdown your system and restart. Open the Mouse Properties
  and check to see if you now have the Enhanced Logitech Mouse
  Control Center.
  
  
4.6  Scrolling/wheel related issues
  
  If your mouse is equipped with a wheel and the wheel does not
  scroll, verify the following:
  
  1)   Verify that the Logitech control panel is installed
    properly. If you click the Start button and select Settings,
    Control Panel, the mouse icon should bring up a Logitech control
    panel. Otherwise reinstall MouseWare.
  
  2)   If your wheel only works in Office 97 compatible
    applications, go to the Buttons page in the mouse control panel
    and verify that the check box "Use Office 97 Compatible Scroll
    Only" is unchecked.
  
  3)   For advanced users: DirectInput may not receive wheel
    information while em_exec.exe is running (this most probably
    happens playing games). Should conflicts arise you will need to
    end task on Em_exec. To end task on Em_exec, press the "CTRL",
    "ALT" and "DEL" keys simultaneously in order for the "Close
    Program" dialogue to appear. Click on Em_exec to highlight it and
    then click on the "End Task" button.
    
    Note: this may cause scrolling to stop working for some
    applications and disables any special functionality provided by
    Logitech MouseWare. To re-enable complete functionality you will
    need to launch Em_exec manually. To do this, double-click on the
    mouse icon in the Windows 9x control panel.
  
  4)   The wheel will not operate in Windows 3.1 or in DOS.
    However, the wheel button will operate as a regular middle
    button.
  
 Please note that the scrolling mouse functions for touchpads do
 only work with Logitech touchpads. This is the case if you can
 find a "Touchpad" tab in the mouse control panel. Alternatively
 you can search for the following key in the registry:
 HKEY_LOCAL_MACHINE\SOFTWARE\Logitech\MouseWare\CurrentVersion\T
 ouchScroll.
 In order to look at the registry click the "Start" button and
 select "Run". Type "regedit" in the open line and click on the
 OK button.
 Note that the information in the Mouseware help file concerning
 touchpad support only applies to Logitech touchpads.

4.7  Cordless Desktop
  
  1) Keyboard loses connection with system
     This can occur if the keyboard channel button is pressed
     while the system is turned off or in suspend mode. Turn the
     system on or resume from suspend and press the keyboard
     channel button located on the right side of the keyboard.
     If the keyboard still does not work, follow the "Connect
     procedure" on the Easy Installation card enclosed with this
     package.
  
  2) Pressing Connect has no response from software
     If you receive no response from the software after the
     connect button is pressed, please do the following:
     - Wait at least 30 seconds before pressing the connect
       button again.
     - Check to see if your mouse and keyboard are working. If
       they are working, you do not need to reconnect them.
     - Press the connect button on the receiver and then press
       the channel button on one of the devices. If the connect
       button flashes, the device did connect successfully.
     
     If the devices are still not working, do the following:
     - Shut down your system
     - Remove the batteries from the devices
     - Restart your system
     - Put the batteries back into the devices
     - Perform the connect procedure again.
  
  3) Keyboard Only Connected -- no cordless features
     If the keyboard is connected to the computer without the
     cordless mouse, you will not receive any cordless software
     features for the keyboard.  This includes the Cordless Page
     in Keyboard Properties, battery status and task bar icons.
  
  4) Battery Status
     - Battery Status Low message appears after little use of the
       keyboard.
       Make sure you are using alkaline batteries in both the
       mouse and keyboard. If you are using alkaline batteries
       and the message still appears, change the batteries in the
       device.
  
     - Battery Status unknown message appears for the keyboard.
       The battery status for the keyboard is activated after 100
       keystrokes. Providing the keyboard is working as expected,
       this message is not a problem. If the keyboard is not
       working, please follow the connect procedure instructions
       on the enclosed Easy Installation Card.
  
  5) Mouse cursor is erratic
  Replace batteries.
  
  6) Keyboard misses keystrokes or keys repeat
  Replace batteries.
  

5.   For more information
  
  For more Troubleshooting information contact our web site at
  www.logitech.com
  
