ComCap - Magenta Serial Port Capture Utility
============================================

Readme for Release 2.6 - 3rd September 2002
-------------------------------------------

ComCap is a simple Windows application designed to capture any ASCII data
received on PC serial communications ports to text files.  Captured data
is optionally shown in scrolling windows, and may be copied to be
clipboard if required.  Data from up to eight serial communication ports
can be captured simultaneously, in separate files.  The capture file names
are automatically generated with a new file being created each day, week
or month, or several times a day.  Captured data may be optionally echoed
to a local or network printer.  ComCap is a system tray application that
can be set to start automatically when windows starts, and remain
unobtrusive.  ComCap will run on Windows 98 and later 32-bit versions of
Windows.  On Windows NT4, 2000, XP and .NET Server, ComCap may be run as a
service, so it automatically starts when the PC boots without needing a
user logged-on.

Although basic communications settings need to be specified (speed,
parity, data bits), there are no flow control settings and data will be
captured irrespective of the usual control lines (so just a 2-wire serial
cable is needed).

Provided that a reasonably continuous flow of data is being received, the
correct settings can usually be deduced within a minute or so, by changing
the speed until readable data appears.  Although ComCap ignores the
control lines, it does display the status of the CTS, DSR and DCD lines,
and also flashes when data is received.  ComCap sets the RTS and DTR lines
when capture is enabled and uses RTS for flow control.  ComCap never
transmits any data and does not support software flow control (Xon/Xoff).

ComCap is primarily designed to capture telephone call logging data from
the serial port provided on most telephone switching systems (PABXs),
typically called Call Data Records (CDR).  Generally, only ASCII data is
saved to the capture file, although there is a raw option.  The saved data
may then be used as input to telephone call management applications that
will cost calls and produce reports on telephone usage.  But ComCap is
application non-specific and will capture anything that arrives on a
serial port.  It has been used for a wide variety of purposes, such as
logging output from test and monitoring equipment and serial printer data.

Please note that ComCap is not designed to monitor data between modems and
PC applications, it requires exclusive access to the serial port so no
other application can use the port at the same time.

The ComCap distribution includes a small application written by a user,
'Concatenation Utility', that allows multiple text file captured by ComCap
to be combined into a single text file that may be easier to import into a
telephone call management application.  There is also a small ‘Test RS232
Signals’ utility that may be useful in testing communication port and
cabling problems.

ComCap should have a minimal overhead on the PC and can just be left
running minimised.  It will run on any PC or lap top capable of running
Windows 98 such as a low end Pentium with 16 Mbytes of memory (which could
be dedicated for data capture).  Although ComCap will probably run on
Windows 95, it is no longer officially supported because the Delphi
compiler is not longer supported on that OS.


Installation
------------

ComCap is usually distributed as a ZIP file, which should first be
unzipped into a temporary folder.  If you do not already have it, the
Winzip application from http://www.winzip.com/ (or from most magazine
cover CD-ROMs, Tucows archives, etc) is strongly recommended.

The program SETUP.EXE should then be run to install ComCap.  About 470
Kbytes of disk space is required for the COMCAP.EXE program and 310 Kbytes
for the service version COMCAPSVC.EXE (this is not installed on Windows
9x).   Two other programs are also installed CONCAT.EXE and SIGNALS.EXE.
These are described later.

If you have received an executable with the name COMCAPS.EXE, this should
be run just like SETUP.EXE to install the software.  If the service
version is already installed, please ignore the error saying so.

A user with administrative level privileges must install ComCap.
Normally, only administrative level users will be able to run ComCap.  To
allow lower level users access to ComCap, it is necessary to apply extra
permissions to the ComCap registry keys.  To do this, run REGEDT32.EXE,
and open the key:  HKEY_LOCAL_MACHINE\SOFTWARE\Magenta-Systems\ComCap.
Then click on ComCap, take Permissions from the main menu, select name
Users and you should see ‘Full Control, Allow’ as a blank box.  Tick it,
then Apply, and non-administrator logons will be able to run ComCap.

Until registered, ComCap will only run for 15 minutes before capture is
automatically stopped.  It will be necessary to restart ComCap to continue
capture.  ComCap may be registered using a secure order form at the web
site:  http://www.magsys.co.uk/comcap/.  Once the order has been
processed, a small file 'userreg.txt' is returned by email, which should
be copied into the ComCap directory.  If ComCap is already running, it
should be exited and restarted to see the new file.  When started, ComCap
will show the name of the individual or company that registered the
software and will run continually.

ComCap is run from Start, Programs, Magenta Systems, then ComCap.  The
ComCap icon will appear in the System Tray, which should be clicked to
restore the main application window.  To auto start ComCap each time
windows is booted, copy the ComCap shortcut into the Startup folder.

If ComCap has been installed on Windows NT4, 2000, XP or NET Server,
‘Magenta ComCap Service’ will be found added to the Services list, with
manual start-up.  Before the ComCap service may be started, the windows
version must be run, Common and Channel Settings specified and capture
tested.  Then the service version may be started, and changed to automatic
start-up, if required.  If the PC reboots, capture will then continue
without the PC needing to be logged-on.

Although the ComCap Service may be used logged-on to the ‘local system
account’, it is better to specify a specific user account with a password.
This ensures that dates and times in ComCap will be formatted according to
that user’s preferences, rather than the American default, and allows
access to network resources.  Echo printing is only possible when using
the account of a user that has the required printer installed.

For testing purposes, a Plessey Call Simulator may be downloaded from the
web site at:  http://www.magsys.co.uk/comcap/callsim.zip.  Note the file
is not indexed on the ComCap web pages.  The Plessey Call Simulator
application creates CDRs for three types of large switch (BTS 7#2, iSDX,
Ericsson), outputting data to a serial port.  The volume and type of
simulated calls may be specified, for a wide range of test purposes.  A
null modem cable will be needed to feed the ComCap port.  It can be used
on the same PC as ComCap, but both COM ports will be needed.


Uninstalling
------------

ComCap may be removed from the Control Panel, Add/Remove Programs, or by
running the program UNINSTAL.EXE in the installation directory.  The
uninstaller will remove all installed programs and files, and all
registry.  It will not remove any capture or log files that ComCap has
created.

Uninstalling ComCap should remove the service version from the NT database
automatically.  If it only the interactive version is required, the
service may be removed manually by typing COMCAPSRV.EXE -UNINSTALL from a
command prompt.


Release History
---------------

This is now in the help file.


Ordering ComCap
---------------

Until registered, ComCap will only run for 15 minutes before capture
is automatically stopped.  It will be necessary to restart ComCap to
continue capture.  ComCap may be registered using a secure order
form at the web site, http://www.magsys.co.uk/comcap/.  Once the order
has been processed, a small file 'userreg.txt' is returned by email,
which should be copied into the ComCap directory.  If ComCap is
already running, it should be exited and restarted to see the new
file.  When started, ComCap will show the name of the individual or
company that registered the software and will run continually.


Distribution
------------

ComCap may be freely distributed via web pages, FTP sites, BBS and
conferencing systems or on CD-ROM in unaltered zip format, but no
charge may be made other than reasonable media or bandwidth cost.  Any
notifications must state that ComCap is shareware until registered
with Magenta Systems Ltd.  Please email Magenta Systems Ltd if you
distribute ComCap in some way, so you can be notified of upgrades or
other important changes.


Copyright Information
---------------------

Copyright Magenta Systems Ltd, England, 2002.

Magenta Systems Ltd
9 Vincent Road
Croydon
CR0 6ED
United Kingdom

Phone 020 8656 3636, International Phone +44 20 8656 3636
Fax 020 8656 8127, International Fax +44 20 8656 8127

Email: comcap@magsys.co.uk
Web: http://www.magsys.co.uk/comcap/
Download: http://www.magsys.co.uk/comcap/comcap.zip

There is also a support conference on the CIX conferencing system,
cix:magsoft.  Information on joining CIX may be found at
http://www.cix.co.uk/ or http://www.conferencing.co.uk


