*****************************************************
               Kagayaki III 
             IZANAI for TEMMA-PC,PCJr Control
*****************************************************
Kagayaki III(R) Copyright(C) 1998-2001 by SeedsBox All rights reserved.
Navigation Edition 2001.4/30

http://www.now21.com/kagayaki/


!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
This manual is made by machine translation.
Grammar can be wrong.
Please forgive me.
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!


-- !!!!! attention !!!!! (Even if an obstacle occurs in machine parts and the human body, I do not bear responsibility)
  - Do not look at the sun directly by telescope, and there is absolutely danger of loss of eyesight.
    Please make all possible measures for safe security when observing the sun.

  - Pay attention so that a gear box,telescope body, and e.t.c does not hit tripods or another thing.

  - Check a gear,clutch beforehand.

  - Communication rate is slow.
    If you need emergency stop,control by hand controler or telescope switch.

  - Star party function. It is remote control. Please keep safety.

  - Keep safety in various phenomena.


-- About IZANAI for TEMMA-PC
  - You do not have to do pole axis setting.
    - You cannot see the polestar in order to observe it on a veranda...
    - Observing is disturbed in by a building...
    - You are weak in pole axial setting...
    - e.t.c...


-- Preparations before setting.
  - Use the low magnification eyepeace.
  - Set focus beforehand.
  - Set a finder beforehand.
    !! Future operation will become comfortable if you will do these three preparations.

  - Connect a TEMMA-PC,PCJr(After this, it is called TEMMA) to PC.

  - Set a pole axis toward the north(if the southern hemisphere,toword the south).
    !! This setting does not have to be correct.

  - Power on.


-- Setting
  1.[Setting]button -> [Telescope]button. Telescope setting window will open.
    Choose "IZANAI for TEMMA-PC".
    Select port[COM1]-[COM4] which is not using.
    Click [ Connect ]button.

  2.Click [GoTo]button(in main screen). Goto window will open.

  3.Click [Setting]button.(in [e.t.c]menu in goto window).
    !! After this, obey instructions of a screen

  4.fix a telescope toward the zenith.
    !! Set telescope west position(if the southern hemisphere,too).

  5.Push [OK]button. (Time, Location and zenith setting will complete).

  !! After this, do not loose clamp.

  6.Slew telescope to a star of zenith neighborhood into the field center by hand box.

  7.Click [OK]button.

  8.Slew a telescope position 180 degrees , and catch the same star in the field of vision center.
    !! Use the hand box.

  9.Click [OK]button.

  !! Setting of mounting is complete. Click [OK]button.
     Next operation is standard star setting.

  1.Choose a star on the screen.(After close the goto window).

  2.Slew telescope to a same star into the field center by hand box.

  3.Click [Std Star]button. Standard star window will open.
    Push [Add]button. 1st std star is set.

  4.Choose another star on the screen which is far from the first star.(After close the goto window).

  5.[GoTo]button(in main screen) -> [ Goto ]button(in goto screen). 
    Your telescope slew to the star that was chosen.
    The result is not correct.
    Move a star to the center of a field with hand box's arrow buttons.

  6.Click [Std Star]button. Standard star window will open.
    Push [Add]button. 2nd std star is set.

  !! 2 standard star is set. Auto navigation became possible.
  !! If you wish more correct navigation, Do the same operation. 3rd standard star will be added.


-- Operations
  - Choose the object from search grid or atlas(right click), what you wont to see.

  - Click [Goto]button on main screen. "Goto"window will open. And click [  Goto  ]button. Slewing will start.

  - When you need stop slewing, click[ Stop ]button.

  - [HS],[NS]button(in [e.t.c]menu in goto window) can change speed.

  - [12V],[24V]button(in [e.t.c]menu in goto window) can follow power supplier.

  - Click [ ----- ]button...
　　　[ -----  ] Even if a telescope mark moves, star atlas does not scroll.
　　　[ Follow ] When a telescope mark comes off from a screen, star atlas scrolls.
　　　[ Center ] Star atlas is scrolled to always keep a telescope mark the center.


-- Observation finish
  - [Setting] -> [Telescope] button. Telescope setting window will open.
    Click [ Disconnect ]button.


-- e.t.c.
  - Use the low magnification eyepeace.

  - In spite of state that a telescope stops, an indicator(ooooo) lights occasionally.
    When an observational error of coordinate data was detected as movement, it occurs.
    There is not a problem.

  - There is the case that a state in "Goto" does not end occasionally.
    In this case, push a [ Stop ]button and then return for a while.

