*****************************************************
               Kagayaki III 
             SKY SENSOR 2000 PC Control
*****************************************************
Kagayaki III(R) Copyright(C) 1998-2001 by SeedsBox All rights reserved.
Navigation Edition 2001.4/30

http://www.now21.com/kagayaki/


!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
This manual is made by machine translation.
Grammar can be wrong.
Please forgive me.
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!


-- !!!!! attention !!!!! (Even if an obstacle occurs in machine parts and the human body, I do not bear responsibility)
  - Do not look at the sun directly by telescope, and there is absolutely danger of loss of eyesight.
    Please make all possible measures for safe security when observing the sun.

  - Pay attention so that a gear box,telescope body, and e.t.c does not hit tripods or another thing.

  - Check a gear,clutch beforehand.

  - Communication rate is slow.
    If you need emergency stop,control by hand controler or telescope switch.

  - Star party function. It is remote control. Please keep safety.

  - Keep safety in various phenomena.


-- Preparations before setting.
  - Use the low magnification eyepeace.
  - Set focus beforehand.
  - Set a finder beforehand.
    !! Future operation will become comfortable if you will do these three preparations.

  - Connect a SKY SENSOR 2000 PC(After this, it is called 2000PC) to PC.

  - Set a pole axis toward the north(if the southern hemisphere,toword the south).
    !! This setting does not have to be correct.

  - Power on.

  - Slew a telescope to the west(if the southern hemisphere,toword the east).
    (According to a 2000PC's manual.)


-- Setting
  - [Setting]button -> [Telescope]button. Telescope setting window will open.
    Choose "SKY SENSOR 2000 PC".
    Select port[COM1]-[COM4] which is not using.
    Click [ Connect ]button.

  - [GoTo]button(in main screen).

  - [Time&Location]button(in [e.t.c]menu in goto window).
    Telescope is set location and time.

  !! After this, do not loose clamp.

  - Choose a star on the screen.(After close the goto window).

  - [GoTo]button(in main screen) -> [ Goto ]button(in goto screen). 
    Your telescope slew to the star that was chosen. The result is not correct.

  - Move a star to the center of a field with 2000PC's arrow buttons.

  - [Synchronize]button(in [e.t.c]menu).

  - Choose another star on the screen which is far from the first star.(After close the goto window).

  - Do the same operation.

  !! 2 standard star is set. Auto navigation became possible.
  !! If you wish more correct navigation, Do the same operation. 3rd standard star will be added.


-- Operations

  - Choose the object from search grid or atlas(right click), what you wont to see.

  - Click [Goto]button on main screen. "Goto"window will open. And click [  Goto  ]button. Slewing will start.

  - When you need stop slewing, click[ Stop ]button.

  - [Hi],[Mid],[Lo]button(in [e.t.c]menu in goto window) can change speed.

  - Click [ ----- ]button...
　　　[ -----  ] Even if a telescope mark moves, star atlas does not scroll.
　　　[ Follow ] When a telescope mark comes off from a screen, star atlas scrolls.
　　　[ Center ] Star atlas is scrolled to always keep a telescope mark the center.


-- Observation finish
  - [Setting] -> [Telescope] button. Telescope setting window will open.
    Click [ Disconnect ]button.


-- e.t.c.
  - Use the low magnification eyepeace.

  - In spite of state that a telescope stops, an indicator(ooooo) lights occasionally.
    When an observational error of coordinate data was detected as movement, it occurs.
    There is not a problem.

  - There is the case that a state in "Goto" does not end occasionally.
    In this case, push a [ Stop ]button and then return for a while.



