*****************************************************
               Kagayaki III 
             IZANAI for SKY SENSOR 3D PC Control
*****************************************************
Kagayaki III(R) Copyright(C) 1998-2001 by SeedsBox All rights reserved.
Navigation Edition 2001.4/30

http://www.now21.com/kagayaki/


!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
This manual is made by machine translation.
Grammar can be wrong.
Please forgive me.
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!


-- !!!!! attention !!!!! (Even if an obstacle occurs in machine parts and the human body, I do not bear responsibility)
  - Do not look at the sun directly by telescope, and there is absolutely danger of loss of eyesight.
    Please make all possible measures for safe security when observing the sun.

  - Pay attention so that a gear box,telescope body, and e.t.c does not hit tripods or another thing.

  - Check a gear,clutch beforehand.

  - Communication rate is slow.
    If you need emergency stop,control by hand controler or telescope switch.

  - Star party function. It is remote control. Please keep safety.

  - Keep safety in various phenomena.


-- About IZANAI for SKY SENSOR 3D
  - You do not have to do pole axis setting.
    - You cannot see the polestar in order to observe it on a veranda...
    - Observing is disturbed in by a building...
    - You are weak in pole axial setting...
    - e.t.c...


-- Preparations before setting.
  - Use the low magnification eyepeace.
  - Set focus beforehand.
  - Set a finder beforehand.
    !! Future operation will become comfortable if you will do these three preparations.

  - If a declination setting circles of your telescope is movable(GP, e.t.c), set it precisely beforehand.

  - Connect a SKY SENSOR 3D(After this, it is called 3D) to PC.

  - Set a pole axis toward the north(if the southern hemisphere,toword the south).
    !! This setting does not have to be correct.

  - Power on.


-- Setting
  - Push [I]button on the 3D's panel.
    A button of a 3D's panel will not work.

  - [Setting]button -> [Telescope]button. Telescope setting window will open.
    Choose "IZANAI for SKYSENSOR 3D".
    Select port[COM1]-[COM4] which is not using.
    Click [ Connect ]button.

  - [GoTo]button(in main screen). "Goto" window will open.

  - If your telescope is with encoder, click [With Encoder]button(in [e.t.c]menu in goto window).

  - Click [Setting]button(in [e.t.c]menu in goto window).
    !! After this, obey instructions of a screen

  - Slew a telescope toward the west.
    Match declination setting circles with zero degree "precisely".
    Right ascension setting does not have to be correct.
    Even if you loose clamp and turn it by hand, there is not a problem.

  - Click [OK]button. (Time and location is set).

  !! If your telescope does not have encoder,never loose clamp after now.

  - Choose a star on the screen.(After close the goto window).

  - Slew telescope to a same star into the field center by 3D's control panel.
    !! Click [I Command]button, 3D's control panel will be workable.

  - Click [Std Star]button. Standard star window will open.
    Push [Add]button. 1st std star is set.

  - Choose another star on the screen which is far from the first star.(After close the goto window).

  - [GoTo]button(in main screen) -> [ Goto ]button(in goto screen). 
    Your telescope slew to the star that was chosen.
    The result is not correct.
    Move a star to the center of a field with 3D's control panel.
    !! Click [I Command]button, 3D's control panel will be workable.

  - Click [Std Star]button. Standard star window will open.
    Push [Add]button. 2nd std star is set.

  !! 2 standard star is set. Auto navigation became possible.
  !! If you wish more correct navigation, Do the same operation. 3rd standard star will be added.


-- Operations

  - Choose the object from search grid or atlas(right click), what you wont to see.

  - Click [Goto]button on main screen. "Goto"window will open. And click [  Goto  ]button. Slewing will start.
    (When slewing over the meridian, it takes long time.)

  - When you need stop slewing, click[ Stop ]button.

  - If you need use the 3D's panel,click[I Commnad]button(in [e.t.c]menu in goto window).

  - Click [ ----- ]button...
　　　[ -----  ] Even if a telescope mark moves, star atlas does not scroll.
　　　[ Follow ] When a telescope mark comes off from a screen, star atlas scrolls.
　　　[ Center ] Star atlas is scrolled to always keep a telescope mark the center.

  - Arrow buttons on the screen are not effective.


-- Observation finish
  - [Setting] -> [Telescope] button. Telescope setting window will open.
    Click [ Disconnect ]button.


-- e.t.c.

  -As for 3D, speed of communication is slow. 
   !! In case of emergency, power off 3D.

  - Use the low magnification eyepeace.

  - In spite of state that a telescope stops, an indicator(ooooo) lights occasionally.
    When an observational error of coordinate data was detected as movement, it occurs.
    There is not a problem.

  - There is the case that a state in "Goto" does not end occasionally.
    In this case, click a [ Stop ]button and then return for a while.

  - 180 degrees turn over right ascension.
    This hardly occurs.
    As for this phenomenon, a cause is indistinct.


