Quick Navigation
| Background
| System Summary
| Motherboard
| Processor
| BIOS
| PCI/AGP Devices
| Memory Modules
| Memory (SMBIOS)
| Disk
| ATAPI
| Storage (ASPI)
| Logical Drives
| USB Devices
| Printers
| Slots (SMBIOS)
| Ports (SMBIOS)
| Network
| Monitor
| Video
| Hardware Monitoring
| Diagnostics
| Software
Background
| Background
| Version | ASTRA32 v.3.81
| URL | www.astra32.com
| Network Name | A2KKV
| User Name | KKV1
| Report Date | December 23, 2020
| Report Time | 14:45:09
| OS Version | MS Windows 7 Professional x64 Edition (6.1.7601 Service Pack 1)
| Registered To | Sysinfo Lab
| License Type | Professional for 1 computer
| Command Line | /LL lang\a32en.lng /RTJXHCE examples\astra32
| Disabled Tests | UDMA
System Summary
| Processor
| Processor | Intel Xeon E3-1246 v3 3500 MHz
| CPU Clock | 3491.9 MHz (35.0 x 99.8 MHz)
| Level 1 Cache | 4 x 32 kB + 4 x 32 kB (data+instr.)
| Level 2 Cache | 4 x 256 kB
| Level 3 Cache | 1 x 8 MB
| Motherboard
| System Name | Gigabyte Technology Co., Ltd. B85M-D3V-A
| Board Model | Gigabyte Technology Co., Ltd. B85M-D3V-A
| BIOS Version | AMI BIOS 08.00.10
| Chipset Name | Intel B85 (Lynx Point)
| Northbridge Vendor | Intel Corporation
| Northbridge | Xeon E3-1200 v3 Processor DRAM Controller
| Southbridge Vendor | Intel Corporation
| Southbridge | B85 Express LPC Controller
| DMI/SMBIOS Version | 2.7
| Memory
| Memory Size | 15.97 GB
| System Memory | 16350 MB
| Memory Module | 8 GB DDR3-1866 (PC3-14900) SDRAM (Kllisre)
| Memory Module | 8 GB DDR3-1866 (PC3-14900) SDRAM (Kingston)
| Storage
| Disk Model | SPCC Solid State Disk
| Disk Size | 114473 MB (111.79 GB)
| Disk Model | WDC WD1001FALS-00J7B0
| Disk Size | 953869 MB (931.51 GB)
| Disk Model | Samsung SSD 860 EVO 250GB
| Disk Size | 238475 MB (232.89 GB)
| Disk Model | ST3500412AS
| Disk Size | 476940 MB (465.76 GB)
| CD/DVD Model | PIONEER DVD-RW DVR-217F
| CD/DVD Speed | 16x (Write: 40x)
| Video
| Monitor Vendor | BenQ
| Monitor Model | BenQ GW2470
| Video Chip Vendor | Nvidia Corp
| Video Chip | GP104 [GeForce GTX 1070]
| Video Memory Size | 8 GB GDDR5 (Micron)
| Sound
| Sound Chip Vendor | Intel Corporation
| Sound Chip | 8 Series/C220 Series Chipset Family HD Audio Controller
| Sound Chip Vendor | Nvidia Corp
| Sound Chip | GP104 High Definition Audio Controller
| AC'97/HDA Codec Name | NVidia GPU GP104 HDMI/DP
| Sound Chip Vendor | VIA Technologies Inc (Was: IC Ensemble Inc)
| Sound Chip | VT1720/4 Envy24PT PCI Multi-Channel Audio Controller
| Printer
| Printer Vendor | Canon
| Printer Model | LaserBase MF3110 Scanner/Printer
| Operating System
| Operating System | MS Windows 7 Professional x64 Edition (6.1.7601 Service Pack 1)
| Windows Folder | G:\Windows
| Modem
| Modem Vendor | Intel Corporation
| Modem Model | 8 Series/C220 Series Chipset Family MEI Controller #1
| Network
| Network Name | A2KKV
| Adapter Vendor | Realtek Semiconductor
| Adapter Name | RTL8111/8168/8411 PCI Express Gigabit Ethernet Controller
| Interface Description | Realtek PCIe GbE Family Controller
| MAC Address | 1C-1B-0D-B1-81-06
| Interface Description | VirtualBox Host-Only Ethernet Adapter
| MAC Address | 0A-00-27-00-00-10
| Ports
| LPT Ports | LPT1(0378h)
| COM Ports | COM1(03F8h)
Motherboard
| System
| System Vendor | Gigabyte Technology Co., Ltd.
| Product Name | B85M-D3V-A
| Version | To be filled by O.E.M.
| Serial Number | To be filled by O.E.M.
| UUID | 1C021B030D04B1058106060700080009
| Wake-up Type | Power Switch
| SKU Number | To be filled by O.E.M.
| Family | To be filled by O.E.M.
| Motherboard
| Motherboard Vendor | Unknown (0001)
| Vendor URL | Unknown
| Board Model | Gigabyte Technology Co., Ltd. B85M-D3V-A
| Version | x.x
| Serial Number | To be filled by O.E.M.
| Asset Tag | To be filled by O.E.M.
| BIOS Version | AMI BIOS 08.00.10
| BIOS Date | 04/13/12
| Chipset Name | Intel B85 (Lynx Point)
| Northbridge Vendor | Intel Corporation
| Northbridge | Xeon E3-1200 v3 Processor DRAM Controller
| Southbridge Vendor | Intel Corporation
| Southbridge | B85 Express LPC Controller
| Onboard Device 1
| Description | To Be Filled By O.E.M.
| Device Type | Video
| Status | Enabled
| Onboard Device 2
| Description | Onboard LAN
| Device Type | Ethernet
| Status | Enabled
| Configuration Options
| To Be Filled By O.E.M.
| System Enclosure
| Manufacturer | Gigabyte Technology Co., Ltd.
| Type | Desktop
| Version | To Be Filled By O.E.M.
| Serial Number | To Be Filled By O.E.M.
| Asset Tag | To Be Filled By O.E.M.
| Boot-up State | Safe
| Power Supply State | Safe
| Thermal State | Safe
| Security Status | None
| OEM-defined | 00000000h
| Height | 0.0 sm
| Power Cords | 1
| Contained Element | 0
CPU
| CPU
| Processor | Intel Xeon E3-1246 v3 3500 MHz
| Coprocessor | Internal
| CPU Clock | 3491.9 MHz
| Level 1 Cache | 4 x 32 kB + 4 x 32 kB (data+instr.)
| Level 2 Cache | 4 x 256 kB
| Level 3 Cache | 1 x 8 MB
| Code Name | Haswell-WS
| Manufacturing Process | 22 nm
| FSB Clock | 99.8 MHz
| Multiplier | 35.0
| Expected Clock | 3500 MHz
| Overclocking Support | Not Supported
| Max Turbo Clock | 3900.0 MHz
| Turbo Boost | 2/3/4/4 (Enabled)
| Turbo Clock (1-2 core) | 3900 MHz
| Turbo Clock (3 core) | 3800 MHz
| Turbo Clock (4 core) | 3700 MHz
| Socket Type | Socket 1150 FCLGA
| Package Temperature | 39 °C (102 °F)
| Temperature Core 1 | 38 °C (100 °F)
| Temperature Core 2 | 36 °C (97 °F)
| Temperature Core 3 | 36 °C (97 °F)
| Temperature Core 4 | 38 °C (100 °F)
| Maximum Temperature (Tjmax) | 100 °C (212 °F)
| Core Voltage | 1.096 V
| Vendor | GenuineIntel
| Processor Name | Intel(R) Xeon(R) CPU E3-1246 v3 @ 3.50GHz
| Processor Type | Original OEM Processor
| CPUID | Family: 6, Model: 12, Stepping: 3
| Ext. Family/Model | Family: -, Model: 3
| CPU Signature | 000306C3h
| Number of Cores | 4
| Logical Cores Count | 8
| Core Stepping | C-0
| sSpec Number | SR1QZ
| Microcode Revision | 1Ch
| Max TDP | 84 Wattes
| Power Limit 1 (Time) | 84.0 Wattes (Unlimited)
| Power Limit 2 (Time) | 105.0 Wattes (Unlimited)
| Internal Graphics | Intel HD Graphics (Disabled)
| Transistor Count | 1400 million
| Die Size | 177 mm2
| Launch Date | May, 2014
| Recommended Price (USD) | $276
| Instruction Set
| Floating-Point Unit On-Chip | Supported
| IA MMX Technology | Supported
| SSE Instruction Set | Supported
| SSE2 Instruction Set | Supported
| SSE3 Instruction Set | Supported
| Supplemental SSE3 Instruction Set | Supported
| SSE4.1 Instruction Set | Supported
| SSE4.2 Instruction Set | Supported
| Advanced Vector Extensions (AVX) | Supported
| Advanced Vector Extensions 2 (AVX2) | Supported
| AVX-512 Foundation Instructions | Not Supported
| AVX-512 Prefetch Instructions | Not Supported
| AVX-512 Exponential and Reciprocal | Not Supported
| AVX-512 Conflict Detection | Not Supported
| AVX-512 Byte and Word Instructions | Not Supported
| AVX-512 Doubleword and Quadword | Not Supported
| AVX-512 Vector Length Extensions | Not Supported
| AVX-512 Integer Fused Multiply-Add | Not Supported
| AVX-512 Vector Bit Manipulation | Not Supported
| AVX-512 QVNNI Instructions | Not Supported
| AVX-512 QFMA Instructions | Not Supported
| AVX-512 VBMI2 Instructions | Not Supported
| AVX-512 VNNI Instructions | Not Supported
| AVX-512 BITALG Instructions | Not Supported
| Galois Field NI/Affine Transformation | Not Supported
| VEX-encoded AES-NI (VAES) | Not Supported
| VEX-encoded PCLMUL (VPCL) | Not Supported
| PCOMMIT Instruction | Not Supported
| CLWB Instruction | Not Supported
| PREFETCHWT1 Instruction | Not Supported
| Software Guard Extensions (SGX) | Not Supported
| SGX Launch Configuration | Not Supported
| FMA Instructions Set | Supported
| AES Instructions Set | Supported
| Intel Extended Memory 64 Tech. | Supported
| Intel Architecture - 64 (IA-64) | Not Supported
| AMD MMX Instruction Extensions | Not Supported
| AMD 3DNow! Instructions | Not Supported
| AMD 3DNow! Extensions | Not Supported
| AMD 3DNow! Prefetch | Not Supported
| AMD SSE4A Extensions | Not Supported
| AMD eXtended OPeration (XOP) | Not Supported
| AMD Misaligned SSE | Not Supported
| AMD64 Architecture | Not Supported
| Cyrix Extended MMX | Not Supported
| CMPXCHG8 Instruction Supported | Supported
| CMPXCHG16 Instruction Supported | Supported
| Fast System Call | Supported
| Conditional Move Instruction | Supported
| CLFLUSH Insruction Supported | Supported
| Fast Save and Restore | Supported
| Monitor/MWAIT Instructions | Supported
| SYSCALL/SYSRET Instructions | Not Supported
| LAHF/SAHF Instructions | Supported
| POPCNT Insruction Supported | Supported
| XSAVE Insructions Supported | Supported
| OS Supports XSAVE Instructions | Supported
| PCLMULQDQ Instruction Supported | Supported
| MOVBE Insruction Supported | Supported
| F16C Insruction Supported | Supported
| RDTSCP Insruction Supported | Supported
| RDRAND Insruction Supported | Supported
| (RD/WR)(FS/GS) BASE Instructions | Supported
| Bit Manipulation 1 Instructions | Supported
| Bit Manipulation 1 Instructions | Supported
| Enhanced REP MOVSB/STOSB | Supported
| INVPCID Instruction | Supported
| XSAVEOPT Instruction | Supported
| RDSEED Instruction | Not Supported
| ADCX/ADOX Instructions | Not Supported
| CLAC/STAC Instructions | Not Supported
| SCLFLUSHOPT Instruction | Not Supported
| RDPID Instruction | Not Supported
| VPOPCNT[D/Q] Instructions | Not Supported
| Fast Short REP MOV Instruction | Not Supported
| PCONFIG Instruction | Not Supported
| WBNOINVD Instruction | Not Supported
| WaitPKG Instructions | Not Supported
| CLDEMOTE Instruction | Not Supported
| MOVDIRI Instruction | Not Supported
| MOVDIRI64B Instruction | Not Supported
| RDPRU Instruction | Not Supported
| MCOMMIT Instruction | Not Supported
| AMD Fast Save and Restore | Not Supported
| AMD SKINIT, STGI, DEV Supported | Not Supported
| AMD Light Weight Profiling (LWP) | Not Supported
| AMD FMA4 Insruction Supported | Not Supported
| AMD TBM Insruction Supported | Not Supported
| AMD MONITORX/MWAITX Instructions | Not Supported
| AMD CLZERO Instruction | Not Supported
| Processor Features
| Hypervisor Present | Not Supported
| Virtual Mode Extension | Supported
| Debugging Extension | Supported
| Page Size Extension | Supported
| Time Stamp Counter | Supported
| Model Specific Registers | Supported
| Physical Address Extension | Supported
| Machine Check Exception | Supported
| On-chip APIC Hardware Supported | Supported
| Memory Type Range Registers | Supported
| Page Global Enable | Supported
| Machine Check Architecture | Supported
| Page Attribute Table | Supported
| 36-bit Page Size Extension | Supported
| Processor Serial Number | Not Supported
| Debug Store | Supported
| 64-bit Debug Store | Supported
| Self-Snoop | Supported
| Hyper-Threading Technology | Supported
| Pending Break Enable | Supported
| CPL-Qualified Debug Store | Supported
| L1 Context ID | Not Supported
| Send Task Priority Messages | Supported
| Direct Cache Access | Not Supported
| Performance Capabilities MSR | Supported
| x2APIC Architecture | Supported
| Advanced Bit Manipulation | Supported
| OS Visible Workaround | Not Supported
| Instruction Based Sampling | Not Supported
| 1-GB Large Page | Supported
| Process Context Identifiers | Supported
| Time Stamp Counter Deadline | Supported
| Time Stamp Counter Adjust | Supported
| Intel Virtualization Technology | Supported
| Intel Trusted Execution Technology | Supported
| Supervisor Mode Execution Protection | Supported
| Hardware Lock Elision | Not Supported
| Restricted Transactional Memory | Not Supported
| Quality of Service Monitoring | Not Supported
| Quality of Service Enforcement | Not Supported
| Deprecated FPU CS and FPU DS | Supported
| Memory Protection Extensions (MPX) | Not Supported
| Processor Trace (PT) | Not Supported
| Secure Hash Algorithm Ext. (SHA) | Not Supported
| Debug Interface MSR | Supported
| User-Mode Instruction Prevention | Not Supported
| Protection Keys for User-Mode Pages | Not Supported
| 5 Level Page Table | Not Supported
| Total Memory Encryption (TME) | Not Supported
| Speculation Control (IBRS and IBPB) | Not Supported
| Single Thread Indirect Branch Predictors | Not Supported
| L1 Data Cache (L1D) Flush | Not Supported
| ARCH_CAPABILITIES MSR | Not Supported
| Speculative Store Bypass Disable (SSBD) | Not Supported
| Intel Turbo Boost Technology | Supported, Enabled
| Intel Turbo Boost Max Technology 3.0 | Not Supported
| Intel Execute Disable Bit | Supported
| Hybrid Processor | Not Supported
| AMD Secure Virtual Machine | Not Supported
| AMD Model-Specific Registers | Not Supported
| AMD Multiprocessing Capable | Not Supported
| AMD CMP Legacy Mode | Not Supported
| AMD CR8 in Legacy Mode | Not Supported
| AMD Ext. APIC Register Space | Not Supported
| AMD Watchdog Timer | Not Supported
| AMD Translation Cache Extension | Not Supported
| AMD Topology Extensions | Not Supported
| AMD Core Performance Counter Ext. | Not Supported
| AMD NB Performance Counter Ext. | Not Supported
| AMD Streaming Performance Monitor | Not Supported
| AMD Data Breakpoint Extension | Not Supported
| AMD Performance TSC | Not Supported
| AMD L2I Performance Counter Ext. | Not Supported
| AMD IRPERF Performance Counter | Not Supported
| AMD Always Save/Restore FP Error Pointers | Not Supported
| AMD Indirect Branch Prediction Barrier | Not Supported
| AMD Indirect Branch Restricted Speculation | Not Supported
| AMD IBRS Always On Mode | Not Supported
| AMD IBRS Preferred | Not Supported
| AMD Single Thread Indirect Branch Predictor | Not Supported
| AMD STIBP Always On Mode | Not Supported
| AMD Speculative Store Bypass Disable (SSBD) | Not Supported
| AMD SSBD Not Needed | Not Supported
| AMD VIRT_SPEC_CTRL MSR | Not Supported
| Power Management
| ACPI Supported | Supported
| Thermal Monitor Supported | Supported
| Thermal Monitor 2 | Supported
| Enhanced SpeedStep Technology | Supported
| Digital Thermal Sensor | Supported
| Always Running APIC Timer | Supported
| Invariant TSC | Supported
| Power Limit Notification | Supported
| Extended Clock Modulation Duty | Supported
| Package Thermal Management | Supported
| Hardware Coordination Feedback | Supported
| ACNT2 Capability | Not Supported
| Performance-Energy Bias | Not Supported
| Hardware-Managed P-State Base Support | Not Supported
| Hardware Duty Cycle Programming (HDC) | Not Supported
| AMD Temperature Sensor | Not Supported
| AMD Frequency ID Control | Not Supported
| AMD Voltage ID Control | Not Supported
| AMD Thermal Trip | Not Supported
| AMD Thermal Monitoring | Not Supported
| AMD Software Thermal Control | Not Supported
| AMD 100MHz Multiplier Steps | Not Supported
| AMD Hardware P-State Control | Not Supported
| AMD Effective Frequency Interface | Not Supported
| AMD Processor Feedback Interface | Not Supported
| AMD Processor Accumulator | Not Supported
| AMD Connected Standby | Not Supported
| AMD Running Average Power Limit | Not Supported
| AMD MCA Overflow Recovery | Not Supported
| AMD Software Uncorr. Error Containment/Recovery | Not Supported
| AMD Hardware Assert (HWA) | Not Supported
| AMD Scalable MCA | Not Supported
CPU Cache
| Level 1 Instruction Cache
| Size | 4 x 32 kB
| Associativity | 8-way
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 64
| Associativity | 8-way
| TLB 2/4M Pages |
| Number of Entries | 8
| Associativity | full
| Level 1 Data Cache
| Size | 4 x 32 kB
| Associativity | 8-way
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 1024
| Associativity | 8-way
| TLB 2/4M Pages |
| Number of Entries | 1024
| Associativity | 8-way
| Level 2 Cache
| Size | 4 x 256 kB
| Associativity | 8-way
| Line Size | 64 byte
| Level 3 Cache
| Size | 1 x 8 MB
| Associativity | 16-way
| Line Size | 64 byte
CPU (SMBIOS)
| Processor
| Processor Vendor | Intel
| Processor Version | Intel(R) Xeon(R) CPU E3-1246 v3 @ 3.50GHz
| Current Speed | 3700 MHz
| External Clock | 100 MHz
| Voltage | 1.0 V
| Processor Upgrade | Other
| Processor Status | CPU Enabled
| Socket Designation | SOCKET 0
| Processor Type | Central Processor
| Processor Family | Intel Xeon
| Processor ID1 | 000306C3h
| Processor ID2 | BFEBFBFFh
| Max Speed | 7000 MHz
| Socket Status | CPU Socket Populated
| Serial Number |
| Asset Tag | Fill By OEM
| Part Number | Fill By OEM
| CPU Core Count | 4 (Enabled: 1)
| CPU Thread Count | 2
| Structure Length | 2Ah
CPU (SMBIOS) Cache
| Level 1 Cache
| Installed Size | 256 kB
| Operational Mode | Write Back
| Current SRAM Type | Unknown
| Status | Enabled
| Socket Designation | CPU Internal L1
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 256 kB
| Supported SRAM Type | Unknown
| Cache Speed | Unknown
| Error Correction | Single-bit ECC
| System Cache Type | Other
| Associativity | 8-way Set-Associative
| Structure Length | 13h
| Level 2 Cache
| Installed Size | 1 MB
| Operational Mode | Write Back
| Current SRAM Type | Unknown
| Status | Enabled
| Socket Designation | CPU Internal L2
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 1 MB
| Supported SRAM Type | Unknown
| Cache Speed | Unknown
| Error Correction | Single-bit ECC
| System Cache Type | Unified
| Associativity | 8-way Set-Associative
| Structure Length | 13h
| Level 3 Cache
| Installed Size | 8 MB
| Operational Mode | Write Back
| Current SRAM Type | Unknown
| Status | Enabled
| Socket Designation | CPU Internal L3
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 8 MB
| Supported SRAM Type | Unknown
| Cache Speed | Unknown
| Error Correction | Single-bit ECC
| System Cache Type | Unified
| Associativity | 16-way Set-Associative
| Structure Length | 13h
BIOS
| BIOS
| Motherboard Vendor | Unknown (0001)
| Vendor URL | Unknown
| BIOS Version | AMI BIOS 08.00.10
| BIOS Date | 04/13/12
| BIOS Copyright | 04/13/12(C)2010 American Megatrends, Inc. All Rights Reserved
| Motherboard ID | BIOS Date: 08/24/16 16:14:27 Ver: 04.06.05
| BIOS ID | 63-0100-000001-00101111-041312-Chipset
| BIOS Size | 512 kB
| Processor | 686
| Chipset ID | Chipset
| BIOS Revision | 0100
| MP Specification Ver. | 1.4
| MP Table Address | 000Fh:D450h
| Number of CPU/Cores | 4
| DMI/SMBIOS Version | 2.7
| DMI/SMBIOS Structures | 77
| SMBIOS
| BIOS Vendor | American Megatrends Inc.
| BIOS Version | F4a
| BIOS Date | 08/24/2016
| BIOS ROM Size | 4 MB
| System BIOS Version | 4.6
| Starting Segment | F000h
| Current Language | en|US|iso8859-1
| Number of Languages | 4
| Structure Length | 18h
| Bus Supported
| PCI is Supported | Supported
| AGP is Supported | Not Supported
| USB is Supported | Supported
| ISA is Supported | Not Supported
| VLBus is Supported | Not Supported
| MCA is Supported | Not Supported
| EISA is Supported | Not Supported
| PC Card is Supported | Not Supported
| Boot Options
| Selectable Boot | Supported
| Boot From CD | Supported
| ATAPI ZIP Drive Boot | Not Supported
| LS-120 Boot | Not Supported
| BIOS Boot Specification | Supported
| Boot From PC Card | Not Supported
| Network Service Boot Supported | Not Supported
| I2O Boot | Not Supported
| 1394 Boot | Not Supported
| BIOS Features
| BIOS Characteristics | Supported
| ACPI Supported | Supported
| PnP is Supported | Not Supported
| APM is Supported | Not Supported
| ESCD Support | Not Supported
| Enhanced Disk Drive (EDD) | Supported
| BIOS is Upgradeable (Flash) | Supported
| BIOS ROM is Socketed | Supported
| BIOS Shadowing is Allowed | Supported
| Smart Battery Supported | Not Supported
| Targeted Content Distribution | Supported
| UEFI Specification is Supported | Supported
| Virtual Machine | Not Supported
| Int 13h - 5.25"/360kB Floppy | Not Supported
| Int 13h - 5.25"/1.2MB Floppy | Supported
| Int 13h - 3.5"/720kB Floppy | Supported
| Int 13h - 3.5"/2.88MB Floppy | Supported
| Int 5h, Print Screen Service | Supported
| Int 9h, 8042 Keyboard Services | Supported
| Int 14h, Serial Services | Supported
| Int 17h, Printer Services | Supported
| Int 10h, CGA/Mono Video Services | Not Supported
| Int 13h - Floppy for NEC 9800 | Not Supported
| Int 13h - Floppy for Toshiba | Not Supported
| NEC PC-98 | Not Supported
| OEM SMBIOS Strings
| To Be Filled By O.E.M.
| To Be Filled By O.E.M.
| To Be Filled By O.E.M.
| To Be Filled By O.E.M.
| To Be Filled By O.E.M.
| Other SMBIOS Structures
| Hardware Security (24)
| System Boot Information (32)
| Management Device (34)
| Voltage Probe (26)
| Management Device Threshold Data (36)
| Management Device Component (35)
| Temperature Probe (28)
| Management Device Threshold Data (36)
| Management Device Component (35)
| Cooling Device (27)
| Management Device Threshold Data (36)
| Management Device Component (35)
| Cooling Device (27)
| Management Device Threshold Data (36)
| Management Device Component (35)
| Electrical Current Probe (29)
| Management Device Threshold Data (36)
| Management Device Component (35)
| Voltage Probe (26)
| Temperature Probe (28)
| Cooling Device (27)
| Electrical Current Probe (29)
| System Power Supply (39)
| Memory Device Mapped Address (20)
| Memory Device Mapped Address (20)
| Memory Array Mapped Address (19)
| Unknown (136)
| Unknown (131)
PCI/AGP Devices
| Bus: 00h, Device: 00h, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (0C08h) | Xeon E3-1200 v3 Processor DRAM Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5000h) | Unknown
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 06h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 0, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24441
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_8086&DEV_0C08&SUBSYS_50001458&REV_06
| Compatible ID | PCI\VEN_8086&DEV_0C08&REV_06
| Parent ID | ACPI_HAL\PNP0C08
| Bus: 00h, Device: 01h, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (0C01h) | 4th Gen Core/Xeon E3-1200 v3 Processor PCI Express x16 Controller
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | 06h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | E000h - EFFFh
| Memory Address | F6000000h - F70FFFFFh
| Memory Address | E0000000h - F1FFFFFFh
| System IRQ | 16
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 8.0 GB/s (Current: 2.5 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 2
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard PCI-to-PCI bridge
| Device Class | System
| Device Location | PCI bus 0, device 1, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24441
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | pci
| Hardware ID | PCI\VEN_8086&DEV_0C01&SUBSYS_50001458&REV_06
| Compatible ID | PCI\VEN_8086&DEV_0C01&REV_06
| Parent ID | ACPI_HAL\PNP0C08
| Bus: 00h, Device: 14h, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C31h) | 8 Series/C220 Series Chipset Family USB xHCI Host Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5007h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 05h
| Interface | 30h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | F7200000h - F720FFFFh
| Driver
| Driver Status | The device is working properly
| Manufacturer | Intel(R) Corporation
| Device Description | Intel(R) USB 3.0 eXtensible Host Controller
| Device Class | USB
| Device Location | PCI bus 0, device 20, function 0
| Driver Provider | Intel(R) Corporation
| Driver Version | 5.0.4.43
| Driver Date | 5-11-2017
| Inf File | oem36.inf
| Service Name | iusb3xhc
| Hardware ID | PCI\VEN_8086&DEV_8C31&SUBSYS_50071458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C31&REV_05
| Parent ID | ACPI_HAL\PNP0C08
| Bus: 00h, Device: 16h, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C3Ah) | 8 Series/C220 Series Chipset Family MEI Controller #1
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (1C3Ah) | Unknown
| Class (07h) | Communication
| SubClass (80h) | Other
| Revision | 04h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | F721A000h - F721A00Fh
| System IRQ | 11
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | INTEL
| Device Description | Intel(R) 8 Series/C220 Series Management Engine Interface - 8C3A
| Device Class | System
| Device Location | PCI bus 0, device 22, function 0
| Driver Provider | INTEL
| Driver Version | 0.0.0.1
| Driver Date | 1-4-2013
| Inf File | oem34.inf
| Hardware ID | PCI\VEN_8086&DEV_8C3A&SUBSYS_1C3A1458&REV_04
| Compatible ID | PCI\VEN_8086&DEV_8C3A&REV_04
| Parent ID | ACPI_HAL\PNP0C08
| Bus: 00h, Device: 1Ah, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C2Dh) | 8 Series/C220 Series Chipset Family USB Enhanced Host Controller #2
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5006h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 05h
| Interface | 20h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | F7218000h - F72183FFh
| System IRQ | 16
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | Standard Enhanced PCI to USB Host Controller
| Device Class | USB
| Device Location | PCI bus 0, device 26, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24138
| Driver Date | 6-21-2006
| Inf File | usbport.inf
| Service Name | usbehci
| Hardware ID | PCI\VEN_8086&DEV_8C2D&SUBSYS_50061458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C2D&REV_05
| Parent ID | ACPI_HAL\PNP0C08
| Bus: 00h, Device: 1Bh, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C20h) | 8 Series/C220 Series Chipset Family HD Audio Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (A002h) | Unknown
| Class (04h) | Multimedia
| SubClass (03h) | Hi-definition Audio
| Revision | 05h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | F7210000h - F7213FFFh
| System IRQ | 22
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 1.0
| Device/Port Type | Root Complex Integrated Endpoint
| Link Speed | Unknown (0) (Current: Unknown (0))
| Link Width | x0 (Current: x0)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | High Definition Audio Controller
| Device Class | System
| Device Location | PCI bus 0, device 27, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.23403
| Driver Date | 3-25-2016
| Inf File | hdaudbus.inf
| Service Name | HDAudBus
| Hardware ID | PCI\VEN_8086&DEV_8C20&SUBSYS_A0021458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C20&REV_05
| Parent ID | ACPI_HAL\PNP0C08
| Bus: 00h, Device: 1Ch, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C10h) | 8 Series/C220 Series Chipset Family PCI Express Root Port 1
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | D5h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 16
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 5.0 GB/s (Current: 2.5 GB/s)
| Link Width | x1 (Current: x0)
| Link Port Number | 1
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard PCI-to-PCI bridge
| Device Class | System
| Device Location | PCI bus 0, device 28, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24441
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | pci
| Hardware ID | PCI\VEN_8086&DEV_8C10&SUBSYS_50011458&REV_D5
| Compatible ID | PCI\VEN_8086&DEV_8C10&REV_D5
| Parent ID | ACPI_HAL\PNP0C08
| Bus: 00h, Device: 1Ch, Function: 02h
| Vendor (8086h) | Intel Corporation
| Device (8C14h) | 8 Series/C220 Series Chipset Family PCI Express Root Port 3
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | D5h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | D000h - DFFFh
| Memory Address | F7100000h - F71FFFFFh
| Memory Address | F2100000h - F21FFFFFh
| System IRQ | 18
| Interrupt Pin | INTC#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 5.0 GB/s (Current: 2.5 GB/s)
| Link Width | x1 (Current: x1)
| Link Port Number | 3
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard PCI-to-PCI bridge
| Device Class | System
| Device Location | PCI bus 0, device 28, function 2
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24441
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | pci
| Hardware ID | PCI\VEN_8086&DEV_8C14&SUBSYS_50011458&REV_D5
| Compatible ID | PCI\VEN_8086&DEV_8C14&REV_D5
| Parent ID | ACPI_HAL\PNP0C08
| Bus: 00h, Device: 1Ch, Function: 03h
| Vendor (8086h) | Intel Corporation
| Device (244Eh) | 82801FB Hub Interface to PCI Bridge (ICH6 C0 step)
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | D5h
| Interface | 01h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | C000h - CFFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 19
| Interrupt Pin | INTD#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 5.0 GB/s (Current: 2.5 GB/s)
| Link Width | x1 (Current: x1)
| Link Port Number | 4
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Intel
| Device Description | Intel(R) 82801 PCI Bridge - 244E
| Device Class | System
| Device Location | PCI bus 4, device 0, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24441
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | pci
| Hardware ID | PCI\VEN_8086&DEV_244E&SUBSYS_88921458&REV_41
| Compatible ID | PCI\VEN_8086&DEV_244E&REV_41
| Parent ID | PCI\VEN_8086&DEV_244E&SUBSYS_50011458&REV_D5
| Bus: 00h, Device: 1Dh, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C26h) | 8 Series/C220 Series Chipset Family USB Enhanced Host Controller #1
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5006h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 05h
| Interface | 20h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | F7217000h - F72173FFh
| System IRQ | 23
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | Standard Enhanced PCI to USB Host Controller
| Device Class | USB
| Device Location | PCI bus 0, device 29, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24138
| Driver Date | 6-21-2006
| Inf File | usbport.inf
| Service Name | usbehci
| Hardware ID | PCI\VEN_8086&DEV_8C26&SUBSYS_50061458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C26&REV_05
| Parent ID | ACPI_HAL\PNP0C08
| Bus: 00h, Device: 1Fh, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C50h) | B85 Express LPC Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5001h) | Unknown
| Class (06h) | Bridge
| SubClass (01h) | PCI/ISA
| Revision | 05h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard ISA bridge
| Device Class | System
| Device Location | PCI bus 0, device 31, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24441
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | msisadrv
| Hardware ID | PCI\VEN_8086&DEV_8C50&SUBSYS_50011458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C50&REV_05
| Parent ID | ACPI_HAL\PNP0C08
| Bus: 00h, Device: 1Fh, Function: 02h
| Vendor (8086h) | Intel Corporation
| Device (8C02h) | 8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (B005h) | Unknown
| Class (01h) | Storage
| SubClass (06h) | Serial ATA
| Revision | 05h
| Interface | 01h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Base I/O Port | 0000F070h - 0000F077h
| Base I/O Port | 0000F060h - 0000F063h
| Base I/O Port | 0000F050h - 0000F057h
| Base I/O Port | 0000F040h - 0000F043h
| Base I/O Port | 0000F020h - 0000F03Fh
| Memory Address | F7216000h - F72167FFh
| System IRQ | 19
| Interrupt Pin | INTB#
| Driver
| Driver Status | The device is working properly
| Manufacturer | Standard AHCI 1.0 Serial ATA Controller
| Device Description | Standard AHCI 1.0 Serial ATA Controller
| Device Class | hdc
| Device Location | PCI bus 0, device 31, function 2
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.23403
| Driver Date | 6-21-2006
| Inf File | mshdc.inf
| Service Name | msahci
| Hardware ID | PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C02&REV_05
| Parent ID | ACPI_HAL\PNP0C08
| Bus: 00h, Device: 1Fh, Function: 03h
| Vendor (8086h) | Intel Corporation
| Device (8C22h) | 8 Series/C220 Series Chipset Family SMBus Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5001h) | Unknown
| Class (0Ch) | Serial
| SubClass (05h) | SMBus Controller
| Revision | 05h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Not Supported
| I/O Access | Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| SMBus Port | F000h
| Memory Address | F7215000h - F72150FFh
| Base I/O Port | 0000F000h - 0000F01Fh
| System IRQ | 10
| Interrupt Pin | INTC#
| Driver
| Driver Status | The device is working properly
| Manufacturer | INTEL
| Device Description | Intel(R) 8 Series/C220 Series SMBus Controller - 8C22
| Device Class | System
| Device Location | PCI bus 0, device 31, function 3
| Driver Provider | INTEL
| Driver Version | 10.1.1.45
| Driver Date | 1-2-2018
| Inf File | oem38.inf
| Hardware ID | PCI\VEN_8086&DEV_8C22&SUBSYS_50011458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C22&REV_05
| Parent ID | ACPI_HAL\PNP0C08
| Bus: 01h, Device: 00h, Function: 00h
| Vendor (10DEh) | Nvidia Corp
| Device (1B81h) | GP104 [GeForce GTX 1070]
| Subsys Vendor (10DEh) | Nvidia Corp
| Subsystem ID (119Dh) | Unknown
| Class (03h) | Display
| SubClass (00h) | VGA
| Revision | A1h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | F6000000h - F6FFFFFFh
| Memory Address | E0000000h - EFFFFFFFh
| Memory Address | F0000000h - F1FFFFFFh
| Base I/O Port | 0000E000h - 0000E07Fh
| System IRQ | 16
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 8.0 GB/s (Current: 2.5 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | NVIDIA
| Device Description | NVIDIA GeForce GTX 1070
| Device Class | Display
| Device Location | PCI bus 1, device 0, function 0
| Driver Provider | NVIDIA
| Driver Version | 26.21.14.4219
| Driver Date | 1-29-2020
| Inf File | oem15.inf
| Service Name | nvlddmkm
| Hardware ID | PCI\VEN_10DE&DEV_1B81&SUBSYS_119D10DE&REV_A1
| Compatible ID | PCI\VEN_10DE&DEV_1B81&REV_A1
| Parent ID | PCI\VEN_8086&DEV_0C01&SUBSYS_50001458&REV_06
| Bus: 01h, Device: 00h, Function: 01h
| Vendor (10DEh) | Nvidia Corp
| Device (10F0h) | GP104 High Definition Audio Controller
| Subsys Vendor (10DEh) | Nvidia Corp
| Subsystem ID (119Dh) | Unknown
| Class (04h) | Multimedia
| SubClass (03h) | Hi-definition Audio
| Revision | A1h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | F7080000h - F7083FFFh
| System IRQ | 17
| Interrupt Pin | INTB#
| AC'97/HDA Capabilities
| AC'97/HDA Codec Name | NVidia GPU GP104 HDMI/DP
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 8.0 GB/s (Current: 2.5 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | High Definition Audio Controller
| Device Class | System
| Device Location | PCI bus 1, device 0, function 1
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.23403
| Driver Date | 3-25-2016
| Inf File | hdaudbus.inf
| Service Name | HDAudBus
| Hardware ID | PCI\VEN_10DE&DEV_10F0&SUBSYS_119D10DE&REV_A1
| Compatible ID | PCI\VEN_10DE&DEV_10F0&REV_A1
| Parent ID | PCI\VEN_8086&DEV_0C01&SUBSYS_50001458&REV_06
| Bus: 03h, Device: 00h, Function: 00h
| Vendor (10ECh) | Realtek Semiconductor
| Device (8168h) | RTL8111/8168/8411 PCI Express Gigabit Ethernet Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (E000h) | GA-EP45-DS5 Motherboard
| Class (02h) | Network
| SubClass (00h) | Ethernet
| Revision | 0Ch
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | 0000D000h - 0000D0FFh
| Memory Address | F7100000h - F7100FFFh
| Memory Address | F2100000h - F2103FFFh
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 2.5 GB/s (Current: 2.5 GB/s)
| Link Width | x1 (Current: x1)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Realtek
| Device Description | Realtek PCIe GbE Family Controller
| Device Class | Net
| Device Location | PCI bus 3, device 0, function 0
| Driver Provider | Realtek
| Driver Version | 7.127.701.2019
| Driver Date | 7-1-2019
| Inf File | oem33.inf
| Service Name | RTL8167
| Hardware ID | PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_0C
| Compatible ID | PCI\VEN_10EC&DEV_8168&REV_0C
| Parent ID | PCI\VEN_8086&DEV_8C14&SUBSYS_50011458&REV_D5
| Bus: 04h, Device: 00h, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (244Eh) | 82801 Family (ICH2/3/4/5/6/7/8/9,63xxESB) Hub Interface to PCI Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | 41h
| Interface | 01h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | C000h - CFFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 19
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | Intel
| Device Description | Intel(R) 82801 PCI Bridge - 244E
| Device Class | System
| Device Location | PCI bus 0, device 28, function 3
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24441
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | pci
| Hardware ID | PCI\VEN_8086&DEV_244E&SUBSYS_50011458&REV_D5
| Compatible ID | PCI\VEN_8086&DEV_244E&REV_D5
| Parent ID | ACPI_HAL\PNP0C08
| Bus: 05h, Device: 00h, Function: 00h
| Vendor (1412h) | VIA Technologies Inc (Was: IC Ensemble Inc)
| Device (1724h) | VT1720/4 Envy24PT PCI Multi-Channel Audio Controller
| Subsys Vendor (1412h) | VIA Technologies Inc (Was: IC Ensemble Inc)
| Subsystem ID (3631h) | M-Audio Revolution 5.1
| Class (04h) | Multimedia
| SubClass (01h) | Audio
| Revision | 01h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Not Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | 0000C080h - 0000C09Fh
| Base I/O Port | 0000C000h - 0000C07Fh
| System IRQ | 19
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | M-Audio
| Device Description | M-Audio Revolution 5.1
| Device Class | MEDIA
| Device Location | PCI bus 5, device 0, function 0
| Driver Provider | M-Audio
| Driver Version | 5.10.0.5064
| Driver Date | 3-12-2008
| Inf File | oem49.inf
| Service Name | REVO51
| Hardware ID | PCI\VEN_1412&DEV_1724&SUBSYS_36311412&REV_01
| Compatible ID | PCI\VEN_1412&DEV_1724&REV_01
| Parent ID | PCI\VEN_8086&DEV_244E&SUBSYS_88921458&REV_41
Memory Modules
| Memory Slot 1
| Memory Type | 8 GB DDR3-1866 (PC3-14900) SDRAM
| Manufacturer | Kllisre
| Module Type | Unbuffered DIMM
| Number of Ranks/Banks | 2 Ranks, 8 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| JEDEC Timings | CL-tRCD-tRP-tRAS-tWR-tRC @ Frequency
| JEDEC Profile 1 | 13.0-11-10-30-15-42 @ 933MHz
| JEDEC Profile 2 | 11.0-11-10-30-15-42 @ 933MHz
| JEDEC Profile 3 | 10.0-11-10-30-15-42 @ 933MHz
| JEDEC Profile 4 | 9.0-10-9-28-13-38 @ 841MHz
| JEDEC Profile 5 | 8.0-9-8-25-12-34 @ 747MHz
| JEDEC Profile 6 | 7.0-8-7-22-10-30 @ 654MHz
| JEDEC Profile 7 | 6.0-7-6-19-9-26 @ 560MHz
| JEDEC Profile 8 | 5.0-6-5-16-8-21 @ 467MHz
| Refresh Rate | 7.8 us (2X 85-95 C)
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | 1.50 V
| Max Case Temperature | 95 °C (203 °F)
| SPD Revision | 1.1
| Part Number | KHX1866C10D3/8G
| Manufacturing Location | 7
| Manufacture Date | January 2019 (1903h)
| Serial Number | 522C5B2Ch
| Revision Code | None
| EPP Support | Not Supported
| XMP Support | Not Supported
| Memory Slot 3
| Memory Type | 8 GB DDR3-1866 (PC3-14900) SDRAM
| Manufacturer | Kingston
| Module Type | Unbuffered DIMM
| Number of Ranks/Banks | 2 Ranks, 8 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| JEDEC Timings | CL-tRCD-tRP-tRAS-tWR-tRC @ Frequency
| JEDEC Profile 1 | 13.0-11-10-30-15-42 @ 933MHz
| JEDEC Profile 2 | 11.0-11-10-30-15-42 @ 933MHz
| JEDEC Profile 3 | 10.0-11-10-30-15-42 @ 933MHz
| JEDEC Profile 4 | 9.0-10-9-28-13-38 @ 841MHz
| JEDEC Profile 5 | 8.0-9-8-25-12-34 @ 747MHz
| JEDEC Profile 6 | 7.0-8-7-22-10-30 @ 654MHz
| JEDEC Profile 7 | 6.0-7-6-19-9-26 @ 560MHz
| JEDEC Profile 8 | 5.0-6-5-16-8-21 @ 467MHz
| Refresh Rate | 7.8 us (2X 85-95 C)
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | 1.50 V
| Max Case Temperature | 95 °C (203 °F)
| SPD Revision | 1.1
| Part Number | KHX1866C10D3/8G
| Manufacturing Location | 7
| Manufacture Date | May 2015 (1519h)
| Serial Number | 66117105h
| Revision Code | None
| EPP Support | Not Supported
| XMP Support | Not Supported
Memory (SMBIOS)
| Physical Memory Array 1
| Maximum Capacity | 32768 MB
| Location | System Board or Motherboard
| Use | System Memory
| Memory Error Correct. | None
| Memory Devices | 2
| Structure Length | 17h
| Memory Device 1
| Size | 8192 MB
| Form Factor | DIMM
| Memory Type | DDR3
| Speed | 1600 MHz
| Configured Speed | 1600 MHz
| Device Locator | ChannelA-DIMM0
| Bank Locator | BANK 0
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | Synchronous
| Manufacturer | 1319
| Serial Number | 522C5B2C
| Asset Tag | 9876543210
| Part Number | KHX1866C10D3/8G
| Structure Length | 22h
| Memory Device 2
| Size | Not Installed
| Form Factor | DIMM
| Memory Type | Unknown
| Speed | Unknown
| Device Locator | ChannelA-DIMM1
| Bank Locator | BANK 1
| Total Width | 0 bits
| Data Width | 0 bits
| Device Set | 00h
| Type Detail | None
| Manufacturer | [Empty]
| Serial Number | [Empty]
| Asset Tag | 9876543210
| Part Number | [Empty]
| Structure Length | 22h
| Memory Device 3
| Size | 8192 MB
| Form Factor | DIMM
| Memory Type | DDR3
| Speed | 1600 MHz
| Configured Speed | 1600 MHz
| Device Locator | ChannelB-DIMM0
| Bank Locator | BANK 2
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | Synchronous
| Manufacturer | Kingston
| Serial Number | 66117105
| Asset Tag | 9876543210
| Part Number | KHX1866C10D3/8G
| Structure Length | 22h
| Memory Device 4
| Size | Not Installed
| Form Factor | DIMM
| Memory Type | Unknown
| Speed | Unknown
| Device Locator | ChannelB-DIMM1
| Bank Locator | BANK 3
| Total Width | 0 bits
| Data Width | 0 bits
| Device Set | 00h
| Type Detail | None
| Manufacturer | [Empty]
| Serial Number | [Empty]
| Asset Tag | 9876543210
| Part Number | [Empty]
| Structure Length | 22h
Disk
| Secondary/Master Drive
| Disk Model | SPCC Solid State Disk
| Disk Size | 114473 MB (111.79 GB)
| Interface Type | Serial ATA III (SATA/600)
| Form Factor | 2.5"
| Rotation Rate | SSD
| Geometry | Heads: 16, Sectors: 63, Tracks: 16383
| Compatibility | ACS-4
| Serial Number | 2A40079618DB00135162
| Controller Revision | SBFM61.3
| Disk Marketing Size | 120034 MB (120.03 GB)
| Buffer Size | Unknown
| Buffer Type | Not Specified
| Disk Temperature | 33 °C (91 °F)
| Disk Health Status | Good
| SSD Remaining Life | 100 %
| Total Host Writes | 3.31 TB
| Logical Drives | I:
| ECC bytes | None
| Security Erase Time | 20 min
| Enh. Security Erase | 60 min
| Current APM Value | None
| Acoustic Management | None
| Location (Vendor) | Intel Corporation
| Location (Device) | 8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
| Device Location | Secondary/Master
| Transfer Modes
| SATA Speed | 600 MB/s, Active: 600 MB/s
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 6 (UltraDMA/133), Active: 5 (UltraDMA/100)
| Sectors per Interrupt | 16, Active: 16
| Disk Features
| SATA NCQ Command | Supported
| SSD TRIM Command | Supported
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Supported
| Double Word I/O | Supported
| Standard Standby Timer | Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| S.M.A.R.T. | Supported, Enabled
| S.M.A.R.T. Self-test | Supported, Enabled
| S.M.A.R.T. Error Logging | Supported, Enabled
| Security Mode Feature Set | Supported, Disabled
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Not Supported
| Write Cache | Supported, Enabled
| Look-ahead | Supported, Enabled
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Not Supported
| Host Protected Area | Supported, Enabled
| Write Verify Command | Not Supported
| Write Buffer Command | Supported, Enabled
| Read Buffer Command | Supported, Enabled
| NOP Command | Supported, Enabled
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Supported, Enabled
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Not Supported
| Removable Media Status | Not Supported
| Power-up in Standby | Not Supported
| Set Features Req. to Spinup | Not Supported
| Set Max Security Extension | Supported, Disabled
| Automatic Acoustic Management | Not Supported
| 48-bit Address | Supported, Enabled
| Device Configuration Overlay | Supported, Enabled
| Flush Cache Command | Supported, Enabled
| Flush Cache Ext Command | Supported, Enabled
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Supported, Enabled
| Write DMA/Multiple FUA EXT | Supported, Enabled
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Not Supported
| S.M.A.R.T.
| ID | Attribute Name | Threshold | Worst | Value | Raw Value
| 1 | Raw Read Error Rate | 50 | 100 | 100 | 0
| 9 | Power On Hours Count | 0 | 100 | 100 | 3632
| 12 | Drive Power Cycle Count | 0 | 100 | 100 | 1701
| 168 | SATA PHY Error Count | 0 | 100 | 100 | 0
| 170 | Available Reserved Space | 0 | 100 | 100 | 483
| 173 | Average Erase Count | 0 | 100 | 100 | 2490434
| 192 | Unsafe Shutdown Count | 0 | 100 | 100 | 85
| 194 | Drive Temperature | 0 | 67 | 67 | 141736083489
| 218 | Flash ROM ECC Correction Count | 50 | 100 | 100 | 0
| 231 | SSD Remaining Life | 0 | 100 | 100 | 98
| 241 | Total Host Writes | 0 | 100 | 100 | 3386
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | SPCC Solid State Disk ATA Device
| Device Class | DiskDrive
| Device Location | Channel 1, Target 0, Lun 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.23403
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | IDE\DiskSPCC_Solid_State_Disk___________________SBFM61.3
| Compatible ID | GenDisk
| Parent ID | PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
| 8th/Slave Drive
| Disk Model | WDC WD1001FALS-00J7B0
| Disk Size | 953869 MB (931.51 GB)
| Interface Type | Serial ATA II (SATA/300)
| Geometry | Heads: 16, Sectors: 63, Tracks: 16383
| Compatibility | ATA8-ACS
| Serial Number | WD-WMATV0357962
| Controller Revision | 05.00K05
| Disk Marketing Size | 1000204 MB (1000.2 GB)
| Buffer Size | 32 MB
| Buffer Type | Not Specified
| Disk Temperature | 42 °C (108 °F)
| Reallocated Sectors | 0
| Disk Health Status | Good
| Logical Drives | E:, F:, H:
| ECC bytes | 50
| Security Erase Time | 194 min
| Enh. Security Erase | 194 min
| Current APM Value | None
| Acoustic Management | FEh (80h Recommended) - Disabled
| Location (Vendor) | Intel Corporation
| Location (Device) | 8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
| Device Location | 8th/Slave
| Transfer Modes
| SATA Speed | 300 MB/s
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 6 (UltraDMA/133), Active: 5 (UltraDMA/100)
| Sectors per Interrupt | 16, Active: 16
| Disk Features
| SATA NCQ Command | Supported
| SSD TRIM Command | Not Supported
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Supported
| Double Word I/O | Not Supported
| Standard Standby Timer | Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| S.M.A.R.T. | Supported, Enabled
| S.M.A.R.T. Self-test | Supported, Enabled
| S.M.A.R.T. Error Logging | Supported, Enabled
| Security Mode Feature Set | Supported, Disabled
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Not Supported
| Write Cache | Supported, Enabled
| Look-ahead | Supported, Enabled
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Not Supported
| Host Protected Area | Supported, Enabled
| Write Verify Command | Not Supported
| Write Buffer Command | Supported, Enabled
| Read Buffer Command | Supported, Enabled
| NOP Command | Supported, Enabled
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Supported, Enabled
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Not Supported
| Removable Media Status | Not Supported
| Power-up in Standby | Supported, Disabled
| Set Features Req. to Spinup | Supported, Enabled
| Set Max Security Extension | Supported, Disabled
| Automatic Acoustic Management | Supported, Disabled
| 48-bit Address | Supported, Enabled
| Device Configuration Overlay | Supported, Enabled
| Flush Cache Command | Supported, Enabled
| Flush Cache Ext Command | Supported, Enabled
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Supported, Enabled
| Write DMA/Multiple FUA EXT | Not Supported
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Supported, Enabled
| S.M.A.R.T.
| ID | Attribute Name | Threshold | Worst | Value | Raw Value
| 1 | Raw Read Error Rate | 51 | 200 | 200 | 0
| 3 | Spin-up Time | 21 | 253 | 253 | 6500
| 4 | Start/Stop Count | 0 | 68 | 68 | 32639
| 5 | Reallocated Sectors Count | 140 | 200 | 200 | 0
| 7 | Seek Error Rate | 51 | 253 | 100 | 0
| 9 | Power On Hours Count | 0 | 45 | 45 | 40331
| 10 | Spin-up Retry Count | 51 | 100 | 100 | 0
| 11 | Recalibration Retries | 51 | 100 | 100 | 0
| 12 | Drive Power Cycle Count | 0 | 78 | 78 | 22728
| 192 | Power-Off Retract Count | 0 | 198 | 198 | 2052
| 193 | Load/Unload Cycle Count | 0 | 190 | 190 | 32529
| 194 | Drive Temperature | 0 | 89 | 108 | 42
| 196 | Reallocation Event Count | 0 | 200 | 200 | 0
| 197 | Current Pending Sectors | 0 | 200 | 200 | 0
| 198 | Uncorrectable Sectors | 0 | 200 | 200 | 0
| 199 | UltraDMA CRC Error Rate | 0 | 200 | 200 | 312
| 200 | Write Error Rate | 51 | 183 | 200 | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | WDC WD1001FALS-00J7B0 ATA Device
| Device Class | DiskDrive
| Device Location | Channel 2, Target 0, Lun 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.23403
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | IDE\DiskWDC_WD1001FALS-00J7B0___________________05.00K05
| Compatible ID | GenDisk
| Parent ID | PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
| 8th/Slave Drive
| Disk Model | Samsung SSD 860 EVO 250GB
| Disk Size | 238475 MB (232.89 GB)
| Interface Type | Serial ATA III (SATA/600)
| Form Factor | 2.5"
| Rotation Rate | SSD
| Geometry | Heads: 16, Sectors: 63, Tracks: 16383
| Compatibility | ACS-4 revision 94
| Serial Number | S3Y9NB0K275545B
| Controller Revision | RVT01B6Q
| Disk Marketing Size | 250059 MB (250.06 GB)
| Buffer Size | Unknown
| Buffer Type | Not Specified
| Disk Temperature | 39 °C (102 °F)
| Reallocated Sectors | 0
| Disk Health Status | Good
| SSD Remaining Life | 100 %
| Total Host Writes | 6.58 TB
| Logical Drives | C:, D:, G:
| ECC bytes | None
| Security Erase Time | 4 min
| Enh. Security Erase | 8 min
| Current APM Value | None
| Acoustic Management | None
| Location (Vendor) | Intel Corporation
| Location (Device) | 8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
| Device Location | 8th/Slave
| Transfer Modes
| SATA Speed | 600 MB/s, Active: 600 MB/s
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 6 (UltraDMA/133), Active: 5 (UltraDMA/100)
| Sectors per Interrupt | 1, Active: 1
| Disk Features
| SATA NCQ Command | Supported
| SSD TRIM Command | Supported
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Supported
| Double Word I/O | Supported
| Standard Standby Timer | Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| S.M.A.R.T. | Supported, Enabled
| S.M.A.R.T. Self-test | Supported, Enabled
| S.M.A.R.T. Error Logging | Supported, Enabled
| Security Mode Feature Set | Supported, Disabled
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Not Supported
| Write Cache | Supported, Enabled
| Look-ahead | Supported, Enabled
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Not Supported
| Host Protected Area | Supported, Enabled
| Write Verify Command | Not Supported
| Write Buffer Command | Supported, Enabled
| Read Buffer Command | Supported, Enabled
| NOP Command | Supported, Enabled
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Supported, Enabled
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Not Supported
| Removable Media Status | Not Supported
| Power-up in Standby | Not Supported
| Set Features Req. to Spinup | Not Supported
| Set Max Security Extension | Supported, Disabled
| Automatic Acoustic Management | Not Supported
| 48-bit Address | Supported, Enabled
| Device Configuration Overlay | Supported, Enabled
| Flush Cache Command | Supported, Enabled
| Flush Cache Ext Command | Supported, Enabled
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Supported, Enabled
| Write DMA/Multiple FUA EXT | Supported, Enabled
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Supported, Enabled
| S.M.A.R.T.
| ID | Attribute Name | Threshold | Worst | Value | Raw Value
| 5 | Reallocated Sectors Count | 10 | 100 | 100 | 0
| 9 | Power On Hours Count | 0 | 97 | 97 | 11541
| 12 | Drive Power Cycle Count | 0 | 93 | 93 | 6429
| 177 | Wear Leveling Count | 0 | 98 | 98 | 23
| 179 | Used Reserved Block Count (Total) | 10 | 100 | 100 | 0
| 181 | Program Fail Count | 10 | 100 | 100 | 0
| 182 | Erase Fail Count | 10 | 100 | 100 | 0
| 183 | Runtime Bad Block | 10 | 100 | 100 | 0
| 187 | Uncorrectable Errors | 0 | 100 | 100 | 0
| 190 | Airflow Temperature | 0 | 47 | 61 | 39
| 195 | Hardware ECC Recovered | 0 | 200 | 200 | 0
| 199 | UltraDMA CRC Error Rate | 0 | 99 | 99 | 3
| 235 | POR Recovery Count | 0 | 99 | 99 | 272
| 241 | Total Host Writes | 0 | 99 | 99 | 14120793738
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | Samsung SSD 860 EVO 250GB ATA Device
| Device Class | DiskDrive
| Device Location | Channel 3, Target 0, Lun 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.23403
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | IDE\DiskSamsung_SSD_860_EVO_250GB_______________RVT01B6Q
| Compatible ID | GenDisk
| Parent ID | PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
| 8th/Slave Drive
| Disk Model | ST3500412AS
| Disk Size | 476940 MB (465.76 GB)
| Interface Type | Serial ATA II (SATA/300)
| Rotation Rate | 5900 rpm
| Geometry | Heads: 16, Sectors: 63, Tracks: 16383
| Compatibility | ATA8-ACS revision 41
| Serial Number | 6VV25CDT
| Controller Revision | CC32
| Disk Marketing Size | 500108 MB (500.11 GB)
| Buffer Size | 16 MB
| Buffer Type | Not Specified
| Disk Temperature | 35 °C (95 °F)
| Reallocated Sectors | 1991
| Disk Health Status | Bad
| Total Host Writes | 1.02 TB
| Total Host Reads | 789.29 GB
| Logical Drives | J:
| ECC bytes | 4
| Security Erase Time | 96 min
| Enh. Security Erase | 96 min
| Current APM Value | C0h
| Acoustic Management | 00h (FEh Recommended) - Enabled
| Location (Vendor) | Intel Corporation
| Location (Device) | 8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
| Device Location | 8th/Slave
| Transfer Modes
| SATA Speed | 300 MB/s
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 6 (UltraDMA/133), Active: 5 (UltraDMA/100)
| Sectors per Interrupt | 16, Active: 16
| Disk Features
| SATA NCQ Command | Supported
| SSD TRIM Command | Not Supported
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Supported
| Double Word I/O | Not Supported
| Standard Standby Timer | Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| S.M.A.R.T. | Supported, Enabled
| S.M.A.R.T. Self-test | Supported, Enabled
| S.M.A.R.T. Error Logging | Supported, Enabled
| Security Mode Feature Set | Supported, Disabled
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Not Supported
| Write Cache | Supported, Enabled
| Look-ahead | Supported, Enabled
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Not Supported
| Host Protected Area | Supported, Enabled
| Write Verify Command | Not Supported
| Write Buffer Command | Supported, Enabled
| Read Buffer Command | Supported, Enabled
| NOP Command | Not Supported
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Supported, Enabled
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Supported, Enabled
| Removable Media Status | Not Supported
| Power-up in Standby | Supported, Disabled
| Set Features Req. to Spinup | Supported, Disabled
| Set Max Security Extension | Supported, Disabled
| Automatic Acoustic Management | Supported, Enabled
| 48-bit Address | Supported, Enabled
| Device Configuration Overlay | Supported, Enabled
| Flush Cache Command | Supported, Enabled
| Flush Cache Ext Command | Supported, Enabled
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Supported, Enabled
| Write DMA/Multiple FUA EXT | Supported, Enabled
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Supported, Enabled
| S.M.A.R.T.
| ID | Attribute Name | Threshold | Worst | Value | Raw Value
| 1 | Raw Read Error Rate | 6 | 90 | 120 | 243460323
| 3 | Spin-up Time | 0 | 97 | 97 | 0
| 4 | Start/Stop Count | 20 | 71 | 71 | 30122
| 5 | Reallocated Sectors Count | 36 | 52 | 52 | 1991
| 7 | Seek Error Rate | 30 | 60 | 84 | 265538621
| 9 | Power On Hours Count | 0 | 79 | 79 | 18882
| 10 | Spin-up Retry Count | 97 | 100 | 100 | 0
| 12 | Drive Power Cycle Count | 20 | 87 | 87 | 13710
| 183 | SATA Downshift Error Count | 0 | 94 | 94 | 6
| 184 | End to End Error Detection | 99 | 100 | 100 | 0
| 187 | Uncorrectable Errors | 0 | 1 | 1 | 1907
| 188 | Command Timeout | 0 | 1 | 100 | 175
| 189 | High Fly Writes | 0 | 100 | 100 | 0
| 190 | Airflow Temperature | 45 | 39 | 65 | 43639111715
| 194 | Drive Temperature | 0 | 61 | 35 | 25769803811
| 195 | Hardware ECC Recovered | 0 | 22 | 38 | 243460323
| 197 | Current Pending Sectors | 0 | 99 | 100 | 0
| 198 | Uncorrectable Sectors | 0 | 99 | 100 | 0
| 199 | UltraDMA CRC Error Rate | 0 | 200 | 200 | 0
| 240 | Head Flying Hours | 0 | 253 | 100 | 88411901834003
| 241 | Total Host Writes | 0 | 253 | 100 | 2194415541
| 242 | Total Host Reads | 0 | 253 | 100 | 1655269662
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | ST3500412AS ATA Device
| Device Class | DiskDrive
| Device Location | Channel 4, Target 0, Lun 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.23403
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | IDE\DiskST3500412AS_____________________________CC32____
| Compatible ID | GenDisk
| Parent ID | PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
ATAPI
| ATAPI
| ATAPI Model | PIONEER DVD-RW DVR-217F
| ATAPI Type | DVD+-RW DL/CD-RW
| Interface Type | Serial ATA I
| Physical Interface | Serial ATAPI
| ATAPI Name | PIONEER DVD-RW DVR-217F
| Vendor Specific | 09/03/04 PIONEER
| CD Read Speed | 16x (Current: 16x)
| CD Write Speed | 40x (Current: 32x)
| Buffer Size | 1.95 MB
| Loading Mechanism | Tray Type
| Rotation Control | CLV
| Read Retry Count | 3
| Write Retry Count | 0
| Compatibility | ATA/ATAPI-7
| Serial Number | IEDP052900WL
| Controller Revision | 1.07
| Logical Drives | K:
| Command DRQ Type | Accelerated DRQ
| Command Packet Size | 12 bytes
| Location (Vendor) | Intel Corporation
| Location (Device) | 8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
| Transfer Modes
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 4 (UltraDMA/66), Active: 2 (UltraDMA/33)
| Reading Features
| CD-R Disk Read | Supported
| CD-RW Disk Read | Supported
| DVD-ROM Disk Read | Supported
| DVD-RAM Disk Read | Supported
| DVD-R Disk Read | Supported
| DVD-R DL Disk Read | Supported
| DVD-RW Disk Read | Supported
| DVD-RW DL Disk Read | Not Supported
| DVD+R Disk Read | Supported
| DVD+R DL Disk Read | Supported
| DVD+RW Disk Read | Supported
| DVD+RW DL Disk Read | Not Supported
| BD-ROM Disk Read | Not Supported
| BD-R Disk Read | Not Supported
| BD-RE Disk Read | Not Supported
| HD DVD-ROM Disk Read | Not Supported
| HD DVD-RAM Disk Read | Not Supported
| HD DVD-R Disk Read | Not Supported
| HD DVD-R DL Disk Read | Not Supported
| HD DVD-RW Disk Read | Not Supported
| HD DVD-RW DL Disk Read | Not Supported
| Read Packet Using Method 2 | Supported
| Read Mode2 Form1 Sectors | Supported
| Read Mode2 Form2 Sectors | Supported
| Multisession Disk Read | Supported
| READ-CD Command on AudioCD | Supported
| Read Bar Code Capable | Not Supported
| Read Lead-in (CD-Text) | Supported
| Writing Features
| CD-R Disk Write | Supported
| CD-RW Disk Write | Supported
| DVD-RAM Disk Write | Not Supported
| DVD-R Disk Write | Supported
| DVD-R DL Disk Write | Supported
| DVD-RW Disk Write | Supported
| DVD+R Disk Write | Supported
| DVD+R DL Disk Write | Supported
| DVD+RW Disk Write | Supported
| DVD+RW DL Disk Write | Not Supported
| BD-R Disk Write | Not Supported
| BD-RE Disk Write | Not Supported
| HD DVD-R Disk Write | Not Supported
| HD DVD-R DL Disk Write | Not Supported
| HD DVD-RAM Disk Write | Not Supported
| HD DVD-RW Disk Write | Not Supported
| HD DVD-RW DL Disk Write | Not Supported
| Test Write Mode Support | Supported
| Buffer Underrun Protection | Supported
| Other Features
| Audio Play Support | Supported
| CD-DA Stream is Accurate | Supported
| Composite Audio/Video | Not Supported
| Digital Output on Port 1 | Not Supported
| Digital Output on Port 2 | Not Supported
| Support Subcode R-W | Not Supported
| Support Subcode R-W D&C | Not Supported
| C2 Pointers Supported | Supported
| ISRC Supported | Supported
| UPC Supported | Supported
| ATAPI Features
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Not Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| ATA Software Reset | Not Supported
| Overlap Operation | Not Supported
| Command Queuing | Not Supported
| Interleaving DMA | Not Supported
| S.M.A.R.T. | Not Supported
| S.M.A.R.T. Self-test | Not Supported
| S.M.A.R.T. Error Logging | Not Supported
| Security Mode Feature Set | Not Supported
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Supported, Enabled
| Write Cache | Not Supported
| Look-ahead | Not Supported
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Supported, Enabled
| Host Protected Area | Not Supported
| Write Verify Command | Not Supported
| Write Buffer Command | Not Supported
| Read Buffer Command | Not Supported
| NOP Command | Not Supported
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Not Supported
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Not Supported
| Removable Media Status | Not Supported
| Power-up in Standby | Not Supported
| Set Features Req. to Spinup | Not Supported
| Set Max Security Extension | Not Supported
| Automatic Acoustic Management | Not Supported
| 48-bit Address | Not Supported
| Device Configuration Overlay | Not Supported
| Flush Cache Command | Not Supported
| Flush Cache Ext Command | Not Supported
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Not Supported
| Write DMA/Multiple FUA EXT | Not Supported
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Not Supported
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard CD-ROM drives)
| Device Description | CD-ROM Drive
| Friendly Name | PIONEER DVD-RW DVR-217F ATA Device
| Device Class | CDROM
| Device Location | Channel 5, Target 0, Lun 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.23403
| Driver Date | 6-21-2006
| Inf File | cdrom.inf
| Service Name | cdrom
| Hardware ID | IDE\CdRomPIONEER_DVD-RW__DVR-217F________________1.07____
| Compatible ID | GenCdRom
| Parent ID | PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
Storage (ASPI)
| Host: 3, Target: 0, LUN: 0
| Device Name | Generic USB SD Reader
| Device Type | Disk Drive
| Compatibility | Not Standard
| Vendor Specific |
| Serial Number |
| Controller Revision | 1.00
| Logical Drives | M:
| Location | Host: 3, Target: 0, LUN: 0
| Bus Width | 8-bit
| Address Width | 8-bit
| Location (Vendor) | Alcor Micro
| Location (Device) | USB 52-in-1 Card Reader/Writer
| ASPI Device Features
| Removable Medium | Yes
| Read Cache | Not Supported
| Write Cache | Not Supported
| Read Reallocate | Not Supported
| Write Reallocate | Not Supported
| Terminate I/O Process | Not Supported
| Normal ACA | Not Supported
| Hierarchical Support | Not Supported
| Embedded Array Controller | Not Supported
| Protection Information | Not Supported
| Enclosure Services | Not Supported
| Multi-Ported Device | Not Supported
| Medium Changer | Not Supported
| Relative Addressing | Not Supported
| Synchronous Transfer | Not Supported
| Linked Commands | Not Supported
| Soft Reset | Not Supported
| Quick Arbitration | Not Supported
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | Generic USB SD Reader USB Device
| Device Class | DiskDrive
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.23403
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | USBSTOR\DiskGeneric_USB_SD_Reader___1.00
| Compatible ID | USBSTOR\Disk
| Parent ID | USB\VID_058F&PID_6362&REV_0129
| Host: 3, Target: 0, LUN: 0
| Device Name | Generic USB CF Reader
| Device Type | Disk Drive
| Compatibility | Not Standard
| Vendor Specific |
| Serial Number |
| Controller Revision | 1.01
| Logical Drives | N:
| Location | Host: 3, Target: 0, LUN: 0
| Bus Width | 8-bit
| Address Width | 8-bit
| Location (Vendor) | Alcor Micro
| Location (Device) | USB 52-in-1 Card Reader/Writer
| ASPI Device Features
| Removable Medium | Yes
| Read Cache | Not Supported
| Write Cache | Not Supported
| Read Reallocate | Not Supported
| Write Reallocate | Not Supported
| Terminate I/O Process | Not Supported
| Normal ACA | Not Supported
| Hierarchical Support | Not Supported
| Embedded Array Controller | Not Supported
| Protection Information | Not Supported
| Enclosure Services | Not Supported
| Multi-Ported Device | Not Supported
| Medium Changer | Not Supported
| Relative Addressing | Not Supported
| Synchronous Transfer | Not Supported
| Linked Commands | Not Supported
| Soft Reset | Not Supported
| Quick Arbitration | Not Supported
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | Generic USB CF Reader USB Device
| Device Class | DiskDrive
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.23403
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | USBSTOR\DiskGeneric_USB_CF_Reader___1.01
| Compatible ID | USBSTOR\Disk
| Parent ID | USB\VID_058F&PID_6362&REV_0129
| Host: 3, Target: 0, LUN: 0
| Device Name | Generic USB SM Reader
| Device Type | Disk Drive
| Compatibility | Not Standard
| Vendor Specific |
| Serial Number |
| Controller Revision | 1.02
| Logical Drives | O:
| Location | Host: 3, Target: 0, LUN: 0
| Bus Width | 8-bit
| Address Width | 8-bit
| Location (Vendor) | Alcor Micro
| Location (Device) | USB 52-in-1 Card Reader/Writer
| ASPI Device Features
| Removable Medium | Yes
| Read Cache | Not Supported
| Write Cache | Not Supported
| Read Reallocate | Not Supported
| Write Reallocate | Not Supported
| Terminate I/O Process | Not Supported
| Normal ACA | Not Supported
| Hierarchical Support | Not Supported
| Embedded Array Controller | Not Supported
| Protection Information | Not Supported
| Enclosure Services | Not Supported
| Multi-Ported Device | Not Supported
| Medium Changer | Not Supported
| Relative Addressing | Not Supported
| Synchronous Transfer | Not Supported
| Linked Commands | Not Supported
| Soft Reset | Not Supported
| Quick Arbitration | Not Supported
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | Generic USB SM Reader USB Device
| Device Class | DiskDrive
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.23403
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | USBSTOR\DiskGeneric_USB_SM_Reader___1.02
| Compatible ID | USBSTOR\Disk
| Parent ID | USB\VID_058F&PID_6362&REV_0129
| Host: 3, Target: 0, LUN: 0
| Device Name | Generic USB MS Reader
| Device Type | Disk Drive
| Compatibility | Not Standard
| Vendor Specific |
| Serial Number |
| Controller Revision | 1.03
| Logical Drives | P:
| Location | Host: 3, Target: 0, LUN: 0
| Bus Width | 8-bit
| Address Width | 8-bit
| Location (Vendor) | Alcor Micro
| Location (Device) | USB 52-in-1 Card Reader/Writer
| ASPI Device Features
| Removable Medium | Yes
| Read Cache | Not Supported
| Write Cache | Not Supported
| Read Reallocate | Not Supported
| Write Reallocate | Not Supported
| Terminate I/O Process | Not Supported
| Normal ACA | Not Supported
| Hierarchical Support | Not Supported
| Embedded Array Controller | Not Supported
| Protection Information | Not Supported
| Enclosure Services | Not Supported
| Multi-Ported Device | Not Supported
| Medium Changer | Not Supported
| Relative Addressing | Not Supported
| Synchronous Transfer | Not Supported
| Linked Commands | Not Supported
| Soft Reset | Not Supported
| Quick Arbitration | Not Supported
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | Generic USB MS Reader USB Device
| Device Class | DiskDrive
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.23403
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | USBSTOR\DiskGeneric_USB_MS_Reader___1.03
| Compatible ID | USBSTOR\Disk
| Parent ID | USB\VID_058F&PID_6362&REV_0129
Logical Drives
| Local Drives
| C:[SYSTEM]
| Drive Letter | C:
| Drive Type | Fixed Disk
| Volume Label | SYSTEM
| File System | FAT
| Volume Serial Number | F81A-AC7C
| Total Size | 100.93 MB
| Free Space | 9.05 MB (9.0%)
| Location | Samsung SSD 860 EVO 250GB (S3Y9NB0K275545B)
| D:[UTILITIES]
| Drive Letter | D:
| Drive Type | Fixed Disk
| Volume Label | UTILITIES
| File System | FAT32
| Volume Serial Number | 441A-C1C0
| Total Size | 4.99 GB
| Free Space | 1.49 GB (30.0%)
| Location | Samsung SSD 860 EVO 250GB (S3Y9NB0K275545B)
| E:[WIN10]
| Drive Letter | E:
| Drive Type | Fixed Disk
| Volume Label | WIN10
| File System | NTFS
| Volume Serial Number | E8C6-391A
| Total Size | 30.0 GB
| Free Space | 29.84 GB (99.5%)
| Location | WDC WD1001FALS-00J7B0 (WD-WMATV0357962)
| F:[WINXP]
| Drive Letter | F:
| Drive Type | Fixed Disk
| Volume Label | WINXP
| File System | NTFS
| Volume Serial Number | 4EC7-F3C6
| Total Size | 10.0 GB
| Free Space | 2.25 GB (22.5%)
| Location | WDC WD1001FALS-00J7B0 (WD-WMATV0357962)
| G:[WIN7]
| Drive Letter | G:
| Drive Type | Fixed Disk
| Volume Label | WIN7
| File System | NTFS
| Volume Serial Number | 2648-A498
| Total Size | 227.79 GB
| Free Space | 138.35 GB (60.7%)
| Location | Samsung SSD 860 EVO 250GB (S3Y9NB0K275545B)
| H:[MUSIC]
| Drive Letter | H:
| Drive Type | Fixed Disk
| Volume Label | MUSIC
| File System | NTFS
| Volume Serial Number | 56C9-FD1A
| Total Size | 891.51 GB
| Free Space | 191.96 GB (21.5%)
| Location | WDC WD1001FALS-00J7B0 (WD-WMATV0357962)
| I:[WIN7MAX]
| Drive Letter | I:
| Drive Type | Fixed Disk
| Volume Label | WIN7MAX
| File System | NTFS
| Volume Serial Number | B822-7007
| Total Size | 111.79 GB
| Free Space | 16.68 GB (14.9%)
| Location | SPCC Solid State Disk (2A40079618DB00135162)
| J:[WIN7MAXDATA]
| Drive Letter | J:
| Drive Type | Fixed Disk
| Volume Label | WIN7MAXDATA
| File System | NTFS
| Volume Serial Number | 4487-0B4F
| Total Size | 465.76 GB
| Free Space | 245.07 GB (52.6%)
| Location | ST3500412AS (6VV25CDT)
| K:
| Drive Letter | K:
| Drive Type | Optical Drive
| Location | PIONEER DVD-RW DVR-217F
| M:
| Drive Letter | M:
| Drive Type | Removable Disk
| Location | Generic USB SD Reader
| N:
| Drive Letter | N:
| Drive Type | Removable Disk
| Location | Generic USB CF Reader
| O:
| Drive Letter | O:
| Drive Type | Removable Disk
| Location | Generic USB SM Reader
| P:
| Drive Letter | P:
| Drive Type | Removable Disk
| Location | Generic USB MS Reader
USB Devices
| USB Device 1
| Vendor (8087h) | Intel Corp.
| Device (8000h) | Integrated Rate Matching Hub
| Manufacturer |
| Product |
| Serial Number |
| Device Version | 0.05
| Class (09h) | Hub
| SubClass (00h) | Unused
| Protocol (01h) | Single TT
| Configuration |
| USB Version | 2.00
| Speed | 480 Mb/s
| Transfer Type | Interrupt
| Data Packet Size | 64 bytes
| Max Power | Remote Wakeup
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Generic USB Hub)
| Device Description | Generic USB Hub
| Device Class | USB
| Device Location | Port_#0001.Hub_#0002
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24138
| Driver Date | 6-21-2006
| Inf File | usb.inf
| Service Name | usbhub
| Hardware ID | USB\VID_8087&PID_8000&REV_0005
| Compatible ID | USB\Class_09&SubClass_00&Prot_00
| Parent ID | PCI\VEN_8086&DEV_8C26&SUBSYS_50061458&REV_05
| Interface 1
| Class (09h) | Hub
| SubClass (00h) | Unused
| Protocol (00h) | Full Speed (or Root) Hub
| Interface |
| USB Device 2
| Vendor (8087h) | Intel Corp.
| Device (8008h) | Integrated Rate Matching Hub
| Manufacturer |
| Product |
| Serial Number |
| Device Version | 0.05
| Class (09h) | Hub
| SubClass (00h) | Unused
| Protocol (01h) | Single TT
| Configuration |
| USB Version | 2.00
| Speed | 480 Mb/s
| Transfer Type | Interrupt
| Data Packet Size | 64 bytes
| Max Power | Remote Wakeup
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Generic USB Hub)
| Device Description | Generic USB Hub
| Device Class | USB
| Device Location | Port_#0001.Hub_#0001
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24138
| Driver Date | 6-21-2006
| Inf File | usb.inf
| Service Name | usbhub
| Hardware ID | USB\VID_8087&PID_8008&REV_0005
| Compatible ID | USB\Class_09&SubClass_00&Prot_00
| Parent ID | PCI\VEN_8086&DEV_8C2D&SUBSYS_50061458&REV_05
| Interface 1
| Class (09h) | Hub
| SubClass (00h) | Unused
| Protocol (00h) | Full Speed (or Root) Hub
| Interface |
| USB Device 3
| Vendor (093Ah) | Pixart Imaging
| Device (2532h) | Gaming Mouse
| Manufacturer | PixArt
| Product | Gaming Mouse
| Serial Number |
| Device Version | 1.00
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Protocol (00h) | Unknown
| Configuration |
| USB Version | 2.00
| Speed | 480 Mb/s
| Transfer Type | Interrupt
| Data Packet Size | 8 bytes
| Max Power | 100 mA Remote Wakeup
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | USB Composite Device
| Device Class | USB
| Device Location | Port_#0004.Hub_#0001
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24138
| Driver Date | 6-21-2006
| Inf File | usb.inf
| Service Name | usbccgp
| Hardware ID | USB\VID_093A&PID_2532&REV_0100
| Compatible ID | IUSB3\DevClass_00&SubClass_00&Prot_00
| Parent ID | PCI\VEN_8086&DEV_8C31&SUBSYS_50071458&REV_05
| Interface 1
| Class (03h) | Human Interface Devices
| SubClass (01h) | Boot Interface Subclass
| Protocol (02h) | Mouse
| Interface |
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | USB Input Device
| Device Class | HIDClass
| Device Location | 0000.0014.0000.004.000.000.000.000.000
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24386
| Driver Date | 6-21-2006
| Inf File | input.inf
| Service Name | HidUsb
| Hardware ID | USB\VID_093A&PID_2532&REV_0100&MI_00
| Compatible ID | USB\Class_03&SubClass_01&Prot_02
| Parent ID | USB\VID_093A&PID_2532&REV_0100
| Interface 2
| Class (03h) | Human Interface Devices
| SubClass (00h) | No Subclass
| Protocol (01h) | Keyboard
| Interface |
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | USB Input Device
| Device Class | HIDClass
| Device Location | 0000.0014.0000.004.000.000.000.000.000
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24386
| Driver Date | 6-21-2006
| Inf File | input.inf
| Service Name | HidUsb
| Hardware ID | USB\VID_093A&PID_2532&REV_0100&MI_01
| Compatible ID | USB\Class_03&SubClass_00&Prot_01
| Parent ID | USB\VID_093A&PID_2532&REV_0100
| USB Device 4
| Vendor (058Fh) | Alcor Micro
| Device (6362h) | USB 52-in-1 Card Reader/Writer
| Manufacturer | Generic
| Product | Mass Storage Device
| Serial Number | 058F312D81B
| Device Version | 1.29
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Protocol (00h) | Unknown
| Configuration |
| USB Version | 2.00
| Speed | 480 Mb/s
| Transfer Type | Bulk
| Data Packet Size | 64 bytes
| Max Power | 250 mA
| Driver
| Driver Status | The device is working properly
| Manufacturer | Compatible USB storage device
| Device Description | USB Mass Storage Device
| Device Class | USB
| Device Location | Port_#0006.Hub_#0001
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.23403
| Driver Date | 6-21-2006
| Inf File | usbstor.inf
| Service Name | USBSTOR
| Hardware ID | USB\VID_058F&PID_6362&REV_0129
| Compatible ID | USB\Class_08&SubClass_06&Prot_50
| Parent ID | PCI\VEN_8086&DEV_8C31&SUBSYS_50071458&REV_05
| Interface 1
| Class (08h) | Mass Storage
| SubClass (06h) | SCSI
| Protocol (50h) | Bulk (Zip)
| Interface |
| USB Device 5
| Vendor (04A9h) | Canon
| Device (2660h) | LaserBase MF3110 Scanner/Printer
| Manufacturer | Canon,Inc.
| Product | MF3110
| Serial Number | 2363E2124558
| Device Version | 0.00
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Protocol (00h) | Unknown
| Configuration |
| USB Version | 2.00
| Speed | 480 Mb/s
| Transfer Type | Bulk/Interrupt
| Data Packet Size | 64 bytes
| Max Power | 2 mA Self-Powered
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | USB Composite Device
| Device Class | USB
| Device Location | Port_#0012.Hub_#0001
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24138
| Driver Date | 6-21-2006
| Inf File | usb.inf
| Service Name | usbccgp
| Hardware ID | USB\VID_04A9&PID_2660&REV_0000
| Compatible ID | IUSB3\DevClass_00&SubClass_00&Prot_00
| Parent ID | PCI\VEN_8086&DEV_8C31&SUBSYS_50071458&REV_05
| Interface 1
| Class (FFh) | Vendor Specific Class
| SubClass (00h) | Unknown
| Protocol (FFh) | Unknown
| Interface |
| Driver
| Driver Status | The device is working properly
| Manufacturer | Canon
| Device Description | Canon MF3110
| Device Class | Image
| Device Location | 0000.0014.0000.012.000.000.000.000.000
| Driver Provider | Canon
| Driver Version | 11.3.0.0
| Driver Date | 2-1-2007
| Inf File | oem40.inf
| Service Name | usbscan
| Hardware ID | USB\VID_04A9&PID_2660&REV_0000&MI_00
| Compatible ID | USB\Class_ff&SubClass_00&Prot_ff
| Parent ID | USB\VID_04A9&PID_2660&REV_0000
| Interface 2
| Class (07h) | Printer
| SubClass (01h) | Printer
| Protocol (02h) | Bidirectional
| Interface |
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | USB Printing Support
| Device Class | USB
| Device Location | 0000.0014.0000.012.000.000.000.000.000
| Driver Provider | Microsoft
| Driver Version | 6.1.7600.16385
| Driver Date | 6-21-2006
| Inf File | usbprint.inf
| Service Name | usbprint
| Hardware ID | USB\VID_04A9&PID_2660&REV_0000&MI_01
| Compatible ID | USB\Class_07&SubClass_01&Prot_02
| Parent ID | USB\VID_04A9&PID_2660&REV_0000
Physical Printers
| USB Printer 1
| Vendor (04A9h) | Canon
| Device (2660h) | LaserBase MF3110 Scanner/Printer
| Manufacturer | Canon,Inc.
| Product | MF3110
| Serial Number | 2363E2124558
| Device Version | 0.00
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Protocol (00h) | Unknown
| Configuration |
| USB Version | 2.00
| Speed | 480 Mb/s
| Transfer Type | Bulk/Interrupt
| Data Packet Size | 64 bytes
| Max Power | 2 mA Self-Powered
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | USB Composite Device
| Device Class | USB
| Device Location | Port_#0012.Hub_#0001
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24138
| Driver Date | 6-21-2006
| Inf File | usb.inf
| Service Name | usbccgp
| Hardware ID | USB\VID_04A9&PID_2660&REV_0000
| Compatible ID | IUSB3\DevClass_00&SubClass_00&Prot_00
| Parent ID | PCI\VEN_8086&DEV_8C31&SUBSYS_50071458&REV_05
Installed Printers
| Local Printers
| Installed Printer 1
| Printer Name | Microsoft XPS Document Writer
| Printer Port | XPSPort:
| Default Printer | No
| Printer Type | Local
| Print Processor | winprint
| Data Type | RAW
| Installed Printer 2
| Printer Name | Fax
| Printer Port | SHRFAX:
| Default Printer | No
| Printer Type | Local
| Print Processor | winprint
| Data Type | RAW
| Installed Printer 3
| Printer Name | Canon MF5700 Series
| Printer Port | USB001
| Default Printer | Yes
| Printer Type | Local
| Print Processor | winprint
| Data Type | RAW
Slots (SMBIOS)
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 16x or x16
| Slot Designation | J6B2
| Slot Length | Long Length
| Slot ID | 0
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J6B1
| Slot Length | Short Length
| Slot ID | 1
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 8x or x8
| Slot Designation | J6D1
| Slot Length | Short Length
| Slot ID | 2
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 16x or x16
| Slot Designation | J7B1
| Slot Length | Short Length
| Slot ID | 3
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J8B4
| Slot Length | Short Length
| Slot ID | 4
| Slot PCI
| Slot Type | PCI
| Current Usage | In Use
| Data Bus Width | 32 bit
| Slot Designation | J8B3
| Slot Length | Short Length
| Slot ID | 6
Ports (SMBIOS)
| Port 1 Mouse Port
| Int. Connector Type | None
| Ext. Connector Type | PS/2
| Port Type | Mouse Port
| Int. Designator | J1A1
| Ext. Designator | PS2Mouse
| Port 2 Keyboard Port
| Int. Connector Type | None
| Ext. Connector Type | PS/2
| Port Type | Keyboard Port
| Int. Designator | J1A1
| Ext. Designator | Keyboard
| Port 3 Other
| Int. Connector Type | None
| Ext. Connector Type | Mini-Centronics Type-14
| Port Type | Other
| Int. Designator | J2A1
| Ext. Designator | TV Out
| Port 4 Serial Port 16550A Compatible
| Int. Connector Type | None
| Ext. Connector Type | DB-9 pin male
| Port Type | Serial Port 16550A Compatible
| Int. Designator | J2A2A
| Ext. Designator | COM A
| Port 5 Video Port
| Int. Connector Type | None
| Ext. Connector Type | DB-15 pin female
| Port Type | Video Port
| Int. Designator | J2A2B
| Ext. Designator | Video
| Port 6 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J3A1
| Ext. Designator | USB1
| Port 7 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J3A1
| Ext. Designator | USB2
| Port 8 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J3A1
| Ext. Designator | USB3
| Port 9 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9A1 - TPM HDR
| Ext. Designator |
| Port 10 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9C1 - PCIE DOCKING CONN
| Ext. Designator |
| Port 11 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J2B3 - CPU FAN
| Ext. Designator |
| Port 12 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J6C2 - EXT HDMI
| Ext. Designator |
| Port 13 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J3C1 - GMCH FAN
| Ext. Designator |
| Port 14 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J1D1 - ITP
| Ext. Designator |
| Port 15 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9E2 - MDC INTPSR
| Ext. Designator |
| Port 16 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9E4 - MDC INTPSR
| Ext. Designator |
| Port 17 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9E3 - LPC HOT DOCKING
| Ext. Designator |
| Port 18 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9E1 - SCAN MATRIX
| Ext. Designator |
| Port 19 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9G1 - LPC SIDE BAND
| Ext. Designator |
| Port 20 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J8F1 - UNIFIED
| Ext. Designator |
| Port 21 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J6F1 - LVDS
| Ext. Designator |
| Port 22 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J2F1 - LAI FAN
| Ext. Designator |
| Port 23 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J2G1 - GFX VID
| Ext. Designator |
| Port 24 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J1G6 - AC JACK
| Ext. Designator |
Network
| Network
| Network Name | A2KKV
| User Name | KKV1
| User Role | Administrator
| Logon Domain | A2KKV
| Interface 1
| Adapter Vendor | Realtek Semiconductor
| Adapter Name | RTL8111/8168/8411 PCI Express Gigabit Ethernet Controller
| Subsys Vendor | Giga-Byte Technology
| Subsystem ID | GA-EP45-DS5 Motherboard
| Bus Type | PCI Express 2.0 x1
| Description | Realtek PCIe GbE Family Controller
| MAC Address | 1C-1B-0D-B1-81-06
| Adapter Type | Ethernet
| Link Speed | 100.0 Mbps
| MTU Size | 1500 byte
| Adapter Status | Enabled
| Operational Status | Operational
| DHCP Server | 192.168.1.1
| IP Address | 192.168.1.61
| IP Address Subnet Mask | 255.255.255.0
| Gateway | 192.168.1.1
| DNS Server | 192.168.1.1
| Interface 2
| Description | VirtualBox Host-Only Ethernet Adapter
| MAC Address | 0A-00-27-00-00-10
| Adapter Type | Ethernet
| Link Speed | 1000.0 Mbps
| MTU Size | 1500 byte
| Adapter Status | Enabled
| Operational Status | Operational
| DHCP Enabled | No
| IP Address | 192.168.56.1
| IP Address Subnet Mask | 255.255.255.0
| Gateway | 0.0.0.0
Monitor
| Monitor
| Monitor Vendor | BenQ
| Monitor Model | BenQ GW2470
| Viewable Size | 23.8" (60.4 sm)
| Serial Number | 21573
| Manufacture Date | August 2016
| EDID Version | 1.3
| Monitor ID | BNQ78D9
| Aspect Ratio | 16:9
| Horizontal Size | 527 mm
| Vertical Size | 296 mm
| Gamma Factor | 2.200
| Display Type | RGB Color
| Input Signal | Digital
| Internal Model | BenQ GW2470
| Internal Number | K8G00916019
| Vertical Frequency | 50-76 Hz
| Horizontal Frequency | 30-83 kHz
| DPMS Features
| Active Off | Supported
| Suspend | Not Supported
| Standby | Not Supported
| Supported Modes
| Mode 1 | 640x480 @ 60 Hz (VGA)
| Mode 2 | 640x480 @ 75 Hz (VESA)
| Mode 3 | 720x400 @ 70 Hz (VGA)
| Mode 4 | 800x600 @ 60 Hz (VESA)
| Mode 5 | 800x600 @ 75 Hz (VESA)
| Mode 6 | 832x624 @ 75 Hz (Mac II)
| Mode 7 | 1024x768 @ 60 Hz (VESA)
| Mode 8 | 1024x768 @ 75 Hz (VESA)
| Mode 9 | 1152x870 @ 75 Hz (Mac II)
| Mode 10 | 1280x720 @ 60 Hz
| Mode 11 | 1280x800 @ 60 Hz
| Mode 12 | 1280x1024 @ 60 Hz
| Mode 13 | 1280x1024 @ 75 Hz (VESA)
| Mode 14 | 1600x900 @ 60 Hz
| Mode 15 | 1680x1050 @ 60 Hz
| Mode 16 | 1920x1080 @ 60 Hz (Recommended)
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard monitor types)
| Device Description | Generic PnP Monitor
| Device Class | Monitor
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.24521
| Driver Date | 6-21-2006
| Inf File | monitor.inf
| Service Name | monitor
| Hardware ID | MONITOR\BNQ78D9
| Compatible ID | *PNP09FF
| Parent ID | PCI\VEN_10DE&DEV_1B81&SUBSYS_119D10DE&REV_A1
Video
| Video
| Video Chip Vendor | Nvidia Corp
| Video Chip | GP104 [GeForce GTX 1070]
| Subsystem Vendor | Nvidia Corp
| Full Name | Nvidia GeForce GTX 1070
| Code Name | GP104-A
| Revision | A1h
| Video Memory Size | 8 GB
| Memory Type | 256-bit GDDR5 (Micron)
| GPU Type | Desktop Discrete
| Video BIOS Version | Version 86.04.50.00.1E
| Video BIOS Date | 10/17/16
| GPU Manufacturer | TSMC
| Unified Shaders | 1920
| Pixel Pipelines (ROPS) | 64
| Current Resolution | 1920x1080 32bpp @ 75 Hz
| Driver Version | R442.19
| Bus Type | PCI Express 3.0 x16
| Base Clocks
| Base Core Clock | 1556 MHz
| Base Memory Clock | 2002 MHz (Effective: 8008 MHz)
| Memory Bandwidth | 256.3 GB/s
| Boost Clocks
| Boost Core Clock | 1746 MHz
| Boost Memory Clock | 2002 MHz (Effective: 8008 MHz)
| Memory Bandwidth | 256.3 GB/s
| Hardware Monitoring
| Core Temperature | 36 °C (97 °F)
| Current Core Clock | 139 MHz
| Current Memory Clock | 202 MHz (Effective: 808 MHz)
| Core Usage | 0 %
| Memory Usage | 2 %
| Memory Controller Usage | 3 %
| Video Engine Usage | 0 %
| Bus Interface Load | 0 %
| Fan Speed | 0 rpm
| Fan Speed | 0 %
| Performance Profile 0
| Core Clock | 1962 MHz
| Memory Clock | 2002 MHz
| Performance Profile 2
| Core Clock | 3802 MHz
| Memory Clock | 1901 MHz
| Performance Profile 5
| Core Clock | 139 MHz
| Memory Clock | 405 MHz
| Performance Profile 8
| Core Clock | 139 MHz
| Memory Clock | 202 MHz
| PCI-E Capabilities
| PCI Express Version | 3.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 8.0 GB/s (Current: 2.5 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | NVIDIA
| Device Description | NVIDIA GeForce GTX 1070
| Device Class | Display
| Device Location | PCI bus 1, device 0, function 0
| Driver Provider | NVIDIA
| Driver Version | 26.21.14.4219
| Driver Date | 1-29-2020
| Inf File | oem15.inf
| Service Name | nvlddmkm
| Hardware ID | PCI\VEN_10DE&DEV_1B81&SUBSYS_119D10DE&REV_A1
| Compatible ID | PCI\VEN_10DE&DEV_1B81&REV_A1
| Parent ID | PCI\VEN_8086&DEV_0C01&SUBSYS_50001458&REV_06
Hardware Monitoring
| Processor
| Processor | Intel Xeon E3-1246 v3 3500 MHz
| Core Voltage | 0.754 V
| Package Temperature | 39 °C (102 °F)
| Core 1
| Temperature Core | 38 °C (100 °F)
| Core Clock | 798.2 MHz (Original: 3500 MHz)
| FSB Clock | 99.8 MHz
| Multiplier | 8.0
| Core 2
| Temperature Core | 36 °C (97 °F)
| Core Clock | 798.2 MHz (Original: 3500 MHz)
| FSB Clock | 99.8 MHz
| Multiplier | 8.0
| Core 3
| Temperature Core | 36 °C (97 °F)
| Core Clock | 798.2 MHz (Original: 3500 MHz)
| FSB Clock | 99.8 MHz
| Multiplier | 8.0
| Core 4
| Temperature Core | 38 °C (100 °F)
| Core Clock | 798.2 MHz (Original: 3500 MHz)
| FSB Clock | 99.8 MHz
| Multiplier | 8.0
| Video Card
| Video Chip | GP104 [GeForce GTX 1070]
| Core Temperature | 36 °C (97 °F)
| Current Core Clock | 139 MHz (Original: 1556 MHz)
| Current Memory Clock | 202 MHz (Original: 2002 MHz)
| Core Usage | 0 %
| Memory Usage | 2 %
| Memory Controller Usage | 3 %
| Video Engine Usage | 0 %
| Bus Interface Load | 0 %
| Fan Speed | 0 rpm
| Fan Speed | 0 %
| Disk Drive 1
| Disk Model | SPCC Solid State Disk
| Disk Temperature | 33 °C (91 °F)
| Total Host Writes | 3.31 TB
| Disk Drive 2
| Disk Model | WDC WD1001FALS-00J7B0
| Disk Temperature | 42 °C (108 °F)
| Disk Drive 3
| Disk Model | Samsung SSD 860 EVO 250GB
| Disk Temperature | 39 °C (102 °F)
| Total Host Writes | 6.58 TB
| Disk Drive 4
| Disk Model | ST3500412AS
| Disk Temperature | 35 °C (95 °F)
| Total Host Writes | 1.02 TB
| Total Host Reads | 789.29 GB
Drivers Troubleshooter
| List of Problem Devices
| All devices are working properly
Disk Diagnostics
| Disk 1 Status
| Disk Model | SPCC Solid State Disk
| Disk Size | 114473 MB (111.79 GB)
| Interface Type | Serial ATA III (SATA/600)
| Serial Number | 2A40079618DB00135162
| Controller Revision | SBFM61.3
| Disk Marketing Size | 120034 MB (120.03 GB)
| Buffer Size | Unknown
| Location (Vendor) | Intel Corporation
| Location (Device) | 8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
| Device Location | Secondary/Master
| Disk Temperature | 33 °C (91 °F)
| Disk Health Status | Good
| SSD Remaining Life | 100 %
| Total Host Writes | 3.31 TB
| Disk 2 Status
| Disk Model | WDC WD1001FALS-00J7B0
| Disk Size | 953869 MB (931.51 GB)
| Interface Type | Serial ATA II (SATA/300)
| Serial Number | WD-WMATV0357962
| Controller Revision | 05.00K05
| Disk Marketing Size | 1000204 MB (1000.2 GB)
| Buffer Size | 32767.5 kB
| Location (Vendor) | Intel Corporation
| Location (Device) | 8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
| Device Location | 8th/Slave
| Disk Temperature | 42 °C (108 °F)
| Reallocated Sectors | 0
| Disk Health Status | Good
| Disk 3 Status
| Disk Model | Samsung SSD 860 EVO 250GB
| Disk Size | 238475 MB (232.89 GB)
| Interface Type | Serial ATA III (SATA/600)
| Serial Number | S3Y9NB0K275545B
| Controller Revision | RVT01B6Q
| Disk Marketing Size | 250059 MB (250.06 GB)
| Buffer Size | Unknown
| Location (Vendor) | Intel Corporation
| Location (Device) | 8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
| Device Location | 8th/Slave
| Disk Temperature | 39 °C (102 °F)
| Reallocated Sectors | 0
| Disk Health Status | Good
| SSD Remaining Life | 100 %
| Total Host Writes | 6.58 TB
| Disk 4 Status
| Disk Model | ST3500412AS
| Disk Size | 476940 MB (465.76 GB)
| Interface Type | Serial ATA II (SATA/300)
| Serial Number | 6VV25CDT
| Controller Revision | CC32
| Disk Marketing Size | 500108 MB (500.11 GB)
| Buffer Size | 16384.0 kB
| Location (Vendor) | Intel Corporation
| Location (Device) | 8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
| Device Location | 8th/Slave
| Disk Temperature | 35 °C (95 °F)
| Reallocated Sectors | 1991
| Disk Health Status | Bad
| Total Host Writes | 1.02 TB
| Total Host Reads | 789.29 GB
Windows
| Windows
| Operating System | MS Windows 7 Professional x64 Edition (6.1.7601 Service Pack 1)
| OS Language | English (United States)
| Windows Folder | G:\Windows
| Installation Date | February 10, 2020
| Kernel Type | Multiprocessor Free
| Registered Owner | KKV1
| Registered Organization |
| Product ID | 00371-OEM-8992671-00407
| Product Key | XXXXX-XXXXX-XXXXX-XXXXX-XXXXX
| System UpTime | 0 Hour(s) 15 Minutes 7 Seconds
| IE Version | 9.11.9600.19596
| DirectX Version | DirectX 11
| Regional Settings
| Country | Russia
| Language | Russian
| Time Zone | Romance Standard Time (GMT+3)
| Currency Name | Russian Ruble
| Measurment System | Metric
| ANSI Code Page | 1251
| OEM Code Page | 866
Installed Programs
| Installed Programs
| Program Name | Version | Publisher | Date | Size |
| ASTRA32 - Advanced System Information Tool | 3.81 | Sysinfo Lab |  |  |
Installed Hotfixes
| Installed Hotfixes
| Hotfix for Microsoft Windows (KB2496898) |
| Hotfix for Microsoft Windows (KB2990941) |
| Hotfix for Microsoft Windows (KB3006137) |