  +------------------------------------------------------------------------+
  |    This report is created by ASTRA32 v.3.81     Dec-23-2020 14:45:09   |
  +------------------------------------------------------------------------+
                                   A2KKV
                                   
     Registered To:                Sysinfo Lab
     License Type:                 Professional for 1 computer
                                   
     Disabled Tests:               UDMA
                  +-----------------------------------------+
                  |              System Summary             |
                  +-----------------------------------------+
  Processor 
     Processor:                    Intel Xeon E3-1246 v3 3500 MHz
     CPU Clock:                    3491.9 MHz (35.0 x 99.8 MHz)
     Level 1 Cache:                4 x 32 kB + 4 x 32 kB (data+instr.)
     Level 2 Cache:                4 x 256 kB
     Level 3 Cache:                1 x 8 MB
  Motherboard
     System Name:                  Gigabyte Technology Co., Ltd. B85M-D3V-A
     Board Model:                  Gigabyte Technology Co., Ltd. B85M-D3V-A
     BIOS Version:                 AMI BIOS 08.00.10
     Chipset Name:                 Intel B85 (Lynx Point)
     Northbridge Vendor:           Intel Corporation
     Northbridge:                  Xeon E3-1200 v3 Processor DRAM Controller
     Southbridge Vendor:           Intel Corporation
     Southbridge:                  B85 Express LPC Controller
     DMI/SMBIOS Version:           2.7
  Memory
     Memory Size:                  15.97 GB
     System Memory:                16350 MB
     Memory Module:                8 GB DDR3-1866 (PC3-14900) SDRAM (Kllisre)
     Memory Module:                8 GB DDR3-1866 (PC3-14900) SDRAM (Kingston)
  Storage
     Disk Model:                   SPCC Solid State Disk
     Disk Size:                    114473 MB (111.79 GB)
     Disk Model:                   WDC WD1001FALS-00J7B0
     Disk Size:                    953869 MB (931.51 GB)
     Disk Model:                   Samsung SSD 860 EVO 250GB
     Disk Size:                    238475 MB (232.89 GB)
     Disk Model:                   ST3500412AS
     Disk Size:                    476940 MB (465.76 GB)
     CD/DVD Model:                 PIONEER DVD-RW  DVR-217F
     CD/DVD Speed:                 16x (Write: 40x)
  Video
     Monitor Vendor:               BenQ
     Monitor Model:                BenQ GW2470
     Video Chip Vendor:            Nvidia Corp
     Video Chip:                   GP104 [GeForce GTX 1070]
     Video Memory Size:            8 GB GDDR5 (Micron)
  Sound
     Sound Chip Vendor:            Intel Corporation
     Sound Chip:                   8 Series/C220 Series Chipset Family HD Audio Controller
     Sound Chip Vendor:            Nvidia Corp
     Sound Chip:                   GP104 High Definition Audio Controller
     AC'97/HDA Codec Name:         NVidia GPU GP104 HDMI/DP
     Sound Chip Vendor:            VIA Technologies Inc (Was: IC Ensemble Inc)
     Sound Chip:                   VT1720/4 Envy24PT PCI Multi-Channel Audio Controller
  Printer
     Printer Vendor:               Canon
     Printer Model:                LaserBase MF3110 Scanner/Printer
  Operating System
     Operating System:             MS Windows 7 Professional x64 Edition (6.1.7601 Service Pack 1)
     Windows Folder:               G:\Windows
  Modem
     Modem Vendor:                 Intel Corporation
     Modem Model:                  8 Series/C220 Series Chipset Family MEI Controller #1
  Network
     Network Name:                 A2KKV
     Adapter Vendor:               Realtek Semiconductor
     Adapter Name:                 RTL8111/8168/8411 PCI Express Gigabit Ethernet Controller
     Interface Description:        Realtek PCIe GbE Family Controller
     MAC Address:                  1C-1B-0D-B1-81-06
     Interface Description:        VirtualBox Host-Only Ethernet Adapter
     MAC Address:                  0A-00-27-00-00-10
  Ports
     LPT Ports:                    LPT1(0378h) 
     COM Ports:                    COM1(03F8h) 
                                   
                  +-----------------------------------------+
                  |               Motherboard               |
                  +-----------------------------------------+
  System
     System Vendor:                Gigabyte Technology Co., Ltd.
     Product Name:                 B85M-D3V-A
     Version:                      To be filled by O.E.M.
     Serial Number:                To be filled by O.E.M.
     UUID:                         1C021B030D04B1058106060700080009
     Wake-up Type:                 Power Switch
     SKU Number:                   To be filled by O.E.M.
     Family:                       To be filled by O.E.M.
  Motherboard
     Motherboard Vendor:           Unknown (0001)
     Vendor URL:                   Unknown
     Board Model:                  Gigabyte Technology Co., Ltd. B85M-D3V-A
     Version:                      x.x
     Serial Number:                To be filled by O.E.M.
     Asset Tag:                    To be filled by O.E.M.
     BIOS Version:                 AMI BIOS 08.00.10
     BIOS Date:                    04/13/12
     Chipset Name:                 Intel B85 (Lynx Point)
     Northbridge Vendor:           Intel Corporation
     Northbridge:                  Xeon E3-1200 v3 Processor DRAM Controller
     Southbridge Vendor:           Intel Corporation
     Southbridge:                  B85 Express LPC Controller
  Onboard Device 1
     Description:                  To Be Filled By O.E.M.
     Device Type:                  Video
     Status:                       Enabled
  Onboard Device 2
     Description:                  Onboard LAN
     Device Type:                  Ethernet
     Status:                       Enabled
  Configuration Options
     To Be Filled By O.E.M.
  System Enclosure
     Manufacturer:                 Gigabyte Technology Co., Ltd.
     Type:                         Desktop
     Version:                      To Be Filled By O.E.M.
     Serial Number:                To Be Filled By O.E.M.
     Asset Tag:                    To Be Filled By O.E.M.
     Boot-up State:                Safe
     Power Supply State:           Safe
     Thermal State:                Safe
     Security Status:              None
     OEM-defined:                  00000000h
     Height:                       0.0 sm
     Power Cords:                  1
     Contained Element:            0
                                   
                  +-----------------------------------------+
                  |                  CPU                    |
                  +-----------------------------------------+
  CPU 
     Processor:                    Intel Xeon E3-1246 v3 3500 MHz
     Coprocessor:                  Internal
     CPU Clock:                    3491.9 MHz
     Level 1 Cache:                4 x 32 kB + 4 x 32 kB (data+instr.)
     Level 2 Cache:                4 x 256 kB
     Level 3 Cache:                1 x 8 MB
     Code Name:                    Haswell-WS
     Manufacturing Process:        22 nm
     FSB Clock:                    99.8 MHz
     Multiplier:                   35.0
     Expected Clock:               3500 MHz
     Overclocking Support:         Not Supported
     Max Turbo Clock:              3900.0 MHz
     Turbo Boost:                  2/3/4/4 (Enabled)
     Turbo Clock (1-2 core):       3900 MHz
     Turbo Clock (3 core):         3800 MHz
     Turbo Clock (4 core):         3700 MHz
     Socket Type:                  Socket 1150 FCLGA
     Package Temperature:          39 °C (102 °F)
     Temperature Core 1:           38 °C (100 °F)
     Temperature Core 2:           36 °C (97 °F)
     Temperature Core 3:           36 °C (97 °F)
     Temperature Core 4:           38 °C (100 °F)
     Maximum Temperature (Tjmax):  100 °C (212 °F)
     Core Voltage:                 1.096 V
     Vendor:                       GenuineIntel
     Processor Name:               Intel(R) Xeon(R) CPU E3-1246 v3 @ 3.50GHz
     Processor Type:               Original OEM Processor
     CPUID:                        Family: 6, Model: 12, Stepping: 3
     Ext. Family/Model:            Family: -, Model: 3
     CPU Signature:                000306C3h
     Number of Cores:              4
     Logical Cores Count:          8
     Core Stepping:                C-0
     sSpec Number:                 SR1QZ
     Microcode Revision:           1Ch
     Max TDP:                      84 Wattes
     Power Limit 1 (Time):         84.0 Wattes (Unlimited)
     Power Limit 2 (Time):         105.0 Wattes (Unlimited)
     Internal Graphics:            Intel HD Graphics (Disabled)
     Transistor Count:             1400 million
     Die Size:                     177 mm2
     Launch Date:                  May, 2014
     Recommended Price (USD):      $276
  Instruction Set
     Floating-Point Unit On-Chip:             [X]
     IA MMX Technology:                       [X]
     SSE Instruction Set:                     [X]
     SSE2 Instruction Set:                    [X]
     SSE3 Instruction Set:                    [X]
     Supplemental SSE3 Instruction Set:       [X]
     SSE4.1 Instruction Set:                  [X]
     SSE4.2 Instruction Set:                  [X]
     Advanced Vector Extensions (AVX):        [X]
     Advanced Vector Extensions 2 (AVX2):     [X]
     AVX-512 Foundation Instructions:         [ ]
     AVX-512 Prefetch Instructions:           [ ]
     AVX-512 Exponential and Reciprocal:      [ ]
     AVX-512 Conflict Detection:              [ ]
     AVX-512 Byte and Word Instructions:      [ ]
     AVX-512 Doubleword and Quadword:         [ ]
     AVX-512 Vector Length Extensions:        [ ]
     AVX-512 Integer Fused Multiply-Add:      [ ]
     AVX-512 Vector Bit Manipulation:         [ ]
     AVX-512 QVNNI Instructions:              [ ]
     AVX-512 QFMA Instructions:               [ ]
     AVX-512 VBMI2 Instructions:              [ ]
     AVX-512 VNNI Instructions:               [ ]
     AVX-512 BITALG Instructions:             [ ]
     Galois Field NI/Affine Transformation:   [ ]
     VEX-encoded AES-NI (VAES):               [ ]
     VEX-encoded PCLMUL (VPCL):               [ ]
     PCOMMIT Instruction:                     [ ]
     CLWB Instruction:                        [ ]
     PREFETCHWT1 Instruction:                 [ ]
     Software Guard Extensions (SGX):         [ ]
     SGX Launch Configuration:                [ ]
     FMA Instructions Set:                    [X]
     AES Instructions Set:                    [X]
     Intel Extended Memory 64 Tech.:          [X]
     Intel Architecture - 64 (IA-64):         [ ]
     AMD MMX Instruction Extensions:          [ ]
     AMD 3DNow! Instructions:                 [ ]
     AMD 3DNow! Extensions:                   [ ]
     AMD 3DNow! Prefetch:                     [ ]
     AMD SSE4A Extensions:                    [ ]
     AMD eXtended OPeration (XOP):            [ ]
     AMD Misaligned SSE:                      [ ]
     AMD64 Architecture:                      [ ]
     Cyrix Extended MMX:                      [ ]
     CMPXCHG8 Instruction Supported:          [X]
     CMPXCHG16 Instruction Supported:         [X]
     Fast System Call:                        [X]
     Conditional Move Instruction:            [X]
     CLFLUSH Insruction Supported:            [X]
     Fast Save and Restore:                   [X]
     Monitor/MWAIT Instructions:              [X]
     SYSCALL/SYSRET Instructions:             [ ]
     LAHF/SAHF Instructions:                  [X]
     POPCNT Insruction Supported:             [X]
     XSAVE Insructions Supported:             [X]
     OS Supports XSAVE Instructions:          [X]
     PCLMULQDQ Instruction Supported:         [X]
     MOVBE Insruction Supported:              [X]
     F16C Insruction Supported:               [X]
     RDTSCP Insruction Supported:             [X]
     RDRAND Insruction Supported:             [X]
     (RD/WR)(FS/GS) BASE Instructions:        [X]
     Bit Manipulation 1 Instructions:         [X]
     Bit Manipulation 1 Instructions:         [X]
     Enhanced REP MOVSB/STOSB:                [X]
     INVPCID Instruction:                     [X]
     XSAVEOPT Instruction:                    [X]
     RDSEED Instruction:                      [ ]
     ADCX/ADOX Instructions:                  [ ]
     CLAC/STAC Instructions:                  [ ]
     SCLFLUSHOPT Instruction:                 [ ]
     RDPID Instruction:                       [ ]
     VPOPCNT[D/Q] Instructions:               [ ]
     Fast Short REP MOV Instruction:          [ ]
     PCONFIG Instruction:                     [ ]
     WBNOINVD Instruction:                    [ ]
     WaitPKG Instructions:                    [ ]
     CLDEMOTE Instruction:                    [ ]
     MOVDIRI Instruction:                     [ ]
     MOVDIRI64B Instruction:                  [ ]
     RDPRU Instruction:                       [ ]
     MCOMMIT Instruction:                     [ ]
     AMD Fast Save and Restore:               [ ]
     AMD SKINIT, STGI, DEV Supported:         [ ]
     AMD Light Weight Profiling (LWP):        [ ]
     AMD FMA4 Insruction Supported:           [ ]
     AMD TBM Insruction Supported:            [ ]
     AMD MONITORX/MWAITX Instructions:        [ ]
     AMD CLZERO Instruction:                  [ ]
  Processor Features
     Hypervisor Present:                      [ ]
     Virtual Mode Extension:                  [X]
     Debugging Extension:                     [X]
     Page Size Extension:                     [X]
     Time Stamp Counter:                      [X]
     Model Specific Registers:                [X]
     Physical Address Extension:              [X]
     Machine Check Exception:                 [X]
     On-chip APIC Hardware Supported:         [X]
     Memory Type Range Registers:             [X]
     Page Global Enable:                      [X]
     Machine Check Architecture:              [X]
     Page Attribute Table:                    [X]
     36-bit Page Size Extension:              [X]
     Processor Serial Number:                 [ ]
     Debug Store:                             [X]
     64-bit Debug Store:                      [X]
     Self-Snoop:                              [X]
     Hyper-Threading Technology:              [X]
     Pending Break Enable:                    [X]
     CPL-Qualified Debug Store:               [X]
     L1 Context ID:                           [ ]
     Send Task Priority Messages:             [X]
     Direct Cache Access:                     [ ]
     Performance Capabilities MSR:            [X]
     x2APIC Architecture:                     [X]
     Advanced Bit Manipulation:               [X]
     OS Visible Workaround:                   [ ]
     Instruction Based Sampling:              [ ]
     1-GB Large Page:                         [X]
     Process Context Identifiers:             [X]
     Time Stamp Counter Deadline:             [X]
     Time Stamp Counter Adjust:               [X]
     Intel Virtualization Technology:         [X]
     Intel Trusted Execution Technology:      [X]
     Supervisor Mode Execution Protection:    [X]
     Hardware Lock Elision:                   [ ]
     Restricted Transactional Memory:         [ ]
     Quality of Service Monitoring:           [ ]
     Quality of Service Enforcement:          [ ]
     Deprecated FPU CS and FPU DS:            [X]
     Memory Protection Extensions (MPX):      [ ]
     Processor Trace (PT):                    [ ]
     Secure Hash Algorithm Ext. (SHA):        [ ]
     Debug Interface MSR:                     [X]
     User-Mode Instruction Prevention:        [ ]
     Protection Keys for User-Mode Pages:     [ ]
     5 Level Page Table:                      [ ]
     Total Memory Encryption (TME):           [ ]
     Speculation Control (IBRS and IBPB):     [ ]
     Single Thread Indirect Branch Predictors:[ ]
     L1 Data Cache (L1D) Flush:               [ ]
     ARCH_CAPABILITIES MSR:                   [ ]
     Speculative Store Bypass Disable (SSBD): [ ]
     Intel Turbo Boost Technology:            [X] enabled
     Intel Turbo Boost Max Technology 3.0:    [ ]
     Intel Execute Disable Bit:               [X]
     Hybrid Processor:                        [ ]
     AMD Secure Virtual Machine:              [ ]
     AMD Model-Specific Registers:            [ ]
     AMD Multiprocessing Capable:             [ ]
     AMD CMP Legacy Mode:                     [ ]
     AMD CR8 in Legacy Mode:                  [ ]
     AMD Ext. APIC Register Space:            [ ]
     AMD Watchdog Timer:                      [ ]
     AMD Translation Cache Extension:         [ ]
     AMD Topology Extensions:                 [ ]
     AMD Core Performance Counter Ext.:       [ ]
     AMD NB Performance Counter Ext.:         [ ]
     AMD Streaming Performance Monitor:       [ ]
     AMD Data Breakpoint Extension:           [ ]
     AMD Performance TSC:                     [ ]
     AMD L2I Performance Counter Ext.:        [ ]
     AMD IRPERF Performance Counter:          [ ]
     AMD Always Save/Restore FP Error Pointers:[ ]
     AMD Indirect Branch Prediction Barrier:  [ ]
     AMD Indirect Branch Restricted Speculation:[ ]
     AMD IBRS Always On Mode:                 [ ]
     AMD IBRS Preferred:                      [ ]
     AMD Single Thread Indirect Branch Predictor:[ ]
     AMD STIBP Always On Mode:                [ ]
     AMD Speculative Store Bypass Disable (SSBD):[ ]
     AMD SSBD Not Needed:                     [ ]
     AMD VIRT_SPEC_CTRL MSR:                  [ ]
  Power Management
     ACPI Supported:                          [X]
     Thermal Monitor Supported:               [X]
     Thermal Monitor 2:                       [X]
     Enhanced SpeedStep Technology:           [X]
     Digital Thermal Sensor:                  [X]
     Always Running APIC Timer:               [X]
     Invariant TSC:                           [X]
     Power Limit Notification:                [X]
     Extended Clock Modulation Duty:          [X]
     Package Thermal Management:              [X]
     Hardware Coordination Feedback:          [X]
     ACNT2 Capability:                        [ ]
     Performance-Energy Bias:                 [ ]
     Hardware-Managed P-State Base Support:   [ ]
     Hardware Duty Cycle Programming (HDC):   [ ]
     AMD Temperature Sensor:                  [ ]
     AMD Frequency ID Control:                [ ]
     AMD Voltage ID Control:                  [ ]
     AMD Thermal Trip:                        [ ]
     AMD Thermal Monitoring:                  [ ]
     AMD Software Thermal Control:            [ ]
     AMD 100MHz Multiplier Steps:             [ ]
     AMD Hardware P-State Control:            [ ]
     AMD Effective Frequency Interface:       [ ]
     AMD Processor Feedback Interface:        [ ]
     AMD Processor Accumulator:               [ ]
     AMD Connected Standby:                   [ ]
     AMD Running Average Power Limit:         [ ]
     AMD MCA Overflow Recovery:               [ ]
     AMD Software Uncorr. Error Containment/Recovery:[ ]
     AMD Hardware Assert (HWA):               [ ]
     AMD Scalable MCA:                        [ ]
                                   
                  +-----------------------------------------+
                  |                CPU Cache                |
                  +-----------------------------------------+
  Level 1 Instruction Cache
     Size:                         4 x 32 kB
     Associativity:                8-way
     Line Size:                    64 byte
     TLB 4K Pages:                 
       Number of Entries:          64
       Associativity:              8-way
     TLB 2/4M Pages:               
       Number of Entries:          8
       Associativity:              full
  Level 1 Data Cache
     Size:                         4 x 32 kB
     Associativity:                8-way
     Line Size:                    64 byte
     TLB 4K Pages:                 
       Number of Entries:          1024
       Associativity:              8-way
     TLB 2/4M Pages:               
       Number of Entries:          1024
       Associativity:              8-way
  Level 2 Cache
     Size:                         4 x 256 kB
     Associativity:                8-way
     Line Size:                    64 byte
  Level 3 Cache
     Size:                         1 x 8 MB
     Associativity:                16-way
     Line Size:                    64 byte
                                   
                  +-----------------------------------------+
                  |              CPU (SMBIOS)               |
                  +-----------------------------------------+
  Processor 
     Processor Vendor:             Intel
     Processor Version:            Intel(R) Xeon(R) CPU E3-1246 v3 @ 3.50GHz
     Current Speed:                3700 MHz
     External Clock:               100 MHz
     Voltage:                      1.0 V
     Processor Upgrade:            Other
     Processor Status:             CPU Enabled
     Socket Designation:           SOCKET 0
     Processor Type:               Central Processor
     Processor Family:             Intel Xeon
     Processor ID1:                000306C3h
     Processor ID2:                BFEBFBFFh
     Max Speed:                    7000 MHz
     Socket Status:                CPU Socket Populated
     Serial Number:                
     Asset Tag:                    Fill By OEM
     Part Number:                  Fill By OEM
     CPU Core Count:               4 (Enabled: 1)
     CPU Thread Count:             2
     Structure Length:             2Ah
                                   
                  +-----------------------------------------+
                  |            CPU (SMBIOS) Cache           |
                  +-----------------------------------------+
  Level 1 Cache
     Installed Size:               256 kB
     Operational Mode:             Write Back
     Current SRAM Type:            Unknown
     Status:                       Enabled
     Socket Designation:           CPU Internal L1
     Cache Socketed:               Not Socketed
     Location:                     Internal
     Maximum Cache Size:           256 kB
     Supported SRAM Type:          Unknown
     Cache Speed:                  Unknown
     Error Correction:             Single-bit ECC
     System Cache Type:            Other
     Associativity:                8-way Set-Associative
     Structure Length:             13h
  Level 2 Cache
     Installed Size:               1 MB
     Operational Mode:             Write Back
     Current SRAM Type:            Unknown
     Status:                       Enabled
     Socket Designation:           CPU Internal L2
     Cache Socketed:               Not Socketed
     Location:                     Internal
     Maximum Cache Size:           1 MB
     Supported SRAM Type:          Unknown
     Cache Speed:                  Unknown
     Error Correction:             Single-bit ECC
     System Cache Type:            Unified
     Associativity:                8-way Set-Associative
     Structure Length:             13h
  Level 3 Cache
     Installed Size:               8 MB
     Operational Mode:             Write Back
     Current SRAM Type:            Unknown
     Status:                       Enabled
     Socket Designation:           CPU Internal L3
     Cache Socketed:               Not Socketed
     Location:                     Internal
     Maximum Cache Size:           8 MB
     Supported SRAM Type:          Unknown
     Cache Speed:                  Unknown
     Error Correction:             Single-bit ECC
     System Cache Type:            Unified
     Associativity:                16-way Set-Associative
     Structure Length:             13h
                                   
                  +-----------------------------------------+
                  |                  BIOS                   |
                  +-----------------------------------------+
  BIOS
     Motherboard Vendor:           Unknown (0001)
     Vendor URL:                   Unknown
     BIOS Version:                 AMI BIOS 08.00.10
     BIOS Date:                    04/13/12
     BIOS Copyright:               04/13/12(C)2010 American Megatrends, Inc. All Rights Reserved
     Motherboard ID:               BIOS Date: 08/24/16 16:14:27 Ver: 04.06.05
     BIOS ID:                      63-0100-000001-00101111-041312-Chipset
     BIOS Size:                    512 kB
     Processor:                    686
     Chipset ID:                   Chipset
     BIOS Revision:                0100
     MP Specification Ver.:        1.4
     MP Table Address:             000Fh:D450h
     Number of CPU/Cores:          4
     DMI/SMBIOS Version:           2.7
     DMI/SMBIOS Structures:        77
  SMBIOS
     BIOS Vendor:                  American Megatrends Inc.
     BIOS Version:                 F4a
     BIOS Date:                    08/24/2016
     BIOS ROM Size:                4 MB
     System BIOS Version:          4.6
     Starting Segment:             F000h
     Current Language:             en|US|iso8859-1
     Number of Languages:          4
     Structure Length:             18h
  Bus Supported
     PCI is Supported:                    [X]
     AGP is Supported:                    [ ]
     USB is Supported:                    [X]
     ISA is Supported:                    [ ]
     VLBus is Supported:                  [ ]
     MCA is Supported:                    [ ]
     EISA is Supported:                   [ ]
     PC Card is Supported:                [ ]
  Boot Options
     Selectable Boot:                     [X]
     Boot From CD:                        [X]
     ATAPI ZIP Drive Boot:                [ ]
     LS-120 Boot:                         [ ]
     BIOS Boot Specification:             [X]
     Boot From PC Card:                   [ ]
     Network Service Boot Supported:      [ ]
     I2O Boot:                            [ ]
     1394 Boot:                           [ ]
  BIOS Features
     BIOS Characteristics:                [X]
     ACPI Supported:                      [X]
     PnP is Supported:                    [ ]
     APM is Supported:                    [ ]
     ESCD Support:                        [ ]
     Enhanced Disk Drive (EDD):           [X]
     BIOS is Upgradeable (Flash):         [X]
     BIOS ROM is Socketed:                [X]
     BIOS Shadowing is Allowed:           [X]
     Smart Battery Supported:             [ ]
     Targeted Content Distribution:       [X]
     UEFI Specification is Supported:     [X]
     Virtual Machine:                     [ ]
     Int 13h - 5.25"/360kB Floppy:        [ ]
     Int 13h - 5.25"/1.2MB Floppy:        [X]
     Int 13h - 3.5"/720kB Floppy:         [X]
     Int 13h - 3.5"/2.88MB Floppy:        [X]
     Int 5h, Print Screen Service:        [X]
     Int 9h, 8042 Keyboard Services:      [X]
     Int 14h, Serial Services:            [X]
     Int 17h, Printer Services:           [X]
     Int 10h, CGA/Mono Video Services:    [ ]
     Int 13h - Floppy for NEC 9800:       [ ]
     Int 13h - Floppy for Toshiba:        [ ]
     NEC PC-98:                           [ ]
  OEM SMBIOS Strings
     To Be Filled By O.E.M.
     To Be Filled By O.E.M.
     To Be Filled By O.E.M.
     To Be Filled By O.E.M.
     To Be Filled By O.E.M.
  Other SMBIOS Structures
     Hardware Security (24)
     System Boot Information (32)
     Management Device (34)
     Voltage Probe (26)
     Management Device Threshold Data (36)
     Management Device Component (35)
     Temperature Probe (28)
     Management Device Threshold Data (36)
     Management Device Component (35)
     Cooling Device (27)
     Management Device Threshold Data (36)
     Management Device Component (35)
     Cooling Device (27)
     Management Device Threshold Data (36)
     Management Device Component (35)
     Electrical Current Probe (29)
     Management Device Threshold Data (36)
     Management Device Component (35)
     Voltage Probe (26)
     Temperature Probe (28)
     Cooling Device (27)
     Electrical Current Probe (29)
     System Power Supply (39)
     Memory Device Mapped Address (20)
     Memory Device Mapped Address (20)
     Memory Array Mapped Address (19)
     Unknown (136)
     Unknown (131)
                                   
                  +-----------------------------------------+
                  |             PCI/AGP Devices             |
                  +-----------------------------------------+
  Bus: 00h, Device: 00h, Function: 00h         
     Vendor (8086h):               Intel Corporation
     Device (0C08h):               Xeon E3-1200 v3 Processor DRAM Controller
     Subsys Vendor (1458h):        Giga-Byte Technology
     Subsystem ID (5000h):         Unknown
     Class (06h):                  Bridge
     SubClass (00h):               PCI/CPU
     Revision:                     06h
     Interface:                    00h
  Device Properties
     Device Timing:                Fast
     Memory Access:                [X]
     I/O Access:                   [ ]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard system devices)
     Device Description:           PCI standard host CPU bridge
     Device Class:                 System
     Device Location:              PCI bus 0, device 0, function 0
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24441
     Driver Date:                  6-21-2006
     Inf File:                     machine.inf
     Hardware ID:                  PCI\VEN_8086&DEV_0C08&SUBSYS_50001458&REV_06
     Compatible ID:                PCI\VEN_8086&DEV_0C08&REV_06
     Parent ID:                    ACPI_HAL\PNP0C08
                                   
  Bus: 00h, Device: 01h, Function: 00h         
     Vendor (8086h):               Intel Corporation
     Device (0C01h):               4th Gen Core/Xeon E3-1200 v3 Processor PCI Express x16 Controller
     Class (06h):                  Bridge
     SubClass (04h):               PCI/PCI
     Revision:                     06h
     Interface:                    00h
  Device Properties
     Device Timing:                Fast
     Memory Access:                [X]
     I/O Access:                   [X]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Base I/O Port:                E000h - EFFFh
     Memory Address:               F6000000h - F70FFFFFh
     Memory Address:               E0000000h - F1FFFFFFh
     System IRQ:                   16
     Interrupt Pin:                INTA#
  PCI-E Capabilities
     PCI Express Version:          3.0
     Device/Port Type:             Root Port of PCI-E Root Complex
     Link Speed:                   8.0 GB/s (Current: 2.5 GB/s)
     Link Width:                   x16 (Current: x16)
     Link Port Number:             2
     Physical Slot Number:         0
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard system devices)
     Device Description:           PCI standard PCI-to-PCI bridge
     Device Class:                 System
     Device Location:              PCI bus 0, device 1, function 0
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24441
     Driver Date:                  6-21-2006
     Inf File:                     machine.inf
     Service Name:                 pci
     Hardware ID:                  PCI\VEN_8086&DEV_0C01&SUBSYS_50001458&REV_06
     Compatible ID:                PCI\VEN_8086&DEV_0C01&REV_06
     Parent ID:                    ACPI_HAL\PNP0C08
                                   
  Bus: 00h, Device: 14h, Function: 00h         
     Vendor (8086h):               Intel Corporation
     Device (8C31h):               8 Series/C220 Series Chipset Family USB xHCI Host Controller
     Subsys Vendor (1458h):        Giga-Byte Technology
     Subsystem ID (5007h):         Unknown
     Class (0Ch):                  Serial
     SubClass (03h):               USB
     Revision:                     05h
     Interface:                    30h
  Device Properties
     Device Timing:                Medium
     Memory Access:                [X]
     I/O Access:                   [ ]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Memory Address:               F7200000h - F720FFFFh
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 Intel(R) Corporation
     Device Description:           Intel(R) USB 3.0 eXtensible Host Controller
     Device Class:                 USB
     Device Location:              PCI bus 0, device 20, function 0
     Driver Provider:              Intel(R) Corporation
     Driver Version:               5.0.4.43
     Driver Date:                  5-11-2017
     Inf File:                     oem36.inf
     Service Name:                 iusb3xhc
     Hardware ID:                  PCI\VEN_8086&DEV_8C31&SUBSYS_50071458&REV_05
     Compatible ID:                PCI\VEN_8086&DEV_8C31&REV_05
     Parent ID:                    ACPI_HAL\PNP0C08
                                   
  Bus: 00h, Device: 16h, Function: 00h         
     Vendor (8086h):               Intel Corporation
     Device (8C3Ah):               8 Series/C220 Series Chipset Family MEI Controller #1
     Subsys Vendor (1458h):        Giga-Byte Technology
     Subsystem ID (1C3Ah):         Unknown
     Class (07h):                  Communication
     SubClass (80h):               Other
     Revision:                     04h
     Interface:                    00h
  Device Properties
     Device Timing:                Fast
     Memory Access:                [X]
     I/O Access:                   [ ]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Memory Address:               F721A000h - F721A00Fh
     System IRQ:                   11
     Interrupt Pin:                INTA#
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 INTEL
     Device Description:           Intel(R) 8 Series/C220 Series Management Engine Interface - 8C3A
     Device Class:                 System
     Device Location:              PCI bus 0, device 22, function 0
     Driver Provider:              INTEL
     Driver Version:               0.0.0.1
     Driver Date:                  1-4-2013
     Inf File:                     oem34.inf
     Hardware ID:                  PCI\VEN_8086&DEV_8C3A&SUBSYS_1C3A1458&REV_04
     Compatible ID:                PCI\VEN_8086&DEV_8C3A&REV_04
     Parent ID:                    ACPI_HAL\PNP0C08
                                   
  Bus: 00h, Device: 1Ah, Function: 00h         
     Vendor (8086h):               Intel Corporation
     Device (8C2Dh):               8 Series/C220 Series Chipset Family USB Enhanced Host Controller #2
     Subsys Vendor (1458h):        Giga-Byte Technology
     Subsystem ID (5006h):         Unknown
     Class (0Ch):                  Serial
     SubClass (03h):               USB
     Revision:                     05h
     Interface:                    20h
  Device Properties
     Device Timing:                Medium
     Memory Access:                [X]
     I/O Access:                   [ ]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Memory Address:               F7218000h - F72183FFh
     System IRQ:                   16
     Interrupt Pin:                INTA#
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard USB Host Controller)
     Device Description:           Standard Enhanced PCI to USB Host Controller
     Device Class:                 USB
     Device Location:              PCI bus 0, device 26, function 0
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24138
     Driver Date:                  6-21-2006
     Inf File:                     usbport.inf
     Service Name:                 usbehci
     Hardware ID:                  PCI\VEN_8086&DEV_8C2D&SUBSYS_50061458&REV_05
     Compatible ID:                PCI\VEN_8086&DEV_8C2D&REV_05
     Parent ID:                    ACPI_HAL\PNP0C08
                                   
  Bus: 00h, Device: 1Bh, Function: 00h         
     Vendor (8086h):               Intel Corporation
     Device (8C20h):               8 Series/C220 Series Chipset Family HD Audio Controller
     Subsys Vendor (1458h):        Giga-Byte Technology
     Subsystem ID (A002h):         Unknown
     Class (04h):                  Multimedia
     SubClass (03h):               Hi-definition Audio
     Revision:                     05h
     Interface:                    00h
  Device Properties
     Device Timing:                Fast
     Memory Access:                [X]
     I/O Access:                   [ ]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Memory Address:               F7210000h - F7213FFFh
     System IRQ:                   22
     Interrupt Pin:                INTA#
  PCI-E Capabilities
     PCI Express Version:          1.0
     Device/Port Type:             Root Complex Integrated Endpoint
     Link Speed:                   Unknown (0) (Current: Unknown (0))
     Link Width:                   x0 (Current: x0)
     Link Port Number:             0
     Physical Slot Number:         0
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 Microsoft
     Device Description:           High Definition Audio Controller
     Device Class:                 System
     Device Location:              PCI bus 0, device 27, function 0
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.23403
     Driver Date:                  3-25-2016
     Inf File:                     hdaudbus.inf
     Service Name:                 HDAudBus
     Hardware ID:                  PCI\VEN_8086&DEV_8C20&SUBSYS_A0021458&REV_05
     Compatible ID:                PCI\VEN_8086&DEV_8C20&REV_05
     Parent ID:                    ACPI_HAL\PNP0C08
                                   
  Bus: 00h, Device: 1Ch, Function: 00h         
     Vendor (8086h):               Intel Corporation
     Device (8C10h):               8 Series/C220 Series Chipset Family PCI Express Root Port 1
     Class (06h):                  Bridge
     SubClass (04h):               PCI/PCI
     Revision:                     D5h
     Interface:                    00h
  Device Properties
     Device Timing:                Fast
     Memory Access:                [ ]
     I/O Access:                   [ ]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Memory Address:               FFF00000h - 000FFFFFh
     System IRQ:                   16
     Interrupt Pin:                INTA#
  PCI-E Capabilities
     PCI Express Version:          2.0
     Device/Port Type:             Root Port of PCI-E Root Complex
     Link Speed:                   5.0 GB/s (Current: 2.5 GB/s)
     Link Width:                   x1 (Current: x0)
     Link Port Number:             1
     Physical Slot Number:         0
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard system devices)
     Device Description:           PCI standard PCI-to-PCI bridge
     Device Class:                 System
     Device Location:              PCI bus 0, device 28, function 0
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24441
     Driver Date:                  6-21-2006
     Inf File:                     machine.inf
     Service Name:                 pci
     Hardware ID:                  PCI\VEN_8086&DEV_8C10&SUBSYS_50011458&REV_D5
     Compatible ID:                PCI\VEN_8086&DEV_8C10&REV_D5
     Parent ID:                    ACPI_HAL\PNP0C08
                                   
  Bus: 00h, Device: 1Ch, Function: 02h         
     Vendor (8086h):               Intel Corporation
     Device (8C14h):               8 Series/C220 Series Chipset Family PCI Express Root Port 3
     Class (06h):                  Bridge
     SubClass (04h):               PCI/PCI
     Revision:                     D5h
     Interface:                    00h
  Device Properties
     Device Timing:                Fast
     Memory Access:                [X]
     I/O Access:                   [X]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Base I/O Port:                D000h - DFFFh
     Memory Address:               F7100000h - F71FFFFFh
     Memory Address:               F2100000h - F21FFFFFh
     System IRQ:                   18
     Interrupt Pin:                INTC#
  PCI-E Capabilities
     PCI Express Version:          2.0
     Device/Port Type:             Root Port of PCI-E Root Complex
     Link Speed:                   5.0 GB/s (Current: 2.5 GB/s)
     Link Width:                   x1 (Current: x1)
     Link Port Number:             3
     Physical Slot Number:         0
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard system devices)
     Device Description:           PCI standard PCI-to-PCI bridge
     Device Class:                 System
     Device Location:              PCI bus 0, device 28, function 2
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24441
     Driver Date:                  6-21-2006
     Inf File:                     machine.inf
     Service Name:                 pci
     Hardware ID:                  PCI\VEN_8086&DEV_8C14&SUBSYS_50011458&REV_D5
     Compatible ID:                PCI\VEN_8086&DEV_8C14&REV_D5
     Parent ID:                    ACPI_HAL\PNP0C08
                                   
  Bus: 00h, Device: 1Ch, Function: 03h         
     Vendor (8086h):               Intel Corporation
     Device (244Eh):               82801FB Hub Interface to PCI Bridge (ICH6 C0 step)
     Class (06h):                  Bridge
     SubClass (04h):               PCI/PCI
     Revision:                     D5h
     Interface:                    01h
  Device Properties
     Device Timing:                Fast
     Memory Access:                [X]
     I/O Access:                   [X]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Base I/O Port:                C000h - CFFFh
     Memory Address:               FFF00000h - 000FFFFFh
     System IRQ:                   19
     Interrupt Pin:                INTD#
  PCI-E Capabilities
     PCI Express Version:          2.0
     Device/Port Type:             Root Port of PCI-E Root Complex
     Link Speed:                   5.0 GB/s (Current: 2.5 GB/s)
     Link Width:                   x1 (Current: x1)
     Link Port Number:             4
     Physical Slot Number:         0
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 Intel
     Device Description:           Intel(R) 82801 PCI Bridge - 244E
     Device Class:                 System
     Device Location:              PCI bus 4, device 0, function 0
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24441
     Driver Date:                  6-21-2006
     Inf File:                     machine.inf
     Service Name:                 pci
     Hardware ID:                  PCI\VEN_8086&DEV_244E&SUBSYS_88921458&REV_41
     Compatible ID:                PCI\VEN_8086&DEV_244E&REV_41
     Parent ID:                    PCI\VEN_8086&DEV_244E&SUBSYS_50011458&REV_D5
                                   
  Bus: 00h, Device: 1Dh, Function: 00h         
     Vendor (8086h):               Intel Corporation
     Device (8C26h):               8 Series/C220 Series Chipset Family USB Enhanced Host Controller #1
     Subsys Vendor (1458h):        Giga-Byte Technology
     Subsystem ID (5006h):         Unknown
     Class (0Ch):                  Serial
     SubClass (03h):               USB
     Revision:                     05h
     Interface:                    20h
  Device Properties
     Device Timing:                Medium
     Memory Access:                [X]
     I/O Access:                   [ ]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Memory Address:               F7217000h - F72173FFh
     System IRQ:                   23
     Interrupt Pin:                INTA#
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard USB Host Controller)
     Device Description:           Standard Enhanced PCI to USB Host Controller
     Device Class:                 USB
     Device Location:              PCI bus 0, device 29, function 0
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24138
     Driver Date:                  6-21-2006
     Inf File:                     usbport.inf
     Service Name:                 usbehci
     Hardware ID:                  PCI\VEN_8086&DEV_8C26&SUBSYS_50061458&REV_05
     Compatible ID:                PCI\VEN_8086&DEV_8C26&REV_05
     Parent ID:                    ACPI_HAL\PNP0C08
                                   
  Bus: 00h, Device: 1Fh, Function: 00h         
     Vendor (8086h):               Intel Corporation
     Device (8C50h):               B85 Express LPC Controller
     Subsys Vendor (1458h):        Giga-Byte Technology
     Subsystem ID (5001h):         Unknown
     Class (06h):                  Bridge
     SubClass (01h):               PCI/ISA
     Revision:                     05h
     Interface:                    00h
  Device Properties
     Device Timing:                Medium
     Memory Access:                [X]
     I/O Access:                   [X]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard system devices)
     Device Description:           PCI standard ISA bridge
     Device Class:                 System
     Device Location:              PCI bus 0, device 31, function 0
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24441
     Driver Date:                  6-21-2006
     Inf File:                     machine.inf
     Service Name:                 msisadrv
     Hardware ID:                  PCI\VEN_8086&DEV_8C50&SUBSYS_50011458&REV_05
     Compatible ID:                PCI\VEN_8086&DEV_8C50&REV_05
     Parent ID:                    ACPI_HAL\PNP0C08
                                   
  Bus: 00h, Device: 1Fh, Function: 02h         
     Vendor (8086h):               Intel Corporation
     Device (8C02h):               8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
     Subsys Vendor (1458h):        Giga-Byte Technology
     Subsystem ID (B005h):         Unknown
     Class (01h):                  Storage
     SubClass (06h):               Serial ATA
     Revision:                     05h
     Interface:                    01h
  Device Properties
     Device Timing:                Medium
     Memory Access:                [X]
     I/O Access:                   [X]
     Bus Master:                   [X]
     66 MHz Speed Support:         [X]
  Device Resources
     Base I/O Port:                0000F070h - 0000F077h
     Base I/O Port:                0000F060h - 0000F063h
     Base I/O Port:                0000F050h - 0000F057h
     Base I/O Port:                0000F040h - 0000F043h
     Base I/O Port:                0000F020h - 0000F03Fh
     Memory Address:               F7216000h - F72167FFh
     System IRQ:                   19
     Interrupt Pin:                INTB#
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 Standard AHCI 1.0 Serial ATA Controller
     Device Description:           Standard AHCI 1.0 Serial ATA Controller
     Device Class:                 hdc
     Device Location:              PCI bus 0, device 31, function 2
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.23403
     Driver Date:                  6-21-2006
     Inf File:                     mshdc.inf
     Service Name:                 msahci
     Hardware ID:                  PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
     Compatible ID:                PCI\VEN_8086&DEV_8C02&REV_05
     Parent ID:                    ACPI_HAL\PNP0C08
                                   
  Bus: 00h, Device: 1Fh, Function: 03h         
     Vendor (8086h):               Intel Corporation
     Device (8C22h):               8 Series/C220 Series Chipset Family SMBus Controller
     Subsys Vendor (1458h):        Giga-Byte Technology
     Subsystem ID (5001h):         Unknown
     Class (0Ch):                  Serial
     SubClass (05h):               SMBus Controller
     Revision:                     05h
     Interface:                    00h
  Device Properties
     Device Timing:                Medium
     Memory Access:                [ ]
     I/O Access:                   [X]
     Bus Master:                   [ ]
     66 MHz Speed Support:         [ ]
  Device Resources
     SMBus Port:                   F000h
     Memory Address:               F7215000h - F72150FFh
     Base I/O Port:                0000F000h - 0000F01Fh
     System IRQ:                   10
     Interrupt Pin:                INTC#
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 INTEL
     Device Description:           Intel(R) 8 Series/C220 Series SMBus Controller - 8C22
     Device Class:                 System
     Device Location:              PCI bus 0, device 31, function 3
     Driver Provider:              INTEL
     Driver Version:               10.1.1.45
     Driver Date:                  1-2-2018
     Inf File:                     oem38.inf
     Hardware ID:                  PCI\VEN_8086&DEV_8C22&SUBSYS_50011458&REV_05
     Compatible ID:                PCI\VEN_8086&DEV_8C22&REV_05
     Parent ID:                    ACPI_HAL\PNP0C08
                                   
  Bus: 01h, Device: 00h, Function: 00h         
     Vendor (10DEh):               Nvidia Corp
     Device (1B81h):               GP104 [GeForce GTX 1070]
     Subsys Vendor (10DEh):        Nvidia Corp
     Subsystem ID (119Dh):         Unknown
     Class (03h):                  Display
     SubClass (00h):               VGA
     Revision:                     A1h
     Interface:                    00h
  Device Properties
     Device Timing:                Fast
     Memory Access:                [X]
     I/O Access:                   [X]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Memory Address:               F6000000h - F6FFFFFFh
     Memory Address:               E0000000h - EFFFFFFFh
     Memory Address:               F0000000h - F1FFFFFFh
     Base I/O Port:                0000E000h - 0000E07Fh
     System IRQ:                   16
     Interrupt Pin:                INTA#
  PCI-E Capabilities
     PCI Express Version:          3.0
     Device/Port Type:             Legacy PCI-E Endpoint
     Link Speed:                   8.0 GB/s (Current: 2.5 GB/s)
     Link Width:                   x16 (Current: x16)
     Link Port Number:             0
     Physical Slot Number:         0
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 NVIDIA
     Device Description:           NVIDIA GeForce GTX 1070
     Device Class:                 Display
     Device Location:              PCI bus 1, device 0, function 0
     Driver Provider:              NVIDIA
     Driver Version:               26.21.14.4219
     Driver Date:                  1-29-2020
     Inf File:                     oem15.inf
     Service Name:                 nvlddmkm
     Hardware ID:                  PCI\VEN_10DE&DEV_1B81&SUBSYS_119D10DE&REV_A1
     Compatible ID:                PCI\VEN_10DE&DEV_1B81&REV_A1
     Parent ID:                    PCI\VEN_8086&DEV_0C01&SUBSYS_50001458&REV_06
                                   
  Bus: 01h, Device: 00h, Function: 01h         
     Vendor (10DEh):               Nvidia Corp
     Device (10F0h):               GP104 High Definition Audio Controller
     Subsys Vendor (10DEh):        Nvidia Corp
     Subsystem ID (119Dh):         Unknown
     Class (04h):                  Multimedia
     SubClass (03h):               Hi-definition Audio
     Revision:                     A1h
     Interface:                    00h
  Device Properties
     Device Timing:                Fast
     Memory Access:                [X]
     I/O Access:                   [ ]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Memory Address:               F7080000h - F7083FFFh
     System IRQ:                   17
     Interrupt Pin:                INTB#
  AC'97/HDA Capabilities
     AC'97/HDA Codec Name:         NVidia GPU GP104 HDMI/DP
  PCI-E Capabilities
     PCI Express Version:          3.0
     Device/Port Type:             PCI-E Endpoint
     Link Speed:                   8.0 GB/s (Current: 2.5 GB/s)
     Link Width:                   x16 (Current: x16)
     Link Port Number:             0
     Physical Slot Number:         0
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 Microsoft
     Device Description:           High Definition Audio Controller
     Device Class:                 System
     Device Location:              PCI bus 1, device 0, function 1
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.23403
     Driver Date:                  3-25-2016
     Inf File:                     hdaudbus.inf
     Service Name:                 HDAudBus
     Hardware ID:                  PCI\VEN_10DE&DEV_10F0&SUBSYS_119D10DE&REV_A1
     Compatible ID:                PCI\VEN_10DE&DEV_10F0&REV_A1
     Parent ID:                    PCI\VEN_8086&DEV_0C01&SUBSYS_50001458&REV_06
                                   
  Bus: 03h, Device: 00h, Function: 00h         
     Vendor (10ECh):               Realtek Semiconductor
     Device (8168h):               RTL8111/8168/8411 PCI Express Gigabit Ethernet Controller
     Subsys Vendor (1458h):        Giga-Byte Technology
     Subsystem ID (E000h):         GA-EP45-DS5 Motherboard
     Class (02h):                  Network
     SubClass (00h):               Ethernet
     Revision:                     0Ch
     Interface:                    00h
  Device Properties
     Device Timing:                Fast
     Memory Access:                [X]
     I/O Access:                   [X]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Base I/O Port:                0000D000h - 0000D0FFh
     Memory Address:               F7100000h - F7100FFFh
     Memory Address:               F2100000h - F2103FFFh
  PCI-E Capabilities
     PCI Express Version:          2.0
     Device/Port Type:             PCI-E Endpoint
     Link Speed:                   2.5 GB/s (Current: 2.5 GB/s)
     Link Width:                   x1 (Current: x1)
     Link Port Number:             0
     Physical Slot Number:         0
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 Realtek
     Device Description:           Realtek PCIe GbE Family Controller
     Device Class:                 Net
     Device Location:              PCI bus 3, device 0, function 0
     Driver Provider:              Realtek
     Driver Version:               7.127.701.2019
     Driver Date:                  7-1-2019
     Inf File:                     oem33.inf
     Service Name:                 RTL8167
     Hardware ID:                  PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_0C
     Compatible ID:                PCI\VEN_10EC&DEV_8168&REV_0C
     Parent ID:                    PCI\VEN_8086&DEV_8C14&SUBSYS_50011458&REV_D5
                                   
  Bus: 04h, Device: 00h, Function: 00h         
     Vendor (8086h):               Intel Corporation
     Device (244Eh):               82801 Family (ICH2/3/4/5/6/7/8/9,63xxESB) Hub Interface to PCI Bridge
     Class (06h):                  Bridge
     SubClass (04h):               PCI/PCI
     Revision:                     41h
     Interface:                    01h
  Device Properties
     Device Timing:                Fast
     Memory Access:                [X]
     I/O Access:                   [X]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Base I/O Port:                C000h - CFFFh
     Memory Address:               FFF00000h - 000FFFFFh
     System IRQ:                   19
     Interrupt Pin:                INTA#
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 Intel
     Device Description:           Intel(R) 82801 PCI Bridge - 244E
     Device Class:                 System
     Device Location:              PCI bus 0, device 28, function 3
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24441
     Driver Date:                  6-21-2006
     Inf File:                     machine.inf
     Service Name:                 pci
     Hardware ID:                  PCI\VEN_8086&DEV_244E&SUBSYS_50011458&REV_D5
     Compatible ID:                PCI\VEN_8086&DEV_244E&REV_D5
     Parent ID:                    ACPI_HAL\PNP0C08
                                   
  Bus: 05h, Device: 00h, Function: 00h         
     Vendor (1412h):               VIA Technologies Inc (Was: IC Ensemble Inc)
     Device (1724h):               VT1720/4 Envy24PT PCI Multi-Channel Audio Controller
     Subsys Vendor (1412h):        VIA Technologies Inc (Was: IC Ensemble Inc)
     Subsystem ID (3631h):         M-Audio Revolution 5.1
     Class (04h):                  Multimedia
     SubClass (01h):               Audio
     Revision:                     01h
     Interface:                    00h
  Device Properties
     Device Timing:                Medium
     Memory Access:                [ ]
     I/O Access:                   [X]
     Bus Master:                   [X]
     66 MHz Speed Support:         [ ]
  Device Resources
     Base I/O Port:                0000C080h - 0000C09Fh
     Base I/O Port:                0000C000h - 0000C07Fh
     System IRQ:                   19
     Interrupt Pin:                INTA#
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 M-Audio
     Device Description:           M-Audio Revolution 5.1
     Device Class:                 MEDIA
     Device Location:              PCI bus 5, device 0, function 0
     Driver Provider:              M-Audio
     Driver Version:               5.10.0.5064
     Driver Date:                  3-12-2008
     Inf File:                     oem49.inf
     Service Name:                 REVO51
     Hardware ID:                  PCI\VEN_1412&DEV_1724&SUBSYS_36311412&REV_01
     Compatible ID:                PCI\VEN_1412&DEV_1724&REV_01
     Parent ID:                    PCI\VEN_8086&DEV_244E&SUBSYS_88921458&REV_41
                                   
                  +-----------------------------------------+
                  |              Memory Modules             |
                  +-----------------------------------------+
  Memory Slot 1
     Memory Type:                  8 GB DDR3-1866 (PC3-14900) SDRAM
     Manufacturer:                 Kllisre
     Module Type:                  Unbuffered DIMM
     Number of Ranks/Banks:        2 Ranks, 8 Banks
     Module Attributes:            Unbuffered
     Error Checking:               None
     JEDEC Timings:                CL-tRCD-tRP-tRAS-tWR-tRC @ Frequency
     JEDEC Profile 1:              13.0-11-10-30-15-42 @ 933MHz
     JEDEC Profile 2:              11.0-11-10-30-15-42 @ 933MHz
     JEDEC Profile 3:              10.0-11-10-30-15-42 @ 933MHz
     JEDEC Profile 4:              9.0-10-9-28-13-38 @ 841MHz
     JEDEC Profile 5:              8.0-9-8-25-12-34 @ 747MHz
     JEDEC Profile 6:              7.0-8-7-22-10-30 @ 654MHz
     JEDEC Profile 7:              6.0-7-6-19-9-26 @ 560MHz
     JEDEC Profile 8:              5.0-6-5-16-8-21 @ 467MHz
     Refresh Rate:                 7.8 us (2X 85-95 C)
     Data Width:                   64 bits
     SDRAM Width:                  x8
     Voltage Interface:            1.50 V
     Max Case Temperature:         95 °C (203 °F)
     SPD Revision:                 1.1
     Part Number:                  KHX1866C10D3/8G   
     Manufacturing Location:       7
     Manufacture Date:             January 2019 (1903h)
     Serial Number:                522C5B2Ch
     Revision Code:                None
     EPP Support:                  [ ]
     XMP Support:                  [ ]
                                   
  Memory Slot 3
     Memory Type:                  8 GB DDR3-1866 (PC3-14900) SDRAM
     Manufacturer:                 Kingston
     Module Type:                  Unbuffered DIMM
     Number of Ranks/Banks:        2 Ranks, 8 Banks
     Module Attributes:            Unbuffered
     Error Checking:               None
     JEDEC Timings:                CL-tRCD-tRP-tRAS-tWR-tRC @ Frequency
     JEDEC Profile 1:              13.0-11-10-30-15-42 @ 933MHz
     JEDEC Profile 2:              11.0-11-10-30-15-42 @ 933MHz
     JEDEC Profile 3:              10.0-11-10-30-15-42 @ 933MHz
     JEDEC Profile 4:              9.0-10-9-28-13-38 @ 841MHz
     JEDEC Profile 5:              8.0-9-8-25-12-34 @ 747MHz
     JEDEC Profile 6:              7.0-8-7-22-10-30 @ 654MHz
     JEDEC Profile 7:              6.0-7-6-19-9-26 @ 560MHz
     JEDEC Profile 8:              5.0-6-5-16-8-21 @ 467MHz
     Refresh Rate:                 7.8 us (2X 85-95 C)
     Data Width:                   64 bits
     SDRAM Width:                  x8
     Voltage Interface:            1.50 V
     Max Case Temperature:         95 °C (203 °F)
     SPD Revision:                 1.1
     Part Number:                  KHX1866C10D3/8G   
     Manufacturing Location:       7
     Manufacture Date:             May 2015 (1519h)
     Serial Number:                66117105h
     Revision Code:                None
     EPP Support:                  [ ]
     XMP Support:                  [ ]
                                   
                  +-----------------------------------------+
                  |             Memory (SMBIOS)             |
                  +-----------------------------------------+
  Physical Memory Array 1
     Maximum Capacity:             32768 MB
     Location:                     System Board or Motherboard
     Use:                          System Memory
     Memory Error Correct.:        None
     Memory Devices:               2
     Structure Length:             17h
  Memory Device 1
     Size:                         8192 MB
     Form Factor:                  DIMM
     Memory Type:                  DDR3
     Speed:                        1600 MHz
     Configured Speed:             1600 MHz
     Device Locator:               ChannelA-DIMM0
     Bank Locator:                 BANK 0
     Total Width:                  64 bits
     Data Width:                   64 bits
     Device Set:                   00h
     Type Detail:                  Synchronous
     Manufacturer:                 1319
     Serial Number:                522C5B2C
     Asset Tag:                    9876543210
     Part Number:                  KHX1866C10D3/8G
     Structure Length:             22h
  Memory Device 2
     Size:                         Not Installed
     Form Factor:                  DIMM
     Memory Type:                  Unknown
     Speed:                        Unknown
     Device Locator:               ChannelA-DIMM1
     Bank Locator:                 BANK 1
     Total Width:                  0 bits
     Data Width:                   0 bits
     Device Set:                   00h
     Type Detail:                  None
     Manufacturer:                 [Empty]
     Serial Number:                [Empty]
     Asset Tag:                    9876543210
     Part Number:                  [Empty]
     Structure Length:             22h
  Memory Device 3
     Size:                         8192 MB
     Form Factor:                  DIMM
     Memory Type:                  DDR3
     Speed:                        1600 MHz
     Configured Speed:             1600 MHz
     Device Locator:               ChannelB-DIMM0
     Bank Locator:                 BANK 2
     Total Width:                  64 bits
     Data Width:                   64 bits
     Device Set:                   00h
     Type Detail:                  Synchronous
     Manufacturer:                 Kingston
     Serial Number:                66117105
     Asset Tag:                    9876543210
     Part Number:                  KHX1866C10D3/8G
     Structure Length:             22h
  Memory Device 4
     Size:                         Not Installed
     Form Factor:                  DIMM
     Memory Type:                  Unknown
     Speed:                        Unknown
     Device Locator:               ChannelB-DIMM1
     Bank Locator:                 BANK 3
     Total Width:                  0 bits
     Data Width:                   0 bits
     Device Set:                   00h
     Type Detail:                  None
     Manufacturer:                 [Empty]
     Serial Number:                [Empty]
     Asset Tag:                    9876543210
     Part Number:                  [Empty]
     Structure Length:             22h
                                   
                  +-----------------------------------------+
                  |                  Disk                   |
                  +-----------------------------------------+
  Secondary/Master Drive
     Disk Model:                   SPCC Solid State Disk
     Disk Size:                    114473 MB (111.79 GB)
     Interface Type:               Serial ATA III (SATA/600)
     Form Factor:                  2.5"
     Rotation Rate:                SSD
     Geometry:                     Heads: 16, Sectors: 63, Tracks: 16383
     Compatibility:                ACS-4
     Serial Number:                2A40079618DB00135162
     Controller Revision:          SBFM61.3
     Disk Marketing Size:          120034 MB (120.03 GB)
     Buffer Size:                  Unknown
     Buffer Type:                  Not Specified
     Disk Temperature:             33 °C (91 °F)
     Disk Health Status:           Good
     SSD Remaining Life:           100 %
     Total Host Writes:            3.31 TB
     Logical Drives:               I:
     ECC bytes:                    None
     Security Erase Time:          20 min
     Enh. Security Erase:          60 min
     Current APM Value:            None
     Acoustic Management:          None
     Location (Vendor):            Intel Corporation
     Location (Device):            8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
     Device Location:              Secondary/Master
  Transfer Modes
     SATA Speed:                   600 MB/s, Active: 600 MB/s
     PIO Mode Support:             4
     SW DMA Mode Support:          Not Supported
     MW DMA Mode Support:          2, Active: None
     UDMA Mode Support:            6 (UltraDMA/133), Active: 5 (UltraDMA/100)
     Sectors per Interrupt:        16, Active: 16
  Disk Features
     SATA NCQ Command:                    [X]
     SSD TRIM Command:                    [X]
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [X]
     Double Word I/O:                     [X]
     Standard Standby Timer:              [X]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [X]
     S.M.A.R.T.:                          [X] enabled
     S.M.A.R.T. Self-test:                [X] enabled
     S.M.A.R.T. Error Logging:            [X] enabled
     Security Mode Feature Set:           [X] disabled
     Removable Media:                     [ ]
     Power Management:                    [X] enabled
     PACKET Command:                      [ ]
     Write Cache:                         [X] enabled
     Look-ahead:                          [X] enabled
     Release Interrupt:                   [ ]
     Service Interrupt:                   [ ]
     Device Reset Command:                [ ]
     Host Protected Area:                 [X] enabled
     Write Verify Command:                [ ]
     Write Buffer Command:                [X] enabled
     Read Buffer Command:                 [X] enabled
     NOP Command:                         [X] enabled
     Identify Device DMA Command:         [ ]
     Download Microcode Command:          [X] enabled
     Read/Write DMA Queued:               [ ]
     CFA Feature Set:                     [ ]
     Advanced Power Management:           [ ]
     Removable Media Status:              [ ]
     Power-up in Standby:                 [ ]
     Set Features Req. to Spinup:         [ ]
     Set Max Security Extension:          [X] disabled
     Automatic Acoustic Management:       [ ]
     48-bit Address:                      [X] enabled
     Device Configuration Overlay:        [X] enabled
     Flush Cache Command:                 [X] enabled
     Flush Cache Ext Command:             [X] enabled
     Media Serial Number:                 [ ]
     Media Card Pass Through:             [ ]
     Streaming Feature Set:               [ ]
     General Purpose Logging:             [X] enabled
     Write DMA/Multiple FUA EXT:          [X] enabled
     Write DMA Queued FUA EXT:            [ ]
     World Wide Name:                     [ ]
  S.M.A.R.T.
     ID  | Attribute Name                 |Threshold|Worst|Value| Raw Value
     ----+--------------------------------+---------+-----+-----+-----------
     1   | Raw Read Error Rate            |       50|  100|  100|     0
     9   | Power On Hours Count           |        0|  100|  100|  3632
     12  | Drive Power Cycle Count        |        0|  100|  100|  1701
     168 | SATA PHY Error Count           |        0|  100|  100|     0
     170 | Available Reserved Space       |        0|  100|  100|   483
     173 | Average Erase Count            |        0|  100|  100| 2490434
     192 | Unsafe Shutdown Count          |        0|  100|  100|    85
     194 | Drive Temperature              |        0|   67|   67| 141736083489
     218 | Flash ROM ECC Correction Count |       50|  100|  100|     0
     231 | SSD Remaining Life             |        0|  100|  100|    98
     241 | Total Host Writes              |        0|  100|  100|  3386
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard disk drives)
     Device Description:           Disk drive
     Friendly Name:                SPCC Solid State Disk ATA Device
     Device Class:                 DiskDrive
     Device Location:              Channel 1, Target 0, Lun 0
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.23403
     Driver Date:                  6-21-2006
     Inf File:                     disk.inf
     Service Name:                 disk
     Hardware ID:                  IDE\DiskSPCC_Solid_State_Disk___________________SBFM61.3
     Compatible ID:                GenDisk
     Parent ID:                    PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
                                   
  8th/Slave Drive
     Disk Model:                   WDC WD1001FALS-00J7B0
     Disk Size:                    953869 MB (931.51 GB)
     Interface Type:               Serial ATA II (SATA/300)
     Geometry:                     Heads: 16, Sectors: 63, Tracks: 16383
     Compatibility:                ATA8-ACS
     Serial Number:                WD-WMATV0357962
     Controller Revision:          05.00K05
     Disk Marketing Size:          1000204 MB (1000.2 GB)
     Buffer Size:                  32 MB
     Buffer Type:                  Not Specified
     Disk Temperature:             42 °C (108 °F)
     Reallocated Sectors:          0
     Disk Health Status:           Good
     Logical Drives:               E:, F:, H:
     ECC bytes:                    50
     Security Erase Time:          194 min
     Enh. Security Erase:          194 min
     Current APM Value:            None
     Acoustic Management:          FEh (80h Recommended) - Disabled
     Location (Vendor):            Intel Corporation
     Location (Device):            8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
     Device Location:              8th/Slave
  Transfer Modes
     SATA Speed:                   300 MB/s
     PIO Mode Support:             4
     SW DMA Mode Support:          Not Supported
     MW DMA Mode Support:          2, Active: None
     UDMA Mode Support:            6 (UltraDMA/133), Active: 5 (UltraDMA/100)
     Sectors per Interrupt:        16, Active: 16
  Disk Features
     SATA NCQ Command:                    [X]
     SSD TRIM Command:                    [ ]
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [X]
     Double Word I/O:                     [ ]
     Standard Standby Timer:              [X]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [X]
     S.M.A.R.T.:                          [X] enabled
     S.M.A.R.T. Self-test:                [X] enabled
     S.M.A.R.T. Error Logging:            [X] enabled
     Security Mode Feature Set:           [X] disabled
     Removable Media:                     [ ]
     Power Management:                    [X] enabled
     PACKET Command:                      [ ]
     Write Cache:                         [X] enabled
     Look-ahead:                          [X] enabled
     Release Interrupt:                   [ ]
     Service Interrupt:                   [ ]
     Device Reset Command:                [ ]
     Host Protected Area:                 [X] enabled
     Write Verify Command:                [ ]
     Write Buffer Command:                [X] enabled
     Read Buffer Command:                 [X] enabled
     NOP Command:                         [X] enabled
     Identify Device DMA Command:         [ ]
     Download Microcode Command:          [X] enabled
     Read/Write DMA Queued:               [ ]
     CFA Feature Set:                     [ ]
     Advanced Power Management:           [ ]
     Removable Media Status:              [ ]
     Power-up in Standby:                 [X] disabled
     Set Features Req. to Spinup:         [X] enabled
     Set Max Security Extension:          [X] disabled
     Automatic Acoustic Management:       [X] disabled
     48-bit Address:                      [X] enabled
     Device Configuration Overlay:        [X] enabled
     Flush Cache Command:                 [X] enabled
     Flush Cache Ext Command:             [X] enabled
     Media Serial Number:                 [ ]
     Media Card Pass Through:             [ ]
     Streaming Feature Set:               [ ]
     General Purpose Logging:             [X] enabled
     Write DMA/Multiple FUA EXT:          [ ]
     Write DMA Queued FUA EXT:            [ ]
     World Wide Name:                     [X] enabled
  S.M.A.R.T.
     ID  | Attribute Name            |Threshold|Worst|Value| Raw Value
     ----+---------------------------+---------+-----+-----+-----------
     1   | Raw Read Error Rate       |       51|  200|  200|     0
     3   | Spin-up Time              |       21|  253|  253|  6500
     4   | Start/Stop Count          |        0|   68|   68| 32639
     5   | Reallocated Sectors Count |      140|  200|  200|     0
     7   | Seek Error Rate           |       51|  253|  100|     0
     9   | Power On Hours Count      |        0|   45|   45| 40331
     10  | Spin-up Retry Count       |       51|  100|  100|     0
     11  | Recalibration Retries     |       51|  100|  100|     0
     12  | Drive Power Cycle Count   |        0|   78|   78| 22728
     192 | Power-Off Retract Count   |        0|  198|  198|  2052
     193 | Load/Unload Cycle Count   |        0|  190|  190| 32529
     194 | Drive Temperature         |        0|   89|  108|    42
     196 | Reallocation Event Count  |        0|  200|  200|     0
     197 | Current Pending Sectors   |        0|  200|  200|     0
     198 | Uncorrectable Sectors     |        0|  200|  200|     0
     199 | UltraDMA CRC Error Rate   |        0|  200|  200|   312
     200 | Write Error Rate          |       51|  183|  200|     0
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard disk drives)
     Device Description:           Disk drive
     Friendly Name:                WDC WD1001FALS-00J7B0 ATA Device
     Device Class:                 DiskDrive
     Device Location:              Channel 2, Target 0, Lun 0
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.23403
     Driver Date:                  6-21-2006
     Inf File:                     disk.inf
     Service Name:                 disk
     Hardware ID:                  IDE\DiskWDC_WD1001FALS-00J7B0___________________05.00K05
     Compatible ID:                GenDisk
     Parent ID:                    PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
                                   
  8th/Slave Drive
     Disk Model:                   Samsung SSD 860 EVO 250GB
     Disk Size:                    238475 MB (232.89 GB)
     Interface Type:               Serial ATA III (SATA/600)
     Form Factor:                  2.5"
     Rotation Rate:                SSD
     Geometry:                     Heads: 16, Sectors: 63, Tracks: 16383
     Compatibility:                ACS-4 revision 94
     Serial Number:                S3Y9NB0K275545B
     Controller Revision:          RVT01B6Q
     Disk Marketing Size:          250059 MB (250.06 GB)
     Buffer Size:                  Unknown
     Buffer Type:                  Not Specified
     Disk Temperature:             39 °C (102 °F)
     Reallocated Sectors:          0
     Disk Health Status:           Good
     SSD Remaining Life:           100 %
     Total Host Writes:            6.58 TB
     Logical Drives:               C:, D:, G:
     ECC bytes:                    None
     Security Erase Time:          4 min
     Enh. Security Erase:          8 min
     Current APM Value:            None
     Acoustic Management:          None
     Location (Vendor):            Intel Corporation
     Location (Device):            8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
     Device Location:              8th/Slave
  Transfer Modes
     SATA Speed:                   600 MB/s, Active: 600 MB/s
     PIO Mode Support:             4
     SW DMA Mode Support:          Not Supported
     MW DMA Mode Support:          2, Active: None
     UDMA Mode Support:            6 (UltraDMA/133), Active: 5 (UltraDMA/100)
     Sectors per Interrupt:        1, Active: 1
  Disk Features
     SATA NCQ Command:                    [X]
     SSD TRIM Command:                    [X]
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [X]
     Double Word I/O:                     [X]
     Standard Standby Timer:              [X]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [X]
     S.M.A.R.T.:                          [X] enabled
     S.M.A.R.T. Self-test:                [X] enabled
     S.M.A.R.T. Error Logging:            [X] enabled
     Security Mode Feature Set:           [X] disabled
     Removable Media:                     [ ]
     Power Management:                    [X] enabled
     PACKET Command:                      [ ]
     Write Cache:                         [X] enabled
     Look-ahead:                          [X] enabled
     Release Interrupt:                   [ ]
     Service Interrupt:                   [ ]
     Device Reset Command:                [ ]
     Host Protected Area:                 [X] enabled
     Write Verify Command:                [ ]
     Write Buffer Command:                [X] enabled
     Read Buffer Command:                 [X] enabled
     NOP Command:                         [X] enabled
     Identify Device DMA Command:         [ ]
     Download Microcode Command:          [X] enabled
     Read/Write DMA Queued:               [ ]
     CFA Feature Set:                     [ ]
     Advanced Power Management:           [ ]
     Removable Media Status:              [ ]
     Power-up in Standby:                 [ ]
     Set Features Req. to Spinup:         [ ]
     Set Max Security Extension:          [X] disabled
     Automatic Acoustic Management:       [ ]
     48-bit Address:                      [X] enabled
     Device Configuration Overlay:        [X] enabled
     Flush Cache Command:                 [X] enabled
     Flush Cache Ext Command:             [X] enabled
     Media Serial Number:                 [ ]
     Media Card Pass Through:             [ ]
     Streaming Feature Set:               [ ]
     General Purpose Logging:             [X] enabled
     Write DMA/Multiple FUA EXT:          [X] enabled
     Write DMA Queued FUA EXT:            [ ]
     World Wide Name:                     [X] enabled
  S.M.A.R.T.
     ID  | Attribute Name                    |Threshold|Worst|Value| Raw Value
     ----+-----------------------------------+---------+-----+-----+-----------
     5   | Reallocated Sectors Count         |       10|  100|  100|     0
     9   | Power On Hours Count              |        0|   97|   97| 11541
     12  | Drive Power Cycle Count           |        0|   93|   93|  6429
     177 | Wear Leveling Count               |        0|   98|   98|    23
     179 | Used Reserved Block Count (Total) |       10|  100|  100|     0
     181 | Program Fail Count                |       10|  100|  100|     0
     182 | Erase Fail Count                  |       10|  100|  100|     0
     183 | Runtime Bad Block                 |       10|  100|  100|     0
     187 | Uncorrectable Errors              |        0|  100|  100|     0
     190 | Airflow Temperature               |        0|   47|   61|    39
     195 | Hardware ECC Recovered            |        0|  200|  200|     0
     199 | UltraDMA CRC Error Rate           |        0|   99|   99|     3
     235 | POR Recovery Count                |        0|   99|   99|   272
     241 | Total Host Writes                 |        0|   99|   99| 14120793738
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard disk drives)
     Device Description:           Disk drive
     Friendly Name:                Samsung SSD 860 EVO 250GB ATA Device
     Device Class:                 DiskDrive
     Device Location:              Channel 3, Target 0, Lun 0
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.23403
     Driver Date:                  6-21-2006
     Inf File:                     disk.inf
     Service Name:                 disk
     Hardware ID:                  IDE\DiskSamsung_SSD_860_EVO_250GB_______________RVT01B6Q
     Compatible ID:                GenDisk
     Parent ID:                    PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
                                   
  8th/Slave Drive
     Disk Model:                   ST3500412AS
     Disk Size:                    476940 MB (465.76 GB)
     Interface Type:               Serial ATA II (SATA/300)
     Rotation Rate:                5900 rpm
     Geometry:                     Heads: 16, Sectors: 63, Tracks: 16383
     Compatibility:                ATA8-ACS revision 41
     Serial Number:                6VV25CDT
     Controller Revision:          CC32
     Disk Marketing Size:          500108 MB (500.11 GB)
     Buffer Size:                  16 MB
     Buffer Type:                  Not Specified
     Disk Temperature:             35 °C (95 °F)
     Reallocated Sectors:          1991
     Disk Health Status:           Bad
     Total Host Writes:            1.02 TB
     Total Host Reads:             789.29 GB
     Logical Drives:               J:
     ECC bytes:                    4
     Security Erase Time:          96 min
     Enh. Security Erase:          96 min
     Current APM Value:            C0h
     Acoustic Management:          00h (FEh Recommended) - Enabled
     Location (Vendor):            Intel Corporation
     Location (Device):            8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
     Device Location:              8th/Slave
  Transfer Modes
     SATA Speed:                   300 MB/s
     PIO Mode Support:             4
     SW DMA Mode Support:          Not Supported
     MW DMA Mode Support:          2, Active: None
     UDMA Mode Support:            6 (UltraDMA/133), Active: 5 (UltraDMA/100)
     Sectors per Interrupt:        16, Active: 16
  Disk Features
     SATA NCQ Command:                    [X]
     SSD TRIM Command:                    [ ]
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [X]
     Double Word I/O:                     [ ]
     Standard Standby Timer:              [X]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [X]
     S.M.A.R.T.:                          [X] enabled
     S.M.A.R.T. Self-test:                [X] enabled
     S.M.A.R.T. Error Logging:            [X] enabled
     Security Mode Feature Set:           [X] disabled
     Removable Media:                     [ ]
     Power Management:                    [X] enabled
     PACKET Command:                      [ ]
     Write Cache:                         [X] enabled
     Look-ahead:                          [X] enabled
     Release Interrupt:                   [ ]
     Service Interrupt:                   [ ]
     Device Reset Command:                [ ]
     Host Protected Area:                 [X] enabled
     Write Verify Command:                [ ]
     Write Buffer Command:                [X] enabled
     Read Buffer Command:                 [X] enabled
     NOP Command:                         [ ]
     Identify Device DMA Command:         [ ]
     Download Microcode Command:          [X] enabled
     Read/Write DMA Queued:               [ ]
     CFA Feature Set:                     [ ]
     Advanced Power Management:           [X] enabled
     Removable Media Status:              [ ]
     Power-up in Standby:                 [X] disabled
     Set Features Req. to Spinup:         [X] disabled
     Set Max Security Extension:          [X] disabled
     Automatic Acoustic Management:       [X] enabled
     48-bit Address:                      [X] enabled
     Device Configuration Overlay:        [X] enabled
     Flush Cache Command:                 [X] enabled
     Flush Cache Ext Command:             [X] enabled
     Media Serial Number:                 [ ]
     Media Card Pass Through:             [ ]
     Streaming Feature Set:               [ ]
     General Purpose Logging:             [X] enabled
     Write DMA/Multiple FUA EXT:          [X] enabled
     Write DMA Queued FUA EXT:            [ ]
     World Wide Name:                     [X] enabled
  S.M.A.R.T.
     ID  | Attribute Name             |Threshold|Worst|Value| Raw Value
     ----+----------------------------+---------+-----+-----+-----------
     1   | Raw Read Error Rate        |        6|   90|  120| 243460323
     3   | Spin-up Time               |        0|   97|   97|     0
     4   | Start/Stop Count           |       20|   71|   71| 30122
     5   |!Reallocated Sectors Count  |       36|   52|   52|  1991
     7   | Seek Error Rate            |       30|   60|   84| 265538621
     9   | Power On Hours Count       |        0|   79|   79| 18882
     10  | Spin-up Retry Count        |       97|  100|  100|     0
     12  | Drive Power Cycle Count    |       20|   87|   87| 13710
     183 | SATA Downshift Error Count |        0|   94|   94|     6
     184 | End to End Error Detection |       99|  100|  100|     0
     187 | Uncorrectable Errors       |        0|    1|    1|  1907
     188 | Command Timeout            |        0|    1|  100|   175
     189 | High Fly Writes            |        0|  100|  100|     0
     190 | Airflow Temperature        |       45|   39|   65| 43639111715
     194 | Drive Temperature          |        0|   61|   35| 25769803811
     195 | Hardware ECC Recovered     |        0|   22|   38| 243460323
     197 | Current Pending Sectors    |        0|   99|  100|     0
     198 | Uncorrectable Sectors      |        0|   99|  100|     0
     199 | UltraDMA CRC Error Rate    |        0|  200|  200|     0
     240 | Head Flying Hours          |        0|  253|  100| 88411901834003
     241 | Total Host Writes          |        0|  253|  100| 2194415541
     242 | Total Host Reads           |        0|  253|  100| 1655269662
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard disk drives)
     Device Description:           Disk drive
     Friendly Name:                ST3500412AS ATA Device
     Device Class:                 DiskDrive
     Device Location:              Channel 4, Target 0, Lun 0
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.23403
     Driver Date:                  6-21-2006
     Inf File:                     disk.inf
     Service Name:                 disk
     Hardware ID:                  IDE\DiskST3500412AS_____________________________CC32____
     Compatible ID:                GenDisk
     Parent ID:                    PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
                                   
                  +-----------------------------------------+
                  |                  ATAPI                  |
                  +-----------------------------------------+
   ATAPI
     ATAPI Model:                  PIONEER DVD-RW  DVR-217F
     ATAPI Type:                   DVD+-RW DL/CD-RW
     Interface Type:               Serial ATA I
     Physical Interface:           Serial ATAPI
     ATAPI Name:                   PIONEER DVD-RW  DVR-217F
     Vendor Specific:              09/03/04  PIONEER
     CD Read Speed:                16x (Current: 16x)
     CD Write Speed:               40x (Current: 32x)
     Buffer Size:                  1.95 MB
     Loading Mechanism:            Tray Type
     Rotation Control:             CLV
     Read Retry Count:             3
     Write Retry Count:            0
     Compatibility:                ATA/ATAPI-7
     Serial Number:                IEDP052900WL
     Controller Revision:          1.07
     Logical Drives:               K:
     Command DRQ Type:             Accelerated DRQ
     Command Packet Size:          12 bytes
     Location (Vendor):            Intel Corporation
     Location (Device):            8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
  Transfer Modes
     PIO Mode Support:             4
     SW DMA Mode Support:          Not Supported
     MW DMA Mode Support:          2, Active: None
     UDMA Mode Support:            4 (UltraDMA/66), Active: 2 (UltraDMA/33)
  Reading Features
     CD-R Disk Read:                      [X]
     CD-RW Disk Read:                     [X]
     DVD-ROM Disk Read:                   [X]
     DVD-RAM Disk Read:                   [X]
     DVD-R Disk Read:                     [X]
     DVD-R DL Disk Read:                  [X]
     DVD-RW Disk Read:                    [X]
     DVD-RW DL Disk Read:                 [ ]
     DVD+R Disk Read:                     [X]
     DVD+R DL Disk Read:                  [X]
     DVD+RW Disk Read:                    [X]
     DVD+RW DL Disk Read:                 [ ]
     BD-ROM Disk Read:                    [ ]
     BD-R Disk Read:                      [ ]
     BD-RE Disk Read:                     [ ]
     HD DVD-ROM Disk Read:                [ ]
     HD DVD-RAM Disk Read:                [ ]
     HD DVD-R Disk Read:                  [ ]
     HD DVD-R DL Disk Read:               [ ]
     HD DVD-RW Disk Read:                 [ ]
     HD DVD-RW DL Disk Read:              [ ]
     Read Packet Using Method 2:          [X]
     Read Mode2 Form1 Sectors:            [X]
     Read Mode2 Form2 Sectors:            [X]
     Multisession Disk Read:              [X]
     READ-CD Command on AudioCD:          [X]
     Read Bar Code Capable:               [ ]
     Read Lead-in (CD-Text):              [X]
  Writing Features
     CD-R Disk Write:                     [X]
     CD-RW Disk Write:                    [X]
     DVD-RAM Disk Write:                  [ ]
     DVD-R Disk Write:                    [X]
     DVD-R DL Disk Write:                 [X]
     DVD-RW Disk Write:                   [X]
     DVD+R Disk Write:                    [X]
     DVD+R DL Disk Write:                 [X]
     DVD+RW Disk Write:                   [X]
     DVD+RW DL Disk Write:                [ ]
     BD-R Disk Write:                     [ ]
     BD-RE Disk Write:                    [ ]
     HD DVD-R Disk Write:                 [ ]
     HD DVD-R DL Disk Write:              [ ]
     HD DVD-RAM Disk Write:               [ ]
     HD DVD-RW Disk Write:                [ ]
     HD DVD-RW DL Disk Write:             [ ]
     Test Write Mode Support:             [X]
     Buffer Underrun Protection:          [X]
  Other Features
     Audio Play Support:                  [X]
     CD-DA Stream is Accurate:            [X]
     Composite Audio/Video:               [ ]
     Digital Output on Port 1:            [ ]
     Digital Output on Port 2:            [ ]
     Support Subcode R-W:                 [ ]
     Support Subcode R-W D&C:             [ ]
     C2 Pointers Supported:               [X]
     ISRC Supported:                      [X]
     UPC Supported:                       [X]
  ATAPI Features
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [ ]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [X]
     ATA Software Reset:                  [ ]
     Overlap Operation:                   [ ]
     Command Queuing:                     [ ]
     Interleaving DMA:                    [ ]
     S.M.A.R.T.:                          [ ]
     S.M.A.R.T. Self-test:                [ ]
     S.M.A.R.T. Error Logging:            [ ]
     Security Mode Feature Set:           [ ]
     Removable Media:                     [ ]
     Power Management:                    [X] enabled
     PACKET Command:                      [X] enabled
     Write Cache:                         [ ]
     Look-ahead:                          [ ]
     Release Interrupt:                   [ ]
     Service Interrupt:                   [ ]
     Device Reset Command:                [X] enabled
     Host Protected Area:                 [ ]
     Write Verify Command:                [ ]
     Write Buffer Command:                [ ]
     Read Buffer Command:                 [ ]
     NOP Command:                         [ ]
     Identify Device DMA Command:         [ ]
     Download Microcode Command:          [ ]
     Read/Write DMA Queued:               [ ]
     CFA Feature Set:                     [ ]
     Advanced Power Management:           [ ]
     Removable Media Status:              [ ]
     Power-up in Standby:                 [ ]
     Set Features Req. to Spinup:         [ ]
     Set Max Security Extension:          [ ]
     Automatic Acoustic Management:       [ ]
     48-bit Address:                      [ ]
     Device Configuration Overlay:        [ ]
     Flush Cache Command:                 [ ]
     Flush Cache Ext Command:             [ ]
     Media Serial Number:                 [ ]
     Media Card Pass Through:             [ ]
     Streaming Feature Set:               [ ]
     General Purpose Logging:             [ ]
     Write DMA/Multiple FUA EXT:          [ ]
     Write DMA Queued FUA EXT:            [ ]
     World Wide Name:                     [ ]
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard CD-ROM drives)
     Device Description:           CD-ROM Drive
     Friendly Name:                PIONEER DVD-RW  DVR-217F ATA Device
     Device Class:                 CDROM
     Device Location:              Channel 5, Target 0, Lun 0
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.23403
     Driver Date:                  6-21-2006
     Inf File:                     cdrom.inf
     Service Name:                 cdrom
     Hardware ID:                  IDE\CdRomPIONEER_DVD-RW__DVR-217F________________1.07____
     Compatible ID:                GenCdRom
     Parent ID:                    PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
                                   
                  +-----------------------------------------+
                  |              Storage (ASPI)             |
                  +-----------------------------------------+
  Host: 3, Target: 0, LUN: 0         
     Device Name:                  Generic USB SD Reader
     Device Type:                  Disk Drive
     Compatibility:                Not Standard
     Vendor Specific:              
     Serial Number:                
     Controller Revision:          1.00
     Logical Drives:               M:
     Location:                     Host: 3, Target: 0, LUN: 0
     Bus Width:                    8-bit
     Address Width:                8-bit
     Location (Vendor):            Alcor Micro
     Location (Device):            USB 52-in-1 Card Reader/Writer
  ASPI Device Features
     Removable Medium:                    Yes
     Read Cache:                          [ ]
     Write Cache:                         [ ]
     Read Reallocate:                     [ ]
     Write Reallocate:                    [ ]
     Terminate I/O Process:               [ ]
     Normal ACA:                          [ ]
     Hierarchical Support:                [ ]
     Embedded Array Controller:           [ ]
     Protection Information:              [ ]
     Enclosure Services:                  [ ]
     Multi-Ported Device:                 [ ]
     Medium Changer:                      [ ]
     Relative Addressing:                 [ ]
     Synchronous Transfer:                [ ]
     Linked Commands:                     [ ]
     Soft Reset:                          [ ]
     Quick Arbitration:                   [ ]
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard disk drives)
     Device Description:           Disk drive
     Friendly Name:                Generic USB SD Reader USB Device
     Device Class:                 DiskDrive
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.23403
     Driver Date:                  6-21-2006
     Inf File:                     disk.inf
     Service Name:                 disk
     Hardware ID:                  USBSTOR\DiskGeneric_USB_SD_Reader___1.00
     Compatible ID:                USBSTOR\Disk
     Parent ID:                    USB\VID_058F&PID_6362&REV_0129
                                   
  Host: 3, Target: 0, LUN: 0         
     Device Name:                  Generic USB CF Reader
     Device Type:                  Disk Drive
     Compatibility:                Not Standard
     Vendor Specific:              
     Serial Number:                
     Controller Revision:          1.01
     Logical Drives:               N:
     Location:                     Host: 3, Target: 0, LUN: 0
     Bus Width:                    8-bit
     Address Width:                8-bit
     Location (Vendor):            Alcor Micro
     Location (Device):            USB 52-in-1 Card Reader/Writer
  ASPI Device Features
     Removable Medium:                    Yes
     Read Cache:                          [ ]
     Write Cache:                         [ ]
     Read Reallocate:                     [ ]
     Write Reallocate:                    [ ]
     Terminate I/O Process:               [ ]
     Normal ACA:                          [ ]
     Hierarchical Support:                [ ]
     Embedded Array Controller:           [ ]
     Protection Information:              [ ]
     Enclosure Services:                  [ ]
     Multi-Ported Device:                 [ ]
     Medium Changer:                      [ ]
     Relative Addressing:                 [ ]
     Synchronous Transfer:                [ ]
     Linked Commands:                     [ ]
     Soft Reset:                          [ ]
     Quick Arbitration:                   [ ]
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard disk drives)
     Device Description:           Disk drive
     Friendly Name:                Generic USB CF Reader USB Device
     Device Class:                 DiskDrive
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.23403
     Driver Date:                  6-21-2006
     Inf File:                     disk.inf
     Service Name:                 disk
     Hardware ID:                  USBSTOR\DiskGeneric_USB_CF_Reader___1.01
     Compatible ID:                USBSTOR\Disk
     Parent ID:                    USB\VID_058F&PID_6362&REV_0129
                                   
  Host: 3, Target: 0, LUN: 0         
     Device Name:                  Generic USB SM Reader
     Device Type:                  Disk Drive
     Compatibility:                Not Standard
     Vendor Specific:              
     Serial Number:                
     Controller Revision:          1.02
     Logical Drives:               O:
     Location:                     Host: 3, Target: 0, LUN: 0
     Bus Width:                    8-bit
     Address Width:                8-bit
     Location (Vendor):            Alcor Micro
     Location (Device):            USB 52-in-1 Card Reader/Writer
  ASPI Device Features
     Removable Medium:                    Yes
     Read Cache:                          [ ]
     Write Cache:                         [ ]
     Read Reallocate:                     [ ]
     Write Reallocate:                    [ ]
     Terminate I/O Process:               [ ]
     Normal ACA:                          [ ]
     Hierarchical Support:                [ ]
     Embedded Array Controller:           [ ]
     Protection Information:              [ ]
     Enclosure Services:                  [ ]
     Multi-Ported Device:                 [ ]
     Medium Changer:                      [ ]
     Relative Addressing:                 [ ]
     Synchronous Transfer:                [ ]
     Linked Commands:                     [ ]
     Soft Reset:                          [ ]
     Quick Arbitration:                   [ ]
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard disk drives)
     Device Description:           Disk drive
     Friendly Name:                Generic USB SM Reader USB Device
     Device Class:                 DiskDrive
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.23403
     Driver Date:                  6-21-2006
     Inf File:                     disk.inf
     Service Name:                 disk
     Hardware ID:                  USBSTOR\DiskGeneric_USB_SM_Reader___1.02
     Compatible ID:                USBSTOR\Disk
     Parent ID:                    USB\VID_058F&PID_6362&REV_0129
                                   
  Host: 3, Target: 0, LUN: 0         
     Device Name:                  Generic USB MS Reader
     Device Type:                  Disk Drive
     Compatibility:                Not Standard
     Vendor Specific:              
     Serial Number:                
     Controller Revision:          1.03
     Logical Drives:               P:
     Location:                     Host: 3, Target: 0, LUN: 0
     Bus Width:                    8-bit
     Address Width:                8-bit
     Location (Vendor):            Alcor Micro
     Location (Device):            USB 52-in-1 Card Reader/Writer
  ASPI Device Features
     Removable Medium:                    Yes
     Read Cache:                          [ ]
     Write Cache:                         [ ]
     Read Reallocate:                     [ ]
     Write Reallocate:                    [ ]
     Terminate I/O Process:               [ ]
     Normal ACA:                          [ ]
     Hierarchical Support:                [ ]
     Embedded Array Controller:           [ ]
     Protection Information:              [ ]
     Enclosure Services:                  [ ]
     Multi-Ported Device:                 [ ]
     Medium Changer:                      [ ]
     Relative Addressing:                 [ ]
     Synchronous Transfer:                [ ]
     Linked Commands:                     [ ]
     Soft Reset:                          [ ]
     Quick Arbitration:                   [ ]
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard disk drives)
     Device Description:           Disk drive
     Friendly Name:                Generic USB MS Reader USB Device
     Device Class:                 DiskDrive
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.23403
     Driver Date:                  6-21-2006
     Inf File:                     disk.inf
     Service Name:                 disk
     Hardware ID:                  USBSTOR\DiskGeneric_USB_MS_Reader___1.03
     Compatible ID:                USBSTOR\Disk
     Parent ID:                    USB\VID_058F&PID_6362&REV_0129
                                   
                  +-----------------------------------------+
                  |              Logical Drives             |
                  +-----------------------------------------+
  Local Drives
  C:[SYSTEM]
     Drive Letter:                 C:
     Drive Type:                   Fixed Disk
     Volume Label:                 SYSTEM
     File System:                  FAT
     Volume Serial Number:         F81A-AC7C
     Total Size:                   100.93 MB
     Free Space:                   9.05 MB (9.0%)
     Location:                     Samsung SSD 860 EVO 250GB (S3Y9NB0K275545B)
  D:[UTILITIES]
     Drive Letter:                 D:
     Drive Type:                   Fixed Disk
     Volume Label:                 UTILITIES
     File System:                  FAT32
     Volume Serial Number:         441A-C1C0
     Total Size:                   4.99 GB
     Free Space:                   1.49 GB (30.0%)
     Location:                     Samsung SSD 860 EVO 250GB (S3Y9NB0K275545B)
  E:[WIN10]
     Drive Letter:                 E:
     Drive Type:                   Fixed Disk
     Volume Label:                 WIN10
     File System:                  NTFS
     Volume Serial Number:         E8C6-391A
     Total Size:                   30.0 GB
     Free Space:                   29.84 GB (99.5%)
     Location:                     WDC WD1001FALS-00J7B0 (WD-WMATV0357962)
  F:[WINXP]
     Drive Letter:                 F:
     Drive Type:                   Fixed Disk
     Volume Label:                 WINXP
     File System:                  NTFS
     Volume Serial Number:         4EC7-F3C6
     Total Size:                   10.0 GB
     Free Space:                   2.25 GB (22.5%)
     Location:                     WDC WD1001FALS-00J7B0 (WD-WMATV0357962)
  G:[WIN7]
     Drive Letter:                 G:
     Drive Type:                   Fixed Disk
     Volume Label:                 WIN7
     File System:                  NTFS
     Volume Serial Number:         2648-A498
     Total Size:                   227.79 GB
     Free Space:                   138.35 GB (60.7%)
     Location:                     Samsung SSD 860 EVO 250GB (S3Y9NB0K275545B)
  H:[MUSIC]
     Drive Letter:                 H:
     Drive Type:                   Fixed Disk
     Volume Label:                 MUSIC
     File System:                  NTFS
     Volume Serial Number:         56C9-FD1A
     Total Size:                   891.51 GB
     Free Space:                   191.96 GB (21.5%)
     Location:                     WDC WD1001FALS-00J7B0 (WD-WMATV0357962)
  I:[WIN7MAX]
     Drive Letter:                 I:
     Drive Type:                   Fixed Disk
     Volume Label:                 WIN7MAX
     File System:                  NTFS
     Volume Serial Number:         B822-7007
     Total Size:                   111.79 GB
     Free Space:                   16.68 GB (14.9%)
     Location:                     SPCC Solid State Disk (2A40079618DB00135162)
  J:[WIN7MAXDATA]
     Drive Letter:                 J:
     Drive Type:                   Fixed Disk
     Volume Label:                 WIN7MAXDATA
     File System:                  NTFS
     Volume Serial Number:         4487-0B4F
     Total Size:                   465.76 GB
     Free Space:                   245.07 GB (52.6%)
     Location:                     ST3500412AS (6VV25CDT)
  K:
     Drive Letter:                 K:
     Drive Type:                   Optical Drive
     Location:                     PIONEER DVD-RW  DVR-217F
  M:
     Drive Letter:                 M:
     Drive Type:                   Removable Disk
     Location:                     Generic USB SD Reader
  N:
     Drive Letter:                 N:
     Drive Type:                   Removable Disk
     Location:                     Generic USB CF Reader
  O:
     Drive Letter:                 O:
     Drive Type:                   Removable Disk
     Location:                     Generic USB SM Reader
  P:
     Drive Letter:                 P:
     Drive Type:                   Removable Disk
     Location:                     Generic USB MS Reader
                                   
                  +-----------------------------------------+
                  |               USB Devices               |
                  +-----------------------------------------+
  USB Device 1
     Vendor (8087h):               Intel Corp.
     Device (8000h):               Integrated Rate Matching Hub
     Manufacturer:                 
     Product:                      
     Serial Number:                
     Device Version:               0.05
     Class (09h):                  Hub
     SubClass (00h):               Unused
     Protocol (01h):               Single TT
     Configuration:                
     USB Version:                  2.00
     Speed:                        480 Mb/s
     Transfer Type:                Interrupt
     Data Packet Size:             64 bytes
     Max Power:                    Remote Wakeup
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Generic USB Hub)
     Device Description:           Generic USB Hub
     Device Class:                 USB
     Device Location:              Port_#0001.Hub_#0002
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24138
     Driver Date:                  6-21-2006
     Inf File:                     usb.inf
     Service Name:                 usbhub
     Hardware ID:                  USB\VID_8087&PID_8000&REV_0005
     Compatible ID:                USB\Class_09&SubClass_00&Prot_00
     Parent ID:                    PCI\VEN_8086&DEV_8C26&SUBSYS_50061458&REV_05
  Interface 1
     Class (09h):                  Hub
     SubClass (00h):               Unused
     Protocol (00h):               Full Speed (or Root) Hub
     Interface:                    
                                   
  USB Device 2
     Vendor (8087h):               Intel Corp.
     Device (8008h):               Integrated Rate Matching Hub
     Manufacturer:                 
     Product:                      
     Serial Number:                
     Device Version:               0.05
     Class (09h):                  Hub
     SubClass (00h):               Unused
     Protocol (01h):               Single TT
     Configuration:                
     USB Version:                  2.00
     Speed:                        480 Mb/s
     Transfer Type:                Interrupt
     Data Packet Size:             64 bytes
     Max Power:                    Remote Wakeup
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Generic USB Hub)
     Device Description:           Generic USB Hub
     Device Class:                 USB
     Device Location:              Port_#0001.Hub_#0001
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24138
     Driver Date:                  6-21-2006
     Inf File:                     usb.inf
     Service Name:                 usbhub
     Hardware ID:                  USB\VID_8087&PID_8008&REV_0005
     Compatible ID:                USB\Class_09&SubClass_00&Prot_00
     Parent ID:                    PCI\VEN_8086&DEV_8C2D&SUBSYS_50061458&REV_05
  Interface 1
     Class (09h):                  Hub
     SubClass (00h):               Unused
     Protocol (00h):               Full Speed (or Root) Hub
     Interface:                    
                                   
  USB Device 3
     Vendor (093Ah):               Pixart Imaging
     Device (2532h):               Gaming Mouse
     Manufacturer:                 PixArt
     Product:                      Gaming Mouse
     Serial Number:                
     Device Version:               1.00
     Class (00h):                  Unknown
     SubClass (00h):               Unknown
     Protocol (00h):               Unknown
     Configuration:                
     USB Version:                  2.00
     Speed:                        480 Mb/s
     Transfer Type:                Interrupt
     Data Packet Size:             8 bytes
     Max Power:                    100 mA Remote Wakeup
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard USB Host Controller)
     Device Description:           USB Composite Device
     Device Class:                 USB
     Device Location:              Port_#0004.Hub_#0001
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24138
     Driver Date:                  6-21-2006
     Inf File:                     usb.inf
     Service Name:                 usbccgp
     Hardware ID:                  USB\VID_093A&PID_2532&REV_0100
     Compatible ID:                IUSB3\DevClass_00&SubClass_00&Prot_00
     Parent ID:                    PCI\VEN_8086&DEV_8C31&SUBSYS_50071458&REV_05
  Interface 1
     Class (03h):                  Human Interface Devices
     SubClass (01h):               Boot Interface Subclass
     Protocol (02h):               Mouse
     Interface:                    
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard system devices)
     Device Description:           USB Input Device
     Device Class:                 HIDClass
     Device Location:              0000.0014.0000.004.000.000.000.000.000
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24386
     Driver Date:                  6-21-2006
     Inf File:                     input.inf
     Service Name:                 HidUsb
     Hardware ID:                  USB\VID_093A&PID_2532&REV_0100&MI_00
     Compatible ID:                USB\Class_03&SubClass_01&Prot_02
     Parent ID:                    USB\VID_093A&PID_2532&REV_0100
  Interface 2
     Class (03h):                  Human Interface Devices
     SubClass (00h):               No Subclass
     Protocol (01h):               Keyboard
     Interface:                    
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard system devices)
     Device Description:           USB Input Device
     Device Class:                 HIDClass
     Device Location:              0000.0014.0000.004.000.000.000.000.000
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24386
     Driver Date:                  6-21-2006
     Inf File:                     input.inf
     Service Name:                 HidUsb
     Hardware ID:                  USB\VID_093A&PID_2532&REV_0100&MI_01
     Compatible ID:                USB\Class_03&SubClass_00&Prot_01
     Parent ID:                    USB\VID_093A&PID_2532&REV_0100
                                   
  USB Device 4
     Vendor (058Fh):               Alcor Micro
     Device (6362h):               USB 52-in-1 Card Reader/Writer
     Manufacturer:                 Generic
     Product:                      Mass Storage Device
     Serial Number:                058F312D81B
     Device Version:               1.29
     Class (00h):                  Unknown
     SubClass (00h):               Unknown
     Protocol (00h):               Unknown
     Configuration:                
     USB Version:                  2.00
     Speed:                        480 Mb/s
     Transfer Type:                Bulk
     Data Packet Size:             64 bytes
     Max Power:                    250 mA
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 Compatible USB storage device
     Device Description:           USB Mass Storage Device
     Device Class:                 USB
     Device Location:              Port_#0006.Hub_#0001
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.23403
     Driver Date:                  6-21-2006
     Inf File:                     usbstor.inf
     Service Name:                 USBSTOR
     Hardware ID:                  USB\VID_058F&PID_6362&REV_0129
     Compatible ID:                USB\Class_08&SubClass_06&Prot_50
     Parent ID:                    PCI\VEN_8086&DEV_8C31&SUBSYS_50071458&REV_05
  Interface 1
     Class (08h):                  Mass Storage
     SubClass (06h):               SCSI
     Protocol (50h):               Bulk (Zip)
     Interface:                    
                                   
  USB Device 5
     Vendor (04A9h):               Canon
     Device (2660h):               LaserBase MF3110 Scanner/Printer
     Manufacturer:                 Canon,Inc.
     Product:                      MF3110
     Serial Number:                2363E2124558
     Device Version:               0.00
     Class (00h):                  Unknown
     SubClass (00h):               Unknown
     Protocol (00h):               Unknown
     Configuration:                
     USB Version:                  2.00
     Speed:                        480 Mb/s
     Transfer Type:                Bulk/Interrupt
     Data Packet Size:             64 bytes
     Max Power:                    2 mA Self-Powered
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard USB Host Controller)
     Device Description:           USB Composite Device
     Device Class:                 USB
     Device Location:              Port_#0012.Hub_#0001
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24138
     Driver Date:                  6-21-2006
     Inf File:                     usb.inf
     Service Name:                 usbccgp
     Hardware ID:                  USB\VID_04A9&PID_2660&REV_0000
     Compatible ID:                IUSB3\DevClass_00&SubClass_00&Prot_00
     Parent ID:                    PCI\VEN_8086&DEV_8C31&SUBSYS_50071458&REV_05
  Interface 1
     Class (FFh):                  Vendor Specific Class
     SubClass (00h):               Unknown
     Protocol (FFh):               Unknown
     Interface:                    
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 Canon
     Device Description:           Canon MF3110
     Device Class:                 Image
     Device Location:              0000.0014.0000.012.000.000.000.000.000
     Driver Provider:              Canon
     Driver Version:               11.3.0.0
     Driver Date:                  2-1-2007
     Inf File:                     oem40.inf
     Service Name:                 usbscan
     Hardware ID:                  USB\VID_04A9&PID_2660&REV_0000&MI_00
     Compatible ID:                USB\Class_ff&SubClass_00&Prot_ff
     Parent ID:                    USB\VID_04A9&PID_2660&REV_0000
  Interface 2
     Class (07h):                  Printer
     SubClass (01h):               Printer
     Protocol (02h):               Bidirectional
     Interface:                    
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 Microsoft
     Device Description:           USB Printing Support
     Device Class:                 USB
     Device Location:              0000.0014.0000.012.000.000.000.000.000
     Driver Provider:              Microsoft
     Driver Version:               6.1.7600.16385
     Driver Date:                  6-21-2006
     Inf File:                     usbprint.inf
     Service Name:                 usbprint
     Hardware ID:                  USB\VID_04A9&PID_2660&REV_0000&MI_01
     Compatible ID:                USB\Class_07&SubClass_01&Prot_02
     Parent ID:                    USB\VID_04A9&PID_2660&REV_0000
                                   
                  +-----------------------------------------+
                  |            Physical Printers            |
                  +-----------------------------------------+
  USB Printer 1
     Vendor (04A9h):               Canon
     Device (2660h):               LaserBase MF3110 Scanner/Printer
     Manufacturer:                 Canon,Inc.
     Product:                      MF3110
     Serial Number:                2363E2124558
     Device Version:               0.00
     Class (00h):                  Unknown
     SubClass (00h):               Unknown
     Protocol (00h):               Unknown
     Configuration:                
     USB Version:                  2.00
     Speed:                        480 Mb/s
     Transfer Type:                Bulk/Interrupt
     Data Packet Size:             64 bytes
     Max Power:                    2 mA Self-Powered
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard USB Host Controller)
     Device Description:           USB Composite Device
     Device Class:                 USB
     Device Location:              Port_#0012.Hub_#0001
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24138
     Driver Date:                  6-21-2006
     Inf File:                     usb.inf
     Service Name:                 usbccgp
     Hardware ID:                  USB\VID_04A9&PID_2660&REV_0000
     Compatible ID:                IUSB3\DevClass_00&SubClass_00&Prot_00
     Parent ID:                    PCI\VEN_8086&DEV_8C31&SUBSYS_50071458&REV_05
                                   
                  +-----------------------------------------+
                  |            Installed Printers           |
                  +-----------------------------------------+
  Local Printers
  Installed Printer 1
     Printer Name:                 Microsoft XPS Document Writer
     Printer Port:                 XPSPort:
     Default Printer:              No
     Printer Type:                 Local
     Print Processor:              winprint
     Data Type:                    RAW
                                   
  Installed Printer 2
     Printer Name:                 Fax
     Printer Port:                 SHRFAX:
     Default Printer:              No
     Printer Type:                 Local
     Print Processor:              winprint
     Data Type:                    RAW
                                   
  Installed Printer 3
     Printer Name:                 Canon MF5700 Series
     Printer Port:                 USB001
     Default Printer:              Yes
     Printer Type:                 Local
     Print Processor:              winprint
     Data Type:                    RAW
                                   
                  +-----------------------------------------+
                  |              Slots (SMBIOS)             |
                  +-----------------------------------------+
  Slot PCI Express
     Slot Type:                    PCI Express
     Current Usage:                In Use
     Data Bus Width:               16x or x16
     Slot Designation:             J6B2
     Slot Length:                  Long Length
     Slot ID:                      0
  Slot PCI Express
     Slot Type:                    PCI Express
     Current Usage:                In Use
     Data Bus Width:               1x or x1
     Slot Designation:             J6B1
     Slot Length:                  Short Length
     Slot ID:                      1
  Slot PCI Express
     Slot Type:                    PCI Express
     Current Usage:                In Use
     Data Bus Width:               8x or x8
     Slot Designation:             J6D1
     Slot Length:                  Short Length
     Slot ID:                      2
  Slot PCI Express
     Slot Type:                    PCI Express
     Current Usage:                In Use
     Data Bus Width:               16x or x16
     Slot Designation:             J7B1
     Slot Length:                  Short Length
     Slot ID:                      3
  Slot PCI Express
     Slot Type:                    PCI Express
     Current Usage:                In Use
     Data Bus Width:               1x or x1
     Slot Designation:             J8B4
     Slot Length:                  Short Length
     Slot ID:                      4
  Slot PCI
     Slot Type:                    PCI
     Current Usage:                In Use
     Data Bus Width:               32 bit
     Slot Designation:             J8B3
     Slot Length:                  Short Length
     Slot ID:                      6
                                   
                  +-----------------------------------------+
                  |              Ports (SMBIOS)             |
                  +-----------------------------------------+
  Port 1 Mouse Port
     Int. Connector Type:          None
     Ext. Connector Type:          PS/2
     Port Type:                    Mouse Port
     Int. Designator:              J1A1
     Ext. Designator:              PS2Mouse
  Port 2 Keyboard Port
     Int. Connector Type:          None
     Ext. Connector Type:          PS/2
     Port Type:                    Keyboard Port
     Int. Designator:              J1A1
     Ext. Designator:              Keyboard
  Port 3 Other
     Int. Connector Type:          None
     Ext. Connector Type:          Mini-Centronics Type-14
     Port Type:                    Other
     Int. Designator:              J2A1
     Ext. Designator:              TV Out
  Port 4 Serial Port 16550A Compatible
     Int. Connector Type:          None
     Ext. Connector Type:          DB-9 pin male
     Port Type:                    Serial Port 16550A Compatible
     Int. Designator:              J2A2A
     Ext. Designator:              COM A
  Port 5 Video Port
     Int. Connector Type:          None
     Ext. Connector Type:          DB-15 pin female
     Port Type:                    Video Port
     Int. Designator:              J2A2B
     Ext. Designator:              Video
  Port 6 USB
     Int. Connector Type:          None
     Ext. Connector Type:          USB
     Port Type:                    USB
     Int. Designator:              J3A1
     Ext. Designator:              USB1
  Port 7 USB
     Int. Connector Type:          None
     Ext. Connector Type:          USB
     Port Type:                    USB
     Int. Designator:              J3A1
     Ext. Designator:              USB2
  Port 8 USB
     Int. Connector Type:          None
     Ext. Connector Type:          USB
     Port Type:                    USB
     Int. Designator:              J3A1
     Ext. Designator:              USB3
  Port 9 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J9A1 - TPM HDR
     Ext. Designator:              
  Port 10 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J9C1 - PCIE DOCKING CONN
     Ext. Designator:              
  Port 11 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J2B3 - CPU FAN
     Ext. Designator:              
  Port 12 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J6C2 - EXT HDMI
     Ext. Designator:              
  Port 13 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J3C1 - GMCH FAN
     Ext. Designator:              
  Port 14 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J1D1 - ITP
     Ext. Designator:              
  Port 15 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J9E2 - MDC INTPSR
     Ext. Designator:              
  Port 16 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J9E4 - MDC INTPSR
     Ext. Designator:              
  Port 17 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J9E3 - LPC HOT DOCKING
     Ext. Designator:              
  Port 18 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J9E1 - SCAN MATRIX
     Ext. Designator:              
  Port 19 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J9G1 - LPC SIDE BAND
     Ext. Designator:              
  Port 20 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J8F1 - UNIFIED
     Ext. Designator:              
  Port 21 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J6F1 - LVDS
     Ext. Designator:              
  Port 22 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J2F1 - LAI FAN
     Ext. Designator:              
  Port 23 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J2G1 - GFX VID
     Ext. Designator:              
  Port 24 Other
     Int. Connector Type:          Other
     Ext. Connector Type:          None
     Port Type:                    Other
     Int. Designator:              J1G6 - AC JACK
     Ext. Designator:              
                                   
                  +-----------------------------------------+
                  |                 Network                 |
                  +-----------------------------------------+
  Network
     Network Name:                 A2KKV
     User Name:                    KKV1
     User Role:                    Administrator
     Logon Domain:                 A2KKV
  Interface 1
     Adapter Vendor:               Realtek Semiconductor
     Adapter Name:                 RTL8111/8168/8411 PCI Express Gigabit Ethernet Controller
     Subsys Vendor:                Giga-Byte Technology
     Subsystem ID:                 GA-EP45-DS5 Motherboard
     Bus Type:                     PCI Express 2.0 x1
     Description:                  Realtek PCIe GbE Family Controller
     MAC Address:                  1C-1B-0D-B1-81-06
     Adapter Type:                 Ethernet
     Link Speed:                   100.0 Mbps
     MTU Size:                     1500 byte
     Adapter Status:               Enabled
     Operational Status:           Operational
     DHCP Server:                  192.168.1.1
     IP Address:                   192.168.1.61
     IP Address Subnet Mask:       255.255.255.0
     Gateway:                      192.168.1.1
     DNS Server:                   192.168.1.1
  Interface 2
     Description:                  VirtualBox Host-Only Ethernet Adapter
     MAC Address:                  0A-00-27-00-00-10
     Adapter Type:                 Ethernet
     Link Speed:                   1000.0 Mbps
     MTU Size:                     1500 byte
     Adapter Status:               Enabled
     Operational Status:           Operational
     DHCP Enabled:             No
     IP Address:                   192.168.56.1
     IP Address Subnet Mask:       255.255.255.0
     Gateway:                      0.0.0.0
                                   
                  +-----------------------------------------+
                  |                 Monitor                 |
                  +-----------------------------------------+
  Monitor
     Monitor Vendor:               BenQ
     Monitor Model:                BenQ GW2470
     Viewable Size:                23.8" (60.4 sm)
     Serial Number:                21573
     Manufacture Date:             August 2016
     EDID Version:                 1.3
     Monitor ID:                   BNQ78D9
     Aspect Ratio:                 16:9
     Horizontal Size:              527 mm
     Vertical Size:                296 mm
     Gamma Factor:                 2.200
     Display Type:                 RGB Color
     Input Signal:                 Digital
     Internal Model:               BenQ GW2470
     Internal Number:              K8G00916019
     Vertical Frequency:           50-76 Hz
     Horizontal Frequency:         30-83 kHz
  DPMS Features
     Active Off:                   [X]
     Suspend:                      [ ]
     Standby:                      [ ]
  Supported Modes
     Mode 1:                       640x480   @ 60 Hz (VGA)
     Mode 2:                       640x480   @ 75 Hz (VESA)
     Mode 3:                       720x400   @ 70 Hz (VGA)
     Mode 4:                       800x600   @ 60 Hz (VESA)
     Mode 5:                       800x600   @ 75 Hz (VESA)
     Mode 6:                       832x624   @ 75 Hz (Mac II)
     Mode 7:                       1024x768  @ 60 Hz (VESA)
     Mode 8:                       1024x768  @ 75 Hz (VESA)
     Mode 9:                       1152x870  @ 75 Hz (Mac II)
     Mode 10:                      1280x720  @ 60 Hz
     Mode 11:                      1280x800  @ 60 Hz
     Mode 12:                      1280x1024 @ 60 Hz
     Mode 13:                      1280x1024 @ 75 Hz (VESA)
     Mode 14:                      1600x900  @ 60 Hz
     Mode 15:                      1680x1050 @ 60 Hz
     Mode 16:                      1920x1080 @ 60 Hz (Recommended)
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 (Standard monitor types)
     Device Description:           Generic PnP Monitor
     Device Class:                 Monitor
     Driver Provider:              Microsoft
     Driver Version:               6.1.7601.24521
     Driver Date:                  6-21-2006
     Inf File:                     monitor.inf
     Service Name:                 monitor
     Hardware ID:                  MONITOR\BNQ78D9
     Compatible ID:                *PNP09FF
     Parent ID:                    PCI\VEN_10DE&DEV_1B81&SUBSYS_119D10DE&REV_A1
                                   
                  +-----------------------------------------+
                  |                  Video                  |
                  +-----------------------------------------+
  Video
     Video Chip Vendor:            Nvidia Corp
     Video Chip:                   GP104 [GeForce GTX 1070]
     Subsystem Vendor:             Nvidia Corp
     Full Name:                    Nvidia GeForce GTX 1070
     Code Name:                    GP104-A
     Revision:                     A1h
     Video Memory Size:            8 GB
     Memory Type:                  256-bit GDDR5 (Micron)
     GPU Type:                     Desktop Discrete
     Video BIOS Version:           Version 86.04.50.00.1E 
     Video BIOS Date:              10/17/16
     GPU Manufacturer:             TSMC
     Unified Shaders:              1920
     Pixel Pipelines (ROPS):       64
     Current Resolution:           1920x1080 32bpp @ 75 Hz
     Driver Version:               R442.19
     Bus Type:                     PCI Express 3.0 x16
  Base Clocks
     Base Core Clock:              1556 MHz
     Base Memory Clock:            2002 MHz (Effective: 8008 MHz)
     Memory Bandwidth:             256.3 GB/s
  Boost Clocks
     Boost Core Clock:             1746 MHz
     Boost Memory Clock:           2002 MHz (Effective: 8008 MHz)
     Memory Bandwidth:             256.3 GB/s
  Hardware Monitoring
     Core Temperature:             36 °C (97 °F)
     Current Core Clock:           139 MHz
     Current Memory Clock:         202 MHz (Effective: 808 MHz)
     Core Usage:                   0 %
     Memory Usage:                 2 %
     Memory Controller Usage:      3 %
     Video Engine Usage:           0 %
     Bus Interface Load:           0 %
     Fan Speed:                    0 rpm
     Fan Speed:                    0 %
  Performance Profile 0
     Core Clock:                   1962 MHz
     Memory Clock:                 2002 MHz
  Performance Profile 2
     Core Clock:                   3802 MHz
     Memory Clock:                 1901 MHz
  Performance Profile 5
     Core Clock:                   139 MHz
     Memory Clock:                 405 MHz
  Performance Profile 8
     Core Clock:                   139 MHz
     Memory Clock:                 202 MHz
  PCI-E Capabilities
     PCI Express Version:          3.0
     Device/Port Type:             Legacy PCI-E Endpoint
     Link Speed:                   8.0 GB/s (Current: 2.5 GB/s)
     Link Width:                   x16 (Current: x16)
     Link Port Number:             0
     Physical Slot Number:         0
  Driver
     Driver Status:                The device is working properly
     Manufacturer:                 NVIDIA
     Device Description:           NVIDIA GeForce GTX 1070
     Device Class:                 Display
     Device Location:              PCI bus 1, device 0, function 0
     Driver Provider:              NVIDIA
     Driver Version:               26.21.14.4219
     Driver Date:                  1-29-2020
     Inf File:                     oem15.inf
     Service Name:                 nvlddmkm
     Hardware ID:                  PCI\VEN_10DE&DEV_1B81&SUBSYS_119D10DE&REV_A1
     Compatible ID:                PCI\VEN_10DE&DEV_1B81&REV_A1
     Parent ID:                    PCI\VEN_8086&DEV_0C01&SUBSYS_50001458&REV_06
                                   
                  +-----------------------------------------+
                  |           Hardware Monitoring           |
                  +-----------------------------------------+
  Processor 
     Processor:                    Intel Xeon E3-1246 v3 3500 MHz
     Core Voltage:                 0.754 V
     Package Temperature:          39 °C (102 °F)
  Core 1
     Temperature Core:             38 °C (100 °F)
     Core Clock:                   798.2 MHz (Original: 3500 MHz)
     FSB Clock:                    99.8 MHz
     Multiplier:                   8.0
  Core 2
     Temperature Core:             36 °C (97 °F)
     Core Clock:                   798.2 MHz (Original: 3500 MHz)
     FSB Clock:                    99.8 MHz
     Multiplier:                   8.0
  Core 3
     Temperature Core:             36 °C (97 °F)
     Core Clock:                   798.2 MHz (Original: 3500 MHz)
     FSB Clock:                    99.8 MHz
     Multiplier:                   8.0
  Core 4
     Temperature Core:             38 °C (100 °F)
     Core Clock:                   798.2 MHz (Original: 3500 MHz)
     FSB Clock:                    99.8 MHz
     Multiplier:                   8.0
  Video Card 
     Video Chip:                   GP104 [GeForce GTX 1070]
     Core Temperature:             36 °C (97 °F)
     Current Core Clock:           139 MHz (Original: 1556 MHz)
     Current Memory Clock:         202 MHz (Original: 2002 MHz)
     Core Usage:                   0 %
     Memory Usage:                 2 %
     Memory Controller Usage:      3 %
     Video Engine Usage:           0 %
     Bus Interface Load:           0 %
     Fan Speed:                    0 rpm
     Fan Speed:                    0 %
  Disk Drive 1 
     Disk Model:                   SPCC Solid State Disk
     Disk Temperature:             33 °C (91 °F)
     Total Host Writes:            3.31 TB
  Disk Drive 2 
     Disk Model:                   WDC WD1001FALS-00J7B0
     Disk Temperature:             42 °C (108 °F)
  Disk Drive 3 
     Disk Model:                   Samsung SSD 860 EVO 250GB
     Disk Temperature:             39 °C (102 °F)
     Total Host Writes:            6.58 TB
  Disk Drive 4 
     Disk Model:                   ST3500412AS
     Disk Temperature:             35 °C (95 °F)
     Total Host Writes:            1.02 TB
     Total Host Reads:             789.29 GB
                                   
                  +-----------------------------------------+
                  |          Drivers Troubleshooter         |
                  +-----------------------------------------+
  List of Problem Devices
     All devices are working properly
                                   
                  +-----------------------------------------+
                  |            Disk Diagnostics             |
                  +-----------------------------------------+
  Disk 1 Status
     Disk Model:                   SPCC Solid State Disk
     Disk Size:                    114473 MB (111.79 GB)
     Interface Type:               Serial ATA III (SATA/600)
     Serial Number:                2A40079618DB00135162
     Controller Revision:          SBFM61.3
     Disk Marketing Size:          120034 MB (120.03 GB)
     Buffer Size:                  Unknown
     Location (Vendor):            Intel Corporation
     Location (Device):            8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
     Device Location:              Secondary/Master
     Disk Temperature:             33 °C (91 °F)
     Disk Health Status:           Good
     SSD Remaining Life:           100 %
     Total Host Writes:            3.31 TB
                                   
  Disk 2 Status
     Disk Model:                   WDC WD1001FALS-00J7B0
     Disk Size:                    953869 MB (931.51 GB)
     Interface Type:               Serial ATA II (SATA/300)
     Serial Number:                WD-WMATV0357962
     Controller Revision:          05.00K05
     Disk Marketing Size:          1000204 MB (1000.2 GB)
     Buffer Size:                  32767.5 kB
     Location (Vendor):            Intel Corporation
     Location (Device):            8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
     Device Location:              8th/Slave
     Disk Temperature:             42 °C (108 °F)
     Reallocated Sectors:          0
     Disk Health Status:           Good
                                   
  Disk 3 Status
     Disk Model:                   Samsung SSD 860 EVO 250GB
     Disk Size:                    238475 MB (232.89 GB)
     Interface Type:               Serial ATA III (SATA/600)
     Serial Number:                S3Y9NB0K275545B
     Controller Revision:          RVT01B6Q
     Disk Marketing Size:          250059 MB (250.06 GB)
     Buffer Size:                  Unknown
     Location (Vendor):            Intel Corporation
     Location (Device):            8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
     Device Location:              8th/Slave
     Disk Temperature:             39 °C (102 °F)
     Reallocated Sectors:          0
     Disk Health Status:           Good
     SSD Remaining Life:           100 %
     Total Host Writes:            6.58 TB
                                   
  Disk 4 Status
     Disk Model:                   ST3500412AS
     Disk Size:                    476940 MB (465.76 GB)
     Interface Type:               Serial ATA II (SATA/300)
     Serial Number:                6VV25CDT
     Controller Revision:          CC32
     Disk Marketing Size:          500108 MB (500.11 GB)
     Buffer Size:                  16384.0 kB
     Location (Vendor):            Intel Corporation
     Location (Device):            8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
     Device Location:              8th/Slave
     Disk Temperature:             35 °C (95 °F)
     Reallocated Sectors:          1991
     Disk Health Status:           Bad
     Total Host Writes:            1.02 TB
     Total Host Reads:             789.29 GB
                                   
                  +-----------------------------------------+
                  |                 Windows                 |
                  +-----------------------------------------+
  Windows
     Operating System:             MS Windows 7 Professional x64 Edition (6.1.7601 Service Pack 1)
     OS Language:                  English (United States)
     Windows Folder:               G:\Windows
     Installation Date:            February 10, 2020
     Kernel Type:                  Multiprocessor Free
     Registered Owner:             KKV1
     Registered Organization:      
     Product ID:                   00371-OEM-8992671-00407
     Product Key:                  XXXXX-XXXXX-XXXXX-XXXXX-XXXXX
     System UpTime:                0 Hour(s) 15 Minutes 7 Seconds
     IE Version:                   9.11.9600.19596
     DirectX Version:              DirectX 11
  Regional Settings
     Country:                      Russia
     Language:                     Russian
     Time Zone:                    Romance Standard Time (GMT+3)
     Currency Name:                Russian Ruble
     Measurment System:            Metric
     ANSI Code Page:               1251
     OEM Code Page:                866
                                   
                  +-----------------------------------------+
                  |            Installed Programs           |
                  +-----------------------------------------+
  Installed Programs
     Program Name                                       | Version        |                      Publisher|       Date|      Size| 
     ---------------------------------------------------+----------------+-------------------------------+-----------+----------+------
     ASTRA32 - Advanced System Information Tool         | 3.81           |                    Sysinfo Lab|           |          | 
                                   
                  +-----------------------------------------+
                  |            Installed Hotfixes           |
                  +-----------------------------------------+
  Installed Hotfixes
     Hotfix for Microsoft Windows (KB2496898):
     Hotfix for Microsoft Windows (KB2990941):
     Hotfix for Microsoft Windows (KB3006137):
                                   
                                [End of Report]                               
