 
              7800 Family Managers for Windows NT 3.5x  
              ========================================


This diskette contains Adaptec's Windows NT solution for the AIC-7800 Family
of Host Adapters.  This includes:

      AHA-2910      PCI-to-Fast SCSI (non-bootable)
      AHA-2940      PCI-to-Fast SCSI
      AHA-2940W     PCI-to-Fast and Wide Single-Ended SCSI
      AHA-2940U     PCI-to-Fast20 SCSI
      AHA-2940UW    PCI-to-Fast20 and Wide Single-Ended SCSI
      AHA-2944W     PCI-to-Fast and Wide Differential SCSI
      AHA-2940AU    PCI-to-Fast20 SCSI
      AHA-3940      MultiChannel PCI-to-Fast SCSI
      AHA-3940W     MultiChannel PCI-to-Fast and Wide SCSI
      AHA-3940U     MultiChannel PCI-to-Fast20 SCSI
      AHA-3940UW    MultiChannel PCI-to-Fast20 and Wide SCSI
      AIC-7850      Single-Chip PCI-to-Fast SCSI
      AIC-7855      Single-Chip PCI-to-Fast SCSI
      AIC-7860      Single-Chip PCI-to-Fast20 SCSI
      AIC-7870      Single-Chip PCI-to-Fast and Wide SCSI
      AIC-7880      Single-Chip PCI-to-Fast20 SCSI

             
The following files on this diskette are required for the installation of  
the 7800 family Windows NT drivers:  
  
     Windows NT 3.5
       \DISK1                   - Disk tag file  
       \TXTSETUP.OEM            - Install script used during NT installation
       \WINNT\3_5\AIC78XX.SYS   - Adaptec 7800 family driver v1.30 for Windows NT 3.5
       \WINNT\3_5\README.TXT    - Readme for installation of driver for Windows NT 3.5
       \WINNT\3_5\OEMSETUP.INF  - Install script used by Windows NT Setup
