
	 Adaptec 7800 Family Managers for NetWare 3.1X and 4.XX
	 ======================================================

This disk contains Adaptec's Novell solution for the AIC-7800 Family of
Host Adapters. This includes AHA-2940s (PCI to SCSI), AHA-2940Ws (PCI
to SCSI with wide channel), AHA-2944Ws (PCI to Wide Differential SCSI),
AHA-3940 (PCI MultiChannel SCSI), AHA-3940Ws (PCI MultiChannel Wide SCSI),
AHA-2910 (PCI to SCSI without BIOS), AIC-7870 (Chip on the motherboard
supporting wide channel), AIC-7850 (Chip on the motherboard supporting
8-bit SCSI channel).

Manager Set 1.2 begins support for Adaptec's new line of double-speed
PCI to SCSI products:  AIC-7880 (Chip on the motherboard),
and AHA-2940UltraWide (PCI to Wide SCSI board).

NOTE: To use CD-ROM's in conjunction with these drivers, EZ-SCSI version 3.03
or above must be installed.

The files included on this diskette which are required for the installation
of the NetWare drivers are as follows:

       \netware\v3_1x\aic7870.dsk
       \netware\v3_1x\aspitran.dsk
       \netware\v3_1x\aspicd.dsk

       \netware\v4_xx\aic7870.dsk
       \netware\v4_xx\aic7870.ddi
       \netware\v4_xx\aspitran.dsk
       \netware\v4_xx\aspicd.dsk
       \netware\v4_xx\aspicd.ddi

If required, please consult your DOS manual on how to move around the
directory tree.

Within a subdirectory, you will find a README.TXT file describing the
driver(s) contained in that subdirectory.


This disk provides the following NetWare drivers:

-----------------------------------------------------------------------------

1.) AIC-7870 Family of Host Adapters Driver For NetWare 386 v3.1x.

	  (\netware\v3_1x)

-----------------------------------------------------------------------------

2.) AIC-7870 Family of Host Adapters Driver For NetWare 386 v4.xx.

	  (\netware\v4_xx)

-----------------------------------------------------------------------------

3.) ASPITRAN.DSK ASPI Transport Layer Manager Driver for NetWare v3.1x and
    v4.xx.

	  (\netware\v3_1x)
		  or
	  (\netware\v4_xx)

-----------------------------------------------------------------------------

4.) AIC7870.DDI Driver definition information file for NetWare v4.xx only.

	  (\netware\v4_xx)

-----------------------------------------------------------------------------

5.) ASPICD.DSK CD-ROM Driver for NetWare v3.1x and v4.xx.

	  (\netware\v3_1x)
		   or
	    (.\netware\v4_xx)

-----------------------------------------------------------------------------

6.) ASPICD.DDI CD-ROM Driver definition information file for NetWare v4.xx
    only.

	    (.\netware\v4_xx)

-----------------------------------------------------------------------------

=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

Problem with DDI file for Netware 4.0X
--------------------------------------
There is a known problem which occurs during the installation of Netware 4.0X.
This problem involves the DDI file used during the initialization of the
host adapter device driver. The problem is that the DDI does not contain all
the possible slot number options available on all PCI systems, as there are
too many combinations. As a result, during the installation procedure, NetWare
will report that it was unable to load the driver in the given amount of time.
The cause of this is because the DDI file does not contain any slot options,
which causes NetWare to be unable to load the driver. Note, however, that this
is not an error. The user simply needs to go to the console screen and manually
enter in the correct slot number and installation will continue.

Problem with Quantum Empire 540S drives
---------------------------------------
A second known problem exists that will hang the server after loading the
host adapter device driver. This problem involves targets that do not support
scanning of multiple luns, with the command line option lun_enable.  The
user simply needs to set the command line option multlun_targets to only scan
targets that support multiple luns.  This problem is known to occur with
Quantum Empire 540S drives.
