ASUS PCI-AV868 Windows Driver V1.40 Release Notes

Date:	July 31, 1995

Xing(TM) Native-MPEG(TM) Driver Support
=======================================
To play a MPEG file:
    Method 1:
	* In Windows, open up the Program Manager window.
	* Select the "Run" command from the Program Manager's "File" menu.
	* Click on the "Browse" button to select an MPEG file.
	* Click on the OK button to launch Media Player and play the selected
	  MPEG file.

    Method 2:
	* Launch Media Player directly and select the appropriate MPEG file
	  using the "Open" command under the File menu.
	* Click on the PLAY button and play the selected MPEG file.

There is a sample file, named "TEST.MPG",in the installed directory.
For more information about Xing(TM) Native-MPEG(TM) Driver, please read the
"XING.TXT" file in the same directory.


All Windows Versions Support For Different Languages
====================================================
The drivers and utilities are fully compatible with all Windows versions,
regardless of the languages.


Resolution Change On The Fly
============================
Setting WinSwitch from HotKey dialog box, you can change screen resolution
immediately by pressing a user-defined key if the color depth and font size
are not changed. Some Windows versions don't use it but by restarting Windows
. The following lists Windows versions which can support this function:

	. Czech Windows
	. Danish Windows
	. Dutch Windows
	. English Windows
	. Finnish Windows
	. French Windows
	. Genman Windows
	. Hungarian Windows
	. Norwegian Windows
	. Russian Windows
	. Spanish Windows


Limitations:
============
1.  In 16.7M colors mode and 32K colors mode, the DCT Rop3 test fails.	This
    is the DCT's bug.

2.  For DBCS (Double Byte Character Set) Windows,  like Chinese Windows and
    Japanese Windows, screen resolution can't be changed on real time. It needs
    to restart Windows.
