

    LEXPS PostScript Language Printer Driver for Microsoft Windows 95
    ----------------------------------------------------------------------
    This driver generates PostScript Level 2 language which will not print
    on printers with only Postscript Level 1 emulation.


    This README file contains the following sections:

    I.    Package Content
    II.   Coexistence with Other PostScript Printer Drivers
    III.  Installation Instructions
    IV.   Envelope Printing in Windows 95
    V.    Application Limitations
    VI.   Specifying the Number of Copies
    VII.  Specifying the Scale
    VIII. Downloading Overlays	


    I.   Package Content
    ====================

       This package contains the following files:

       Filename      Description
       ------------  -----------
       READMEPS.TXT  This file
       LEXPS.DRV     LEXPS printer driver
       LEXPSLNG.DLL  Driver resources file
       LEXPS.HLP     Windows 95 LEXPS printer driver help file
       LEXPS.CNT     Windows 95 LEXPS printer driver help context file
       LEXPS.INF     Setup information for Windows 95 driver
       LEXPS.AVI     Animation file
       PS4079.ICM    Color table file for Lexmark 4079 PS2 printer
       PTAPIW16.DLL  DLL file for download
       LEXMV95.DLL   DLL file for interface to download
       LEXMV95.HLP   Help file for interface to download
       LEXMV95R.DLL  Resource DLL for LEXMV95.DLL
       LEXBCE.DLL    Bidirectional communication file
       LEXBCELM.DLL  Bidirectional communication file for language monitor
       LEXLMPM.DLL   Windows 95 language monitor
       LEXSTART.EXE  Bidirectional communication startup file
       LEXPSEXT.DLL  Driver's shell extension file


    II.  Coexistence with Other PostScript Printer Drivers
    ======================================================

       This driver is intended to coexist peacefully with other Windows printer
       drivers, including PSCRIPT.DRV, Microsoft's PostScript printer driver.
       Installing this driver will not delete any installed drivers and should
       not affect their operation in any way.




----------------------------
    PostScript is a trademark of Adobe Systems Incorporated registered in the
    United States.
    III. Installation Instructions
    ==============================

    IMPORTANT:  SKIP THIS SECTION if you intend to use the INSTALLATION
    UTILITIES provided with your printer to install your printer driver.
    The instructions in this section are provided for your information
    only in case you want to install the printer driver manually.

       Take the following steps to install the LEXPS printer driver.

        1.  Start Windows 95.

        2.  Insert the diskette with the driver in the a: drive.

        3.  Select the Start button on the task bar.   Then select Settings
            and Printers.

        4.  Double-click the Add Printer icon.  The Add Printers Wizard
            dialog box is displayed.

        5.  Select the Next> button.

        6.  Select Local or Network printer and then select the Next> button.

        7.  Make sure the driver diskette is in the a: drive and select the
            Have Disk... button.

        8.  Select the OK button.

        9.  Select the appropriate printer from the list and select the Next>
            button.

        10. If the driver was previously installed, the option to keep the
            existing driver or Replace the existing driver will appear.
            Select Replace existing driver and then select the Next> button.

        11. Select the appropriate printer port (normally LPT1:) and select
            the Next> button.

        12. Type a name for the printer object or use the supplied name.  If
            the driver was previously installed using the supplied name, then
            the new supplied name will have '(Copy #)' appended to it.  This
            is to ensure that two printer objects do not have the same name.
            Select whether this printer object should be the default printer
            or not and select the Next> button.

        13. If you would like a test page to be printed through the driver
            you are installing to test if the driver was installed correctly,
            select Yes or No and then select the Finish button.

            The following files will be copied to your Windows/System
            subdirectory:
                 LEXPS.DRV      LEXPSLNG.DLL  LEXPS.HLP     LEXPS.CNT
                 LEXPS.AVI      PTAPIW16.DLL  LEXMV95.DLL   LEXMV95.HLP
                 LEXBCE.DLL     LEXBCELM.DLL  LEXLMPM.DLL   LEXSTART.EXE
                 LEXPSEXT.DLL   LEXMV95R.DLL
            PS4079.ICM will be copied to your Windows/System/Color
            subdirectory when installing the Lexmark Color 4079 plus PS2.

        14. If you had previously installed the printer driver you may now
            wish to delete the new printer object.  The newly installed
            driver files replace the existing driver files and therefore the
            old printer object was also updated.  By keeping the old printer
            object, any settings, overlays, and user forms will be saved.
            To delete the new printer object, click on the object with the
            right mouse button and select Delete.

        15. To open the printer object, Double-click the object then select
            Printer and Properties.


       Installation of the LEXPS printer driver is now complete.




    IV.  Envelope Printing in Windows 95
    ====================================

       When you design or print an envelope, you must select landscape
       orientation.  This will ensure that the address prints in the
       correct position on the envelope.  To change the orientation to
       Landscape, make the appropriate selection from the driver's Paper
       tab or Printer Setup dialog box in your application.


    V.   Application Limitiations
    =============================

       Some applications, such as Corel Draw, Aldus Pagemaker, and Lotus
       123, generate PostScript language directly instead of using the
       Windows GDI interfaces to the printer driver. As a result, some of
       the features of this driver do not work with these types of
       applications unless the UseDrvPS switch is set in LEXPS.INI in the
       Windows subdirectory. Features that may not work include Overlays,
       Multipage Printing, Negative Page, Negative Image, and selectable
       Fill Resolution.


    VI.  Specifying the Number of Copies
    ====================================

       The Copies control on the Paper tab is independent of a Copies
       option that may be available in the Print dialog box of your
       Windows application. Usually, specifying the number of copies in
       the printer driver Paper tab prints uncollated copies faster.
       Specifying the number of copies from your Windows application may
       slow down printing but may enable you to print collated copies if
       your applications supports this feature. Specifying a multiple
       number of copies in both the printer driver Paper tab and the
       application Print dialog box should be avoided since it may
       produce unpredictable results.


    VII. Specifying the Scale
    =========================

       Some Windows applications directly provide a scaling option. With
       such an application, you should try leaving the printer driver
       scaling at 100 percent and set the desired scaling in the
       application. If this does not produce satisfactory results, then set
       the desired scaling in the printer driver and set the scaling in the
       application to 100 percent. Using variable scaling factors in both
       simultaneously may produce unexpected results.


    VIII.  Downloading Overlays
    ===========================

	An overlay is a template that can be defined and then printed as a
	background on a form before the data from the current job is
	printed.  For instructions on downloading an overlay, see the Help
	section in the Paper tab of the printer driver property sheet.  If
        your overlay contains an image, you must ensure that the data is being
	sent to the printer as Ascii 85.  This option can be selected in the
	printer driver's PostScript tab.  It must be set both when creating
        and downloading the overlay.
       
