Compuprint PageMaster 1035ex/1435ex/1445ex/1455ex
Standard Printer Driver for Microsoft Windows 95 (English language version)


Note : This is the driver for the English language version of Windows 95.
       Do not install this driver on a version of Windows 95 other than the
       English language version as this will cause printer dialog boxes to
       display in English rather than the language of the installed Windows 95
       version.


<Overview of Contents>
     This document explains the items listed below. The driver should be used
     only after this document has been read.

     Introduction
     File Composition
     Installation Guide
     Points to Note


<Introduction>
     The Compuprint PageMaster 1035ex/1435ex/1445ex/1455ex printer driver
     (Standard) has drivers for the following models.

       Compuprint PageMaster 1035ex-MV   : Standard driver for 1035ex  *1
       Compuprint PageMaster 1035ex      : Standard driver for 1035ex  *2
       Compuprint PageMaster 1435ex-MV   : Standard driver for 1435ex  *1
       Compuprint PageMaster 1435ex      : Standard driver for 1435ex  *2
       Compuprint PageMaster 1445ex-MV   : Standard driver for 1445ex  *1
       Compuprint PageMaster 1445ex      : Standard driver for 1445ex  *2
       Compuprint PageMaster 1455ex-MV   : Standard driver for 1455ex  *1
       Compuprint PageMaster 1455ex      : Standard driver for 1455ex  *2
     
     *1:MarkVision driver
     *2:Non-MarkVision driver

     When using MarkVision while printing, the MarkVision enabled driver is
     required. This is the driver that is normally installed.
     MarkVision cannot be used with the non-MarkVision driver.
     The non-MarkVision driver can be used to speed up printing throughput
     if desired. To install the non-MarkVision driver, select the Add Printer
     Wizard in the Printers Folder and follow the instructions.


<File composition>
     The following files are necessary for the standard driver.
      OEMSETUP.INF  Information file used for installing the printer driver.
      CPPMEX.DR_    Compuprint PageMaster 1035ex/1435ex/1445ex/1455ex printer
                    driver module.
      LEXBCE.DL_    Bidirectional communication file.
      LEXBCELM.DL_  Bidirectional communication file for language monitor.
      LEXLMPM.DL_   Windows 95 language monitor.
      LEXSTART.EX_  Bidirectional communication startup file.
      ICONLIB.DLL   Microsoft Universal printer driver icon library. 
      UNIDRV.DLL    Microsoft Universal printer driver library.
      UNIDRV.HLP    Microsoft Universal printer driver help file.
      CPPMEXST.TXT  Contains explanation and points to note for the printer
                    driver.


<Installation Guide>
     The standard printer driver can be installed by either of 2 methods
     described below.

     The Plug and Play function can install the MarkVision driver.
     The Set-up from Printers folder can install all models.

     (1)Plug and Play printer detection.

       (a)Windows 95 automatically detects the printer at installation time or
          during the boot process.

       (b)Plug and Play detection code will prompt the user for the appropriate
          files if they are not resident in the Windows directory, by
          displaying the "New Hardware Found" dialog box.

       (c)From the "New Hardware Found" dialog box select the option "Driver
          from disk provided by hardware manufacturer" and click the "OK"
          push-button.

       (d)The "Install from disk" dialog box is displayed prompting the user to
          select the drive and directory containing the installation disk.

       (e)Insert the printer driver installation disk into the A: drive,
          type "A:\" and click "OK".

       (f)The "Select Device" dialog box appears displaying the model name.
          Click "OK" to continue.

       (g)A dialog appears prompting the user to type the printer name. Type
          an appropriate name or use the one supplied and click "Next>".

       (h)The next dialog prompts the user to print a test page. Select "Yes"
          or "No" and click "Finish".

       (i)Driver files are copied from the installation disk.

       (j)When all files have been copied and the driver is installed a dialog
          appears querying the result of test page printout. Depending on
          whether the test page was printed correctly or not click "Yes" or
          "No".

      The Compuprint PageMaster Windows 95 printer driver (MarkVision driver)
      is now installed.


     (2)Set-up from Printers folder.

       (a)Click the Start button, point to Settings, and then click Printers.

       (b)Double-click Add Printer.

       (c)The Add Printer Wizard appears. Click "Next>".

       (d)Click "Have Disk" from the next dialog and the "Install from disk"
          dialog box is displayed prompting the user to select the drive and
          directory containing the installation disk.

       (e)Insert the printer driver installation disk into the A: drive,
          type "A:\" and click "OK".

       (f)A dialog box appears displaying the model names.
          Select the model name which you will use,
          and click "Next>" to continue.

       (g)A list of available ports appears. Select an appropriate port and
          click "Next>".

       (h)A dialog appears prompting the user to type the printer name. Type
          an appropriate name or use the one supplied and click "Next>".

       (i)The next dialog prompts the user to print a test page. Select "Yes"
          or "No" and click "Finish".

       (j)Driver files are copied from the installation disk.

       (k)When all files have been copied and the driver is installed a dialog
          appears querying the result of test page printout. Depending on
          whether the test page was printed correctly or not click "Yes" or
          "No".

      The Compuprint PageMaster Windows 95 printer driver is now installed.


<Points to Note>
       (1)110, 921600 Baud rates are not supported by Compuprint PageMaster
          1035ex/1435ex/1445ex/1455ex and should not be selected when using
          the serial port.

       (2)Vector Graphics is used as the default Graphics Mode for this driver.
          If problems occur when printing graphics, please switch to Raster
          Graphics.

       (3)When setting the printer memory option ("Device Options"-->
          "Printer memory") this driver only supports settings upto 64MB.
          If more than 64MB are installed in the printer (resident+64MB module)
          please set this setting to 64MB.

       (4)When using Duplex printing :  (Compuprint PageMaster 1455ex)
           When the front page and back page settings, such as paper source,
           paper size or print direction, are the same, the printer will print
           according to example #1.
           When any of these settings are different the printer will print
           according to example #2.

           Example #1 :
             Application     Printer
             ---------------------------------
             Page 1->A4      Page 1 front ->A4
             Page 2->A4      Page 1 back  ->A4
             Page 3->A5      Page 2 front ->A5
             Page 4->A5      Page 2 back  ->A5

           Example #2 :
             Application     Printer
             ---------------------------------
             Page 1->A4      Page 1 front ->A4
             Page 2->A5      Page 2 front ->A5
             Page 3->A5      Page 2 back  ->A5
             Page 4->A5      Page 3 front ->A5


Microsoft and Windows are registered trademarks of Microsoft Corporation.
