        #
        | README file for
        |
        | ELSA MicroLink ISDN/MC
        | Version 2.14
        |
        | Copyright (c) 1993-97 ELSA GmbH, Aachen (Germany)
        |
        |                                     Subsidiary:
        | ELSA GmbH                           ELSA Inc.
        | Sonnenweg 11                        2150 Trade Zone Blvd.
        | D-52070 Aachen                      Suite 101
        | Germany                             San Jose, CA 95131
        |                                     USA
        |
        | Phone      : +49-241-606-0          Phone: +1-408-935-0350
        | Support Fax: +49-241-606-6499       Phone:  1-800-272-ELSA
        | BBS (modem): +49-241-606-9800       Fax  : +1-408-935-0370
        | BBS (ISDN) : +49-241-606-9820       BBS  : +1-408-935-0380
        | CompuServe : GO ELSA                CIS  : GO ELSA
        | WWW        : http://www.elsa.de     WWW  : http://www.elsa.com
        |
        | 03/27/97

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

        Table of Contents

        1.      Overview
        2.      Contents
        3.      Installation
        4.      Notes

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

1.      Overview:

        This file contains notes and changes to the MicroLink
        ISDN drivers.

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

2.      Contents:

        The driver disk contains the following files:

        README.TXT   this file
        LIESMICH.TXT german version of the readme.txt file

        CSSELMC.INF Installation file for Win95.

2.1     Driver for CAPI 2.0 and DSS1 (EURO-ISDN):

        CSSELMC.VXD  CAPI version 2.0 driver for ELSA MicroLink ISDN/MC
        D channel protocol : DSS1 (EURO-ISDN)
        B channel protocols: HDLC transparent, bit transparent,
                             X.75, T.70NL, V.120
                             ISO 8208 (X.25), T.90

               - - - - - - - - - - - - - - - - - - - - - - - -

2.2     Driver for CAPI 2.0 and 1TR6 (national ISDN):

        CSS1TMC.VXD  CAPI version 2.0 driver for ELSA MicroLink ISDN/MC
        D channel protocol : 1TR6 (national ISDN)
        B channel protocols: HDLC transparent, bit transparent,
                             X.75, T.70NL, V.120
                             ISO 8208 (X.25), T.90

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

3.      Installation:

        a.) Install the PCMCIA-Controller

            For installing the PCMCIA-Controller you must choose
            the hardware-assitent.

        b.) Install the driver for the MicroLink ISDN board

            Reboot your system and put the MicroLink ISDN board
            into the pcmcia-slot.
            The driver for your ISDN-Board will be installed
            automatically.

        c.) Restart your computer.

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

4.      Notes:

        The latest information you will always find in the
        Support BBS ELSA ONLINE or on our homepage http://www.elsa.de.

               - - - - - - - - - - - - - - - - - - - - - - - -

        V.120 under CAPI 2.0 and CFOS (version newer than 07/15/96):

        Enter the following AT-command:

            AT B12 S17=1 S76=1

        Now, the ISDN adapter board tries to get a V.120 connection
        erverytime you dial "ATDn" (n = number)..

        If you want to get back to X.75 mode, you have to enter:

            AT&F

               - - - - - - - - - - - - - - - - - - - - - - - -

        Have fun with your ELSA ISDN board.
