        #
        | README file for
        |
        | ELSA ISDNMON
        | Version 2.14
        |
        | Copyright (c) 1993-97 ELSA GmbH, Aachen (Germany)
        |
        |                                     Subsidiary:
        | ELSA GmbH                           ELSA Inc.
        | Sonnenweg 11                        2150 Trade Zone Blvd.
        | D-52070 Aachen                      Suite 101
        | Germany                             San Jose, CA 95131
        |                                     USA
        |
        | Phone      : +49-241-606-0          Phone: +1-408-935-0350
        | Support Fax: +49-241-606-6499       Phone:  1-800-272-ELSA
        | BBS (modem): +49-241-606-9800       Fax  : +1-408-935-0370
        | BBS (ISDN) : +49-241-606-9820       BBS  : +1-408-935-0380
        | CompuServe : GO ELSA                CIS  : GO ELSA
        | WWW        : http://www.elsa.de     WWW  : http://www.elsa.com
        |
        | 03/26/97

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

        Table of Contents

        1.      Overview
        2.      Contents
        3.      Installation
        4.      Usage
        5.      Notes

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

1.      Overview:
        This file contains notes and changes to the ELSA ISDNmonitor
        for Windows 95 and NT.

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

2.      Files:

        README.TXT             This file
        LIESMICH.TXT           German version of this file

        ISDNMON.EXE            ELSA ISDNmonitor for Windows 95 and NT

               - - - - - - - - - - - - - - - - - - - - - - - -

3.      Installation:

        Copy the file ISDNMON.EXE to the desired destination path
        and start it from there.

               - - - - - - - - - - - - - - - - - - - - - - - -

4.      Usage:

        The ELSA ISDNmonitor runs with Windows 95 and NT.
        The main window shows the following information:

        - B-Channels (B1 and B2)

            Con (Yellow LED):
              Off     = B-Channel not active
              Partial = B-Channel requested
              On      = B-Channel active (charged!)

            Tx (Red LED):
              Off     = No Data sent
              On      = Data sent

            Rx (Red LED):
              Off     = No Data received
              On      = Data received

        - S0 Interface

            S0 Power (Green LED):
              Off     = No S0 Power
              On      = S0 Power

            S0 Activation (Green LED):
              Off     = S0 Bus active
              On      = S0 Bus inactive

            TEI (Green LED):
              Off     = No TEI
              On      = Got TEI

            L2 (Green LED):
              Off     = D-Channel not active
              On      = D-Channel active

        In the menu topic "Info" you will find entries called
        "About" and "General Info". In the menu topic "Options" you
        will find the entrie "On Top". With "On Top" you can
        tell ISDNmonitor always to stay on top of all other windows.
        "General Info" gives you further information about your CAPI,
        your driver, your hardware and your ISDNmonitor. If you are
        using an US CAPI-Driver you will find another entry called
        "US Info".

        The value of "On Top" and the window position of the ISDNmonitor
        is saved when the ISDNmonitor is terminated and restored on the
        next aktivation.

               - - - - - - - - - - - - - - - - - - - - - - - -

5.      Notes:

        The ELSA ISDNmonitor for Windows 95 and NT runs only with the
        ELSA CAPI 2.0 Driver Ver. 2.14 or higher.

        With Windows 95 the ACOTEC CAPI Subsystem has to be installed.


